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Thank you.

It may be due to different speeds of the SD drive. I haven't done anything with that code so I'll have to figure out how it works.  I don't have the problem, I will try a few drives here to see if I can reproduce it.

Could you take pictures of the SD cards? The side with the labels, please.

I'll look at the serial ports as well. I don't ever hot swap them so this is new. Hotswapping should not matter at all though.

Thanks,
Elecia


Hi Denis,

I can repeat your SD card issues. I only get them on J7.  I should be able to figure them out tomorrow.

As for J7 vs J8... it is very important that you quit the console before you try to swap serial ports. There cannot be two consoles open. 

Also, the code you have, it is important not to send anything at 9600 baud to J8. (I have a code fix for that.)

Thanks,
Elecia



