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Set up
1. Install bags of clean water and purge inject lines.
2. Fill chambers with 2” of clean water, vac out chambers first if necessary 
3. Plug the Shore cable into the com connector, laptop and power supply (Set to15- 16 VDC)
4. Turn on the run switch on the Shore Cable
5. Type cartridge return  
6. Type “reset pico” 
7. Copy oasis.cfg file to system (use y modem send/receive)
8. Load script files xxx.scp (must this be resp.scp, stir.scp, modlog.scp )
9. Delete old data files (oxy.txt, env.txt etc)
10. Check DOS time and date
11. Power cycle the system with the switch (switch on connector cable)
12. Watch the system run at least 1 cycle 
13. Test stir, flush and inject pumps.
14. Type the oxy.txt files to verify optodes are working
15. Reset pico and delete files again
16. Check vent port.
17. Power the system off and disconnect the power supply
18. Install dummy on console port
19. Charge battery, oil bottle installed

Pre deploy
1. Remove battery charger and plug in power to system
2. Purge gas from batteries, top off oil
3. All inject valves open. Green valves under the chambers
4. Plugs on the bottom of chambers installed
5. Load O2/co2 bag(s)
6. Top off pump compensation 
7. Check that run plug is tethered to console port connector
Deploy
1. Log Homer number?
2. Log Sondardyne beacon number?
3. Turn Strobe and VHF Beacon on
4. Anchors installed
5. Remove release safety pins
6. Inject fluid bag connected and valves on (if installed)
7. Optode covers off 9 of them
8. Batteries plugged in (grease connector)
9. Remove battery oil bottles. Clean up oil drips off the couplers
10. Fill chambers with seawater
11. Install run plug (grease connector)
12. Verify the lights on the chamber controllers are on and blinking


Recovery
1. Remove run plug and install dummy (grease connector)
2. Strobe and VHF Beacon off
3. Inject fluid bag lure valves off
4. Optode covers on 9 of them
5. Install battery oil bottles
6. [bookmark: _GoBack]Charge batteries, dummy off system power connections
7. Wash out chambers and flush lines
8. Wash down elevator

