BRS/OASIS software cheat sheet
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Notes:
· Console port settings: 38400, 8 data bits, No parity, 1stop bit
· To get to Picodos from BRS prompt, Type “reset pico”
· To restart OASIS/ BRS application, type “app” or power cycle for 15 seconds.

Picodos commands used in BRS set up (just the common ones)
1. App	launches BRS application from Picodos.
2. Copy
3. Date
4. Dir
5. Erase
6. Rename
7. Reset	Resets the processor, after reboot system will start BRS app after reboot.
8. Time
9. Type	Displays contents of a text file to screen. At 38400 a big file can take a long time.
10. YS	Y-modem Send, used to transfer files from Picodos to PC.  
11. YR	Y-modem Receive, used to transfer files from PC to Picodos.  

BRS commands, common ones. Some dos commands pass through.
1. Scripts 	Shows the scripts that are currently running.
2. Scripts stop	Stops the current scripts.
3. Rempulse	Used to activate an output point for testing like pumps.
4. Analog		Displays current a/d input values, batt volts, can temp, can pressure
5. DP		Driver Parameter, shows what drivers are doing.
6. Type		Displays contents of a text file to screen. At 38400 a big file can take a long time.
7. Time
8. Date
9. Dir
10. Resetpico	kills BRS app and goes back to picodos.


Stir, Flush and Inject Testing
Use rempulse (remote pulse) command from the BRS prompt.
Rempulse can be used on:
· O2_inject(number)
· Stir(number)
· Flush(number)
· Any other DO defined in the OASIS config
Examples
· Rempulse “o2_inject1 30” = O2 inject pump 1 on for 30 seconds.
· Rempulse “stir2 10” = stir 2 on for 10 seconds.



Transfer files with Y-modem examples
Move oxy.txt to PC. (from BRS prompt)
· Reset Pico to get to picodos.
· Type “YS oxy.txt”
· At Hyperterminal, receive file, y-modem
Move resp.scp from PC to BRS. (from BRS prompt)
· Reset Pico to get to picodos.
· Rename existing resp.scp (optional). Type “rename resp.scp resp1.scp”
· [bookmark: _GoBack]Type “erase resp.scp” if you did not rename existing resp file.
· Type “YR” to start Y-modem receive
· At Hyperterminal, send file, y-modem, select the new resp.scp. 





