diag:208>AT$T9

BURN WIRE ARMED
Battery: OK
diag:209>AT$N9,123

Valid release code-waiting for burn...
diag:210>
Burn Wire Released, unit tilted
diag:210>AT$ES9

remote reset sent

diag:211>AT$T9

BURN WIRE ARMED
Battery: OK
diag:212>AT$N9,123

Valid release code-waiting for burn...
diag:213>
Burn Wire Released, unit tilted
diag:213>AT$N9,123
diag:213>AT$ES9
diag:213>AT$ES9

remote reset sent

diag:214>AT$T9

BURN WIRE ARMED
Battery: OK
diag:215>AT$N9,123

Valid release code-waiting for burn...
diag:216>
Burn Wire Released, unit tilted
diag:216>AT$ES9

remote reset sent

diag:217>ATD9
Command 'atd9' not found
Error
diag:218>ATD9
+++
diag:219>0800 bits/sec
diag:219>
diag:219>AT$T9

BURN WIRE ARMED
Battery: OK
diag:220>AT$N9,123

Valid release code-waiting for burn...
diag:221>
Burn Wire Released, unit tilted
diag:221>AT$ES9

remote reset sent

diag:222>ATD9

CONNECT 00800 bits/sec

node2:~$
node2:~$
node2:~$
node2:~$
node2:~$ +++
diag:223>AT$T9

BURN WIRE ARMED
Battery: OK
diag:224>AT$N9,123

Valid release code-waiting for burn...
diag:225>
Burn Wire Released, unit tilted
diag:225>AT$ES9

remote reset sent

diag:226>ATD9

CONNECT 00800 bits/sec

user:51>

user:51>

Command 'user:45>' not found

Error

user:52>

user:52>

Command 'user:45>' not found

Error

user:53>

user:53>

Command 'user:45>' not found

Error

user:54>

user:54>

Command 'command' not found

Error

user:55>

user:55>

Command 'error' not found

Error

user:56>

user:56>

Command 'user:46>' not found

Error

user:57>

user:57>

Command 'user:46>' not found

Error

user:58>

user:58>

Command 'command' not found

Error

user:59>

user:59>

Command 'error' not found

Error

user:60>

user:60>

Command 'user:47>' not found

Error

user:61>

user:61>

Command 'user:47>' not found

Error

user:62>

user:62>

Command 'command' not found

Error

user:63>

user:63>

Command 'error' Setting up RAMFS, please wait...
not found

Error

user:64>

user:64>

Command 'user:48>' not found

Error

user:65>

user:65>

Command 'user:48>' not found

Error

user:66>

user:66>

Command 'comma:
RX DAERRrRERRUN

INIT: ver.r▒▒͕ɂ▒:^Br▒љ▒չ▒▒ɽ▒a^EQ^E▒Command s (rw,mode=0622)


Setting the System Clock using the Hardware Clock as reference...
Calculating module dependencies... depmod: /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.ieee1394map is not an ELF file
depmod: error reading ELF header /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.pnpbiosmap: No such file or directory
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/loopback.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net_init.o
done.
Loading modules: slhc CSLIP: code copyright 1989 Regents of the University of California
ppp_generic PPP generic driver version 2.4.1
ppp_async ppp_deflate PPP Deflate Compression module registered
bsd_comp PPP BSD Compression module registered
cs8900 Cirrus Logic CS8900A driver for Linux (24-Jan-2004)
eth0: Registered cs8900_eeprom char device (major #253)
eth0: CS8900A rev D at 0xf0000300 irq=47, eeprom ok, addr: 00: C:6A: 0:04: 2
eth0: power management support enabled
sidearm-wdog sidearm-wdog: version 1.3 [Jun 22 2005 09:57:53]

INIT: Entering runlevel: 2
Configuring network interfaces: eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
/dev/hda1: clean, 1394/1957888 files, 109068/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 03:03:43.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 03:03:50 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 03:03:50 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
+++e2 login: AT$s9
diag:227>AT$S9
Remote Sregisters
S00=042  S01=000  S02=000  S03=004  S04=005  S05=000  S06=007
S07=015  S08=100  S09=000  S10=036  S11=000  S12=000  S13=000
S14=000  S15=000  S16=001  S17=001  S18=009  S19=000  S20=000
diag:228>+++
Command '+++' not found
Error
diag:229>AT$T9

BURN WIRE ARMED
Battery: OK
diag:230>AT$N9,123

Valid release code-waiting for burn...
diag:231>
Burn Wire Released, unit tilted
diag:231>AT$ES9

remote reset sent

diag:232>ATD9

CONNECT 00800 bits/sec
+++
diag:233>ATD9

CONNECT 00800 bits/sec
+++
diag:234>AT$ES9

remote reset sent

diag:235>ATD9
Response Not Received
diag:236>ATD9

CONNECT 00800 bits/sec
+++K
diag:237>AT$K9
Invalid Command

diag:238>AT$K9
Invalid Command

diag:239>ATD9

CONNECT 00800 bits/sec
+++
diag:240>AT$ES9

remote reset sent

+++g:241>ATD9
diag:242>AT$T9
CONNECT 00800 bits/sec
BURN WIRE ARMED
Battery: OK
diag:243>AT$N9,123

Valid release code-waiting for burn...
diag:244>
Burn Wire Released, unit tilted
diag:244>AT$ES9

remote reset sent

diag:245>AT$S9
Remote Sregisters
S00=042  S01=000  S02=000  S03=004  S04=005  S05=000  S06=007
S07=015  S08=100  S09=000  S10=036  S11=000  S12=000  S13=000
S14=000  S15=000  S16=001  S17=001  S18=009  S19=000  S20=000
diag:246>ATD9

CONNECT 00800 bits/sec
___+++
diag:247>AT$K9
Invalid Command

diag:248>ATD9

CONNECT 00800 bits/sec
+++
diag:249>AT$ES9

remote reset sent

diag:250>AT$T9

BURN WIRE ARMED
Battery: OK
diag:251>AT$N9,123

Valid release code-waiting for burn...
diag:252>
Burn Wire Released, unit tilted
diag:252>AT$ES9

remote reset sent

diag:253>ATD9

CONNECT 00800 bits/sec                                                                                                    0
Relocating zImage from 00060000 to C0008000 (len=00100000)
Proper ARM zImage ID found. Booting...
Uncompressing Linux............................................................ done, booting the kernel.
Linux version 2.4.9-ac10-rmk2-np1-cerf2 (ops@greenflash) (gcc version 2.95.3 20010315 (release)) #64 Thu Nov 20 10:54:37 PST 2008
Processor: Intel StrongARM-1110 revision 9
Architecture: MBARI SideARM v4.1 - 11/16/2006
On node 0 totalpages: 16384
zone(0): 16384 pages.
zone(1): 0 pages.
zone(2): 0 pages.
Kernel command line: console=ttySA0 cpufreq=191700 root=1f04 rw init=/linuxrc
Calibrating delay loop... 127.38 BogoMIPS
Memory: 64MB = 64MB total
Memory: 62420KB available (1628K code, 291K data, 64K init)
Dentry-cache hash table entries: 8192 (order: 4, 65536 bytes)
Inode-cache hash table entries: 4096 (order: 3, 32768 bytes)
Mount-cache hash table entries: 1024 (order: 1, 8192 bytes)
Buffer-cache hash table entries: 4096 (order: 2, 16384 bytes)
Page-cache hash table entries: 16384 (order: 4, 65536 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Soci.22
  options:  [pm]
SA-1100 PCMCIA (CS release 3.1.22)
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP, IGMP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 4096 bind 4096)
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
NetWinder Floating Point Emulator V0.95 (c) 1998-1999 Rebel.com
FAT: bogus logical sector size 408
UMSDOS: msdos_read_super failed, mount aborted.
FAT: bogus logical sector size 408
FAT: bogus logical sector size 408
Child dir "." (ino #1) of dir ino #1 appears to be a hard link
VFS: Mounted root (jffs2 filesystem).
Freeing init memory: 64K
Setting up RAMFS, please wait...
Executing /sbin/init...
INIT: version 2.78 booting
Mounting local filesystems...
devpts on /dev/pts type devpts (rw,mode=0622)
Setting the System Clock using the Hardware Clock as reference...
Calculating module dependencies... depmod: /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.ieee1394map is not an ELF file
depmod: error reading ELF header /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.pnpbiosmap: No such file or directory
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/loopback.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net_init.o
done.
Loading modules: slhc CSLIP: code copyright 1989 Regents of the University of California
ppp_generic PPP generic driver version 2.4.1
ppp_async ppp_deflate PPP Deflate Compression module registered
bsd_comp PPP BSD Compression module registered
cs8900 Cirrus Logic CS8900A driver for Linux (24-Jan-2004)
eth0: Registered cs8900_eeprom char device (major #253)
eth0: CS8900A rev D at 0xf0000300 irq=47, eeprom ok, addr: 00: C:6A: 0:04: 2
eth0: power management support enabled
sidearm-wdog sidearm-wdog: version 1.3 [Jun 22 2005 09:57:53]

INIT: Entering runlevel: 2
Configuring network interfaces:
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
/dev/hda1: clean, 1399/1957888 files, 109146/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 04:10:05.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 04:10:12 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 04:10:12 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
opse2 login: ops
Password: brynner
node2:~$  loc /dev/ttyS
node2:~$
listPorts loc -statsoc -stats
SIAM version $Name:  $
java.lang.ClassFormatError: (org/mbari/siam/devices/workhorse/StreamingWorkhorseADCP_Stub) unexpected EOF at offset=16437

Stack trace:
   java/lang/Throwable.<init>()V
   java/lang/Throwable.<init>(Ljava/lang/String;)V
   java/lang/ClassFormatError.<init>(Ljava/lang/String;)V
   java/lang/ClassLoader.defineClassImpl(Ljava/lang/String;[BII)Ljava/lang/Class;
   java/lang/ClassLoader.defineClass(Ljava/lang/String;[BIILjava/security/ProtectionDomain;)Ljava/lang/Class;
   java/security/SecureClassLoader.defineClass(Ljava/lang/String;[BIILjava/security/CodeSource;)Ljava/lang/Class;
   java/net/URLClassLoader.findClassImpl([Ljava/net/URL;Ljava/lang/String;)Ljava/lang/Class;
   java/net/URLClassLoader$4.run()Ljava/lang/Object;
   java/security/AccessController.doPrivileged(Ljava/security/PrivilegedAction;Ljava/security/AccessControlContext;)Ljava/lang/Object;
   java/net/URLClassLoader.findClass(Ljava/lang/String;)Ljava/lang/Class;
   com/ibm/oti/vm/URLAppClassLoader.findClass(Ljava/lang/String;)Ljava/lang/Class;
   java/lang/ClassLoader.loadClass(Ljava/lang/String;Z)Ljava/lang/Class;
   com/ibm/oti/vm/URLAppClassLoader.loadClass(Ljava/lang/String;Z)Ljava/lang/Class;
   java/lang/ClassLoader.loadClass(Ljava/lang/String;)Ljava/lang/Class;
   java/lang/Class.forNameImpl(Ljava/lang/String;ZLjava/lang/ClassLoader;)Ljava/lang/Class;
   java/lang/Class.forName(Ljava/lang/String;ZLjava/lang/ClassLoader;)Ljava/lang/Class;
   java/rmi/server/RMIClassLoader.loadClass(Ljava/net/URL;Ljava/lang/String;)Ljava/lang/Class;
   java/rmi/server/RMIClassLoader.loadClass(Ljava/lang/String;Ljava/lang/String;)Ljava/lang/Class;
   com/ibm/oti/rmi/RMIObjectInputStream.resolveClass(Ljava/io/ObjectStreamClass;)Ljava/lang/Class;
   java/io/ObjectInputStream.readNewClassDesc()Ljava/io/ObjectStreamClass;
   java/io/ObjectInputStream.readClassDesc()Ljava/io/ObjectStreamClass;
   java/io/ObjectInputStream.readNewObject()Ljava/lang/Object;
   java/io/ObjectInputStream.readNonPrimitiveContent()Ljava/lang/Object;
   java/io/ObjectInputStream.readObject()Ljava/lang/Object;
   com/ibm/oti/rmi/wire/Protocol.readObject(Ljava/lang/Class;Ljava/io/ObjectInput;)Ljava/lang/Object;
   com/ibm/oti/rmi/UnicastRef.invoke(Ljava/rmi/Remote;Ljava/lang/reflect/Method;[Ljava/lang/Object;J)Ljava/lang/Object;
   org/mbari/siam/moos/deployed/MOOSNodeService_Stub.getDevice(J)Lorg/mbari/siam/distributed/Device;
   org/mbari/siam/operations/utils/PortLister.processNode(Lorg/mbari/siam/distributed/Node;)V
   org/mbari/siam/operations/utils/NodeUtility.run()I
   org/mbari/siam/operations/utils/PortLister.main([Ljava/lang/String;)V

listPorts loc -statsoc -stats
SIAM version $Name:  $

Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  16   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK   1   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  20   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK   1   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  12   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING   4   0   0
 /dev/ttySX7      -                    -        -   -
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15      -                    -        -   -
 /dev/ttySA2      -                    -        -   -

tope2:~$ top
bash: top: command not found
lpde2:~$ lp
SIAM version $Name:  $
+++
diag:254>AT$ES9
Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  24   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  13   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  36   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  13   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  28   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  20   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  11   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -

SIAM version $Name:  $


remote reset sent

diag:255>
Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  25   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  15   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  38   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  15   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  30   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  22   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  13   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -


diag:255>
diag:255>AT$ES9

remote reset sent

diag:256>AT$T9
Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  28   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  19   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  42   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  19   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  35   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  26   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  17   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -

diag:256>ATD9SIAM version $Name:  $
diag:256>AT$T9
Response Not Received
diag:257>
diag:257>
Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  29   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  21   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  45   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  21   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  37   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  29   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  19   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -

              D
Battery: OKRME

diag:257>AT$T9
SIAM version $Name:  $
diag:258>
BURN WIRE ARMED
Battery: OK
diag:258>AT$N9,123

Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  30   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  23   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  47   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  23   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  39   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  31   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  21   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1 Response Not Received
diag:259>  0   0
 /dev/ttySA2      -                    -        -   -

diag:259>AT$N9,123
Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  31   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK  25   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  49   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK  25   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  41   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  33   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING  23   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -

diag:260>AT$N9,123
Burn Wire Released, unit tilted


Valid release code-waiting for burn...
diag:261>
Burn Wire Released, unit tilted
diag:261>AT$ES9

remote reset sent

diag:2620
Relocating zImage from 00060000 to C0008000 (len=00100000)
Proper ARM zImage ID found. Booting...
Uncompressing Linux............................................................ done, booting the kernel.
Linux version 2.4.9-ac10-rmk2-np1-cerf2 (ops@greenflash) (gcc version 2.95.3 20010315 (release)) #64 Thu Nov 20 10:54:37 PST 2008
Processor: Intel StrongARM-1110 revision 9
Architecture: MBARI SideARM v4.1 - 11/16/2006
On node 0 totalpages: 16384
zone(0): 16384 pages.
zone(1): 0 pages.
zone(2): 0 pages.
Kernel command line: console=ttySA0 cpufreq=191700 root=1f04 rw init=/linuxrc
Calibrating delay loop... 127.38 BogoMIPS
Memory: 64MB = 64MB total
Memory: 62420KB available (1628K code, 291K data, 64K init)
Dentry-cache hash table entries: 8192 (order: 4, 65536 bytes)
Inode-cache hash table entries: 4096 (order: 3, 32768 bytes)
Mount-cache hash table entries: 1024 (order: 1, 8192 bytes)
Buffer-cache hash table entries: 4096 (order: 2, 16384 bytes)
Page-cache hash table entries: 16384 (order: 4, 65536 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd v1.8
Journalled Block Device driver loaded
JFFS2 version 2.1. (C) 2001 Red Hat, Inc., designed by Axis Communications AB.
ttySA5 at MEM 0x80050000 (irq = 17) is a SA1100
ttySA6 at MEM 0x80030000 (irq = 16) is a SA1100
ttySA7 at MEM 0x80010000 (irq = 15) is a SA1100
pty: 256 Unix98 ptys configured
SA1100 Real Time Clock driver v1.00
block: queued sectors max/low 41397kB/13799kB, 128 slots per queue
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
Uniform Multi-Platform E-IDE driver Revision: 6.31
ide: Assuming 50MHz system bus speed for PIO modes; override with idebus=xx
loop: loaded (max 8 devices)
SA1100 flash: probing 16-bit flash bus
Using RedBoot partition definition
Creating 5 MTD partitions on "SA1100 flash":
0x00000000-0x00020000 : "I-Boot"
0x00000000-0x00020000 : "RedBoot"
0x00020000-0x00060000 : "Partition 2"
0x00060000-0x00160000 : "Partition 3"
0x00160000-0x00fe0000 : "Partition 4"
Linux Kernel Card Services 3.1.22
  options:  [pm]
SA-1100 PCMCIA (CS release 3.1.22)
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP, IGMP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 4096 bind 4096)
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
NetWinder Floating Point Emulator V0.95 (c) 1998-1999 Rebel.com
FAT: bogus logical sector size 408
UMSDOS: msdos_read_super failed, mount aborted.
FAT: bogus logical sector size 408
FAT: bogus logical sector size 408
Child dir "." (ino #1) of dir ino #1 appears to be a hard link
VFS: Mounted root (jffs2 filesystem).
Freeing init memory: 64K
Setting up RAMFS, please wait...
Executing /sbin/init...
INIT: version 2.78 booting
Mounting local filesystems...
devpts on /dev/pts type devpts (rw,mode=0622)
Setting the System Clock using the Hardware Clock as reference...
Calculating module dependencies... depmod: /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.ieee1394map is not an ELF file
depmod: error reading ELF header /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.pnpbiosmap: No such file or directory
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/loopback.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net_init.o
done.
Loading modules: slhc CSLIP: code copyright 1989 Regents of the University of California
ppp_generic PPP generic driver version 2.4.1
ppp_async ppp_deflate PPP Deflate Compression module registered
bsd_comp PPP BSD Compression module registered
cs8900 Cirrus Logic CS8900A driver for Linux (24-Jan-2004)
eth0: Registered cs8900_eeprom char device (major #253)
eth0: CS8900A rev D at 0xf0000300 irq=47, eeprom ok, addr: 00: C:6A: 0:04: 2
eth0: power management support enabled
sidearm-wdog sidearm-wdog: version 1.3 [Jun 22 2005 09:57:53]

INIT: Entering runlevel: 2
Configuring network interfaces: eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
/dev/hda1: clean, 1400/1957888 files, 109244/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 04:25:02.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 04:25:09 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 04:25:09 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login: ops
Command 'ops' not found
Error
diag:263>ATO

CONNECT 00800 bits/sec

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
opse2 login: ops
Password: brynner
listPorts loc -statsoc -stats
SIAM version $Name:  $

Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING   5   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK   1   0   0
 /dev/ttySX3   1474             Aquadopp     INIT   0   0   0
 /dev/ttySX4      -                    -        -   -
 /dev/ttySX5      -                    -        -   -
 /dev/ttySX6      -                    -        -   -
 /dev/ttySX7      -                    -        -   -
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15      -                    -        -   -
 /dev/ttySA2      -                    -        -   -

node2:~$ +++
diag:264>ATD9

CONNECT 00800 bits/sec
+++
diag:265>AT$ES9

remote reset sent

diag:266>ATD9

CONNECT 00800 bits/sec
+++
diag:267>AT$T9

BURN WIRE ARMED
Battery: OK
diag:268>AT$N9,123

Valid release code-waiting for burn...
diag:269>
Burn Wire Released, unit tilted
diag:269>AT$ES9

remote reset sent

diag:270>eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
/dev/hda1: clean, 1401/1957888 files, 109301/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 04:34:48.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 04:34:55 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 04:34:55 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
node2 login:
diag:270>ato

CONNECT 00800 bits/sec
ops
Password: brynner
listPorts loc -statsoc -stats
SIAM version $Name:  $

Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING   9   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK   1   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING   5   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK   1   0   0
 /dev/ttySX5      -                    -        -   -
 /dev/ttySX6      -                    -        -   -
 /dev/ttySX7      -                    -        -   -
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15      -                    -        -   -
 /dev/ttySA2      -                    -        -   -

exitNode loctNode loc
SIAM version $Name:  $

bg

[1]+  Stopped                 exitNode loc
node2:~$ bg
[1]+ exitNode loc &
!list:~$ !list
listPorts loc -stats
SIAM version $Name:  $

Node 1598 has 14 ports

   Port Name ISI-ID             Service   Status  S   E   R
   --------- ------             -------   ------ --- --- ---
 /dev/ttySX0      -                   -        -   -
 /dev/ttySX1      -                   -        -   -
 /dev/ttySX2      -                   -        -   -
 /dev/ttySX3   1474            Aquadopp SHUTDOWN  11   0   0
 /dev/ttySX4   1524 Optode  slv to 1535       OK   2   0   0
 /dev/ttySX5   1825         300kHz ADCP SAMPLING  18   0   0
 /dev/ttySX6   1828         600kHz ADCP SAMPLING  10   0   0
 /dev/ttySX7   1827        1200kHz ADCP SAMPLING   2   0   0
 /dev/ttySX8      -                   -        -   -
 /dev/ttySX9      -                   -        -   -
/dev/ttySX10      -                   -        -   -
/dev/ttySX11      -                   -        -   -
/dev/ttySX15   1599              MSP430       OK   1   0   0
 /dev/ttySA2      -                   -        -   -

killj9~$ killj9
node2:~$ Caught exception: java.rmi.UnexpectedException: undeclared checked exception
java.rmi.UnexpectedException: undeclared checked exception

Stack trace:
   java/lang/Throwable.<init>()V
   java/lang/Throwable.<init>(Ljava/lang/String;)V
   java/rmi/RemoteException.<init>(Ljava/lang/String;Ljava/lang/Throwable;)V
   java/rmi/UnexpectedException.<init>(Ljava/lang/String;Ljava/lang/Exception;)V
   org/mbari/siam/moos/deployed/MOOSNodeService_Stub.exitApplication()V
   org/mbari/siam/operations/utils/ExitApplication.processNode(Lorg/mbari/siam/distributed/Node;)V
   org/mbari/siam/operations/utils/NodeUtility.run()I
   org/mbari/siam/operations/utils/ExitApplication.main([Ljava/lang/String;)V

Nested exception:
java.io.EOFException

Stack trace:
   java/lang/Throwable.<init>()V
   java/io/DataInputStream.readByte()B
   com/ibm/oti/rmi/wire/StreamProtocolClient.waitReturnHeader()V
   com/ibm/oti/rmi/UnicastRef.invoke(Ljava/rmi/Remote;Ljava/lang/reflect/Method;[Ljava/lang/Object;J)Ljava/lang/Object;
   org/mbari/siam/moos/deployed/MOOSNodeService_Stub.exitApplication()V
   org/mbari/siam/operations/utils/ExitApplication.processNode(Lorg/mbari/siam/distributed/Node;)V
   org/mbari/siam/operations/utils/NodeUtility.run()I
   org/mbari/siam/operations/utils/ExitApplication.main([Ljava/lang/String;)V

rm logs/*
[1]+  Done                    exitNode loc
node2:~$
node2:~$
node2:~$ gosiam
rm logs/*t/hda/siam$ rm logs/*
rm: remove write-protected file `logs/clocks.log'? +
MBARI SideARM v4.1
IBoot version 1.7
  built on Nov 24 2008 at 13:01:12

Copyright 2001,2002 Intrinsyc Software Inc.
Copyright 2004 MBARI

CS8900A found at 0x08000300                                                                                               0
Relocating zImage from 00060000 to C0008000 (len=00100000)
Proper ARM zImage ID found. Booting...
Uncompressing Linux............................................................ done, booting the kernel.
Linux version 2.4.9-ac10-rmk2-np1-cerf2 (ops@greenflash) (gcc version 2.95.3 20010315 (release)) #64 Thu Nov 20 10:54:37 PST 2008
Processor: Intel StrongARM-1110 revision 9
Architecture: MBARI SideARM v4.1 - 11/16/2006
On node 0 totalpages: 16384
zone(0): 16384 pages.
zone(1): 0 pages.
zone(2): 0 pages.
Kernel command line: console=ttySA0 cpufreq=191700 root=1f04 rw init=/linuxrc
Calibrating delay loop... 127.38 BogoMIPS
Memory: 64MB = 64MB total
Memory: 62420KB available (1628K code, 291K data, 64K init)
Dentry-cache hash table entries: 8192 (order: 4, 65536 bytes)
Inode-cache hash table entries: 4096 (order: 3, 32768 bytes)
Mount-cache hash table entries: 1024 (order: 1, 8192 bytes)
Buffer-cache hash table entries: 4096 (order: 2, 16384 bytes)
Page-cache hash table entries: 16384 (order: 4, 65536 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd v1.8
Journalled Block Device driver loaded
JFFS2 version 2.1. (C) 2001 Red Hat, Inc., designed by Axis Communications AB.
ttySA5 at MEM 0x80050000 (irq = 17) is a SA1100
ttySA6 at MEM 0x80030000 (irq = 16) is a SA1100
ttySA7 at MEM 0x80010000 (irq = 15) is a SA1100
pty: 256 Unix98 ptys configured
SA1100 Real Time Clock driver v1.00
block: queued sectors max/low 41397kB/13799kB, 128 slots per queue
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
Uniform Multi-Platform E-IDE driver Revision: 6.31
ide: Assuming 50MHz system bus speed for PIO modes; override with idebus=xx
loop: loaded (max 8 devices)
SA1100 flash: probing 16-bit flash bus
Using RedBoot partition definition
Creating 5 MTD partitions on "SA1100 flash":
0x00000000-0x00020000 : "I-Boot"
0x00000000-0x00020000 : "RedBoot"
0x00020000-0x00060000 : "Partition 2"
0x00060000-0x00160000 : "Partition 3"
0x00160000-0x00fe0000 : "Partition 4"
Linux Kernel Card Services 3.1.22
  options:  [pm]
SA-1100 PCMCIA (CS release 3.1.22)
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP, IGMP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 4096 bind 4096)
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
NetWinder Floating Point Emulator V0.95 (c) 1998-1999 Rebel.com
FAT: bogus logical sector size 408
UMSDOS: msdos_read_super failed, mount aborted.
FAT: bogus logical sector size 408
FAT: bogus logical sector size 408
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
/dev/hda1: clean, 1384/1957888 files, 109050/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 04:45:49.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 04:45:56 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 04:45:56 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
opse2 login: ops
Password: brynner
gosiam~$ gosiam
cd logsmnt/hda/siam$ cd logs
killj9/mnt/hda/siam/logs$ killj9
rm *2:/mnt/hda/siam/logs$ rm *
ym: remove write-protected file `clocks.log'? y
node2:/mnt/hda/siam/logs$ +
MBARI SideARM v4.1
IBoot version 1.7
  built on Nov 24 2008 at 13:01:12

Copyright 2001,2002 Intrinsyc Software Inc.
Copyright 2004 MBARI

CS8900A found at 0x08000300                                                                                               0
Relocating zImage from 00060000 to C0008000 (len=00100000)
Proper ARM zImage ID found. Booting...
Uncompressing Linux............................................................ done, booting the kernel.
Linux version 2.4.9-ac10-rmk2-np1-cerf2 (ops@greenflash) (gcc version 2.95.3 20010315 (release)) #64 Thu Nov 20 10:54:37 PST 2008
Processor: Intel StrongARM-1110 revision 9
Architecture: MBARI SideARM v4.1 - 11/16/2006
On node 0 totalpages: 16384
zone(0): 16384 pages.
zone(1): 0 pages.
zone(2): 0 pages.
Kernel command line: console=ttySA0 cpufreq=191700 root=1f04 rw init=/linuxrc
Calibrating delay loop... 127.38 BogoMIPS
Memory: 64MB = 64MB total
Memory: 62420KB available (1628K code, 291K data, 64K init)
Dentry-cache hash table entries: 8192 (order: 4, 65536 bytes)
Inode-cache hash table entries: 4096 (order: 3, 32768 bytes)
Mount-cache hash table entries: 1024 (order: 1, 8192 bytes)
Buffer-cache hash table entries: 4096 (order: 2, 16384 bytes)
Page-cache hash table entries: 16384 (order: 4, 65536 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd v1.8
Journalled Block Device driver loaded
JFFS2 version 2.1. (C) 2001 Red Hat, Inc., designed by Axis Communications AB.
ttySA5 at MEM 0x80050000 (irq = 17) is a SA1100
ttySA6 at MEM 0x80030000 (irq = 16) is a SA1100
ttySA7 at MEM 0x80010000 (irq = 15) is a SA1100
pty: 256 Unix98 ptys configured
SA1100 Real Time Clock driver v1.00
block: queued sectors max/low 41397kB/13799kB, 128 slots per queue
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
Uniform Multi-Platform E-IDE driver Revision: 6.31
ide: Assuming 50MHz system bus speed for PIO modes; override with idebus=xx
loop: loaded (max 8 devices)
SA1100 flash: probing 16-bit flash bus
Using RedBoot partition definition
Creating 5 MTD partitions on "SA1100 flash":
0x00000000-0x00020000 : "I-Boot"
0x00000000-0x00020000 : "RedBoot"
0x00020000-0x00060000 : "Partition 2"
0x00060000-0x00160000 : "Partition 3"
0x00160000-0x00fe0000 : "Partition 4"
Linux Kernel Card Services 3.1.22
  options:  [pm]
SA-1100 PCMCIA (CS release 3.1.22)
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP, IGMP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 4096 bind 4096)
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
NetWinder Floating Point Emulator V0.95 (c) 1998-1999 Rebel.com
FAT: bogus logical sector size 408
UMSDOS: msdos_read_super failed, mount aborted.
FAT: bogus logical sector size 408
FAT: bogus logical sector size 408
Child dir "." (ino #1) of dir ino #1 appears to be a hard link
VFS: Mounted root (jffs2 filesystem).
Freeing init memory: 64K
Setting up RAMFS, please wait...
Executing /sbin/init...
INIT: version 2.78 booting
Mounting local filesystems...
devpts on /dev/pts type devpts (rw,mode=0622)
Setting the System Clock using the Hardware Clock as reference...
Calculating module dependencies... depmod: /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.ieee1394map is not an ELF file
depmod: error reading ELF header /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.pnpbiosmap: No such file or directory
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/loopback.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net_init.o
done.
Loading modules: slhc CSLIP: code copyright 1989 Regents of the University of California
ppp_generic PPP generic driver version 2.4.1
ppp_async ppp_deflate PPP Deflate Compression module registered
bsd_comp PPP BSD Compression module registered
cs8900 Cirrus Logic CS8900A driver for Linux (24-Jan-2004)
eth0: Registered cs8900_eeprom char device (major #253)
eth0: CS8900A rev D at 0xf0000300 irq=47, eeprom ok, addr: 00: C:6A: 0:04: 2
eth0: power management support enabled
sidearm-wdog sidearm-wdog: version 1.3 [Jun 22 2005 09:57:53]

INIT: Entering runlevel: 2
Configuring network interfaces: eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: SDCFXS-032G, ATA DISK drive
ide0 at 0xf7000000-0xf7000007,0xf700000e on irq 43
hda: 62537328 sectors (32019 MB) w/1KiB Cache, CHS=62041/16/63
Partition check:
 hda: hda1
ide_cs: hda: Vcc = 3.3, Vpp = 0.0
cardmgr[58]: executing: './ide start hda'
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027
cardmgr[58]: + ide.opts configuring default,1,OAZ102514183027,1 partition 1
cardmgr[58]: exiting
running filesystem check on CF filesystem
e2fsck 1.38 (30-Jun- hda:2005)
 hda1
 hda: hda1
/dev/hda1: recovering journal
 hda: hda1
 hda: hda1
Clearing orphaned inode 811010 (uid=0, gid=0, mode=0100644, size=665)
/dev/hda1: clean, 1376/1957888 files, 109012/7817134 blocks
Configuring sa1100_gpio gpio port: SA1100 GPIO v1.3 device (10,224): stencil=0x000FFFF
done.
Configuring sa1100_lddio lddio port: SA1100 LDDIO v1.0 device (10,225): stencil=0x0000FFF
done.
Configuring sa1100_spi spi port: SA1100 SPI v1.3 device (10,223)
done.
Configuring Exar serial ports: xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000000] irq[2] firstminor[0]
ttySX0 at MEM 0x10000000 (irq = 2) is a 16550
ttySX1 at MEM 0x10000020 (irq = 2) is a 16550
ttySX2 at MEM 0x10000040 (irq = 2) is a 16550
ttySX3 at MEM 0x10000060 (irq = 2) is a 16550
ttySX4 at MEM 0x10000080 (irq = 2) is a 16550
ttySX5 at MEM 0x100000a0 (irq = 2) is a 16550
ttySX6 at MEM 0x100000c0 (irq = 2) is a 16550
ttySX7 at MEM 0x100000e0 (irq = 2) is a 16550
xr788: version [1.72 (serial wakeup, the saga continues) Jun 17 2005 15:05:21] base[10000200] irq[3] firstminor[8]
ttySX8 at MEM 0x10000200 (irq = 3) is a 16550
ttySX9 at MEM 0x10000220 (irq = 3) is a 16550
ttySX10 at MEM 0x10000240 (irq = 3) is a 16550
ttySX11 at MEM 0x10000260 (irq = 3) is a 16550
ttySX12 at MEM 0x10000280 (irq = 3) is a 16550
ttySX13 at MEM 0x100002a0 (irq = 3) is a 16550
ttySX14 at MEM 0x100002c0 (irq = 3) is a 16550
ttySX15 at MEM 0x100002e0 (irq = 3) is a 16550
done.
Starting system logger:
Starting kernel logger:
Starting OpenBSD Secure Shell server: sshd.
SIOCADDRT: Network is unreachable
Starting Boa webserver: boa.
mounting filesystems
 hda: hda1
 hda: hda1
kjournald starting.  Commit interval 5 seconds
EXT3 FS 2.4-0.9.6, 11 Aug 2001 on ide0(3,1), internal journal
EXT3-fs: mounted filesystem with ordered data mode.
/dev/hda1 on /mnt/hda type ext3 (rw)

Setting system date/time to 7/10/2015, 04:50:03.
rc.local - try to get DHCP address
Switching interface to DHCP... interfaces_modified Done!
Using /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/arch/arm/mach-sa1100/registers.o

RF Power 0 ON

Run ntpdate
 7 Oct 04:50:10 ntpdate[162]: can't find host in.pool.ntp.org
 7 Oct 04:50:10 ntpdate[162]: no servers can be used, exiting
Start logging clocks
Starting SIAM application:
startnode - do not try ntpdate here for standalone node
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
!             Warning PARENT_HOST not defined                 !
!             Starting node without portal                    !
!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!
done.

**************************************************
** Intrinsyc Linux (I-Linux)                    **
** Copyright 2001,2002 Intrinsyc Software Inc.  **
** Version: 4.4                                 **
** Support: http://support.intrinsyc.com        **
**************************************************
opse2 login: ops
Password: brynner
node2:~$
node2:~$
listPorts loc -statsoc -stats
SIAM version $Name:  $

Node 1598 has 14 ports

   Port Name ISI-ID              Service   Status  S   E   R
   --------- ------              -------   ------ --- --- ---
 /dev/ttySX0      -                    -        -   -
 /dev/ttySX1   1533              SBE-19+ SAMPLING  21   0   0
 /dev/ttySX2   1535 Triplet  slv to 1827       OK   7   0   0
 /dev/ttySX3   1474             Aquadopp SAMPLING  28   0   0
 /dev/ttySX4   1524  Optode  slv to 1535       OK   7   0   0
 /dev/ttySX5   1825          300kHz ADCP SAMPLING  20   0   0
 /dev/ttySX6   1828          600kHz ADCP SAMPLING  13   0   0
 /dev/ttySX7   1827         1200kHz ADCP SAMPLING   5   0   0
 /dev/ttySX8      -                    -        -   -
 /dev/ttySX9      -                    -        -   -
/dev/ttySX10      -                    -        -   -
/dev/ttySX11      -                    -        -   -
/dev/ttySX15   1599               MSP430       OK   1   0   0
 /dev/ttySA2      -                    -        -   -

samplePort loc /dev/ttySX15v/ttySX15
SIAM version $Name:  $
MSP430:
parentID=1598, recordType=1
devid=1599, t=1444193938830, seqNo=1, mdref=0
nBytes=75
$PEDATA, P861.89, T30.49, H28.96, GFL0.00, GFH-0.13, C289.86, TC0.00, *3732

press: 861.89 millibar
tmprt: 30.49 deg C
humid: 28.96 rel %
GF-low: 0 microAmps
GF-high: -0.13 microAmps
heading: 289.86 deg
nTurns: 0 turns
node2:~$ hda: status timeout: status=0xd0 { Busy }
hda: no DRQ after issuing WRITE

[bookmark: _GoBack]node2:~$
node2:~$ SamplePort loc /dev/ttySX15ide0: reset timed-out, status=0xd0
hda: status timeout: status=0xd0 { Busy }
hda: drive not ready for command
SamplePort loc /dev/ttySX15
bash: SamplePort: command not found
node2:~$
node2:~$ ide0: reset timed-out, status=0xd0
end_request: I/O error, dev 03:01 (hda), sector 25954680
end_request: I/O error, dev 03:01 (hda), sector 25954880
end_request: I/O error, dev 03:01 (hda), sector 25954904
end_request: I/O error, dev 03:01 (hda), sector 25954936
end_request: I/O error, dev 03:01 (hda), sector 25955008
end_request: I/O error, dev 03:01 (hda), sector 25955032
end_request: I/O error, dev 03:01 (hda), sector 25955040
end_request: I/O error, dev 03:01 (hda), sector 8
end_request: I/O error, dev 03:01 (hda), sector 12496
end_request: I/O error, dev 03:01 (hda), sector 12616
end_request: I/O error, dev 03:01 (hda), sector 15152
end_request: I/O error, dev 03:01 (hda), sector 25952256
end_request: I/O error, dev 03:01 (hda), sector 30959488
end_request: I/O error, dev 03:01 (hda), sector 30959496
end_request: I/O error, dev 03:01 (hda), sector 30959504
end_request: I/O error, dev 03:01 (hda), sector 25954680
end_request: I/O error, dev 03:01 (hda), sector 30959512
end_request: I/O error, dev 03:01 (hda), sector 30959520
end_request: I/O error, dev 03:01 (hda), sector 30959528
end_request: I/O error, dev 03:01 (hda), sector 30959536
end_request: I/O error, dev 03:01 (hda), sector 30959544
end_request: I/O error, dev 03:01 (hda), sector 30959552
end_request: I/O error, dev 03:01 (hda), sector 30959560
end_request: I/O error, dev 03:01 (hda), sector 138744
end_request: I/O error, dev 03:01 (hda), sector 524304
end_request: I/O error, dev 03:01 (hda), sector 0
end_request: I/O error, dev 03:01 (hda), sector 11520
end_request: I/O error, dev 03:01 (hda), sector 30959568
end_request: I/O error, dev 03:01 (hda), sector 30959576
end_request: I/O error, dev 03:01 (hda), sector 30959584
end_request: I/O error, dev 03:01 (hda), sector 25954496
end_request: I/O error, dev 03:01 (hda), sector 25954568
end_request: I/O error, dev 03:01 (hda), sector 25954368
end_request: I/O error, dev 03:01 (hda), sector 25954440
end_request: I/O error, dev 03:01 (hda), sector 30959592
end_request: I/O error, dev 03:01 (hda), sector 30959600
end_request: I/O error, dev 03:01 (hda), sector 30959608
end_request: I/O error, dev 03:01 (hda), sector 25955048
end_request: I/O error, dev 03:01 (hda), sector 25954800
end_request: I/O error, dev 03:01 (hda), sector 30959616
end_request: I/O error, dev 03:01 (hda), sector 30959624
end_request: I/O error, dev 03:01 (hda), sector 30959632
end_request: I/O error, dev 03:01 (hda), sector 25954496
end_request: I/O error, dev 03:01 (hda), sector 25954568
end_request: I/O error, dev 03:01 (hda), sector 25954368
end_request: I/O error, dev 03:01 (hda), sector 25954440
end_request: I/O error, dev 03:01 (hda), sector 30959640
end_request: I/O error, dev 03:01 (hda), sector 30959648
end_request: I/O error, dev 03:01 (hda), sector 30959656
end_request: I/O error, dev 03:01 (hda), sector 25954680
end_request: I/O error, dev 03:01 (hda), sector 25955008
end_request: I/O error, dev 03:01 (hda), sector 25955008
end_request: I/O error, dev 03:01 (hda), sector 25955008
EXT3-fs error (device ide0(3,1)): ext3_free_branches: Read failure, inode=811026, block=3244376
end_request: I/O error, dev 03:01 (hda), sector 25954904
end_request: I/O error, dev 03:01 (hda), sector 25954936
end_request: I/O error, dev 03:01 (hda), sector 25955040
end_request: I/O error, dev 03:01 (hda), sector 25955056
end_request: I/O error, dev 03:01 (hda), sector 25955064
end_request: I/O error, dev 03:01 (hda), sector 0
end_request: I/O error, dev 03:01 (hda), sector 25954880
end_request: I/O error, dev 03:01 (hda), sector 25954880
end_request: I/O error, dev 03:01 (hda), sector 25954880
EXT3-fs error (device ide0(3,1)): ext3_free_branches: Read failure, inode=811024, block=3244360
end_request: I/O error, dev 03:01 (hda), sector 25955032
end_request: I/O error, dev 03:01 (hda), sector 0
end_request: I/O error, dev 03:01 (hda), sector 30959664
end_request: I/O error, dev 03:01 (hda), sector 30959672
end_request: I/O error, dev 03:01 (hda), sector 30959680
end_request: I/O error, dev 03:01 (hda), sector 30959688
end_request: I/O error, dev 03:01 (hda), sector 30959696
end_request: I/O error, dev 03:01 (hda), sector 30959704
end_request: I/O error, dev 03:01 (hda), sector 30959712
end_request: I/O error, dev 03:01 (hda), sector 30959720
end_request: I/O error, dev 03:01 (hda), sector 30959728
end_request: I/O error, dev 03:01 (hda), sector 25954680
end_request: I/O error, dev 03:01 (hda), sector 30959736
end_request: I/O error, dev 03:01 (hda), sector 30959744
end_request: I/O error, dev 03:01 (hda), sector 30959752
end_request: I/O error, dev 03:01 (hda), sector 25954440
end_request: I/O error, dev 03:01 (hda), sector 25954496
end_request: I/O error, dev 03:01 (hda), sector 25954568
end_request: I/O error, dev 03:01 (hda), sector 25954368
end_request: I/O error, dev 03:01 (hda), sector 30959760
Assertion failure in journal_bmap() at journal.c:581: "ret != 0"
kernel BUG at journal.c:581!
Unable to handle kernel NULL pointer dereference at virtual address 00000000
pgd = c0004000
*pgd = 00000000, *pmd = 00000000
Internal error: Oops: ffffffff
CPU: 0
pc : [<c001d59c>]    lr : [<c0024d00>]
sp : c3a6de10  ip : c3a6ddbc  fp : c3a6de20
r10: 00000000  r9 : 00000000  r8 : c3a6dea0
r7 : c32f29e0  r6 : 00000000  r5 : 00000245  r4 : 00000000
r3 : 00000000  r2 : 00000001  r1 : 00000001  r0 : 00000001
Flags: nZCv  IRQs on  FIQs on  Mode SVC_32  Segment user
Control: C332F17F  Table: C332F17F  DAC: 00000015
Process kjournald (pid: 98, stackpage=c3a6d000)
Stack:
c3a6de00: c0024d00 c001d59c 60000013 ffffffff  c0184be0 c3a6de40 c3a6de24 c007abc0
c3a6de20: c001d564 c0184c98 c0330600 00000000  c0330600 c3a6de60 c3a6de44 c007ab48
c3a6de40: c007ab70 c3a6de74 c0330600 00000000  c3250670 c3a6de74 c3a6de64 c007abf8
c3a6de60: c007aacc c2058c00 c3a6dfc8 c3a6de78  c00779ec c007abf0 c002d740 c0330694
c3a6de80: c0330650 00000000 00000000 00000000  c32503d0 c0330600 c1605480 c3250160
c3a6dea0: c22a0ce0 c26fabc0 c1ecf800 c2058c00  c16054e0 c1b12f20 c17a9e00 c17a9e60
c3a6dec0: c17b4f00 c17b4f60 c1c62c60 c1c62cc0  c1ef59e0 c3a6dee0 c0029304 c00295d8
c3a6dee0: 00000000 0000001a 00000000 c01c8478  c01c8138 c3a6df34 c3a6df30 c3a6df08
c3a6df00: c001915c c0029290 fa050000 c3a6df7c  00000001 c001fb40 00000013 ffffffff
c3a6df20: c01ba040 c3a6dfa4 c3a6df34 c00184c0  c001903c c332c000 f500a000 00000000
c3a6df40: 00000000 c3a6c000 c3f4b920 c3f4ba20  c2242000 60000013 c3a6c000 c3f4ba20
c3a6df60: c3f4ba20 c1e8e000 00000000 c01d6760  c01ba040 c3a6dfa4 c00217a0 60000013
c3a6df80: 00000000 c0330650 c0330600 c344a400  00000002 c344a400 c3a6dfc8 c3a6dfa8
c3a6dfa0: c0330708 00000000 c0330650 c0330600  c344a400 00000002 c344a400 c3a6dffc
c3a6dfc0: c3a6dfcc c007a60c c007736c c01d7238  c032bebc 00011ce3 c3a6c000 c007a4bc
c3a6dfe0: c0330600 c0330694 00000000 00000000  00000000 c3a6e000 c0019c3c c007a4ec
Backtrace:
Function entered at [<c001d558>] from [<c007abc0>]
 r4 = C0184BE0
Function entered at [<c007ab64>] from [<c007ab48>]
 r6 = C0330600  r5 = 00000000  r4 = C0330600
Function entered at [<c007aac0>] from [<c007abf8>]
 r6 = C3250670  r5 = 00000000  r4 = C0330600
Function entered at [<c007abe4>] from [<c00779ec>]
 r4 = C2058C00
Function entered at [<c0077360>] from [<c007a60c>]
Function entered at [<c007a4e0>] from [<c0019c3c>]
 r7 = 00000000  r6 = 00000000  r5 = C0330694  r4 = C0330600
Code: eb001d30 e3a03000 (e5833000) e91ba810 c0175578

Message from syslogd@node402 at Wed Oct  7 05:00:43 2015 ...
node402 kernel: Assertion failure in journal_bmap() at journal.c:581: "ret != 0"
Unable to handle kernel paging request at virtual address 45534146
pgd = c0004000
*pgd = 00000000, *pmd = 00000000
Internal error: Oops: ffffffff
CPU: 0
pc : [<c002d5fc>]    lr : [<45534142>]
sp : c01b9ea0  ip : c01d7238  fp : c01b9ec8
r10: c01d7358  r9 : c01d7b5c  r8 : c01789ec
r7 : 00000004  r6 : 00000001  r5 : c01d735c  r4 : c01d7154
r3 : c01d7238  r2 : c01d735c  r1 : bffffb44  r0 : bffffad8
Flags: Nzcv  IRQs off  FIQs on  Mode SVC_32  Segment kernel
Control: C332F17F  Table: C332F17F  DAC: 0000001D
Process swapper (pid: 0, stackpage=c01b9000)
Stack:
c01b9e80:                                      45534142 c002d5fc 80000093 ffffffff
c01b9ea0: c01d6780 00000000 00000000 c01ba0a0  c01ba0c0 c01d6760 60000093 c01b9edc
c01b9ec0: c01b9ecc c0029794 c002d4b4 c01d6780  c01b9efc c01b9ee0 c002964c c0029768
c01b9ee0: c01ba0c0 00000001 c01d6760 fffffffe  c01b9f24 c01b9f00 c0029304 c00295d8
c01b9f00: 00000000 0000001a 00000000 c01c8478  c01c8138 c01b9f54 c01b9f50 c01b9f28
c01b9f20: c001915c c0029290 fa050000 c01b9f9c  00000001 c0019d14 60000013 ffffffff
c01b9f40: c01c8764 c01b9fa8 c01b9f54 c00184c0  c001903c 00000000 00000000 60000013
c01b9f60: 600000d3 c0019cf4 c01b8000 c01b8000  c01bad6c c0019cf4 6901b119 c01c8764
c01b9f80: c01b9fa8 c01b9fac c01b9f9c c0019d14  c0019d14 60000013 ffffffff c01b9fd0
c01b9fa0: c01b9fac c001961c c0019d00 00004000  c01f45f0 c01c8798 c01c8780 c01bac88
c01b9fc0: 0000001f c01b9fe0 c01b9fd4 c0018030  c00195c0 c01b9ffc c01b9fe4 c0008910
c01b9fe0: c001800c c01c8bb0 c01f8318 c01f8318  00000000 c01ba000 c0008080 c00087d8
Backtrace:
Function entered at [<c002d4a8>] from [<c0029794>]
Function entered at [<c002975c>] from [<c002964c>]
 r4 = C01D6780
Function entered at [<c00295cc>] from [<c0029304>]
 r7 = FFFFFFFE  r6 = C01D6760  r5 = 00000001  r4 = C01BA0C0
Function entered at [<c0029284>] from [<c001915c>]
Function entered at [<c0019030>] from [<c00184c0>]
Function entered at [<c0019cf4>] from [<c001961c>]
Function entered at [<c00195b4>] from [<c0018030>]
Function entered at [<c0018000>] from [<c0008910>]
Function entered at [<c00087cc>] from [<c0008080>]
Code: e590e000 e5903004 (e58e3004) e583e000 e5901008
Kernel panic: Aiee, killing interrupt handler!
In interrupt handler - not syncing
 +
MBARI SideARM v4.1
IBoot version 1.7
  built on Nov 24 2008 at 13:01:12

Copyright 2001,2002 Intrinsyc Software Inc.
Copyright 2004 MBARI

CS8900A found at 0x08000300                                                                                               0
Relocating zImage from 00060000 to C0008000 (len=00100000)
Proper ARM zImage ID found. Booting...
Uncompressing Linux............................................................ done, booting the kernel.
Linux version 2.4.9-ac10-rmk2-np1-cerf2 (ops@greenflash) (gcc version 2.95.3 20010315 (release)) #64 Thu Nov 20 10:54:37 PST 2008
Processor: Intel StrongARM-1110 revision 9
Architecture: MBARI SideARM v4.1 - 11/16/2006
On node 0 totalpages: 16384
zone(0): 16384 pages.
zone(1): 0 pages.
zone(2): 0 pages.
Kernel command line: console=ttySA0 cpufreq=191700 root=1f04 rw init=/linuxrc
Calibrating delay loop... 127.38 BogoMIPS
Memory: 64MB = 64MB total
Memory: 62420KB available (1628K code, 291K data, 64K init)
Dentry-cache hash table entries: 8192 (order: 4, 65536 bytes)
Inode-cache hash table entries: 4096 (order: 3, 32768 bytes)
Mount-cache hash table entries: 1024 (order: 1, 8192 bytes)
Buffer-cache hash table entries: 4096 (order: 2, 16384 bytes)
Page-cache hash table entries: 16384 (order: 4, 65536 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd v1.8
Journalled Block Device driver loaded
JFFS2 version 2.1. (C) 2001 Red Hat, Inc., designed by Axis Communications AB.
ttySA5 at MEM 0x80050000 (irq = 17) is a SA1100
ttySA6 at MEM 0x80030000 (irq = 16) is a SA1100
ttySA7 at MEM 0x80010000 (irq = 15) is a SA1100
pty: 256 Unix98 ptys configured
SA1100 Real Time Clock driver v1.00
block: queued sectors max/low 41397kB/13799kB, 128 slots per queue
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
Uniform Multi-Platform E-IDE driver Revision: 6.31
ide: Assuming 50MHz system bus speed for PIO modes; override with idebus=xx
loop: loaded (max 8 devices)
SA1100 flash: probing 16-bit flash bus
Using RedBoot partition definition
Creating 5 MTD partitions on "SA1100 flash":
0x00000000-0x00020000 : "I-Boot"
0x00000000-0x00020000 : "RedBoot"
0x00020000-0x00060000 : "Partition 2"
0x00060000-0x00160000 : "Partition 3"
0x00160000-0x00fe0000 : "Partition 4"
Linux Kernel Card Services 3.1.22
  options:  [pm]
SA-1100 PCMCIA (CS release 3.1.22)
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP, IGMP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 4096 bind 4096)
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
NetWinder Floating Point Emulator V0.95 (c) 1998-1999 Rebel.com
cs: socket c035c000 timed out during reset.  Try increasing setup_delay.
FAT: bogus logical sector size 408
UMSDOS: msdos_read_super failed, mount aborted.
FAT: bogus logical sector size 408
FAT: bogus logical sector size 408
Child dir "." (ino #1) of dir ino #1 appears to be a hard link
VFS: Mounted root (jffs2 filesystem).
Freeing init memory: 64K
Setting up RAMFS, please wait...
Executing /sbin/init...
INIT: version 2.78 booting
Mounting local filesystems...
devpts on /dev/pts type devpts (rw,mode=0622)
Setting the System Clock using the Hardware Clock as reference...
Calculating module dependencies... depmod: /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.ieee1394map is not an ELF file
depmod: error reading ELF header /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/modules.pnpbiosmap: No such file or directory
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/loopback.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net.o
depmod: *** Unresolved symbols in /lib/modules/2.4.9-ac10-rmk2-np1-cerf2/kernel/drivers/net/net_init.o
done.
Loading modules: slhc CSLIP: code copyright 1989 Regents of the University of California
ppp_generic PPP generic driver version 2.4.1
ppp_async ppp_deflate PPP Deflate Compression module registered
bsd_comp PPP BSD Compression module registered
cs8900 Cirrus Logic CS8900A driver for Linux (24-Jan-2004)
eth0: Registered cs8900_eeprom char device (major #253)
eth0: CS8900A rev D at 0xf0000300 irq=47, eeprom ok, addr: 00: C:6A: 0:04: 2
eth0: power management support enabled
sidearm-wdog sidearm-wdog: version 1.3 [Jun 22 2005 09:57:53]

INIT: Entering runlevel: 2
Configuring network interfaces: eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
NETDEV WATCHDOG: eth0: transmit timed out
eth0: Transmit buffer not free!
Operation failed.
done.
Starting PCMCIA services: cardmgr.
cardmgr[58]: starting, version is 3.1.22
cardmgr[58]: watching 2 sockets
cardmgr[58]: socket 1: ATA/IDE Fixed Disk
cardmgr[58]: executing: 'modprobe ide-cs'
Trying to free nonexistent resource <f7000000-f700000f>
hda: no response (status = 0x80), resetting drive
hda: no response (status = 0x80)
hdb: probing with STATUS(0x00) instead of ALTSTATUS(0x80)
hdb: probing with STATUS(0x00) instead of ALTSTATUS(0x80)
hda: no response (status = 0x80), resetting drive
hda: no response (status = 0x80)
hdb: probing with STATUS(0x00) instead of ALTSTATUS(0x80)
hdb: probing with STATUS(0x00) instead of ALTSTATUS(0x80)
hda: no response (status = 0x80), resetting drive
