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Dive Objective: Five-month deployment of SES at Station M in first long-term deployment at 4000 m.

Deployment Date: ___________

Recovery Date: ___________

Person performing topside checklist: 
_____________

Pre-deployment:

1. Install SES battery shorting plug and deck comms cable.

2. Establish reliable comms with SES through deck comms cable.

3. Run syntax check on mission code.

4. Run predive test program and verify correct operation of the following systems:

a. Turntable rotates

b. Fluorometer returns data

c. External LED lights

d. Internal LED lights

e. Camera returns images

5. Check all flotation mechanically secure.

6. Check imaging chambers compensation water level.

7. Inspect all water hoses and fitting for damage and leaks.

8. Check that Drop Weight is installed properly and free to drop.

9. Remove Drop Weight safety tie.

10. Arm both Drop Weight Releases, noting release codes.

a. Release #1 xmt freq: ___________

b. Release #1 rcv freq: ___________

c. Release #1 activation code: ___________

d. Release #1 release code: ___________

e. Release #2 xmt freq: ___________

f. Release #2 rcv freq: ___________

g. Release #2 activation code: ___________

h. Release #2 release code: ___________

11. Note HomerPro #: ___________

12. Activate Strobe and VHF Beacon, noting Beacon channel number and verifying operation with VHF receiver.

a. Beacon channel number: ___________

13. Unplug Rover deck comms cable and install dummy plug in its place.

14. Check all cable connectors and dummies installed and tight.

15. Check for tools left on and in SES frame.

16. Remove SES hold-down straps.

Deployment:

17. Deploy SES, noting exact time and position of launch.

a. SES launch time: ____________ PDT

b. Latitude: _____________deg

c. Longitude: _____________deg

On Bottom:

18. Use ROV to observe position of SES Sample Turntable. The alignment marks should’ve moved from “open” to “samp”.

