SES Deployment on MARS Rev 1
General:
Scheduled deployment date:
June 30, 2011 
Scheduled recovery date:
October 25, 2011
Deployment Vessel:

Point Lobos
Recovery Vessel:

Point Lobos
Deployment method:  


Special Conditions:  
Cable:  70 meter with ODI connector on one end. 

Test Tank Dates:  

MARS Port:
3
Networking:
Subsurface vlan: 
10.1.13.xxx

Subsurface gateway:
10.1.13.1

MARS O&M reserves address 10.1.13.250 to 10.1.13.255

Only addresses in the range of 10.1.13.2 to 10.1.13.11 can be mapped to externally
Science vlan:

10.91.43.xxx

Science gateway:
10.91.43.1

MARS O&M reserves address 10.91.43.250 to 10.91.43.255

Only addresses in the range of 10.91.43.2 to 10.91.43.11 can be mapped to externally
DNS Server #1:
10.91.128.61

DNS Server #2:
10.91.128.62

NTP Server #1:
10.91.128.55

External mapping address range will be 134.89.42.130 to 134.89.42.139.  

A maximum of 10 addresses can be mapped externally.

MARS O&M needs a list of computers by IP address that may access the externally mapped addresses.  (Maximum of 6)

Note:  For WNS testing, the external address range is 134.89.52.130 to 134.89.52.139

Power Requirement:

48 volts @ ? watts
375 volts @ ? watts
