SES LED light o-ring sizes:
Connector -017
Glass -015