20210412::214100: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210412::214100: GUI: Live mode ON.
20210412::214100: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210412::214100: GUI: WiSSL GUI started at 2021_04_12_21:41:00
20210412::214100: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_12.txt
20210412::214100: GUI: Attempting Communications with Head 1...
20210412::214100: GUI: Attempting Communications with Head 2...
20210412::214101: GUI: Established Communications with Head 1.
20210412::214101: GUI: Established Communications with Head 2.
20210412::214102: Head 1: Initializing Communications with GUI ...
20210412::214102: Head 2: Initializing Communications with GUI ...
20210412::214102: Head 1: Communications Established.
20210412::214102: Head 2: Communications Established.
20210412::214103: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210412::214103: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210412::214103: Head 2: Connection Established with the GUI.
20210412::214104: Head 1: Connection Established with the GUI.
20210412::214104: Head 2: Initializing Subsystems, standby ...
20210412::214104: Head 1: Initializing Subsystems, standby ...
20210412::214104: Head 2: Initializing Hardware, Stand by ...
20210412::214104: Head 1: Initializing Hardware, Stand by ...
20210412::214114: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210412::214114: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210412::214114: Head 1: NtQuery - testing 1 ...
20210412::214114: Head 2: NtQuery - testing 1 ...
20210412::214114: Head 1: clock resolution: 10
20210412::214114: Head 2: clock resolution: 10
20210412::214114: Head 1: NtQuery - testing 2, after setting max res ...
20210412::214115: Head 2: NtQuery - testing 2, after setting max res ...
20210412::214115: Head 1: clock resolution: 10
20210412::214115: Head 2: clock resolution: 10
20210412::214115: Head 1: Initializing Optics Electronics ...
20210412::214115: Head 2: Initializing Optics Electronics ...
20210412::214115: Head 1: Power Laser Controller
20210412::214115: Head 2: Power Laser Controller
20210412::214119: Head 1: Power Scanner Controller
20210412::214119: Head 2: Power Scanner Controller
20210412::214121: Head 1: Power OPTO Sensor
20210412::214121: Head 2: Power OPTO Sensor
20210412::214130: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214130: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 52
20210412::214130: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214141: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210412::214141: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210412::214142: Head 1: Eye Safe Optical Filter check Passed
20210412::214142: Head 2: Eye Safe Optical Filter check Passed
20210412::214142: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210412::214142: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210412::214142: Head 1: Initializing Time Sync Subsystem.
20210412::214142: Head 2: Initializing Time Sync Subsystem.
20210412::214143: Head 1: Initializing CTD Subsystem.
20210412::214143: Head 2: Initializing CTD Subsystem.
20210412::214143: Head 1: CTD Initialization Successful
20210412::214143: Head 2: CTD Initialization Successful
20210412::214143: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210412::214143: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210412::214144: Head 1: Time Sync UDP started, waiting for sync...
20210412::214144: Head 2: Time Sync UDP started, waiting for sync...
20210412::214144: Head 1: Attempting CTD Ethernet connection with ROV...
20210412::214144: Head 2: Attempting CTD Ethernet connection with ROV...
20210412::214151: GUI: Live mode ON.
20210412::214151: GUI: Requesing START operation, Head 2
20210412::214151: GUI: Requesing START operation, Head 1
20210412::214151: Head 2: Received request: START
20210412::214151: Head 1: Received request: START
20210412::214151: Head 2: Starting Scan Operation
20210412::214151: Head 1: Starting Scan Operation
20210412::214152: Head 2: Error: not receiving UDP ZDA...
20210412::214152: Head 1: Error: not receiving UDP ZDA...
20210412::214153: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210412::214153: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210412::214153: Head 1: Eye Safe Optical Filter check Passed
20210412::214153: Head 2: Eye Safe Optical Filter check Passed
20210412::214200: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 106
20210412::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 19C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 1
20210412::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 19C, Laser 17.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210412::214202: Head 2: Error: not receiving UDP ZDA...
20210412::214202: Head 1: Error: not receiving UDP ZDA...
20210412::214204: Head 1: Configured for WATER Processing
20210412::214204: Head 1: Configured for WATER Processing
20210412::214204: Head 1: Configured for WATER Processing
20210412::214205: Head 1: Configured for WATER Processing
20210412::214205: Head 1: Configured for WATER Processing
20210412::214205: Head 1: Configured for WATER Processing
20210412::214205: Head 1: Configured for WATER Processing
20210412::214206: Head 1: Configured for WATER Processing
20210412::214206: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214829_wf.raa
20210412::214206: Head 1: Configured for WATER Processing
20210412::214206: Head 1: Configured for WATER Processing
20210412::214207: Head 1: Configured for WATER Processing
20210412::214207: Head 1: Configured for WATER Processing
20210412::214207: Head 1: Configured for WATER Processing
20210412::214208: Head 1: Configured for WATER Processing
20210412::214208: Head 1: Configured for WATER Processing
20210412::214208: Head 1: Configured for WATER Processing
20210412::214209: Head 1: Configured for WATER Processing
20210412::214209: Head 1: Configured for WATER Processing
20210412::214209: Head 1: Configured for WATER Processing
20210412::214209: Head 1: Configured for WATER Processing
20210412::214213: Head 2: Error: not receiving UDP ZDA...
20210412::214213: Head 1: Error: not receiving UDP ZDA...
20210412::214214: Head 2: Configured for WATER Processing
20210412::214214: Head 2: Configured for WATER Processing
20210412::214214: Head 2: Configured for WATER Processing
20210412::214214: Head 2: Configured for WATER Processing
20210412::214215: Head 2: Configured for WATER Processing
20210412::214215: Head 2: Configured for WATER Processing
20210412::214215: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214839_wf.raa
20210412::214215: Head 2: Configured for WATER Processing
20210412::214216: Head 2: Configured for WATER Processing
20210412::214216: Head 2: Configured for WATER Processing
20210412::214216: Head 2: Configured for WATER Processing
20210412::214217: Head 2: Configured for WATER Processing
20210412::214217: Head 2: Configured for WATER Processing
20210412::214217: Head 2: Configured for WATER Processing
20210412::214218: Head 2: Configured for WATER Processing
20210412::214218: Head 2: Configured for WATER Processing
20210412::214218: Head 2: Configured for WATER Processing
20210412::214219: Head 2: Configured for WATER Processing
20210412::214219: Head 2: Configured for WATER Processing
20210412::214219: Head 2: Configured for WATER Processing
20210412::214219: Head 2: Configured for WATER Processing
20210412::214223: Head 2: Error: not receiving UDP ZDA...
20210412::214225: Head 1: Error: not receiving UDP ZDA...
20210412::214226: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214849_wf.raa
20210412::214230: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 159
20210412::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 24C, OCB 26%, OPB 20C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 24C, OCB 26%, OPB 19C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214233: Head 2: Error: not receiving UDP ZDA...
20210412::214238: Head 1: Error: not receiving UDP ZDA...
20210412::214239: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214859_wf.raa
20210412::214244: Head 2: Error: not receiving UDP ZDA...
20210412::214249: Head 1: Error: not receiving UDP ZDA...
20210412::214254: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214909_wf.raa
20210412::214254: Head 2: Error: not receiving UDP ZDA...
20210412::214300: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 212
20210412::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 20C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 19C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214300: Head 1: Error: not receiving UDP ZDA...
20210412::214304: Head 2: Error: not receiving UDP ZDA...
20210412::214308: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214919_wf.raa
20210412::214311: Head 1: Error: not receiving UDP ZDA...
20210412::214314: Head 2: Error: not receiving UDP ZDA...
20210412::214322: Head 1: Error: not receiving UDP ZDA...
20210412::214322: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214929_wf.raa
20210412::214324: Head 2: Error: not receiving UDP ZDA...
20210412::214330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 19C, Laser 21.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214330: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 266
20210412::214330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214334: Head 1: Error: not receiving UDP ZDA...
20210412::214335: Head 2: Error: not receiving UDP ZDA...
20210412::214337: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214939_wf.raa
20210412::214345: Head 1: Error: not receiving UDP ZDA...
20210412::214345: Head 2: Error: not receiving UDP ZDA...
20210412::214351: GUI: Archiving data to file --> C:\Data\20201017d1\20210412_214949_wf.raa
20210412::214355: Head 1: Error: not receiving UDP ZDA...
20210412::214355: GUI: Live mode ON.
20210412::214355: GUI: Requesing STOP operation, Head 2
20210412::214355: GUI: Requesing STOP operation, Head 1
20210412::214355: Head 2: Error: not receiving UDP ZDA...
20210412::214355: Head 1: Received request: STOP
20210412::214355: Head 2: Received request: STOP
20210412::214356: Head 1: Stopping Scan Operation
20210412::214356: Head 2: Stopping Scan Operation
20210412::214358: Head 2: ProcessingMgr stopped all worker threads.
20210412::214358: Head 2:       Stop finished, may now recover.
20210412::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 22.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 0
20210412::214400: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 319
20210412::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20210412::214401: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20210412::214402: Head 1: Eye Safe Optical Filter check Passed
20210412::214402: Head 1: ProcessingMgr stopped all worker threads.
20210412::214402: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210412::214402: Head 1:       Stop finished, may now recover.
20210412::214402: Head 2: Eye Safe Optical Filter check Passed
20210412::214405: Head 1: Error: not receiving UDP ZDA...
20210412::214405: Head 2: Error: not receiving UDP ZDA...
20210412::214415: Head 1: Error: not receiving UDP ZDA...
20210412::214415: Head 2: Error: not receiving UDP ZDA...
20210412::214426: Head 1: Error: not receiving UDP ZDA...
20210412::214426: Head 2: Error: not receiving UDP ZDA...
20210412::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 22.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214430: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 373
20210412::214430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214436: Head 1: Error: not receiving UDP ZDA...
20210412::214436: Head 2: Error: not receiving UDP ZDA...
20210412::214446: Head 1: Error: not receiving UDP ZDA...
20210412::214446: Head 2: Error: not receiving UDP ZDA...
20210412::214456: Head 1: Error: not receiving UDP ZDA...
20210412::214456: Head 2: Error: not receiving UDP ZDA...
20210412::214500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214500: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 427
20210412::214500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210412::214506: Head 1: Error: not receiving UDP ZDA...
20210412::214507: Head 2: Error: not receiving UDP ZDA...
20210412::214517: Head 1: Error: not receiving UDP ZDA...
20210412::214517: Head 2: Error: not receiving UDP ZDA...
20210412::214522: GUI: Live mode ON.
20210412::214522: GUI: Requesing START operation, Head 1
20210412::214522: GUI: Requesing START operation, Head 2
20210412::214522: Head 1: Received request: START
20210412::214522: Head 2: Received request: START
20210412::214523: Head 1: Starting Scan Operation
20210412::214523: Head 2: Starting Scan Operation
20210412::214524: Head 1: Eye Safe Optical Filter State there 10, not there 20, transition 1
20210412::214524: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210412::214524: Head 1: Eye Safe Optical Filter check Passed
20210412::214524: Head 2: Eye Safe Optical Filter check Passed
20210412::214527: Head 1: Error: not receiving UDP ZDA...
20210412::214527: Head 2: Error: not receiving UDP ZDA...
20210412::214528: Head 1: Configured for WATER Processing
20210412::214529: Head 2: Configured for WATER Processing
20210412::214529: Head 1: Configured for WATER Processing
20210412::214529: Head 2: Configured for WATER Processing
20210412::214529: Head 1: Configured for WATER Processing
20210412::214529: Head 2: Configured for WATER Processing
20210412::214529: Head 1: Configured for WATER Processing
20210412::214529: Head 2: Configured for WATER Processing
20210412::214530: Head 1: Configured for WATER Processing
20210412::214530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 1
20210412::214530: Head 2: Configured for WATER Processing
20210412::214530: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 480
20210412::214530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 24.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 1
20210412::214530: Head 1: Configured for WATER Processing
20210412::214530: Head 2: Configured for WATER Processing
20210412::214530: Head 1: Configured for WATER Processing
20210412::214530: Head 2: Configured for WATER Processing
20210412::214531: Head 1: Configured for WATER Processing
20210412::214531: Head 2: Configured for WATER Processing
20210412::214531: Head 1: Configured for WATER Processing
20210412::214531: Head 2: Configured for WATER Processing
20210412::214531: Head 1: Configured for WATER Processing
20210412::214531: Head 2: Configured for WATER Processing
20210412::214531: Head 1: Configured for WATER Processing
20210412::214532: Head 2: Configured for WATER Processing
20210412::214532: Head 1: Configured for WATER Processing
20210412::214532: Head 2: Configured for WATER Processing
20210412::214532: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215127_tank_dry.raa
20210412::214532: Head 1: Configured for WATER Processing
20210412::214532: Head 2: Configured for WATER Processing
20210412::214532: Head 1: Configured for WATER Processing
20210412::214532: Head 2: Configured for WATER Processing
20210412::214533: Head 1: Configured for WATER Processing
20210412::214533: Head 2: Configured for WATER Processing
20210412::214533: Head 1: Configured for WATER Processing
20210412::214533: Head 2: Configured for WATER Processing
20210412::214533: Head 1: Configured for WATER Processing
20210412::214533: Head 2: Configured for WATER Processing
20210412::214534: Head 1: Configured for WATER Processing
20210412::214534: Head 2: Configured for WATER Processing
20210412::214534: Head 1: Configured for WATER Processing
20210412::214534: Head 2: Configured for WATER Processing
20210412::214534: Head 1: Configured for WATER Processing
20210412::214534: Head 2: Configured for WATER Processing
20210412::214537: Head 2: Error: not receiving UDP ZDA...
20210412::214538: Head 1: Error: not receiving UDP ZDA...
20210412::214542: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215137_tank_dry.raa
20210412::214547: Head 2: Error: not receiving UDP ZDA...
20210412::214551: Head 1: Error: not receiving UDP ZDA...
20210412::214555: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215147_tank_dry.raa
20210412::214558: Head 2: Error: not receiving UDP ZDA...
20210412::214600: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 533
20210412::214600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 23.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214604: Head 1: Error: not receiving UDP ZDA...
20210412::214607: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215157_tank_dry.raa
20210412::214608: Head 2: Error: not receiving UDP ZDA...
20210412::214617: Head 1: Error: not receiving UDP ZDA...
20210412::214618: Head 2: Error: not receiving UDP ZDA...
20210412::214620: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215207_tank_dry.raa
20210412::214627: Head 1: Error: not receiving UDP ZDA...
20210412::214628: Head 2: Error: not receiving UDP ZDA...
20210412::214630: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 587
20210412::214630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214632: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215217_tank_dry.raa
20210412::214638: Head 1: Error: not receiving UDP ZDA...
20210412::214638: Head 2: Error: not receiving UDP ZDA...
20210412::214643: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215227_tank_dry.raa
20210412::214649: Head 2: Error: not receiving UDP ZDA...
20210412::214650: Head 1: Error: not receiving UDP ZDA...
20210412::214655: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215237_tank_dry.raa
20210412::214659: Head 2: Error: not receiving UDP ZDA...
20210412::214700: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 640
20210412::214700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 25.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214701: Head 1: Error: not receiving UDP ZDA...
20210412::214705: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215247_tank_dry.raa
20210412::214709: Head 2: Error: not receiving UDP ZDA...
20210412::214711: Head 1: Error: not receiving UDP ZDA...
20210412::214715: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215257_tank_dry.raa
20210412::214719: Head 2: Error: not receiving UDP ZDA...
20210412::214725: Head 1: Error: not receiving UDP ZDA...
20210412::214729: Head 2: Error: not receiving UDP ZDA...
20210412::214730: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 694
20210412::214730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214730: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215307_tank_dry.raa
20210412::214735: Head 1: Error: not receiving UDP ZDA...
20210412::214740: Head 2: Error: not receiving UDP ZDA...
20210412::214741: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215317_tank_dry.raa
20210412::214747: Head 1: Error: not receiving UDP ZDA...
20210412::214750: Head 2: Error: not receiving UDP ZDA...
20210412::214754: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215327_tank_dry.raa
20210412::214800: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 747
20210412::214800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214800: Head 1: Error: not receiving UDP ZDA...
20210412::214800: Head 2: Error: not receiving UDP ZDA...
20210412::214806: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215337_tank_dry.raa
20210412::214810: Head 1: Error: not receiving UDP ZDA...
20210412::214810: Head 2: Error: not receiving UDP ZDA...
20210412::214816: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215347_tank_dry.raa
20210412::214821: Head 2: Error: not receiving UDP ZDA...
20210412::214821: Head 1: Error: not receiving UDP ZDA...
20210412::214828: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215357_tank_dry.raa
20210412::214830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214830: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 800
20210412::214830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214831: Head 2: Error: not receiving UDP ZDA...
20210412::214832: Head 1: Error: not receiving UDP ZDA...
20210412::214839: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215407_tank_dry.raa
20210412::214841: Head 2: Error: not receiving UDP ZDA...
20210412::214842: Head 1: Error: not receiving UDP ZDA...
20210412::214851: Head 2: Error: not receiving UDP ZDA...
20210412::214851: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215417_tank_dry.raa
20210412::214854: Head 1: Error: not receiving UDP ZDA...
20210412::214900: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 853
20210412::214900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214901: Head 2: Error: not receiving UDP ZDA...
20210412::214903: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215427_tank_dry.raa
20210412::214904: Head 1: Error: not receiving UDP ZDA...
20210412::214912: Head 2: Error: not receiving UDP ZDA...
20210412::214915: Head 1: Error: not receiving UDP ZDA...
20210412::214917: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215437_tank_dry.raa
20210412::214922: Head 2: Error: not receiving UDP ZDA...
20210412::214925: Head 1: Error: not receiving UDP ZDA...
20210412::214930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214930: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 907
20210412::214930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210412::214931: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215447_tank_dry.raa
20210412::214932: Head 2: Error: not receiving UDP ZDA...
20210412::214938: Head 1: Error: not receiving UDP ZDA...
20210412::214942: Head 2: Error: not receiving UDP ZDA...
20210412::214944: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215457_tank_dry.raa
20210412::214949: Head 1: Error: not receiving UDP ZDA...
20210412::214953: Head 2: Error: not receiving UDP ZDA...
20210412::214958: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215507_tank_dry.raa
20210412::214959: Head 1: Error: not receiving UDP ZDA...
20210412::215000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215000: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 960
20210412::215000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215003: Head 2: Error: not receiving UDP ZDA...
20210412::215009: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215517_tank_dry.raa
20210412::215011: Head 1: Error: not receiving UDP ZDA...
20210412::215013: Head 2: Error: not receiving UDP ZDA...
20210412::215021: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215527_tank_dry.raa
20210412::215023: Head 2: Error: not receiving UDP ZDA...
20210412::215023: Head 1: Error: not receiving UDP ZDA...
20210412::215030: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1013
20210412::215030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 29.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 27.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215033: Head 2: Error: not receiving UDP ZDA...
20210412::215034: Head 1: Error: not receiving UDP ZDA...
20210412::215035: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215537_tank_dry.raa
20210412::215044: Head 2: Error: not receiving UDP ZDA...
20210412::215046: Head 1: Error: not receiving UDP ZDA...
20210412::215046: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215547_tank_dry.raa
20210412::215054: Head 2: Error: not receiving UDP ZDA...
20210412::215058: Head 1: Error: not receiving UDP ZDA...
20210412::215058: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215557_tank_dry.raa
20210412::215100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 28.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215100: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1067
20210412::215100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 17.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 29.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215104: Head 2: Error: not receiving UDP ZDA...
20210412::215109: Head 1: Error: not receiving UDP ZDA...
20210412::215112: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215607_tank_dry.raa
20210412::215114: Head 2: Error: not receiving UDP ZDA...
20210412::215120: Head 1: Error: not receiving UDP ZDA...
20210412::215124: Head 2: Error: not receiving UDP ZDA...
20210412::215126: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215617_tank_dry.raa
20210412::215130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215130: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1121
20210412::215130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 29.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215132: Head 1: Error: not receiving UDP ZDA...
20210412::215135: Head 2: Error: not receiving UDP ZDA...
20210412::215136: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215627_tank_dry.raa
20210412::215142: Head 1: Error: not receiving UDP ZDA...
20210412::215145: Head 2: Error: not receiving UDP ZDA...
20210412::215148: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215637_tank_dry.raa
20210412::215153: Head 1: Error: not receiving UDP ZDA...
20210412::215155: Head 2: Error: not receiving UDP ZDA...
20210412::215200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215200: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1174
20210412::215200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 20.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215200: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215647_tank_dry.raa
20210412::215205: Head 2: Error: not receiving UDP ZDA...
20210412::215206: Head 1: Error: not receiving UDP ZDA...
20210412::215214: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215657_tank_dry.raa
20210412::215216: Head 2: Error: not receiving UDP ZDA...
20210412::215219: Head 1: Error: not receiving UDP ZDA...
20210412::215225: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215707_tank_dry.raa
20210412::215226: Head 2: Error: not receiving UDP ZDA...
20210412::215229: Head 1: Error: not receiving UDP ZDA...
20210412::215230: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1228
20210412::215230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215236: Head 2: Error: not receiving UDP ZDA...
20210412::215237: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215717_tank_dry.raa
20210412::215242: Head 1: Error: not receiving UDP ZDA...
20210412::215246: Head 2: Error: not receiving UDP ZDA...
20210412::215250: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215727_tank_dry.raa
20210412::215253: Head 1: Error: not receiving UDP ZDA...
20210412::215256: Head 2: Error: not receiving UDP ZDA...
20210412::215300: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1281
20210412::215300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 29.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215303: Head 1: Error: not receiving UDP ZDA...
20210412::215304: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215737_tank_dry.raa
20210412::215307: Head 2: Error: not receiving UDP ZDA...
20210412::215314: Head 1: Error: not receiving UDP ZDA...
20210412::215314: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215747_tank_dry.raa
20210412::215317: Head 2: Error: not receiving UDP ZDA...
20210412::215324: Head 1: Error: not receiving UDP ZDA...
20210412::215324: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215757_tank_dry.raa
20210412::215327: Head 2: Error: not receiving UDP ZDA...
20210412::215330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215330: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1335
20210412::215330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 30.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215336: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215807_tank_dry.raa
20210412::215336: Head 1: Error: not receiving UDP ZDA...
20210412::215337: Head 2: Error: not receiving UDP ZDA...
20210412::215347: Head 2: Error: not receiving UDP ZDA...
20210412::215348: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215817_tank_dry.raa
20210412::215348: Head 1: Error: not receiving UDP ZDA...
20210412::215357: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215827_tank_dry.raa
20210412::215358: Head 2: Error: not receiving UDP ZDA...
20210412::215358: Head 1: Error: not receiving UDP ZDA...
20210412::215400: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1388
20210412::215400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 17.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210412::215408: Head 2: Error: not receiving UDP ZDA...
20210412::215409: Head 1: Error: not receiving UDP ZDA...
20210412::215412: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215837_tank_dry.raa
20210412::215418: Head 2: Error: not receiving UDP ZDA...
20210412::215420: Head 1: Error: not receiving UDP ZDA...
20210412::215422: GUI: Archiving data to file --> C:\Data\20210412t1\20210412_215847_tank_dry.raa
20210412::215428: GUI: Live mode ON.
20210412::215428: GUI: Requesing STOP operation, Head 2
20210412::215428: GUI: Requesing STOP operation, Head 1
20210412::215428: Head 2: Received request: STOP
20210412::215428: Head 1: Received request: STOP
20210412::215428: Head 2: Stopping Scan Operation
20210412::215428: Head 1: Stopping Scan Operation
20210412::215428: Head 2: Error: not receiving UDP ZDA...
20210412::215430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 29.0C, Dig 46.0C, Scan Az fault 0, gain 3, laser state 0
20210412::215430: System  Initialized, Gain 4, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1441
20210412::215430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 0
20210412::215430: Head 2: ProcessingMgr stopped all worker threads.
20210412::215430: Head 1: ProcessingMgr stopped all worker threads.
20210412::215431: Head 2:       Stop finished, may now recover.
20210412::215431: Head 1:       Stop finished, may now recover.
20210412::215431: Head 1: Error: not receiving UDP ZDA...
20210412::215432: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210412::215433: Head 2: Eye Safe Optical Filter check Passed
20210412::215434: Head 1: Eye Safe Optical Filter State there 10, not there 20, transition 1
20210412::215435: Head 1: Eye Safe Optical Filter check Passed
20210412::215438: Head 2: Error: not receiving UDP ZDA...
20210412::215441: Head 1: Error: not receiving UDP ZDA...
20210412::215456: GUI: Lost Communications with Sensor 1.
20210412::215457: GUI: Lost Communications with Head 2.
20210412::215509: GUI: Attempting Communications with Head 1...
20210412::215509: GUI: Attempting Communications with Head 2...
