20210414::200845: GUI: OnBnClickedOk
20210414::200845: GUI: Exiting the WiSSL GUI..
20210414::200845: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::200845: GUI: Wrote configuration data.
20210414::200849: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::200849: GUI: Live mode ON.
20210414::200849: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::200849: GUI: WiSSL GUI started at 2021_04_14_20:08:49
20210414::200849: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::200850: GUI: Attempting Communications with Head 1...
20210414::200850: GUI: Attempting Communications with Head 2...
20210414::200850: GUI: Established Communications with Head 1.
20210414::200851: Head 1: Initializing Communications with GUI ...
20210414::200852: Head 1: Communications Established.
20210414::200853: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::200853: GUI: Established Communications with Head 2.
20210414::200853: Head 1: Connection Established with the GUI.
20210414::200853: Head 1: Initializing Subsystems, standby ...
20210414::200854: Head 1: Initializing Hardware, Stand by ...
20210414::200854: Head 2: Initializing Communications with GUI ...
20210414::200854: Head 2: Communications Established.
20210414::200855: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::200856: Head 2: Connection Established with the GUI.
20210414::200856: Head 2: Initializing Subsystems, standby ...
20210414::200856: Head 2: Initializing Hardware, Stand by ...
20210414::200900: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210414::200900: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 17
20210414::200900: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210414::200903: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::200903: Head 1: NtQuery - testing 1 ...
20210414::200904: Head 1: clock resolution: 10
20210414::200904: Head 1: NtQuery - testing 2, after setting max res ...
20210414::200904: Head 1: clock resolution: 10
20210414::200905: Head 1: Initializing Optics Electronics ...
20210414::200905: Head 1: Power Laser Controller
20210414::200907: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::200907: Head 2: NtQuery - testing 1 ...
20210414::200907: Head 2: clock resolution: 10
20210414::200908: Head 2: NtQuery - testing 2, after setting max res ...
20210414::200908: Head 2: clock resolution: 10
20210414::200908: Head 2: Initializing Optics Electronics ...
20210414::200909: Head 1: Power Scanner Controller
20210414::200909: Head 2: Power Laser Controller
20210414::200911: Head 1: Power OPTO Sensor
20210414::200912: Head 2: Power Scanner Controller
20210414::200915: Head 2: Power OPTO Sensor
20210414::200930: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::200930: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 71
20210414::200930: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::200931: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::200931: Head 1: Eye Safe Optical Filter check Passed
20210414::200931: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210414::200932: Head 1: Initializing Time Sync Subsystem.
20210414::200932: Head 1: Initializing CTD Subsystem.
20210414::200932: Head 1: CTD Initialization Successful
20210414::200933: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210414::200933: Head 1: Time Sync UDP started, waiting for sync...
20210414::200933: Head 1: Attempting CTD Ethernet connection with ROV...
20210414::200935: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::200935: Head 2: Eye Safe Optical Filter check Passed
20210414::200935: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210414::200936: Head 2: Initializing Time Sync Subsystem.
20210414::200936: Head 2: Initializing CTD Subsystem.
20210414::200936: Head 2: CTD Initialization Successful
20210414::200936: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210414::200937: Head 2: Time Sync UDP started, waiting for sync...
20210414::200937: Head 2: Attempting CTD Ethernet connection with ROV...
20210414::200942: Head 1: Error: not receiving UDP ZDA...
20210414::200945: Head 2: Error: not receiving UDP ZDA...
20210414::200952: Head 1: Error: not receiving UDP ZDA...
20210414::200956: Head 2: Error: not receiving UDP ZDA...
20210414::201000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 18C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201000: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 125
20210414::201000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 19C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201002: Head 1: Error: not receiving UDP ZDA...
20210414::201006: Head 2: Error: not receiving UDP ZDA...
20210414::201012: Head 1: Error: not receiving UDP ZDA...
20210414::201016: Head 2: Error: not receiving UDP ZDA...
20210414::201022: Head 1: Error: not receiving UDP ZDA...
20210414::201026: Head 2: Error: not receiving UDP ZDA...
20210414::201030: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 178
20210414::201030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 26%, OPB 20C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 26%, OPB 19C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201033: Head 1: Error: not receiving UDP ZDA...
20210414::201036: Head 2: Error: not receiving UDP ZDA...
20210414::201043: Head 1: Error: not receiving UDP ZDA...
20210414::201047: Head 2: Error: not receiving UDP ZDA...
20210414::201053: Head 1: Error: not receiving UDP ZDA...
20210414::201057: Head 2: Error: not receiving UDP ZDA...
20210414::201100: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 231
20210414::201100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 20C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 19C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201103: Head 1: Error: not receiving UDP ZDA...
20210414::201107: Head 2: Error: not receiving UDP ZDA...
20210414::201114: Head 1: Error: not receiving UDP ZDA...
20210414::201117: Head 2: Error: not receiving UDP ZDA...
20210414::201124: Head 1: Error: not receiving UDP ZDA...
20210414::201128: Head 2: Error: not receiving UDP ZDA...
20210414::201130: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 284
20210414::201130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201134: Head 1: Error: not receiving UDP ZDA...
20210414::201138: Head 2: Error: not receiving UDP ZDA...
20210414::201144: Head 1: Error: not receiving UDP ZDA...
20210414::201148: Head 2: Error: not receiving UDP ZDA...
20210414::201154: Head 1: Error: not receiving UDP ZDA...
20210414::201158: Head 2: Error: not receiving UDP ZDA...
20210414::201200: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 338
20210414::201200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201205: Head 1: Error: not receiving UDP ZDA...
20210414::201208: Head 2: Error: not receiving UDP ZDA...
20210414::201215: Head 1: Error: not receiving UDP ZDA...
20210414::201219: Head 2: Error: not receiving UDP ZDA...
20210414::201225: Head 1: Error: not receiving UDP ZDA...
20210414::201229: Head 2: Error: not receiving UDP ZDA...
20210414::201230: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 391
20210414::201230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201235: Head 1: Error: not receiving UDP ZDA...
20210414::201239: Head 2: Error: not receiving UDP ZDA...
20210414::201245: GUI: OnBnClickedOk
20210414::201245: GUI: Exiting the WiSSL GUI..
20210414::201245: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::201245: GUI: Wrote configuration data.
20210414::201257: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::201257: GUI: Live mode ON.
20210414::201257: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::201257: GUI: WiSSL GUI started at 2021_04_14_20:12:57
20210414::201257: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::201257: GUI: Attempting Communications with Head 1...
20210414::201257: GUI: Attempting Communications with Head 2...
20210414::201305: GUI: Established Communications with Head 2.
20210414::201305: GUI: Established Communications with Head 1.
20210414::201306: Head 1: Error: not receiving UDP ZDA...
20210414::201306: Head 2: Lost Communications with GUI
20210414::201306: Head 1: Lost Communications with GUI
20210414::201306: Head 2: Initializing Communications with GUI ...
20210414::201307: Head 1: Initializing Communications with GUI ...
20210414::201307: Head 2: Error: not receiving UDP ZDA...
20210414::201307: Head 1: Error: not receiving UDP ZDA...
20210414::201307: Head 2: Error: not receiving UDP ZDA...
20210414::201307: Head 1: Error: not receiving UDP ZDA...
20210414::201307: Head 2: Communications Established.
20210414::201308: Head 1: Communications Established.
20210414::201310: Head 2: Error: not receiving UDP ZDA...
20210414::201316: Head 1: Error: not receiving UDP ZDA...
20210414::201320: Head 2: Error: not receiving UDP ZDA...
20210414::201326: Head 1: Error: not receiving UDP ZDA...
20210414::201330: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 468
20210414::201330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201330: Head 2: Error: not receiving UDP ZDA...
20210414::201330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201336: Head 1: Error: not receiving UDP ZDA...
20210414::201340: Head 2: Error: not receiving UDP ZDA...
20210414::201347: Head 1: Error: not receiving UDP ZDA...
20210414::201350: Head 2: Error: not receiving UDP ZDA...
20210414::201357: Head 1: Error: not receiving UDP ZDA...
20210414::201400: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 521
20210414::201400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201401: Head 2: Error: not receiving UDP ZDA...
20210414::201407: Head 1: Error: not receiving UDP ZDA...
20210414::201411: Head 2: Error: not receiving UDP ZDA...
20210414::201417: Head 1: Error: not receiving UDP ZDA...
20210414::201421: Head 2: Error: not receiving UDP ZDA...
20210414::201427: Head 1: Error: not receiving UDP ZDA...
20210414::201430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201430: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 575
20210414::201430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201431: Head 2: Error: not receiving UDP ZDA...
20210414::201438: Head 1: Error: not receiving UDP ZDA...
20210414::201441: Head 2: Error: not receiving UDP ZDA...
20210414::201448: Head 1: Error: not receiving UDP ZDA...
20210414::201452: Head 2: Error: not receiving UDP ZDA...
20210414::201458: Head 1: Error: not receiving UDP ZDA...
20210414::201500: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 628
20210414::201500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201502: Head 2: Error: not receiving UDP ZDA...
20210414::201508: Head 1: Error: not receiving UDP ZDA...
20210414::201512: Head 2: Error: not receiving UDP ZDA...
20210414::201518: Head 1: Error: not receiving UDP ZDA...
20210414::201522: Head 2: Error: not receiving UDP ZDA...
20210414::201529: Head 1: Error: not receiving UDP ZDA...
20210414::201530: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 681
20210414::201530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201532: Head 2: Error: not receiving UDP ZDA...
20210414::201539: Head 1: Error: not receiving UDP ZDA...
20210414::201543: Head 2: Error: not receiving UDP ZDA...
20210414::201549: Head 1: Error: not receiving UDP ZDA...
20210414::201553: Head 2: Error: not receiving UDP ZDA...
20210414::201559: Head 1: Error: not receiving UDP ZDA...
20210414::201600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 735
20210414::201600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201603: Head 2: Error: not receiving UDP ZDA...
20210414::201609: Head 1: Error: not receiving UDP ZDA...
20210414::201613: Head 2: Error: not receiving UDP ZDA...
20210414::201620: Head 1: Error: not receiving UDP ZDA...
20210414::201623: Head 2: Error: not receiving UDP ZDA...
20210414::201630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 788
20210414::201630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201630: Head 1: Error: not receiving UDP ZDA...
20210414::201630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201634: Head 2: Error: not receiving UDP ZDA...
20210414::201640: Head 1: Error: not receiving UDP ZDA...
20210414::201644: Head 2: Error: not receiving UDP ZDA...
20210414::201650: Head 1: Error: not receiving UDP ZDA...
20210414::201654: Head 2: Error: not receiving UDP ZDA...
20210414::201700: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 841
20210414::201700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201701: Head 1: Error: not receiving UDP ZDA...
20210414::201704: Head 2: Error: not receiving UDP ZDA...
20210414::201711: Head 1: Error: not receiving UDP ZDA...
20210414::201714: Head 2: Error: not receiving UDP ZDA...
20210414::201721: Head 1: Error: not receiving UDP ZDA...
20210414::201725: Head 2: Error: not receiving UDP ZDA...
20210414::201730: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 895
20210414::201730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201731: Head 1: Error: not receiving UDP ZDA...
20210414::201735: Head 2: Error: not receiving UDP ZDA...
20210414::201741: Head 1: Error: not receiving UDP ZDA...
20210414::201745: Head 2: Error: not receiving UDP ZDA...
20210414::201751: Head 1: Error: not receiving UDP ZDA...
20210414::201755: Head 2: Error: not receiving UDP ZDA...
20210414::201800: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 948
20210414::201800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201802: Head 1: Error: not receiving UDP ZDA...
20210414::201805: Head 2: Error: not receiving UDP ZDA...
20210414::201812: Head 1: Error: not receiving UDP ZDA...
20210414::201816: Head 2: Error: not receiving UDP ZDA...
20210414::201822: Head 1: Error: not receiving UDP ZDA...
20210414::201826: Head 2: Error: not receiving UDP ZDA...
20210414::201830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201830: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1002
20210414::201830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210414::201832: Head 1: Error: not receiving UDP ZDA...
20210414::201836: Head 2: Error: not receiving UDP ZDA...
20210414::201843: Head 1: Error: not receiving UDP ZDA...
20210414::201846: Head 2: Error: not receiving UDP ZDA...
20210414::201850: GUI: OnBnClickedOk
20210414::201850: GUI: Exiting the WiSSL GUI..
20210414::201850: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::201850: GUI: Wrote configuration data.
20210414::212439: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::212439: GUI: Live mode ON.
20210414::212440: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::212440: GUI: WiSSL GUI started at 2021_04_14_21:24:40
20210414::212440: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::212440: GUI: Attempting Communications with Head 1...
20210414::212440: GUI: Attempting Communications with Head 2...
20210414::212443: GUI: Established Communications with Head 1.
20210414::212443: GUI: Established Communications with Head 2.
20210414::212444: Head 1: Initializing Communications with GUI ...
20210414::212444: Head 2: Initializing Communications with GUI ...
20210414::212445: Head 2: Communications Established.
20210414::212445: Head 1: Communications Established.
20210414::212446: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::212446: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::212446: Head 2: Connection Established with the GUI.
20210414::212447: Head 1: Connection Established with the GUI.
20210414::212447: Head 2: Initializing Subsystems, standby ...
20210414::212447: Head 1: Initializing Subsystems, standby ...
20210414::212447: Head 2: Initializing Hardware, Stand by ...
20210414::212447: Head 1: Initializing Hardware, Stand by ...
20210414::212456: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::212457: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::212457: Head 1: NtQuery - testing 1 ...
20210414::212457: Head 2: NtQuery - testing 1 ...
20210414::212457: Head 1: clock resolution: 10
20210414::212457: Head 2: clock resolution: 10
20210414::212457: Head 1: NtQuery - testing 2, after setting max res ...
20210414::212458: Head 2: NtQuery - testing 2, after setting max res ...
20210414::212458: Head 1: clock resolution: 10
20210414::212458: Head 2: clock resolution: 10
20210414::212458: Head 1: Initializing Optics Electronics ...
20210414::212458: Head 2: Initializing Optics Electronics ...
20210414::212458: Head 1: Power Laser Controller
20210414::212458: Head 2: Power Laser Controller
20210414::212500: System NOT Initialized, Gain 0, Elec PB 30.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 35
20210414::212500: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212500: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212502: Head 1: Power Scanner Controller
20210414::212502: Head 2: Power Scanner Controller
20210414::212504: Head 1: Power OPTO Sensor
20210414::212504: Head 2: Power OPTO Sensor
20210414::212524: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::212524: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::212525: Head 1: Eye Safe Optical Filter check Passed
20210414::212525: Head 2: Eye Safe Optical Filter check Passed
20210414::212525: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210414::212525: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210414::212525: Head 1: Initializing Time Sync Subsystem.
20210414::212525: Head 2: Initializing Time Sync Subsystem.
20210414::212525: Head 1: Initializing CTD Subsystem.
20210414::212526: Head 2: Initializing CTD Subsystem.
20210414::212526: Head 1: CTD Initialization Successful
20210414::212526: Head 2: CTD Initialization Successful
20210414::212526: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210414::212526: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210414::212526: Head 1: Time Sync UDP started, waiting for sync...
20210414::212527: Head 2: Time Sync UDP started, waiting for sync...
20210414::212527: Head 1: Attempting CTD Ethernet connection with ROV...
20210414::212527: Head 2: Attempting CTD Ethernet connection with ROV...
20210414::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 18C, Laser 0.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212530: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 89
20210414::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 19C, Laser 0.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212535: Head 1: Error: not receiving UDP ZDA...
20210414::212535: Head 2: Error: not receiving UDP ZDA...
20210414::212545: Head 1: Error: not receiving UDP ZDA...
20210414::212545: Head 2: Error: not receiving UDP ZDA...
20210414::212555: Head 1: Error: not receiving UDP ZDA...
20210414::212556: Head 2: Error: not receiving UDP ZDA...
20210414::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 24%, OPB 19C, Laser 19.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212600: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 142
20210414::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 24%, OPB 20C, Laser 20.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212606: Head 1: Error: not receiving UDP ZDA...
20210414::212606: Head 2: Error: not receiving UDP ZDA...
20210414::212616: Head 1: Error: not receiving UDP ZDA...
20210414::212616: Head 2: Error: not receiving UDP ZDA...
20210414::212626: Head 1: Error: not receiving UDP ZDA...
20210414::212626: Head 2: Error: not receiving UDP ZDA...
20210414::212630: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 195
20210414::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 20.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212636: Head 1: Error: not receiving UDP ZDA...
20210414::212636: Head 2: Error: not receiving UDP ZDA...
20210414::212646: Head 1: Error: not receiving UDP ZDA...
20210414::212647: Head 2: Error: not receiving UDP ZDA...
20210414::212657: Head 1: Error: not receiving UDP ZDA...
20210414::212657: Head 2: Error: not receiving UDP ZDA...
20210414::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 19C, Laser 21.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212700: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 249
20210414::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 20C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212707: Head 1: Error: not receiving UDP ZDA...
20210414::212707: Head 2: Error: not receiving UDP ZDA...
20210414::212717: Head 1: Error: not receiving UDP ZDA...
20210414::212717: Head 2: Error: not receiving UDP ZDA...
20210414::212727: Head 1: Error: not receiving UDP ZDA...
20210414::212727: Head 2: Error: not receiving UDP ZDA...
20210414::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 19C, Laser 22.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212730: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 302
20210414::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 20C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212737: Head 1: Error: not receiving UDP ZDA...
20210414::212738: Head 2: Error: not receiving UDP ZDA...
20210414::212748: Head 1: Error: not receiving UDP ZDA...
20210414::212748: Head 2: Error: not receiving UDP ZDA...
20210414::212758: Head 1: Error: not receiving UDP ZDA...
20210414::212758: Head 2: Error: not receiving UDP ZDA...
20210414::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 19C, Laser 22.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212800: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 356
20210414::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 20C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212808: Head 1: Error: not receiving UDP ZDA...
20210414::212808: Head 2: Error: not receiving UDP ZDA...
20210414::212818: Head 1: Error: not receiving UDP ZDA...
20210414::212818: Head 2: Error: not receiving UDP ZDA...
20210414::212828: Head 1: Error: not receiving UDP ZDA...
20210414::212829: Head 2: Error: not receiving UDP ZDA...
20210414::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 19C, Laser 21.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212830: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 409
20210414::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 20C, Laser 23.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212839: Head 1: Error: not receiving UDP ZDA...
20210414::212839: Head 2: Error: not receiving UDP ZDA...
20210414::212849: Head 1: Error: not receiving UDP ZDA...
20210414::212849: Head 2: Error: not receiving UDP ZDA...
20210414::212859: Head 1: Error: not receiving UDP ZDA...
20210414::212859: Head 2: Error: not receiving UDP ZDA...
20210414::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 20C, Laser 22.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212900: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 462
20210414::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 20C, Laser 24.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212909: Head 1: Error: not receiving UDP ZDA...
20210414::212909: Head 2: Error: not receiving UDP ZDA...
20210414::212919: Head 1: Error: not receiving UDP ZDA...
20210414::212920: Head 2: Error: not receiving UDP ZDA...
20210414::212930: Head 1: Error: not receiving UDP ZDA...
20210414::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 23.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212930: Head 2: Error: not receiving UDP ZDA...
20210414::212930: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 516
20210414::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 20C, Laser 24.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::212940: Head 1: Error: not receiving UDP ZDA...
20210414::212940: Head 2: Error: not receiving UDP ZDA...
20210414::212950: Head 1: Error: not receiving UDP ZDA...
20210414::212950: Head 2: Error: not receiving UDP ZDA...
20210414::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 23.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213000: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 569
20210414::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213000: Head 1: Error: not receiving UDP ZDA...
20210414::213000: Head 2: Error: not receiving UDP ZDA...
20210414::213010: Head 1: Error: not receiving UDP ZDA...
20210414::213011: Head 2: Error: not receiving UDP ZDA...
20210414::213021: Head 1: Error: not receiving UDP ZDA...
20210414::213021: Head 2: Error: not receiving UDP ZDA...
20210414::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 23.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213030: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 623
20210414::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 24.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213031: Head 1: Error: not receiving UDP ZDA...
20210414::213031: Head 2: Error: not receiving UDP ZDA...
20210414::213041: Head 1: Error: not receiving UDP ZDA...
20210414::213041: Head 2: Error: not receiving UDP ZDA...
20210414::213051: Head 1: Error: not receiving UDP ZDA...
20210414::213051: Head 2: Error: not receiving UDP ZDA...
20210414::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 23.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213100: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 676
20210414::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 25.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213102: Head 1: Error: not receiving UDP ZDA...
20210414::213102: Head 2: Error: not receiving UDP ZDA...
20210414::213112: Head 1: Error: not receiving UDP ZDA...
20210414::213112: Head 2: Error: not receiving UDP ZDA...
20210414::213122: Head 1: Error: not receiving UDP ZDA...
20210414::213122: Head 2: Error: not receiving UDP ZDA...
20210414::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 24.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213130: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 729
20210414::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 25.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213132: Head 1: Error: not receiving UDP ZDA...
20210414::213132: Head 2: Error: not receiving UDP ZDA...
20210414::213142: Head 1: Error: not receiving UDP ZDA...
20210414::213143: Head 2: Error: not receiving UDP ZDA...
20210414::213152: Head 1: Error: not receiving UDP ZDA...
20210414::213153: Head 2: Error: not receiving UDP ZDA...
20210414::213200: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 783
20210414::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 25.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 24.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213203: Head 1: Error: not receiving UDP ZDA...
20210414::213203: Head 2: Error: not receiving UDP ZDA...
20210414::213213: Head 1: Error: not receiving UDP ZDA...
20210414::213213: Head 2: Error: not receiving UDP ZDA...
20210414::213223: Head 1: Error: not receiving UDP ZDA...
20210414::213223: Head 2: Error: not receiving UDP ZDA...
20210414::213230: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 836
20210414::213230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 25.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 24.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213233: Head 1: Error: not receiving UDP ZDA...
20210414::213233: Head 2: Error: not receiving UDP ZDA...
20210414::213243: Head 1: Error: not receiving UDP ZDA...
20210414::213244: Head 2: Error: not receiving UDP ZDA...
20210414::213254: Head 1: Error: not receiving UDP ZDA...
20210414::213254: Head 2: Error: not receiving UDP ZDA...
20210414::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213300: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 890
20210414::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213304: Head 1: Error: not receiving UDP ZDA...
20210414::213304: Head 2: Error: not receiving UDP ZDA...
20210414::213314: Head 1: Error: not receiving UDP ZDA...
20210414::213314: Head 2: Error: not receiving UDP ZDA...
20210414::213324: Head 1: Error: not receiving UDP ZDA...
20210414::213325: Head 2: Error: not receiving UDP ZDA...
20210414::213330: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 943
20210414::213330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213335: Head 1: Error: not receiving UDP ZDA...
20210414::213335: Head 2: Error: not receiving UDP ZDA...
20210414::213345: Head 1: Error: not receiving UDP ZDA...
20210414::213345: Head 2: Error: not receiving UDP ZDA...
20210414::213355: Head 1: Error: not receiving UDP ZDA...
20210414::213355: Head 2: Error: not receiving UDP ZDA...
20210414::213400: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 996
20210414::213400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213405: Head 1: Error: not receiving UDP ZDA...
20210414::213405: Head 2: Error: not receiving UDP ZDA...
20210414::213415: Head 1: Error: not receiving UDP ZDA...
20210414::213416: Head 2: Error: not receiving UDP ZDA...
20210414::213426: Head 1: Error: not receiving UDP ZDA...
20210414::213426: Head 2: Error: not receiving UDP ZDA...
20210414::213430: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1050
20210414::213430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213436: Head 1: Error: not receiving UDP ZDA...
20210414::213436: Head 2: Error: not receiving UDP ZDA...
20210414::213446: Head 1: Error: not receiving UDP ZDA...
20210414::213446: Head 2: Error: not receiving UDP ZDA...
20210414::213456: Head 1: Error: not receiving UDP ZDA...
20210414::213456: Head 2: Error: not receiving UDP ZDA...
20210414::213500: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1103
20210414::213500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213506: Head 1: Error: not receiving UDP ZDA...
20210414::213507: Head 2: Error: not receiving UDP ZDA...
20210414::213517: Head 1: Error: not receiving UDP ZDA...
20210414::213517: Head 2: Error: not receiving UDP ZDA...
20210414::213527: Head 1: Error: not receiving UDP ZDA...
20210414::213527: Head 2: Error: not receiving UDP ZDA...
20210414::213530: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1156
20210414::213530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213537: Head 1: Error: not receiving UDP ZDA...
20210414::213537: Head 2: Error: not receiving UDP ZDA...
20210414::213547: Head 1: Error: not receiving UDP ZDA...
20210414::213547: Head 2: Error: not receiving UDP ZDA...
20210414::213557: Head 1: Error: not receiving UDP ZDA...
20210414::213558: Head 2: Error: not receiving UDP ZDA...
20210414::213600: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1210
20210414::213600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213608: Head 1: Error: not receiving UDP ZDA...
20210414::213608: Head 2: Error: not receiving UDP ZDA...
20210414::213618: Head 2: Error: not receiving UDP ZDA...
20210414::213619: Head 1: Error: not receiving UDP ZDA...
20210414::213630: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1263
20210414::213630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213630: Head 1: Error: not receiving UDP ZDA...
20210414::213630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213630: Head 2: Error: not receiving UDP ZDA...
20210414::213640: Head 1: Error: not receiving UDP ZDA...
20210414::213640: Head 2: Error: not receiving UDP ZDA...
20210414::213650: Head 1: Error: not receiving UDP ZDA...
20210414::213650: Head 2: Error: not receiving UDP ZDA...
20210414::213659: Head 2: CTD Ethernet connection established.
20210414::213659: Head 1: CTD Ethernet connection established.
20210414::213700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213700: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1317
20210414::213700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213700: Head 1: Error: not receiving UDP ZDA...
20210414::213701: Head 2: Error: not receiving UDP ZDA...
20210414::213711: Head 1: Error: not receiving UDP ZDA...
20210414::213711: Head 2: Error: not receiving UDP ZDA...
20210414::213721: Head 1: Error: not receiving UDP ZDA...
20210414::213721: Head 2: Error: not receiving UDP ZDA...
20210414::213730: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1370
20210414::213730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213731: Head 1: Error: not receiving UDP ZDA...
20210414::213731: Head 2: Error: not receiving UDP ZDA...
20210414::213741: Head 1: Error: not receiving UDP ZDA...
20210414::213741: Head 2: Error: not receiving UDP ZDA...
20210414::213751: Head 1: Error: not receiving UDP ZDA...
20210414::213752: Head 2: Error: not receiving UDP ZDA...
20210414::213800: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1423
20210414::213800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213802: Head 1: Error: not receiving UDP ZDA...
20210414::213802: Head 2: Error: not receiving UDP ZDA...
20210414::213812: Head 1: Error: not receiving UDP ZDA...
20210414::213812: Head 2: Error: not receiving UDP ZDA...
20210414::213822: Head 1: Error: not receiving UDP ZDA...
20210414::213822: Head 2: Error: not receiving UDP ZDA...
20210414::213830: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1477
20210414::213830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213832: Head 1: Error: not receiving UDP ZDA...
20210414::213832: Head 2: Error: not receiving UDP ZDA...
20210414::213843: Head 1: Error: not receiving UDP ZDA...
20210414::213843: Head 2: Error: not receiving UDP ZDA...
20210414::213853: Head 1: Error: not receiving UDP ZDA...
20210414::213853: Head 2: Error: not receiving UDP ZDA...
20210414::213900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213900: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1530
20210414::213900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213903: Head 1: Error: not receiving UDP ZDA...
20210414::213903: Head 2: Error: not receiving UDP ZDA...
20210414::213914: Head 1: Error: not receiving UDP ZDA...
20210414::213914: Head 2: Error: not receiving UDP ZDA...
20210414::213924: Head 1: Error: not receiving UDP ZDA...
20210414::213924: Head 2: Error: not receiving UDP ZDA...
20210414::213930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213930: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1583
20210414::213930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::213934: Head 1: Error: not receiving UDP ZDA...
20210414::213934: Head 2: Error: not receiving UDP ZDA...
20210414::213944: Head 1: Error: not receiving UDP ZDA...
20210414::213945: Head 2: Error: not receiving UDP ZDA...
20210414::213949: Head 1: Comm CTD Error, disconnecting
20210414::213949: Head 2: Comm CTD Error, disconnecting
20210414::213950: Head 1: Warning, CTD not recieved within 2 minutes.
20210414::213950: Head 2: Warning, CTD not recieved within 2 minutes.
20210414::213950: Head 1: Restarting CTD Ethernet connection ...
20210414::213950: Head 2: Restarting CTD Ethernet connection ...
20210414::213955: Head 1: Error: not receiving UDP ZDA...
20210414::213955: Head 2: Error: not receiving UDP ZDA...
20210414::214000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214000: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1637
20210414::214000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214005: Head 1: Error: not receiving UDP ZDA...
20210414::214005: Head 2: Error: not receiving UDP ZDA...
20210414::214015: Head 1: Error: not receiving UDP ZDA...
20210414::214015: Head 2: Error: not receiving UDP ZDA...
20210414::214025: Head 1: Error: not receiving UDP ZDA...
20210414::214025: Head 2: Error: not receiving UDP ZDA...
20210414::214030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214030: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1690
20210414::214030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214035: Head 1: Error: not receiving UDP ZDA...
20210414::214036: Head 2: Error: not receiving UDP ZDA...
20210414::214046: Head 1: Error: not receiving UDP ZDA...
20210414::214046: Head 2: Error: not receiving UDP ZDA...
20210414::214056: Head 1: Error: not receiving UDP ZDA...
20210414::214056: Head 2: Error: not receiving UDP ZDA...
20210414::214100: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1743
20210414::214100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214106: Head 1: Error: not receiving UDP ZDA...
20210414::214106: Head 2: Error: not receiving UDP ZDA...
20210414::214116: Head 1: Error: not receiving UDP ZDA...
20210414::214116: Head 2: Error: not receiving UDP ZDA...
20210414::214126: Head 1: Error: not receiving UDP ZDA...
20210414::214127: Head 2: Error: not receiving UDP ZDA...
20210414::214130: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1797
20210414::214130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214137: Head 1: Error: not receiving UDP ZDA...
20210414::214137: Head 2: Error: not receiving UDP ZDA...
20210414::214147: Head 1: Error: not receiving UDP ZDA...
20210414::214147: Head 2: Error: not receiving UDP ZDA...
20210414::214157: Head 1: Error: not receiving UDP ZDA...
20210414::214157: Head 2: Error: not receiving UDP ZDA...
20210414::214200: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1850
20210414::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214207: Head 1: Error: not receiving UDP ZDA...
20210414::214207: Head 2: Error: not receiving UDP ZDA...
20210414::214217: Head 1: Error: not receiving UDP ZDA...
20210414::214218: Head 2: Error: not receiving UDP ZDA...
20210414::214220: Head 2: CTD Ethernet connection established.
20210414::214220: Head 1: CTD Ethernet connection established.
20210414::214228: Head 1: Error: not receiving UDP ZDA...
20210414::214228: Head 2: Error: not receiving UDP ZDA...
20210414::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214230: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1904
20210414::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214238: Head 1: Error: not receiving UDP ZDA...
20210414::214238: Head 2: Error: not receiving UDP ZDA...
20210414::214248: Head 1: Error: not receiving UDP ZDA...
20210414::214248: Head 2: Error: not receiving UDP ZDA...
20210414::214257: Head 2: Comm CTD Error, disconnecting
20210414::214257: Head 1: Comm CTD Error, disconnecting
20210414::214257: Head 2: Restarting CTD Ethernet connection ...
20210414::214257: Head 1: Restarting CTD Ethernet connection ...
20210414::214258: Head 1: Error: not receiving UDP ZDA...
20210414::214259: Head 2: Error: not receiving UDP ZDA...
20210414::214300: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1957
20210414::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214309: Head 1: Error: not receiving UDP ZDA...
20210414::214309: Head 2: Error: not receiving UDP ZDA...
20210414::214310: GUI: OnBnClickedOk
20210414::214310: GUI: Exiting the WiSSL GUI..
20210414::214310: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::214310: GUI: Wrote configuration data.
20210414::214325: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::214325: GUI: Live mode ON.
20210414::214325: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::214325: GUI: WiSSL GUI started at 2021_04_14_21:43:25
20210414::214325: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::214325: GUI: Attempting Communications with Head 2...
20210414::214325: GUI: Attempting Communications with Head 1...
20210414::214325: GUI: Established Communications with Head 2.
20210414::214325: GUI: Established Communications with Head 1.
20210414::214326: Head 1: Lost Communications with GUI
20210414::214326: Head 2: Lost Communications with GUI
20210414::214326: Head 1: Initializing Communications with GUI ...
20210414::214326: Head 2: Initializing Communications with GUI ...
20210414::214327: Head 1: Error: not receiving UDP ZDA...
20210414::214327: Head 2: Error: not receiving UDP ZDA...
20210414::214327: Head 2: Communications Established.
20210414::214327: Head 1: Communications Established.
20210414::214329: Head 1: Error: not receiving UDP ZDA...
20210414::214329: Head 2: Error: not receiving UDP ZDA...
20210414::214339: Head 1: Error: not receiving UDP ZDA...
20210414::214339: Head 2: Error: not receiving UDP ZDA...
20210414::214349: Head 1: Error: not receiving UDP ZDA...
20210414::214350: Head 2: Error: not receiving UDP ZDA...
20210414::214354: Head 2: CTD Ethernet connection established.
20210414::214354: Head 1: CTD Ethernet connection established.
20210414::214400: Head 1: Error: not receiving UDP ZDA...
20210414::214400: Head 2: Error: not receiving UDP ZDA...
20210414::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 21C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214400: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2037
20210414::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214410: Head 1: Error: not receiving UDP ZDA...
20210414::214410: Head 2: Error: not receiving UDP ZDA...
20210414::214420: Head 1: Error: not receiving UDP ZDA...
20210414::214420: Head 2: Error: not receiving UDP ZDA...
20210414::214430: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2090
20210414::214430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 21C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214430: Head 1: Error: not receiving UDP ZDA...
20210414::214430: Head 2: Error: not receiving UDP ZDA...
20210414::214440: Head 1: Error: not receiving UDP ZDA...
20210414::214441: Head 2: Error: not receiving UDP ZDA...
20210414::214451: Head 1: Error: not receiving UDP ZDA...
20210414::214451: Head 2: Error: not receiving UDP ZDA...
20210414::214500: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2143
20210414::214500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 21C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214501: Head 1: Error: not receiving UDP ZDA...
20210414::214501: Head 2: Error: not receiving UDP ZDA...
20210414::214511: Head 1: Error: not receiving UDP ZDA...
20210414::214511: Head 2: Error: not receiving UDP ZDA...
20210414::214521: Head 1: Error: not receiving UDP ZDA...
20210414::214521: Head 2: Error: not receiving UDP ZDA...
20210414::214530: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2197
20210414::214530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214531: Head 1: Error: not receiving UDP ZDA...
20210414::214532: Head 2: Error: not receiving UDP ZDA...
20210414::214542: Head 1: Error: not receiving UDP ZDA...
20210414::214542: Head 2: Error: not receiving UDP ZDA...
20210414::214552: Head 1: Error: not receiving UDP ZDA...
20210414::214552: Head 2: Error: not receiving UDP ZDA...
20210414::214600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214600: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2250
20210414::214600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210414::214602: Head 1: Error: not receiving UDP ZDA...
20210414::214602: Head 2: Error: not receiving UDP ZDA...
20210414::214606: GUI: Live mode ON.
20210414::214606: GUI: Requesing START operation, Head 2
20210414::214606: GUI: Requesing START operation, Head 1
20210414::214606: Head 2: Received request: START
20210414::214606: Head 1: Received request: START
20210414::214606: Head 2: Starting Scan Operation
20210414::214606: Head 1: Starting Scan Operation
20210414::214608: Head 1: Eye Safe Optical Filter State there 10, not there 20, transition 1
20210414::214608: Head 1: Eye Safe Optical Filter check Passed
20210414::214609: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::214609: Head 2: Eye Safe Optical Filter check Passed
20210414::214612: Head 1: Error: not receiving UDP ZDA...
20210414::214612: Head 2: Error: not receiving UDP ZDA...
20210414::214613: Head 1: Configured for WATER Processing
20210414::214613: Head 1: Configured for WATER Processing
20210414::214613: Head 1: Configured for WATER Processing
20210414::214613: Head 2: Configured for WATER Processing
20210414::214613: Head 1: Configured for WATER Processing
20210414::214614: Head 2: Configured for WATER Processing
20210414::214614: Head 1: Configured for WATER Processing
20210414::214614: Head 2: Configured for WATER Processing
20210414::214614: Head 1: Configured for WATER Processing
20210414::214614: Head 2: Configured for WATER Processing
20210414::214614: Head 1: Configured for WATER Processing
20210414::214615: Head 2: Configured for WATER Processing
20210414::214615: Head 1: Configured for WATER Processing
20210414::214615: Head 2: Configured for WATER Processing
20210414::214615: Head 1: Configured for WATER Processing
20210414::214615: Head 2: Configured for WATER Processing
20210414::214615: Head 1: Configured for WATER Processing
20210414::214615: Head 2: Configured for WATER Processing
20210414::214616: Head 1: Configured for WATER Processing
20210414::214616: Head 2: Configured for WATER Processing
20210414::214616: Head 1: Configured for WATER Processing
20210414::214616: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215146_tank_dry.raa
20210414::214616: Head 2: Configured for WATER Processing
20210414::214616: Head 1: Configured for WATER Processing
20210414::214616: Head 2: Configured for WATER Processing
20210414::214616: Head 1: Configured for WATER Processing
20210414::214617: Head 2: Configured for WATER Processing
20210414::214617: Head 1: Configured for WATER Processing
20210414::214617: Head 2: Configured for WATER Processing
20210414::214617: Head 1: Configured for WATER Processing
20210414::214617: Head 2: Configured for WATER Processing
20210414::214617: Head 1: Configured for WATER Processing
20210414::214618: Head 2: Configured for WATER Processing
20210414::214618: Head 1: Configured for WATER Processing
20210414::214618: Head 2: Configured for WATER Processing
20210414::214618: Head 1: Configured for WATER Processing
20210414::214618: Head 2: Configured for WATER Processing
20210414::214618: Head 1: Configured for WATER Processing
20210414::214618: Head 2: Configured for WATER Processing
20210414::214619: Head 2: Configured for WATER Processing
20210414::214619: Head 2: Configured for WATER Processing
20210414::214623: Head 1: Error: not receiving UDP ZDA...
20210414::214623: Head 2: Error: not receiving UDP ZDA...
20210414::214624: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215156_tank_dry.raa
20210414::214630: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2304
20210414::214630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 18.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 30.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 28.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214633: Head 2: Error: not receiving UDP ZDA...
20210414::214635: Head 1: Error: not receiving UDP ZDA...
20210414::214637: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215206_tank_dry.raa
20210414::214643: Head 2: Error: not receiving UDP ZDA...
20210414::214647: Head 1: Error: not receiving UDP ZDA...
20210414::214653: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215216_tank_dry.raa
20210414::214653: Head 2: Error: not receiving UDP ZDA...
20210414::214658: Head 1: Error: not receiving UDP ZDA...
20210414::214700: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2357
20210414::214700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 30.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 29.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214704: Head 2: Error: not receiving UDP ZDA...
20210414::214705: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215226_tank_dry.raa
20210414::214709: Head 1: Error: not receiving UDP ZDA...
20210414::214714: Head 2: Error: not receiving UDP ZDA...
20210414::214715: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215236_tank_dry.raa
20210414::214719: Head 1: Error: not receiving UDP ZDA...
20210414::214724: Head 2: Error: not receiving UDP ZDA...
20210414::214725: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215246_tank_dry.raa
20210414::214729: Head 1: Error: not receiving UDP ZDA...
20210414::214730: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2410
20210414::214730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 29.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214734: Head 2: Error: not receiving UDP ZDA...
20210414::214735: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215256_tank_dry.raa
20210414::214740: Head 1: Error: not receiving UDP ZDA...
20210414::214744: Head 2: Error: not receiving UDP ZDA...
20210414::214745: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215306_tank_dry.raa
20210414::214750: Head 1: Error: not receiving UDP ZDA...
20210414::214755: Head 2: Error: not receiving UDP ZDA...
20210414::214755: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215316_tank_dry.raa
20210414::214800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 29.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214800: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2464
20210414::214800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214800: Head 1: Error: not receiving UDP ZDA...
20210414::214805: Head 2: Error: not receiving UDP ZDA...
20210414::214805: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215326_tank_dry.raa
20210414::214810: Head 1: Error: not receiving UDP ZDA...
20210414::214815: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215336_tank_dry.raa
20210414::214815: Head 2: Error: not receiving UDP ZDA...
20210414::214821: Head 1: Error: not receiving UDP ZDA...
20210414::214825: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215346_tank_dry.raa
20210414::214825: Head 2: Error: not receiving UDP ZDA...
20210414::214830: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2517
20210414::214830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214831: Head 1: Error: not receiving UDP ZDA...
20210414::214835: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215356_tank_dry.raa
20210414::214835: Head 2: Error: not receiving UDP ZDA...
20210414::214841: Head 1: Error: not receiving UDP ZDA...
20210414::214845: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215406_tank_dry.raa
20210414::214846: Head 2: Error: not receiving UDP ZDA...
20210414::214851: Head 1: Error: not receiving UDP ZDA...
20210414::214855: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_215416_tank_dry.raa
20210414::214856: Head 2: Error: not receiving UDP ZDA...
20210414::214900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 22C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214900: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2571
20210414::214900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::214901: GUI: Live mode ON.
20210414::214901: GUI: Requesing STOP operation, Head 2
20210414::214901: GUI: Requesing STOP operation, Head 1
20210414::214902: Head 1: Error: not receiving UDP ZDA...
20210414::214902: Head 2: Received request: STOP
20210414::214902: Head 1: Received request: STOP
20210414::214902: Head 2: Stopping Scan Operation
20210414::214902: Head 1: Stopping Scan Operation
20210414::214904: Head 1: ProcessingMgr stopped all worker threads.
20210414::214905: Head 1:       Stop finished, may now recover.
20210414::214906: Head 2: Error: not receiving UDP ZDA...
20210414::214906: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::214907: Head 1: Eye Safe Optical Filter check Passed
20210414::214909: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::214909: Head 2: Eye Safe Optical Filter check Passed
20210414::214912: Head 1: Error: not receiving UDP ZDA...
20210414::214916: Head 2: Error: not receiving UDP ZDA...
20210414::214922: Head 1: Error: not receiving UDP ZDA...
20210414::214924: GUI: OnBnClickedOk
20210414::214924: GUI: Exiting the WiSSL GUI..
20210414::214924: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::214924: GUI: Wrote configuration data.
20210414::215451: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::215451: GUI: Live mode ON.
20210414::215451: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::215451: GUI: WiSSL GUI started at 2021_04_14_21:54:51
20210414::215451: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::215451: GUI: Attempting Communications with Head 2...
20210414::215451: GUI: Attempting Communications with Head 1...
20210414::215451: GUI: Established Communications with Head 1.
20210414::215451: GUI: Established Communications with Head 2.
20210414::215452: Head 2: Lost Communications with GUI
20210414::215452: Head 1: Lost Communications with GUI
20210414::215453: Head 2: Error: not receiving UDP ZDA...
20210414::215453: Head 1: Initializing Communications with GUI ...
20210414::215453: Head 1: Error: not receiving UDP ZDA...
20210414::215453: Head 2: Initializing Communications with GUI ...
20210414::215453: Head 1: Error: not receiving UDP ZDA...
20210414::215453: Head 2: ProcessingMgr stopped all worker threads.
20210414::215453: Head 1: Error: not receiving UDP ZDA...
20210414::215453: Head 2:       Stop finished, may now recover.
20210414::215454: Head 1: Error: not receiving UDP ZDA...
20210414::215454: Head 2: Error: not receiving UDP ZDA...
20210414::215454: Head 1: Error: not receiving UDP ZDA...
20210414::215454: Head 2: Error: not receiving UDP ZDA...
20210414::215454: Head 1: Error: not receiving UDP ZDA...
20210414::215454: Head 2: Error: not receiving UDP ZDA...
20210414::215455: Head 2: Error: not receiving UDP ZDA...
20210414::215455: Head 1: Error: not receiving UDP ZDA...
20210414::215455: Head 1: Error: not receiving UDP ZDA...
20210414::215455: Head 2: Error: not receiving UDP ZDA...
20210414::215455: Head 1: Error: not receiving UDP ZDA...
20210414::215455: Head 2: Error: not receiving UDP ZDA...
20210414::215456: Head 1: Error: not receiving UDP ZDA...
20210414::215456: Head 2: Error: not receiving UDP ZDA...
20210414::215456: Head 1: Error: not receiving UDP ZDA...
20210414::215456: Head 2: Error: not receiving UDP ZDA...
20210414::215456: Head 2: Error: not receiving UDP ZDA...
20210414::215456: Head 1: Error: not receiving UDP ZDA...
20210414::215456: Head 1: Error: not receiving UDP ZDA...
20210414::215456: Head 2: Error: not receiving UDP ZDA...
20210414::215457: Head 1: Error: not receiving UDP ZDA...
20210414::215457: Head 2: Error: not receiving UDP ZDA...
20210414::215457: Head 2: Error: not receiving UDP ZDA...
20210414::215457: Head 1: Error: not receiving UDP ZDA...
20210414::215457: Head 1: Error: not receiving UDP ZDA...
20210414::215457: Head 2: Error: not receiving UDP ZDA...
20210414::215458: Head 2: Error: not receiving UDP ZDA...
20210414::215458: Head 1: Error: not receiving UDP ZDA...
20210414::215458: Head 1: Error: not receiving UDP ZDA...
20210414::215458: Head 2: Error: not receiving UDP ZDA...
20210414::215458: Head 1: Error: not receiving UDP ZDA...
20210414::215458: Head 2: Error: not receiving UDP ZDA...
20210414::215459: Head 1: Error: not receiving UDP ZDA...
20210414::215459: Head 2: Error: not receiving UDP ZDA...
20210414::215459: Head 2: Error: not receiving UDP ZDA...
20210414::215459: Head 1: Error: not receiving UDP ZDA...
20210414::215459: Head 2: Error: not receiving UDP ZDA...
20210414::215459: Head 1: Error: not receiving UDP ZDA...
20210414::215459: Head 1: Error: not receiving UDP ZDA...
20210414::215459: Head 2: Error: not receiving UDP ZDA...
20210414::215500: Head 2: Error: not receiving UDP ZDA...
20210414::215500: Head 1: Error: not receiving UDP ZDA...
20210414::215500: Head 1: Error: not receiving UDP ZDA...
20210414::215500: Head 2: Error: not receiving UDP ZDA...
20210414::215500: Head 1: Error: not receiving UDP ZDA...
20210414::215500: Head 2: Error: not receiving UDP ZDA...
20210414::215500: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2629
20210414::215500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 0, laser state 0
20210414::215500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210414::215501: Head 1: Error: not receiving UDP ZDA...
20210414::215501: Head 2: Error: not receiving UDP ZDA...
20210414::215501: Head 1: Error: not receiving UDP ZDA...
20210414::215501: Head 2: Error: not receiving UDP ZDA...
20210414::215501: Head 1: Error: not receiving UDP ZDA...
20210414::215501: Head 2: Error: not receiving UDP ZDA...
20210414::215502: Head 1: Error: not receiving UDP ZDA...
20210414::215502: Head 2: Error: not receiving UDP ZDA...
20210414::215502: Head 1: Error: not receiving UDP ZDA...
20210414::215502: Head 2: Error: not receiving UDP ZDA...
20210414::215502: Head 1: Error: not receiving UDP ZDA...
20210414::215502: Head 2: Error: not receiving UDP ZDA...
20210414::215502: Head 1: Communications Established.
20210414::215502: Head 2: Error: not receiving UDP ZDA...
20210414::215503: Head 1: Error: not receiving UDP ZDA...
20210414::215503: Head 2: Error: not receiving UDP ZDA...
20210414::215503: Head 2: Error: not receiving UDP ZDA...
20210414::215503: Head 2: Communications Established.
20210414::215504: Head 2: Error: not receiving UDP ZDA...
20210414::215508: Head 1: Error: not receiving UDP ZDA...
20210414::215512: Head 2: Error: not receiving UDP ZDA...
20210414::215518: Head 1: Error: not receiving UDP ZDA...
20210414::215522: Head 2: Error: not receiving UDP ZDA...
20210414::215528: Head 1: Error: not receiving UDP ZDA...
20210414::215529: GUI: Live mode ON.
20210414::215529: GUI: Requesing START operation, Head 1
20210414::215529: GUI: Requesing START operation, Head 2
20210414::215529: Head 1: Received request: START
20210414::215529: Head 2: Received request: START
20210414::215530: Head 1: Starting Scan Operation
20210414::215530: Head 2: Starting Scan Operation
20210414::215530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210414::215530: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2681
20210414::215530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 0, laser state 0
20210414::215531: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::215531: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::215531: Head 2: Eye Safe Optical Filter check Passed
20210414::215531: Head 1: Eye Safe Optical Filter check Passed
20210414::215533: Head 2: Error: not receiving UDP ZDA...
20210414::215536: Head 1: Configured for WATER Processing
20210414::215536: Head 1: Configured for WATER Processing
20210414::215536: Head 1: Configured for WATER Processing
20210414::215537: Head 1: Configured for WATER Processing
20210414::215537: Head 1: Configured for WATER Processing
20210414::215537: Head 1: Configured for WATER Processing
20210414::215538: Head 1: Configured for WATER Processing
20210414::215538: Head 1: Configured for WATER Processing
20210414::215538: Head 1: Configured for WATER Processing
20210414::215538: Head 1: Configured for WATER Processing
20210414::215539: Head 1: Configured for WATER Processing
20210414::215539: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220059_tank_dry.raa
20210414::215539: Head 1: Configured for WATER Processing
20210414::215539: Head 1: Configured for WATER Processing
20210414::215540: Head 1: Configured for WATER Processing
20210414::215540: Head 1: Configured for WATER Processing
20210414::215540: Head 1: Configured for WATER Processing
20210414::215541: Head 1: Configured for WATER Processing
20210414::215541: Head 1: Configured for WATER Processing
20210414::215541: Head 1: Configured for WATER Processing
20210414::215542: Head 1: Configured for WATER Processing
20210414::215542: Head 1: Error: not receiving UDP ZDA...
20210414::215543: Head 2: Error: not receiving UDP ZDA...
20210414::215547: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220109_tank_dry.raa
20210414::215548: Head 1: Error: not receiving UDP ZDA...
20210414::215553: Head 2: Error: not receiving UDP ZDA...
20210414::215557: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220119_tank_dry.raa
20210414::215558: Head 2: Configured for WATER Processing
20210414::215558: Head 2: Configured for WATER Processing
20210414::215559: Head 1: Error: not receiving UDP ZDA...
20210414::215559: Head 2: Configured for WATER Processing
20210414::215559: Head 2: Configured for WATER Processing
20210414::215559: Head 2: Configured for WATER Processing
20210414::215600: Head 2: Configured for WATER Processing
20210414::215600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215600: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2735
20210414::215600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215600: Head 2: Configured for WATER Processing
20210414::215600: Head 2: Configured for WATER Processing
20210414::215601: Head 2: Configured for WATER Processing
20210414::215601: Head 2: Configured for WATER Processing
20210414::215601: Head 2: Configured for WATER Processing
20210414::215601: Head 2: Configured for WATER Processing
20210414::215602: Head 2: Configured for WATER Processing
20210414::215602: Head 2: Configured for WATER Processing
20210414::215602: Head 2: Configured for WATER Processing
20210414::215603: Head 2: Configured for WATER Processing
20210414::215603: Head 2: Configured for WATER Processing
20210414::215603: Head 2: Configured for WATER Processing
20210414::215604: Head 2: Configured for WATER Processing
20210414::215604: Head 2: Configured for WATER Processing
20210414::215604: Head 2: Error: not receiving UDP ZDA...
20210414::215607: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220129_tank_dry.raa
20210414::215609: Head 1: Error: not receiving UDP ZDA...
20210414::215613: Head 2: Error: not receiving UDP ZDA...
20210414::215616: GUI: Range graph range changed --> 0.00m..10.00m
20210414::215617: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220139_tank_dry.raa
20210414::215619: Head 1: Error: not receiving UDP ZDA...
20210414::215624: Head 2: Error: not receiving UDP ZDA...
20210414::215627: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220149_tank_dry.raa
20210414::215630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215630: Head 1: Error: not receiving UDP ZDA...
20210414::215630: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2788
20210414::215630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 32.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215634: Head 2: Error: not receiving UDP ZDA...
20210414::215637: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220159_tank_dry.raa
20210414::215640: Head 1: Error: not receiving UDP ZDA...
20210414::215644: Head 2: Error: not receiving UDP ZDA...
20210414::215647: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220209_tank_dry.raa
20210414::215650: Head 1: Error: not receiving UDP ZDA...
20210414::215651: Head 1: Comm CTD Error, disconnecting
20210414::215651: Head 2: Comm CTD Error, disconnecting
20210414::215652: Head 1: Warning, CTD not recieved within 2 minutes.
20210414::215652: Head 2: Warning, CTD not recieved within 2 minutes.
20210414::215652: Head 1: Restarting CTD Ethernet connection ...
20210414::215652: Head 2: Restarting CTD Ethernet connection ...
20210414::215654: Head 2: Error: not receiving UDP ZDA...
20210414::215657: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220219_tank_dry.raa
20210414::215658: GUI: Live mode ON.
20210414::215658: GUI: Requesing STOP operation, Head 2
20210414::215658: GUI: Requesing STOP operation, Head 1
20210414::215658: Head 1: Received request: STOP
20210414::215658: Head 2: Received request: STOP
20210414::215658: Head 1: Stopping Scan Operation
20210414::215658: Head 2: Stopping Scan Operation
20210414::215700: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2842
20210414::215700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 0
20210414::215700: Head 1: Error: not receiving UDP ZDA...
20210414::215700: Head 2: ProcessingMgr stopped all worker threads.
20210414::215701: Head 1: ProcessingMgr stopped all worker threads.
20210414::215701: Head 2:       Stop finished, may now recover.
20210414::215701: Head 1:       Stop finished, may now recover.
20210414::215704: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::215704: Head 2: Eye Safe Optical Filter check Passed
20210414::215704: Head 2: Error: not receiving UDP ZDA...
20210414::215706: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::215707: Head 1: Eye Safe Optical Filter check Passed
20210414::215710: Head 1: Error: not receiving UDP ZDA...
20210414::215715: Head 2: Error: not receiving UDP ZDA...
20210414::215715: GUI: Live mode ON.
20210414::215715: GUI: Requesing START operation, Head 2
20210414::215715: GUI: Requesing START operation, Head 1
20210414::215715: Head 2: Received request: START
20210414::215715: Head 1: Received request: START
20210414::215716: Head 2: Starting Scan Operation
20210414::215716: Head 1: Starting Scan Operation
20210414::215717: Head 1: Eye Safe Optical Filter State there 10, not there 20, transition 1
20210414::215717: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::215717: Head 1: Eye Safe Optical Filter check Passed
20210414::215717: Head 2: Eye Safe Optical Filter check Passed
20210414::215721: Head 1: Error: not receiving UDP ZDA...
20210414::215722: Head 2: Configured for WATER Processing
20210414::215722: Head 1: Configured for WATER Processing
20210414::215722: Head 2: Configured for WATER Processing
20210414::215722: Head 1: Configured for WATER Processing
20210414::215722: Head 1: Configured for WATER Processing
20210414::215722: Head 2: Configured for WATER Processing
20210414::215722: Head 1: Configured for WATER Processing
20210414::215722: Head 2: Configured for WATER Processing
20210414::215723: Head 2: Configured for WATER Processing
20210414::215723: Head 1: Configured for WATER Processing
20210414::215723: Head 1: Configured for WATER Processing
20210414::215723: Head 2: Configured for WATER Processing
20210414::215723: Head 1: Configured for WATER Processing
20210414::215723: Head 2: Configured for WATER Processing
20210414::215724: Head 1: Configured for WATER Processing
20210414::215724: Head 2: Configured for WATER Processing
20210414::215724: Head 1: Configured for WATER Processing
20210414::215724: Head 2: Configured for WATER Processing
20210414::215724: Head 1: Configured for WATER Processing
20210414::215724: Head 2: Configured for WATER Processing
20210414::215725: Head 1: Configured for WATER Processing
20210414::215725: Head 2: Configured for WATER Processing
20210414::215725: Head 1: Configured for WATER Processing
20210414::215725: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220244_tank_dry.raa
20210414::215725: Head 2: Configured for WATER Processing
20210414::215725: Head 1: Configured for WATER Processing
20210414::215725: Head 1: Configured for WATER Processing
20210414::215725: Head 2: Configured for WATER Processing
20210414::215726: Head 1: Configured for WATER Processing
20210414::215726: Head 2: Configured for WATER Processing
20210414::215726: Head 1: Configured for WATER Processing
20210414::215726: Head 1: Configured for WATER Processing
20210414::215726: Head 2: Configured for WATER Processing
20210414::215727: Head 1: Configured for WATER Processing
20210414::215727: Head 2: Configured for WATER Processing
20210414::215727: Head 2: Configured for WATER Processing
20210414::215727: Head 1: Configured for WATER Processing
20210414::215727: Head 2: Configured for WATER Processing
20210414::215727: Head 1: Configured for WATER Processing
20210414::215728: Head 2: Configured for WATER Processing
20210414::215728: Head 2: Configured for WATER Processing
20210414::215728: Head 2: Error: not receiving UDP ZDA...
20210414::215730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215730: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2896
20210414::215730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215731: Head 1: Error: not receiving UDP ZDA...
20210414::215733: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220254_tank_dry.raa
20210414::215736: Head 2: Error: not receiving UDP ZDA...
20210414::215741: Head 1: Error: not receiving UDP ZDA...
20210414::215743: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220304_tank_dry.raa
20210414::215746: Head 2: Error: not receiving UDP ZDA...
20210414::215751: Head 1: Error: not receiving UDP ZDA...
20210414::215752: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220314_tank_dry.raa
20210414::215756: Head 2: Error: not receiving UDP ZDA...
20210414::215800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215800: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2949
20210414::215800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215802: Head 1: Error: not receiving UDP ZDA...
20210414::215803: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220324_tank_dry.raa
20210414::215806: Head 2: Error: not receiving UDP ZDA...
20210414::215812: Head 1: Error: not receiving UDP ZDA...
20210414::215813: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220334_tank_dry.raa
20210414::215817: Head 2: Error: not receiving UDP ZDA...
20210414::215822: Head 1: Error: not receiving UDP ZDA...
20210414::215823: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220344_tank_dry.raa
20210414::215827: Head 2: Error: not receiving UDP ZDA...
20210414::215830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215830: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 3003
20210414::215830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215832: Head 1: Error: not receiving UDP ZDA...
20210414::215833: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220354_tank_dry.raa
20210414::215837: Head 2: Error: not receiving UDP ZDA...
20210414::215843: Head 1: Error: not receiving UDP ZDA...
20210414::215843: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220404_tank_dry.raa
20210414::215847: Head 2: Error: not receiving UDP ZDA...
20210414::215850: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::215850: GUI: Wrote configuration data.
20210414::215853: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220414_tank_dry.raa
20210414::215853: Head 1: Error: not receiving UDP ZDA...
20210414::215857: Head 2: Error: not receiving UDP ZDA...
20210414::215900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215900: System  Initialized, Gain 4, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 3056
20210414::215900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::215901: GUI: Live mode ON.
20210414::215901: GUI: Requesing STOP operation, Head 1
20210414::215901: GUI: Requesing STOP operation, Head 2
20210414::215901: Head 1: Received request: STOP
20210414::215901: Head 2: Received request: STOP
20210414::215902: Head 1: Stopping Scan Operation
20210414::215902: Head 2: Stopping Scan Operation
20210414::215903: Head 1: Error: not receiving UDP ZDA...
20210414::215904: Head 1: ProcessingMgr stopped all worker threads.
20210414::215904: Head 1:       Stop finished, may now recover.
20210414::215908: Head 2: Error: not receiving UDP ZDA...
20210414::215910: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::215910: Head 2: Eye Safe Optical Filter check Passed
20210414::215910: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::215910: Head 1: Eye Safe Optical Filter check Passed
20210414::215913: Head 1: Error: not receiving UDP ZDA...
20210414::215918: Head 2: Error: not receiving UDP ZDA...
20210414::215923: GUI: OnBnClickedOk
20210414::215923: GUI: Exiting the WiSSL GUI..
20210414::215923: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::215923: GUI: Wrote configuration data.
20210414::220040: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::220040: GUI: Live mode ON.
20210414::220040: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::220040: GUI: WiSSL GUI started at 2021_04_14_22:00:40
20210414::220040: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::220040: GUI: Attempting Communications with Head 1...
20210414::220040: GUI: Attempting Communications with Head 2...
20210414::220041: GUI: Established Communications with Head 1.
20210414::220042: Head 1: Initializing Communications with GUI ...
20210414::220042: Head 1: Communications Established.
20210414::220043: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::220043: Head 1: Connection Established with the GUI.
20210414::220043: Head 1: Initializing Subsystems, standby ...
20210414::220044: GUI: Established Communications with Head 2.
20210414::220044: Head 1: Initializing Hardware, Stand by ...
20210414::220045: Head 2: Initializing Communications with GUI ...
20210414::220045: Head 2: Communications Established.
20210414::220046: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::220046: Head 2: Connection Established with the GUI.
20210414::220046: Head 2: Initializing Subsystems, standby ...
20210414::220047: Head 2: Initializing Hardware, Stand by ...
20210414::220053: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::220053: Head 1: NtQuery - testing 1 ...
20210414::220054: Head 1: clock resolution: 10
20210414::220054: Head 1: NtQuery - testing 2, after setting max res ...
20210414::220054: Head 1: clock resolution: 10
20210414::220055: Head 1: Initializing Optics Electronics ...
20210414::220055: Head 1: Power Laser Controller
20210414::220056: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::220057: Head 2: NtQuery - testing 1 ...
20210414::220057: Head 2: clock resolution: 10
20210414::220057: Head 2: NtQuery - testing 2, after setting max res ...
20210414::220058: Head 2: clock resolution: 10
20210414::220058: Head 2: Initializing Optics Electronics ...
20210414::220058: Head 2: Power Laser Controller
20210414::220059: Head 1: Power Scanner Controller
20210414::220100: System NOT Initialized, Gain 0, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 34
20210414::220100: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220100: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220101: Head 1: Power OPTO Sensor
20210414::220102: Head 2: Power Scanner Controller
20210414::220104: Head 2: Power OPTO Sensor
20210414::220121: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210414::220121: Head 1: Eye Safe Optical Filter check Passed
20210414::220122: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210414::220122: Head 1: Initializing Time Sync Subsystem.
20210414::220122: Head 1: Initializing CTD Subsystem.
20210414::220122: Head 1: CTD Initialization Successful
20210414::220123: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210414::220123: Head 1: Time Sync UDP started, waiting for sync...
20210414::220123: Head 1: Attempting CTD Ethernet connection with ROV...
20210414::220124: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::220124: Head 2: Eye Safe Optical Filter check Passed
20210414::220125: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210414::220125: Head 2: Initializing Time Sync Subsystem.
20210414::220125: Head 2: Initializing CTD Subsystem.
20210414::220126: Head 2: CTD Initialization Successful
20210414::220126: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210414::220126: Head 2: Time Sync UDP started, waiting for sync...
20210414::220127: Head 2: Attempting CTD Ethernet connection with ROV...
20210414::220130: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 87
20210414::220130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 26%, OPB 22C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 25%, OPB 21C, Laser 0.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220132: Head 1: Error: not receiving UDP ZDA...
20210414::220135: Head 2: Error: not receiving UDP ZDA...
20210414::220137: GUI: Live mode ON.
20210414::220137: GUI: Requesing START operation, Head 1
20210414::220137: GUI: Requesing START operation, Head 2
20210414::220137: Head 1: Received request: START
20210414::220137: Head 2: Received request: START
20210414::220137: Head 1: Starting Scan Operation
20210414::220137: Head 2: Starting Scan Operation
20210414::220139: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::220139: Head 2: Eye Safe Optical Filter check Passed
20210414::220142: Head 1: Error: not receiving UDP ZDA...
20210414::220142: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210414::220142: Head 1: Eye Safe Optical Filter check Passed
20210414::220143: Head 2: Configured for WATER Processing
20210414::220144: Head 2: Configured for WATER Processing
20210414::220144: Head 2: Configured for WATER Processing
20210414::220144: Head 2: Configured for WATER Processing
20210414::220145: Head 2: Configured for WATER Processing
20210414::220145: Head 2: Configured for WATER Processing
20210414::220145: Head 2: Configured for WATER Processing
20210414::220145: Head 2: Configured for WATER Processing
20210414::220146: Head 2: Configured for WATER Processing
20210414::220146: Head 2: Configured for WATER Processing
20210414::220146: Head 2: Configured for WATER Processing
20210414::220147: Head 2: Configured for WATER Processing
20210414::220147: Head 1: Configured for WATER Processing
20210414::220147: Head 2: Configured for WATER Processing
20210414::220147: Head 1: Configured for WATER Processing
20210414::220147: Head 1: Configured for WATER Processing
20210414::220147: Head 2: Configured for WATER Processing
20210414::220148: Head 1: Configured for WATER Processing
20210414::220148: Head 2: Configured for WATER Processing
20210414::220148: Head 1: Configured for WATER Processing
20210414::220148: Head 2: Configured for WATER Processing
20210414::220148: Head 1: Configured for WATER Processing
20210414::220148: Head 2: Configured for WATER Processing
20210414::220148: Head 1: Configured for WATER Processing
20210414::220148: Head 2: Configured for WATER Processing
20210414::220149: Head 1: Configured for WATER Processing
20210414::220149: Head 2: Configured for WATER Processing
20210414::220149: Head 1: Configured for WATER Processing
20210414::220149: Head 2: Configured for WATER Processing
20210414::220149: Head 1: Configured for WATER Processing
20210414::220149: Head 2: Error: not receiving UDP ZDA...
20210414::220150: Head 1: Configured for WATER Processing
20210414::220150: Head 1: Configured for WATER Processing
20210414::220150: Head 1: Configured for WATER Processing
20210414::220150: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220724_tank_dry.raa
20210414::220151: Head 1: Configured for WATER Processing
20210414::220151: Head 1: Configured for WATER Processing
20210414::220151: Head 1: Configured for WATER Processing
20210414::220152: Head 1: Configured for WATER Processing
20210414::220152: Head 1: Configured for WATER Processing
20210414::220152: Head 1: Configured for WATER Processing
20210414::220152: Head 1: Configured for WATER Processing
20210414::220153: Head 1: Error: not receiving UDP ZDA...
20210414::220155: Head 2: Error: not receiving UDP ZDA...
20210414::220158: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220734_tank_dry.raa
20210414::220200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 25%, OPB 22C, Laser 28.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220200: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 141
20210414::220200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 28C, OCB 25%, OPB 23C, Laser 29.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220203: Head 1: Error: not receiving UDP ZDA...
20210414::220205: Head 2: Error: not receiving UDP ZDA...
20210414::220208: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220744_tank_dry.raa
20210414::220213: Head 1: Error: not receiving UDP ZDA...
20210414::220216: Head 2: Error: not receiving UDP ZDA...
20210414::220219: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220754_tank_dry.raa
20210414::220224: Head 1: Error: not receiving UDP ZDA...
20210414::220226: Head 2: Error: not receiving UDP ZDA...
20210414::220229: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220804_tank_dry.raa
20210414::220230: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 194
20210414::220230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 25%, OPB 23C, Laser 30.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 22C, Laser 29.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220234: Head 1: Error: not receiving UDP ZDA...
20210414::220235: Head 1: CTD Ethernet connection established.
20210414::220235: Head 2: CTD Ethernet connection established.
20210414::220236: Head 2: Error: not receiving UDP ZDA...
20210414::220239: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220814_tank_dry.raa
20210414::220245: Head 1: Error: not receiving UDP ZDA...
20210414::220247: Head 2: Error: not receiving UDP ZDA...
20210414::220249: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220824_tank_dry.raa
20210414::220255: Head 1: Error: not receiving UDP ZDA...
20210414::220257: Head 2: Error: not receiving UDP ZDA...
20210414::220300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220300: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220834_tank_dry.raa
20210414::220300: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 248
20210414::220300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220305: Head 1: Error: not receiving UDP ZDA...
20210414::220307: Head 2: Error: not receiving UDP ZDA...
20210414::220312: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220844_tank_dry.raa
20210414::220317: Head 2: Error: not receiving UDP ZDA...
20210414::220318: Head 1: Error: not receiving UDP ZDA...
20210414::220324: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220854_tank_dry.raa
20210414::220328: Head 2: Error: not receiving UDP ZDA...
20210414::220330: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 301
20210414::220330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220331: Head 1: Error: not receiving UDP ZDA...
20210414::220337: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220904_tank_dry.raa
20210414::220338: Head 2: Error: not receiving UDP ZDA...
20210414::220341: Head 1: Error: not receiving UDP ZDA...
20210414::220344: Head 2: Comm CTD Error, disconnecting
20210414::220344: Head 1: Comm CTD Error, disconnecting
20210414::220345: Head 2: Restarting CTD Ethernet connection ...
20210414::220345: Head 1: Restarting CTD Ethernet connection ...
20210414::220348: Head 2: Error: not receiving UDP ZDA...
20210414::220350: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220914_tank_dry.raa
20210414::220352: Head 1: Error: not receiving UDP ZDA...
20210414::220358: Head 2: Error: not receiving UDP ZDA...
20210414::220400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220400: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 355
20210414::220400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220403: Head 1: Error: not receiving UDP ZDA...
20210414::220405: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220924_tank_dry.raa
20210414::220408: Head 2: Error: not receiving UDP ZDA...
20210414::220413: Head 1: Error: not receiving UDP ZDA...
20210414::220418: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220934_tank_dry.raa
20210414::220419: Head 2: Error: not receiving UDP ZDA...
20210414::220426: Head 1: Error: not receiving UDP ZDA...
20210414::220429: Head 2: Error: not receiving UDP ZDA...
20210414::220430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220430: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 409
20210414::220430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220431: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220944_tank_dry.raa
20210414::220437: Head 1: Error: not receiving UDP ZDA...
20210414::220439: Head 2: Error: not receiving UDP ZDA...
20210414::220445: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_220954_tank_dry.raa
20210414::220447: Head 1: Error: not receiving UDP ZDA...
20210414::220449: Head 2: Error: not receiving UDP ZDA...
20210414::220458: Head 1: Error: not receiving UDP ZDA...
20210414::220458: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221004_tank_dry.raa
20210414::220459: Head 2: Error: not receiving UDP ZDA...
20210414::220500: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 462
20210414::220500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220508: Head 1: Error: not receiving UDP ZDA...
20210414::220510: Head 2: Error: not receiving UDP ZDA...
20210414::220510: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221014_tank_dry.raa
20210414::220518: Head 1: Error: not receiving UDP ZDA...
20210414::220520: Head 2: Error: not receiving UDP ZDA...
20210414::220521: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221024_tank_dry.raa
20210414::220525: Head 1: CTD Ethernet connection established.
20210414::220525: Head 2: CTD Ethernet connection established.
20210414::220528: Head 1: Error: not receiving UDP ZDA...
20210414::220530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220530: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 516
20210414::220530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220530: Head 2: Error: not receiving UDP ZDA...
20210414::220530: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221034_tank_dry.raa
20210414::220539: Head 1: Error: not receiving UDP ZDA...
20210414::220540: Head 2: Error: not receiving UDP ZDA...
20210414::220541: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221044_tank_dry.raa
20210414::220543: Head 1: Comm CTD Error, disconnecting
20210414::220543: Head 2: Comm CTD Error, disconnecting
20210414::220544: Head 1: Restarting CTD Ethernet connection ...
20210414::220544: Head 2: Restarting CTD Ethernet connection ...
20210414::220549: Head 1: Error: not receiving UDP ZDA...
20210414::220551: Head 2: Error: not receiving UDP ZDA...
20210414::220551: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221054_tank_dry.raa
20210414::220559: Head 1: Error: not receiving UDP ZDA...
20210414::220600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220600: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 570
20210414::220600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220601: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221104_tank_dry.raa
20210414::220601: Head 2: Error: not receiving UDP ZDA...
20210414::220609: Head 1: Error: not receiving UDP ZDA...
20210414::220611: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221114_tank_dry.raa
20210414::220611: Head 2: Error: not receiving UDP ZDA...
20210414::220619: Head 1: Error: not receiving UDP ZDA...
20210414::220620: Head 1: CTD Ethernet connection established.
20210414::220620: Head 2: CTD Ethernet connection established.
20210414::220621: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221124_tank_dry.raa
20210414::220621: Head 2: Error: not receiving UDP ZDA...
20210414::220630: Head 1: Error: not receiving UDP ZDA...
20210414::220630: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 623
20210414::220630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210414::220631: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_221134_tank_dry.raa
20210414::220631: Head 2: Error: not receiving UDP ZDA...
20210414::220638: GUI: Live mode ON.
20210414::220638: GUI: Requesing STOP operation, Head 2
20210414::220638: GUI: Requesing STOP operation, Head 1
20210414::220639: Head 2: Received request: STOP
20210414::220639: Head 1: Received request: STOP
20210414::220639: Head 2: Stopping Scan Operation
20210414::220639: Head 1: Stopping Scan Operation
20210414::220640: Head 1: Error: not receiving UDP ZDA...
20210414::220641: Head 1: ProcessingMgr stopped all worker threads.
20210414::220641: Head 2: ProcessingMgr stopped all worker threads.
20210414::220641: Head 1:       Stop finished, may now recover.
20210414::220642: Head 2:       Stop finished, may now recover.
20210414::220642: Head 2: Error: not receiving UDP ZDA...
20210414::220643: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::220644: Head 2: Eye Safe Optical Filter check Passed
20210414::220646: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::220646: Head 1: Eye Safe Optical Filter check Passed
20210414::220650: Head 1: Error: not receiving UDP ZDA...
20210414::220652: Head 2: Error: not receiving UDP ZDA...
20210414::220700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220700: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 676
20210414::220700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220700: Head 1: Error: not receiving UDP ZDA...
20210414::220702: Head 2: Error: not receiving UDP ZDA...
20210414::220710: Head 1: Error: not receiving UDP ZDA...
20210414::220712: Head 2: Error: not receiving UDP ZDA...
20210414::220721: Head 1: Error: not receiving UDP ZDA...
20210414::220722: Head 2: Error: not receiving UDP ZDA...
20210414::220730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220730: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 729
20210414::220730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220731: Head 1: Error: not receiving UDP ZDA...
20210414::220733: Head 2: Error: not receiving UDP ZDA...
20210414::220741: Head 1: Error: not receiving UDP ZDA...
20210414::220743: Head 2: Error: not receiving UDP ZDA...
20210414::220751: Head 1: Error: not receiving UDP ZDA...
20210414::220753: Head 2: Error: not receiving UDP ZDA...
20210414::220800: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 783
20210414::220800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220802: Head 1: Error: not receiving UDP ZDA...
20210414::220803: Head 2: Error: not receiving UDP ZDA...
20210414::220812: Head 1: Error: not receiving UDP ZDA...
20210414::220813: Head 2: Error: not receiving UDP ZDA...
20210414::220822: Head 1: Error: not receiving UDP ZDA...
20210414::220824: Head 2: Error: not receiving UDP ZDA...
20210414::220830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220830: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 836
20210414::220830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220832: Head 1: Error: not receiving UDP ZDA...
20210414::220834: Head 1: Warning, CTD not recieved within 2 minutes.
20210414::220834: Head 2: Warning, CTD not recieved within 2 minutes.
20210414::220834: Head 2: Error: not receiving UDP ZDA...
20210414::220842: Head 1: Error: not receiving UDP ZDA...
20210414::220844: Head 2: Error: not receiving UDP ZDA...
20210414::220852: Head 1: Comm CTD Error, disconnecting
20210414::220852: Head 2: Comm CTD Error, disconnecting
20210414::220852: Head 1: Restarting CTD Ethernet connection ...
20210414::220852: Head 2: Restarting CTD Ethernet connection ...
20210414::220852: Head 1: Error: not receiving UDP ZDA...
20210414::220854: Head 2: Error: not receiving UDP ZDA...
20210414::220900: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 890
20210414::220900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::220913: GUI: Lost Communications with Head 2.
20210414::220913: GUI: Lost Communications with Sensor 1.
20210414::220921: GUI: Attempting Communications with Head 2...
20210414::220931: GUI: Attempting Communications with Head 1...
20210414::220955: GUI: OnBnClickedOk
20210414::220955: GUI: Exiting the WiSSL GUI..
20210414::220955: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::220955: GUI: Wrote configuration data.
20210414::221229: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::221230: GUI: Live mode ON.
20210414::221230: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::221230: GUI: WiSSL GUI started at 2021_04_14_22:12:30
20210414::221230: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::221230: GUI: Attempting Communications with Head 1...
20210414::221230: GUI: Attempting Communications with Head 2...
20210414::221230: GUI: Established Communications with Head 1.
20210414::221230: GUI: Established Communications with Head 2.
20210414::221231: Head 2: Lost Communications with GUI
20210414::221231: Head 1: Lost Communications with GUI
20210414::221231: Head 2: Error: not receiving UDP ZDA...
20210414::221231: Head 1: Error: not receiving UDP ZDA...
20210414::221232: Head 2: Initializing Communications with GUI ...
20210414::221232: Head 1: Initializing Communications with GUI ...
20210414::221232: Head 1: Error: not receiving UDP ZDA...
20210414::221232: Head 2: Error: not receiving UDP ZDA...
20210414::221232: Head 1: Error: not receiving UDP ZDA...
20210414::221232: Head 2: Error: not receiving UDP ZDA...
20210414::221233: Head 1: Error: not receiving UDP ZDA...
20210414::221233: Head 2: Error: not receiving UDP ZDA...
20210414::221233: Head 2: Error: not receiving UDP ZDA...
20210414::221233: Head 1: Error: not receiving UDP ZDA...
20210414::221233: Head 2: Error: not receiving UDP ZDA...
20210414::221233: Head 1: Error: not receiving UDP ZDA...
20210414::221233: Head 2: Error: not receiving UDP ZDA...
20210414::221233: Head 1: Error: not receiving UDP ZDA...
20210414::221234: Head 2: Error: not receiving UDP ZDA...
20210414::221234: Head 1: Error: not receiving UDP ZDA...
20210414::221234: Head 2: Error: not receiving UDP ZDA...
20210414::221234: Head 1: Error: not receiving UDP ZDA...
20210414::221234: Head 2: Error: not receiving UDP ZDA...
20210414::221234: Head 1: Error: not receiving UDP ZDA...
20210414::221235: Head 2: Error: not receiving UDP ZDA...
20210414::221235: Head 1: Error: not receiving UDP ZDA...
20210414::221235: Head 2: Error: not receiving UDP ZDA...
20210414::221235: Head 1: Error: not receiving UDP ZDA...
20210414::221235: Head 2: Error: not receiving UDP ZDA...
20210414::221235: Head 1: Error: not receiving UDP ZDA...
20210414::221236: Head 2: Error: not receiving UDP ZDA...
20210414::221236: Head 1: Error: not receiving UDP ZDA...
20210414::221236: Head 2: Error: not receiving UDP ZDA...
20210414::221236: Head 1: Error: not receiving UDP ZDA...
20210414::221236: Head 2: Error: not receiving UDP ZDA...
20210414::221236: Head 1: Error: not receiving UDP ZDA...
20210414::221236: Head 2: Error: not receiving UDP ZDA...
20210414::221236: Head 1: Error: not receiving UDP ZDA...
20210414::221237: Head 2: Error: not receiving UDP ZDA...
20210414::221237: Head 1: Error: not receiving UDP ZDA...
20210414::221237: Head 2: Error: not receiving UDP ZDA...
20210414::221237: Head 1: Error: not receiving UDP ZDA...
20210414::221237: Head 2: Communications Established.
20210414::221237: Head 1: Communications Established.
20210414::221238: Head 1: Error: not receiving UDP ZDA...
20210414::221239: Head 2: Error: not receiving UDP ZDA...
20210414::221247: Head 1: Error: not receiving UDP ZDA...
20210414::221249: Head 2: Error: not receiving UDP ZDA...
20210414::221257: GUI: OnBnClickedOk
20210414::221257: GUI: Exiting the WiSSL GUI..
20210414::221257: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::221257: GUI: Wrote configuration data.
20210414::221429: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::221429: GUI: Live mode ON.
20210414::221429: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::221429: GUI: WiSSL GUI started at 2021_04_14_22:14:29
20210414::221429: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::221429: GUI: Attempting Communications with Head 1...
20210414::221429: GUI: Attempting Communications with Head 2...
20210414::221429: GUI: Established Communications with Head 2.
20210414::221429: GUI: Established Communications with Head 1.
20210414::221430: Head 1: Initializing Communications with GUI ...
20210414::221430: Head 2: Initializing Communications with GUI ...
20210414::221430: Head 1: Communications Established.
20210414::221431: Head 2: Communications Established.
20210414::221432: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::221432: Head 1: Connection Established with the GUI.
20210414::221432: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::221432: Head 1: Initializing Subsystems, standby ...
20210414::221432: Head 2: Connection Established with the GUI.
20210414::221433: Head 1: Initializing Hardware, Stand by ...
20210414::221433: Head 2: Initializing Subsystems, standby ...
20210414::221433: Head 2: Initializing Hardware, Stand by ...
20210414::221433: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::221434: Head 1: NtQuery - testing 1 ...
20210414::221434: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210414::221434: Head 1: clock resolution: 10
20210414::221434: Head 2: NtQuery - testing 1 ...
20210414::221434: Head 1: NtQuery - testing 2, after setting max res ...
20210414::221434: Head 2: clock resolution: 1
20210414::221434: Head 1: clock resolution: 10
20210414::221435: Head 2: NtQuery - testing 2, after setting max res ...
20210414::221435: Head 1: Initializing Optics Electronics ...
20210414::221435: Head 2: clock resolution: 1
20210414::221435: Head 1: Power Laser Controller
20210414::221435: Head 2: Initializing Optics Electronics ...
20210414::221436: Head 2: Power Laser Controller
20210414::221439: Head 1: Power Scanner Controller
20210414::221439: Head 2: Power Scanner Controller
20210414::221441: Head 1: Power OPTO Sensor
20210414::221441: Head 2: Power OPTO Sensor
20210414::221500: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::221500: Head 1: Eye Safe Optical Filter check Passed
20210414::221500: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::221500: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 55
20210414::221500: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210414::221500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 0.0C, Dig 37.0C, Scan Az fault 1, gain 0, laser state 0
20210414::221500: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210414::221500: Head 2: Eye Safe Optical Filter check Passed
20210414::221500: Head 1: Initializing Time Sync Subsystem.
20210414::221501: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210414::221501: Head 1: Initializing CTD Subsystem.
20210414::221501: Head 2: Initializing Time Sync Subsystem.
20210414::221501: Head 1: CTD Initialization Successful
20210414::221501: Head 2: Initializing CTD Subsystem.
20210414::221501: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210414::221501: Head 2: CTD Initialization Successful
20210414::221502: Head 1: Time Sync UDP started, waiting for sync...
20210414::221502: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210414::221502: Head 1: Attempting CTD Ethernet connection with ROV...
20210414::221502: Head 2: Time Sync UDP started, waiting for sync...
20210414::221502: Head 2: Attempting CTD Ethernet connection with ROV...
20210414::221510: Head 1: Error: not receiving UDP ZDA...
20210414::221511: Head 2: Error: not receiving UDP ZDA...
20210414::221520: Head 1: Error: not receiving UDP ZDA...
20210414::221521: Head 2: Error: not receiving UDP ZDA...
20210414::221530: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 108
20210414::221530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::221530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210414::221531: Head 1: Error: not receiving UDP ZDA...
20210414::221531: Head 2: Error: not receiving UDP ZDA...
20210414::221534: GUI: Live mode ON.
20210414::221534: GUI: Requesing START operation, Head 1
20210414::221534: GUI: Requesing START operation, Head 2
20210414::221534: Head 1: Received request: START
20210414::221534: Head 2: Received request: START
20210414::221535: Head 1: Starting Scan Operation
20210414::221535: Head 2: Starting Scan Operation
20210414::221536: Head 1: Eye Safe Optical Filter State there 11, not there 19, transition 1
20210414::221536: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::221536: Head 1: Eye Safe Optical Filter check Passed
20210414::221536: Head 2: Eye Safe Optical Filter check Passed
20210414::221541: Head 1: Configured for WATER Processing
20210414::221541: Head 1: Configured for WATER Processing
20210414::221541: Head 2: Error: not receiving UDP ZDA...
20210414::221541: Head 1: Configured for WATER Processing
20210414::221542: Head 1: Configured for WATER Processing
20210414::221542: Head 1: Configured for WATER Processing
20210414::221542: Head 1: Configured for WATER Processing
20210414::221542: Head 1: Configured for WATER Processing
20210414::221543: Head 1: Configured for WATER Processing
20210414::221543: Head 1: Configured for WATER Processing
20210414::221543: Head 1: Configured for WATER Processing
20210414::221544: Head 1: Configured for WATER Processing
20210414::221544: Head 1: Configured for WATER Processing
20210414::221544: Head 1: Configured for WATER Processing
20210414::221544: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222045_tank_dry.raa
20210414::221545: Head 1: Configured for WATER Processing
20210414::221545: Head 1: Configured for WATER Processing
20210414::221545: Head 1: Configured for WATER Processing
20210414::221546: Head 1: Configured for WATER Processing
20210414::221546: Head 1: Configured for WATER Processing
20210414::221546: Head 1: Configured for WATER Processing
20210414::221546: Head 1: Configured for WATER Processing
20210414::221547: Head 1: Error: not receiving UDP ZDA...
20210414::221548: Head 2: Configured for WATER Processing
20210414::221548: Head 2: Configured for WATER Processing
20210414::221548: Head 2: Configured for WATER Processing
20210414::221549: Head 2: Configured for WATER Processing
20210414::221549: Head 2: Configured for WATER Processing
20210414::221549: Head 2: Configured for WATER Processing
20210414::221550: Head 2: Configured for WATER Processing
20210414::221550: Head 2: Configured for WATER Processing
20210414::221550: Head 2: Configured for WATER Processing
20210414::221551: Head 2: Configured for WATER Processing
20210414::221551: Head 2: Configured for WATER Processing
20210414::221551: Head 1: Error: not receiving UDP ZDA...
20210414::221551: Head 2: Configured for WATER Processing
20210414::221551: Head 2: Configured for WATER Processing
20210414::221552: Head 2: Configured for WATER Processing
20210414::221552: Head 2: Configured for WATER Processing
20210414::221552: Head 2: Configured for WATER Processing
20210414::221553: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222055_tank_dry.raa
20210414::221553: Head 2: Configured for WATER Processing
20210414::221553: Head 2: Configured for WATER Processing
20210414::221553: Head 2: Configured for WATER Processing
20210414::221554: Head 2: Configured for WATER Processing
20210414::221554: Head 2: Error: not receiving UDP ZDA...
20210414::221600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221600: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 162
20210414::221600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221601: Head 1: Error: not receiving UDP ZDA...
20210414::221602: Head 2: Error: not receiving UDP ZDA...
20210414::221602: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222105_tank_dry.raa
20210414::221612: Head 1: Error: not receiving UDP ZDA...
20210414::221612: Head 2: Error: not receiving UDP ZDA...
20210414::221613: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222115_tank_dry.raa
20210414::221622: Head 1: Error: not receiving UDP ZDA...
20210414::221622: Head 2: Error: not receiving UDP ZDA...
20210414::221622: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222125_tank_dry.raa
20210414::221630: Head 2: CTD Ethernet connection established.
20210414::221630: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 215
20210414::221630: Head 1: CTD Ethernet connection established.
20210414::221630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221632: Head 1: Error: not receiving UDP ZDA...
20210414::221632: Head 2: Error: not receiving UDP ZDA...
20210414::221632: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222135_tank_dry.raa
20210414::221642: Head 1: Error: not receiving UDP ZDA...
20210414::221642: Head 2: Error: not receiving UDP ZDA...
20210414::221643: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222145_tank_dry.raa
20210414::221653: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222155_tank_dry.raa
20210414::221653: Head 1: Error: not receiving UDP ZDA...
20210414::221653: Head 2: Error: not receiving UDP ZDA...
20210414::221700: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 268
20210414::221700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221703: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222205_tank_dry.raa
20210414::221703: Head 1: Error: not receiving UDP ZDA...
20210414::221703: Head 2: Error: not receiving UDP ZDA...
20210414::221713: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222215_tank_dry.raa
20210414::221713: Head 1: Error: not receiving UDP ZDA...
20210414::221713: Head 2: Error: not receiving UDP ZDA...
20210414::221723: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222225_tank_dry.raa
20210414::221723: Head 2: Error: not receiving UDP ZDA...
20210414::221723: Head 1: Error: not receiving UDP ZDA...
20210414::221730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221730: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 322
20210414::221730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 32.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221734: Head 2: Error: not receiving UDP ZDA...
20210414::221734: Head 1: Error: not receiving UDP ZDA...
20210414::221737: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222235_tank_dry.raa
20210414::221744: Head 2: Error: not receiving UDP ZDA...
20210414::221746: Head 1: Error: not receiving UDP ZDA...
20210414::221752: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222245_tank_dry.raa
20210414::221754: Head 2: Error: not receiving UDP ZDA...
20210414::221758: Head 1: Error: not receiving UDP ZDA...
20210414::221800: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 375
20210414::221800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 33.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 32.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221804: Head 2: Error: not receiving UDP ZDA...
20210414::221808: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222255_tank_dry.raa
20210414::221810: Head 1: Error: not receiving UDP ZDA...
20210414::221814: Head 2: Error: not receiving UDP ZDA...
20210414::221821: Head 1: Error: not receiving UDP ZDA...
20210414::221823: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222305_tank_dry.raa
20210414::221825: Head 2: Error: not receiving UDP ZDA...
20210414::221830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 31.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221830: System  Initialized, Gain 4, Elec PB 31.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 429
20210414::221830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 33.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::221833: Head 1: Error: not receiving UDP ZDA...
20210414::221835: Head 2: Error: not receiving UDP ZDA...
20210414::221839: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222315_tank_dry.raa
20210414::221845: Head 1: Error: not receiving UDP ZDA...
20210414::221845: Head 2: Error: not receiving UDP ZDA...
20210414::221854: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_222325_tank_dry.raa
20210414::221855: Head 2: Error: not receiving UDP ZDA...
20210414::221902: GUI: Live mode ON.
20210414::221906: GUI: Lost Communications with Sensor 1.
20210414::221907: GUI: Lost Communications with Head 2.
20210414::221916: GUI: Attempting Communications with Head 1...
20210414::221916: GUI: Attempting Communications with Head 2...
20210414::222002: GUI: Established Communications with Head 1.
20210414::222003: Head 1: Initializing Communications with GUI ...
20210414::222003: Head 1: Communications Established.
20210414::222004: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::222004: Head 1: Connection Established with the GUI.
20210414::222005: Head 1: Initializing Subsystems, standby ...
20210414::222005: Head 1: Initializing Hardware, Stand by ...
20210414::222008: GUI: Established Communications with Head 2.
20210414::222009: Head 2: Initializing Communications with GUI ...
20210414::222010: Head 2: Communications Established.
20210414::222011: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::222011: Head 2: Connection Established with the GUI.
20210414::222012: Head 2: Initializing Subsystems, standby ...
20210414::222012: Head 2: Initializing Hardware, Stand by ...
20210414::222015: Head 2: DAQmx Error: -200324: NI-DAQmx is unable to communicate with the device. Make sure the device is present in and accessible to the system, is not currently being reset, and is not reserved by another driver such as Traditional NI-DAQ (Legacy). 
20210414::222015: Head 2: 
20210414::222020: Head 2: DAQmx Error: -200324: NI-DAQmx is unable to communicate with the device. Make sure the device is present in and accessible to the system, is not currently being reset, and is not reserved by another driver such as Traditional NI-DAQ (Legacy). 
20210414::222021: Head 2: 
20210414::222021: Head 2: DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZIN1  Status Code: -200478
20210414::222021: Head 2: 
20210414::222022: Head 2: DAQmx Error: -200486: Specified channel is not in the task. Channel Name: DAQ1/ai4  Task Name: Sc_AZIN1  Status Code: -200486
20210414::222022: Head 2: 
20210414::222022: Head 2:    Error Initializing DAQ Subsystem
20210414::222024: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::222025: Head 1: NtQuery - testing 1 ...
20210414::222025: Head 1: clock resolution: 10
20210414::222025: Head 1: NtQuery - testing 2, after setting max res ...
20210414::222026: Head 1: clock resolution: 10
20210414::222026: Head 1: Initializing Optics Electronics ...
20210414::222026: Head 1: Power Laser Controller
20210414::222030: System NOT Initialized, Gain 0, Elec PB 32.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 52
20210414::222030: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::222030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210414::222030: Head 1: Power Scanner Controller
20210414::222030: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::222031: Head 2: NtQuery - testing 1 ...
20210414::222031: Head 2: clock resolution: 10
20210414::222031: Head 2: NtQuery - testing 2, after setting max res ...
20210414::222032: Head 2: clock resolution: 10
20210414::222032: Head 2: Initializing Optics Electronics ...
20210414::222032: Head 2: Power Laser Controller
20210414::222032: Head 1: Power OPTO Sensor
20210414::222036: Head 2: Power Scanner Controller
20210414::222038: Head 2: Power OPTO Sensor
20210414::222042: GUI: ERROR: Received Invalid Packet ID: 0
20210414::222043: GUI: Lost Communications with Sensor 1.
20210414::222043: GUI: Attempting Communications with Head 1...
20210414::222047: GUI: OnBnClickedOk
20210414::222047: GUI: Exiting the WiSSL GUI..
20210414::222047: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::222047: GUI: Wrote configuration data.
20210414::223551: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::223551: GUI: Live mode ON.
20210414::223551: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::223551: GUI: WiSSL GUI started at 2021_04_14_22:35:51
20210414::223551: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::223551: GUI: Attempting Communications with Head 1...
20210414::223551: GUI: Attempting Communications with Head 2...
20210414::223613: GUI: Established Communications with Head 1.
20210414::223614: Head 1: Initializing Communications with GUI ...
20210414::223615: Head 1: Communications Established.
20210414::223616: GUI: Established Communications with Head 2.
20210414::223616: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::223617: Head 1: Connection Established with the GUI.
20210414::223617: Head 2: Initializing Communications with GUI ...
20210414::223617: Head 1: Initializing Subsystems, standby ...
20210414::223617: Head 1: Initializing Hardware, Stand by ...
20210414::223618: Head 2: Communications Established.
20210414::223619: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210414::223619: Head 2: Connection Established with the GUI.
20210414::223620: Head 2: Initializing Subsystems, standby ...
20210414::223620: Head 2: Initializing Hardware, Stand by ...
20210414::223630: System NOT Initialized, Gain 0, Elec PB 26.0C, Elec PB 32.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 30
20210414::223630: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223630: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223631: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::223632: Head 1: NtQuery - testing 1 ...
20210414::223632: Head 1: clock resolution: 10
20210414::223632: Head 1: NtQuery - testing 2, after setting max res ...
20210414::223632: Head 1: clock resolution: 10
20210414::223633: Head 1: Initializing Optics Electronics ...
20210414::223633: Head 1: Power Laser Controller
20210414::223637: Head 1: Power Scanner Controller
20210414::223639: Head 1: Power OPTO Sensor
20210414::223639: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210414::223640: Head 2: NtQuery - testing 1 ...
20210414::223640: Head 2: clock resolution: 10
20210414::223640: Head 2: NtQuery - testing 2, after setting max res ...
20210414::223641: Head 2: clock resolution: 10
20210414::223641: Head 2: Initializing Optics Electronics ...
20210414::223641: Head 2: Power Laser Controller
20210414::223645: Head 2: Power Scanner Controller
20210414::223647: Head 2: Power OPTO Sensor
20210414::223659: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::223659: Head 1: Eye Safe Optical Filter check Passed
20210414::223700: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210414::223700: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 32.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 83
20210414::223700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 35%, OPB 19C, Laser 0.0C, Dig 31.0C, Scan Az fault 1, gain 0, laser state 0
20210414::223700: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223700: Head 1: Initializing Time Sync Subsystem.
20210414::223700: Head 1: Initializing CTD Subsystem.
20210414::223700: Head 1: CTD Initialization Successful
20210414::223701: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210414::223701: Head 1: Time Sync UDP started, waiting for sync...
20210414::223701: Head 1: Attempting CTD Ethernet connection with ROV...
20210414::223707: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::223708: Head 2: Eye Safe Optical Filter check Passed
20210414::223708: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210414::223708: Head 2: Initializing Time Sync Subsystem.
20210414::223708: Head 2: Initializing CTD Subsystem.
20210414::223709: Head 2: CTD Initialization Successful
20210414::223709: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210414::223709: Head 2: Time Sync UDP started, waiting for sync...
20210414::223710: Head 2: Attempting CTD Ethernet connection with ROV...
20210414::223710: Head 1: Error: not receiving UDP ZDA...
20210414::223718: Head 2: Error: not receiving UDP ZDA...
20210414::223720: Head 1: Error: not receiving UDP ZDA...
20210414::223728: Head 2: Error: not receiving UDP ZDA...
20210414::223730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 31%, OPB 19C, Laser 20.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 137
20210414::223730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 32%, OPB 20C, Laser 21.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223730: Head 1: Error: not receiving UDP ZDA...
20210414::223738: Head 2: Error: not receiving UDP ZDA...
20210414::223740: Head 1: Error: not receiving UDP ZDA...
20210414::223749: Head 2: Error: not receiving UDP ZDA...
20210414::223751: Head 1: Error: not receiving UDP ZDA...
20210414::223759: Head 2: Error: not receiving UDP ZDA...
20210414::223800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 190
20210414::223800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 30%, OPB 20C, Laser 22.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 29%, OPB 19C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223801: Head 1: Error: not receiving UDP ZDA...
20210414::223809: Head 2: Error: not receiving UDP ZDA...
20210414::223811: Head 1: Error: not receiving UDP ZDA...
20210414::223819: Head 2: Error: not receiving UDP ZDA...
20210414::223821: Head 1: Error: not receiving UDP ZDA...
20210414::223829: Head 2: Error: not receiving UDP ZDA...
20210414::223840: GUI: Lost Communications with Head 2.
20210414::223840: GUI: Lost Communications with Sensor 1.
20210414::223845: GUI: Attempting Communications with Head 1...
20210414::223847: Head 2: Error: not receiving UDP ZDA...
20210414::223848: GUI: Attempting Communications with Head 2...
20210414::223848: GUI: Established Communications with Head 2.
20210414::223858: GUI: Lost Communications with Head 2.
20210414::223909: GUI: Attempting Communications with Head 2...
20210414::223909: GUI: Established Communications with Head 2.
20210414::223910: Head 2: Invalid Packet Acknowledgement Status Read: 0x0.
20210414::223910: Head 2: Lost Communications with GUI
20210414::223911: Head 2: Initializing Communications with GUI ...
20210414::223911: Head 2: Error: not receiving UDP ZDA...
20210414::223911: Head 2: Error: not receiving UDP ZDA...
20210414::223911: Head 2: Communications Established.
20210414::223920: Head 2: Error: not receiving UDP ZDA...
20210414::223930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 25%, OPB 20C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::223931: Head 2: Error: not receiving UDP ZDA...
20210414::223941: Head 2: Error: not receiving UDP ZDA...
20210414::223951: Head 2: Error: not receiving UDP ZDA...
20210414::224000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 25%, OPB 20C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::224001: Head 2: Error: not receiving UDP ZDA...
20210414::224012: Head 2: Error: not receiving UDP ZDA...
20210414::224022: Head 2: Error: not receiving UDP ZDA...
20210414::224030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 20C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::224032: Head 2: Error: not receiving UDP ZDA...
20210414::224042: Head 2: Error: not receiving UDP ZDA...
20210414::224052: Head 2: Error: not receiving UDP ZDA...
20210414::224100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 20C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::224103: Head 2: Error: not receiving UDP ZDA...
20210414::224105: GUI: OnBnClickedOk
20210414::224105: GUI: Exiting the WiSSL GUI..
20210414::224105: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::224105: GUI: Wrote configuration data.
20210414::224107: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::224107: GUI: Live mode ON.
20210414::224107: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210414::224107: GUI: WiSSL GUI started at 2021_04_14_22:41:07
20210414::224107: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_14.txt
20210414::224107: GUI: Attempting Communications with Head 1...
20210414::224107: GUI: Attempting Communications with Head 2...
20210414::224109: GUI: Established Communications with Head 2.
20210414::224110: Head 2: Lost Communications with GUI
20210414::224110: Head 2: Initializing Communications with GUI ...
20210414::224111: Head 2: Communications Established.
20210414::224111: GUI: Established Communications with Head 1.
20210414::224113: Head 2: Error: not receiving UDP ZDA...
20210414::224123: Head 2: Error: not receiving UDP ZDA...
20210414::224129: GUI: Live mode ON.
20210414::224129: GUI: Requesing START operation, Head 2
20210414::224129: GUI: Requesing START operation, Head 1
20210414::224130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 20C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210414::224130: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 282
20210414::224130: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 21C, Laser 25.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210414::224130: Head 2: Received request: START
20210414::224130: Head 2: Starting Scan Operation
20210414::224131: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210414::224132: Head 2: Eye Safe Optical Filter check Passed
20210414::224133: Head 2: Error: not receiving UDP ZDA...
20210414::224140: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224713_tank_dry.raa
20210414::224143: Head 2: Error: not receiving UDP ZDA...
20210414::224148: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224723_tank_dry.raa
20210414::224154: Head 2: Error: not receiving UDP ZDA...
20210414::224157: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224733_tank_dry.raa
20210414::224158: Head 2: Configured for WATER Processing
20210414::224159: Head 2: Configured for WATER Processing
20210414::224159: Head 2: Configured for WATER Processing
20210414::224159: Head 2: Configured for WATER Processing
20210414::224200: Head 2: Configured for WATER Processing
20210414::224200: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 336
20210414::224200: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224200: Head 2: Configured for WATER Processing
20210414::224200: Head 2: Configured for WATER Processing
20210414::224201: Head 2: Configured for WATER Processing
20210414::224201: Head 2: Configured for WATER Processing
20210414::224201: Head 2: Configured for WATER Processing
20210414::224201: Head 2: Configured for WATER Processing
20210414::224202: Head 2: Configured for WATER Processing
20210414::224202: Head 2: Configured for WATER Processing
20210414::224202: Head 2: Configured for WATER Processing
20210414::224203: Head 2: Configured for WATER Processing
20210414::224203: Head 2: Configured for WATER Processing
20210414::224203: Head 2: Configured for WATER Processing
20210414::224204: Head 2: Configured for WATER Processing
20210414::224204: Head 2: Configured for WATER Processing
20210414::224204: Head 2: Configured for WATER Processing
20210414::224204: Head 2: Error: not receiving UDP ZDA...
20210414::224207: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224743_tank_dry.raa
20210414::224214: Head 2: Error: not receiving UDP ZDA...
20210414::224218: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224753_tank_dry.raa
20210414::224219: Head 2: CTD Ethernet connection established.
20210414::224224: Head 2: Error: not receiving UDP ZDA...
20210414::224230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 20C, Laser 25.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224230: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 389
20210414::224230: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 15.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 21C, Laser 26.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224230: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224803_tank_dry.raa
20210414::224234: Head 2: Error: not receiving UDP ZDA...
20210414::224241: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224813_tank_dry.raa
20210414::224245: Head 2: Error: not receiving UDP ZDA...
20210414::224251: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224823_tank_dry.raa
20210414::224255: Head 2: Error: not receiving UDP ZDA...
20210414::224300: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 443
20210414::224300: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 21C, Laser 27.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 20C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224301: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224833_tank_dry.raa
20210414::224305: Head 2: Error: not receiving UDP ZDA...
20210414::224306: Head 2: Comm CTD Error, disconnecting
20210414::224307: Head 2: Restarting CTD Ethernet connection ...
20210414::224311: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224843_tank_dry.raa
20210414::224315: Head 2: Error: not receiving UDP ZDA...
20210414::224321: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224853_tank_dry.raa
20210414::224325: Head 2: Error: not receiving UDP ZDA...
20210414::224330: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 496
20210414::224330: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 21C, Laser 27.0C, Dig 36.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 20C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224331: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224903_tank_dry.raa
20210414::224336: Head 2: Error: not receiving UDP ZDA...
20210414::224341: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224913_tank_dry.raa
20210414::224346: Head 2: Error: not receiving UDP ZDA...
20210414::224351: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224923_tank_dry.raa
20210414::224356: Head 2: Error: not receiving UDP ZDA...
20210414::224400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 20C, Laser 26.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224400: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 550
20210414::224400: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 21C, Laser 28.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224402: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224933_tank_dry.raa
20210414::224406: Head 2: Error: not receiving UDP ZDA...
20210414::224412: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224943_tank_dry.raa
20210414::224417: Head 2: Error: not receiving UDP ZDA...
20210414::224422: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_224953_tank_dry.raa
20210414::224427: Head 2: Error: not receiving UDP ZDA...
20210414::224430: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 604
20210414::224430: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 26.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224432: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225003_tank_dry.raa
20210414::224437: Head 2: Error: not receiving UDP ZDA...
20210414::224442: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225013_tank_dry.raa
20210414::224447: Head 2: Error: not receiving UDP ZDA...
20210414::224452: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225023_tank_dry.raa
20210414::224457: Head 2: Error: not receiving UDP ZDA...
20210414::224500: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 657
20210414::224500: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 28.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 27.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224502: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225033_tank_dry.raa
20210414::224508: Head 2: Error: not receiving UDP ZDA...
20210414::224512: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225043_tank_dry.raa
20210414::224518: Head 2: Error: not receiving UDP ZDA...
20210414::224522: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225053_tank_dry.raa
20210414::224528: Head 2: Error: not receiving UDP ZDA...
20210414::224530: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 710
20210414::224530: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224532: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225103_tank_dry.raa
20210414::224538: Head 2: Error: not receiving UDP ZDA...
20210414::224542: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225113_tank_dry.raa
20210414::224548: Head 2: Error: not receiving UDP ZDA...
20210414::224552: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225123_tank_dry.raa
20210414::224559: Head 2: Error: not receiving UDP ZDA...
20210414::224600: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 764
20210414::224600: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224602: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225133_tank_dry.raa
20210414::224609: Head 2: Error: not receiving UDP ZDA...
20210414::224612: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225143_tank_dry.raa
20210414::224619: Head 2: Error: not receiving UDP ZDA...
20210414::224622: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225153_tank_dry.raa
20210414::224629: Head 2: Error: not receiving UDP ZDA...
20210414::224630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224630: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 817
20210414::224630: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224632: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225203_tank_dry.raa
20210414::224640: Head 2: Error: not receiving UDP ZDA...
20210414::224642: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225213_tank_dry.raa
20210414::224650: Head 2: Error: not receiving UDP ZDA...
20210414::224652: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225223_tank_dry.raa
20210414::224700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224700: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 871
20210414::224700: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224700: Head 2: Error: not receiving UDP ZDA...
20210414::224702: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225233_tank_dry.raa
20210414::224710: Head 2: Error: not receiving UDP ZDA...
20210414::224712: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225243_tank_dry.raa
20210414::224720: Head 2: Error: not receiving UDP ZDA...
20210414::224722: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225253_tank_dry.raa
20210414::224730: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 924
20210414::224730: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 38.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 28.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224731: Head 2: Error: not receiving UDP ZDA...
20210414::224732: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225303_tank_dry.raa
20210414::224741: Head 2: Error: not receiving UDP ZDA...
20210414::224743: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225313_tank_dry.raa
20210414::224751: Head 2: Error: not receiving UDP ZDA...
20210414::224752: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225323_tank_dry.raa
20210414::224800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224800: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 978
20210414::224800: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224801: Head 2: Error: not receiving UDP ZDA...
20210414::224803: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225333_tank_dry.raa
20210414::224811: Head 2: Error: not receiving UDP ZDA...
20210414::224813: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225343_tank_dry.raa
20210414::224822: Head 2: Error: not receiving UDP ZDA...
20210414::224822: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225353_tank_dry.raa
20210414::224830: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1031
20210414::224830: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224832: Head 2: Error: not receiving UDP ZDA...
20210414::224833: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225403_tank_dry.raa
20210414::224842: Head 2: Error: not receiving UDP ZDA...
20210414::224843: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225413_tank_dry.raa
20210414::224852: Head 2: Error: not receiving UDP ZDA...
20210414::224853: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225423_tank_dry.raa
20210414::224900: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1085
20210414::224900: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224903: Head 2: Error: not receiving UDP ZDA...
20210414::224903: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225433_tank_dry.raa
20210414::224913: Head 2: Error: not receiving UDP ZDA...
20210414::224913: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225443_tank_dry.raa
20210414::224923: Head 2: Error: not receiving UDP ZDA...
20210414::224923: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225453_tank_dry.raa
20210414::224930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224930: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1138
20210414::224930: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 22C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::224933: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225503_tank_dry.raa
20210414::224933: Head 2: Error: not receiving UDP ZDA...
20210414::224943: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225513_tank_dry.raa
20210414::224943: Head 2: Error: not receiving UDP ZDA...
20210414::224953: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225523_tank_dry.raa
20210414::224954: Head 2: Error: not receiving UDP ZDA...
20210414::225000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225000: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1191
20210414::225000: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 22C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225003: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225533_tank_dry.raa
20210414::225004: Head 2: Error: not receiving UDP ZDA...
20210414::225013: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225543_tank_dry.raa
20210414::225014: Head 2: Error: not receiving UDP ZDA...
20210414::225023: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225553_tank_dry.raa
20210414::225024: Head 2: Error: not receiving UDP ZDA...
20210414::225030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 21C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225030: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1245
20210414::225030: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 22C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225033: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225603_tank_dry.raa
20210414::225034: Head 2: Error: not receiving UDP ZDA...
20210414::225043: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225613_tank_dry.raa
20210414::225045: Head 2: Error: not receiving UDP ZDA...
20210414::225053: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225623_tank_dry.raa
20210414::225055: Head 2: Error: not receiving UDP ZDA...
20210414::225100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225100: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1298
20210414::225100: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.5Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 22C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225104: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225633_tank_dry.raa
20210414::225105: Head 2: Error: not receiving UDP ZDA...
20210414::225113: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225643_tank_dry.raa
20210414::225115: Head 2: Error: not receiving UDP ZDA...
20210414::225123: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225653_tank_dry.raa
20210414::225125: Head 2: Error: not receiving UDP ZDA...
20210414::225130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225130: System  Initialized, Gain 4, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1351
20210414::225130: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 22.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210414::225134: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225703_tank_dry.raa
20210414::225136: Head 2: Error: not receiving UDP ZDA...
20210414::225144: GUI: Archiving data to file --> C:\Data\20210412t1\20210414_225713_tank_dry.raa
20210414::225146: Head 2: Error: not receiving UDP ZDA...
20210414::225149: GUI: Live mode ON.
20210414::225149: GUI: Requesing STOP operation, Head 2
20210414::225149: GUI: Requesing STOP operation, Head 1
20210414::225149: Head 2: Received request: STOP
20210414::225150: Head 2: Stopping Scan Operation
20210414::225152: Head 2: ProcessingMgr stopped all worker threads.
20210414::225152: Head 2:       Stop finished, may now recover.
20210414::225154: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210414::225154: Head 2: Eye Safe Optical Filter check Passed
20210414::225156: Head 2: Error: not receiving UDP ZDA...
20210414::225200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1404
20210414::225200: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225206: Head 2: Error: not receiving UDP ZDA...
20210414::225216: Head 2: Error: not receiving UDP ZDA...
20210414::225227: Head 2: Error: not receiving UDP ZDA...
20210414::225230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225230: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1458
20210414::225230: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225237: Head 2: Error: not receiving UDP ZDA...
20210414::225247: Head 2: Error: not receiving UDP ZDA...
20210414::225257: Head 2: Error: not receiving UDP ZDA...
20210414::225300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225300: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1511
20210414::225300: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225307: Head 2: Error: not receiving UDP ZDA...
20210414::225318: Head 2: Error: not receiving UDP ZDA...
20210414::225328: Head 2: Error: not receiving UDP ZDA...
20210414::225330: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1564
20210414::225330: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225338: Head 2: Error: not receiving UDP ZDA...
20210414::225348: Head 2: Error: not receiving UDP ZDA...
20210414::225358: Head 2: Error: not receiving UDP ZDA...
20210414::225400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225400: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1618
20210414::225400: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225409: Head 2: Error: not receiving UDP ZDA...
20210414::225419: Head 2: Error: not receiving UDP ZDA...
20210414::225429: Head 2: Error: not receiving UDP ZDA...
20210414::225430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225430: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1671
20210414::225430: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225439: Head 2: Error: not receiving UDP ZDA...
20210414::225449: Head 2: Error: not receiving UDP ZDA...
20210414::225500: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1724
20210414::225500: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225500: Head 2: Error: not receiving UDP ZDA...
20210414::225500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225510: Head 2: Error: not receiving UDP ZDA...
20210414::225520: Head 2: Error: not receiving UDP ZDA...
20210414::225530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225530: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1778
20210414::225530: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225530: Head 2: Error: not receiving UDP ZDA...
20210414::225540: Head 2: Error: not receiving UDP ZDA...
20210414::225551: Head 2: Error: not receiving UDP ZDA...
20210414::225600: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1831
20210414::225600: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225601: Head 2: Error: not receiving UDP ZDA...
20210414::225611: Head 2: Error: not receiving UDP ZDA...
20210414::225621: Head 2: Error: not receiving UDP ZDA...
20210414::225630: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1884
20210414::225630: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225631: Head 2: Error: not receiving UDP ZDA...
20210414::225642: Head 2: Error: not receiving UDP ZDA...
20210414::225652: Head 2: Error: not receiving UDP ZDA...
20210414::225700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225700: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1938
20210414::225700: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225702: Head 2: Error: not receiving UDP ZDA...
20210414::225712: Head 2: Error: not receiving UDP ZDA...
20210414::225722: Head 2: Error: not receiving UDP ZDA...
20210414::225730: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 1991
20210414::225730: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225733: Head 2: Error: not receiving UDP ZDA...
20210414::225743: Head 2: Error: not receiving UDP ZDA...
20210414::225753: Head 2: Error: not receiving UDP ZDA...
20210414::225800: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2044
20210414::225800: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225803: Head 2: Error: not receiving UDP ZDA...
20210414::225813: Head 2: Error: not receiving UDP ZDA...
20210414::225824: Head 2: Error: not receiving UDP ZDA...
20210414::225830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225830: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2098
20210414::225830: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225834: Head 2: Error: not receiving UDP ZDA...
20210414::225844: Head 2: Error: not receiving UDP ZDA...
20210414::225854: Head 2: Error: not receiving UDP ZDA...
20210414::225900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225900: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2152
20210414::225900: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225904: Head 2: Error: not receiving UDP ZDA...
20210414::225915: Head 2: Error: not receiving UDP ZDA...
20210414::225925: Head 2: Error: not receiving UDP ZDA...
20210414::225930: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2205
20210414::225930: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::225935: Head 2: Error: not receiving UDP ZDA...
20210414::225945: Head 2: Error: not receiving UDP ZDA...
20210414::225955: Head 2: Error: not receiving UDP ZDA...
20210414::230000: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2258
20210414::230000: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230006: Head 2: Error: not receiving UDP ZDA...
20210414::230016: Head 2: Error: not receiving UDP ZDA...
20210414::230026: Head 2: Error: not receiving UDP ZDA...
20210414::230030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230030: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2312
20210414::230030: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230036: Head 2: Error: not receiving UDP ZDA...
20210414::230046: Head 2: Error: not receiving UDP ZDA...
20210414::230057: Head 2: Error: not receiving UDP ZDA...
20210414::230100: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2365
20210414::230100: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230107: Head 2: Error: not receiving UDP ZDA...
20210414::230117: Head 2: Error: not receiving UDP ZDA...
20210414::230127: Head 2: Error: not receiving UDP ZDA...
20210414::230130: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2418
20210414::230130: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230137: Head 2: Error: not receiving UDP ZDA...
20210414::230148: Head 2: Error: not receiving UDP ZDA...
20210414::230158: Head 2: Error: not receiving UDP ZDA...
20210414::230200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2472
20210414::230200: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230208: Head 2: Error: not receiving UDP ZDA...
20210414::230218: Head 2: Error: not receiving UDP ZDA...
20210414::230228: Head 2: Error: not receiving UDP ZDA...
20210414::230230: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2525
20210414::230230: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230239: Head 2: Error: not receiving UDP ZDA...
20210414::230249: Head 2: Error: not receiving UDP ZDA...
20210414::230259: Head 2: Error: not receiving UDP ZDA...
20210414::230300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230300: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2579
20210414::230300: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230309: Head 2: Error: not receiving UDP ZDA...
20210414::230320: Head 2: Error: not receiving UDP ZDA...
20210414::230330: Head 2: Error: not receiving UDP ZDA...
20210414::230330: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2632
20210414::230330: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230340: Head 2: Error: not receiving UDP ZDA...
20210414::230350: Head 2: Error: not receiving UDP ZDA...
20210414::230400: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2685
20210414::230400: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230400: Head 2: Error: not receiving UDP ZDA...
20210414::230411: Head 2: Error: not receiving UDP ZDA...
20210414::230421: Head 2: Error: not receiving UDP ZDA...
20210414::230430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230430: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2739
20210414::230430: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230431: Head 2: Error: not receiving UDP ZDA...
20210414::230441: Head 2: Error: not receiving UDP ZDA...
20210414::230451: Head 2: Error: not receiving UDP ZDA...
20210414::230500: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2792
20210414::230500: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230502: Head 2: Error: not receiving UDP ZDA...
20210414::230512: Head 2: Error: not receiving UDP ZDA...
20210414::230522: Head 2: Error: not receiving UDP ZDA...
20210414::230530: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2845
20210414::230530: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230532: Head 2: Error: not receiving UDP ZDA...
20210414::230542: Head 2: Error: not receiving UDP ZDA...
20210414::230553: Head 2: Error: not receiving UDP ZDA...
20210414::230600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230600: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2899
20210414::230600: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230603: Head 2: Error: not receiving UDP ZDA...
20210414::230613: Head 2: Error: not receiving UDP ZDA...
20210414::230623: Head 2: Error: not receiving UDP ZDA...
20210414::230630: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2952
20210414::230630: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230633: Head 2: Error: not receiving UDP ZDA...
20210414::230644: Head 2: Error: not receiving UDP ZDA...
20210414::230654: Head 2: Error: not receiving UDP ZDA...
20210414::230700: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 3005
20210414::230700: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230704: Head 2: Error: not receiving UDP ZDA...
20210414::230714: Head 2: Error: not receiving UDP ZDA...
20210414::230724: Head 2: Error: not receiving UDP ZDA...
20210414::230730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230730: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 3059
20210414::230730: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230735: Head 2: Error: not receiving UDP ZDA...
20210414::230745: Head 2: Error: not receiving UDP ZDA...
20210414::230755: Head 2: Error: not receiving UDP ZDA...
20210414::230800: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 3112
20210414::230800: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 31.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230805: Head 2: Error: not receiving UDP ZDA...
20210414::230815: Head 2: Error: not receiving UDP ZDA...
20210414::230826: Head 2: Error: not receiving UDP ZDA...
20210414::230830: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 3165
20210414::230830: Head #1, Init state OK, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 24%, OPB 23C, Laser 30.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::230843: GUI: Lost Communications with Sensor 1.
20210414::230844: GUI: Lost Communications with Head 2.
20210414::230852: GUI: Attempting Communications with Head 2...
20210414::230902: GUI: Attempting Communications with Head 1...
20210414::230942: GUI: Established Communications with Head 2.
20210414::230943: Head 2: Lost Communications with GUI
20210414::230943: Head 2: Error: not receiving UDP ZDA...
20210414::230943: Head 2: Initializing Communications with GUI ...
20210414::230943: Head 2: Error: not receiving UDP ZDA...
20210414::230944: Head 2: Error: not receiving UDP ZDA...
20210414::230944: Head 2: Error: not receiving UDP ZDA...
20210414::230944: Head 2: Error: not receiving UDP ZDA...
20210414::230945: Head 2: Communications Established.
20210414::230947: Head 2: Error: not receiving UDP ZDA...
20210414::230957: Head 2: Error: not receiving UDP ZDA...
20210414::231000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231008: Head 2: Error: not receiving UDP ZDA...
20210414::231018: Head 2: Error: not receiving UDP ZDA...
20210414::231028: Head 2: Error: not receiving UDP ZDA...
20210414::231030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231038: Head 2: Error: not receiving UDP ZDA...
20210414::231048: Head 2: Error: not receiving UDP ZDA...
20210414::231059: Head 2: Error: not receiving UDP ZDA...
20210414::231100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231109: Head 2: Error: not receiving UDP ZDA...
20210414::231119: Head 2: Error: not receiving UDP ZDA...
20210414::231129: Head 2: Error: not receiving UDP ZDA...
20210414::231130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231139: Head 2: Error: not receiving UDP ZDA...
20210414::231150: Head 2: Error: not receiving UDP ZDA...
20210414::231200: Head 2: Error: not receiving UDP ZDA...
20210414::231200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231210: Head 2: Error: not receiving UDP ZDA...
20210414::231220: Head 2: Error: not receiving UDP ZDA...
20210414::231230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231230: Head 2: Error: not receiving UDP ZDA...
20210414::231241: Head 2: Error: not receiving UDP ZDA...
20210414::231251: Head 2: Error: not receiving UDP ZDA...
20210414::231300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231301: Head 2: Error: not receiving UDP ZDA...
20210414::231311: Head 2: Error: not receiving UDP ZDA...
20210414::231321: Head 2: Error: not receiving UDP ZDA...
20210414::231330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231332: Head 2: Error: not receiving UDP ZDA...
20210414::231342: Head 2: Error: not receiving UDP ZDA...
20210414::231352: Head 2: Error: not receiving UDP ZDA...
20210414::231400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231402: Head 2: Error: not receiving UDP ZDA...
20210414::231412: Head 2: Error: not receiving UDP ZDA...
20210414::231423: Head 2: Error: not receiving UDP ZDA...
20210414::231430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231433: Head 2: Error: not receiving UDP ZDA...
20210414::231443: Head 2: Error: not receiving UDP ZDA...
20210414::231453: Head 2: Error: not receiving UDP ZDA...
20210414::231500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231503: Head 2: Error: not receiving UDP ZDA...
20210414::231514: Head 2: Error: not receiving UDP ZDA...
20210414::231524: Head 2: Error: not receiving UDP ZDA...
20210414::231530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231534: Head 2: Error: not receiving UDP ZDA...
20210414::231544: Head 2: Error: not receiving UDP ZDA...
20210414::231554: Head 2: Error: not receiving UDP ZDA...
20210414::231600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231605: Head 2: Error: not receiving UDP ZDA...
20210414::231615: Head 2: Error: not receiving UDP ZDA...
20210414::231625: Head 2: Error: not receiving UDP ZDA...
20210414::231630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231635: Head 2: Error: not receiving UDP ZDA...
20210414::231645: Head 2: Error: not receiving UDP ZDA...
20210414::231656: Head 2: Error: not receiving UDP ZDA...
20210414::231700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231706: Head 2: Error: not receiving UDP ZDA...
20210414::231716: Head 2: Error: not receiving UDP ZDA...
20210414::231726: Head 2: Error: not receiving UDP ZDA...
20210414::231730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231736: Head 2: Error: not receiving UDP ZDA...
20210414::231747: Head 2: Error: not receiving UDP ZDA...
20210414::231759: Head 2: Error: not receiving UDP ZDA...
20210414::231800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231809: Head 2: Error: not receiving UDP ZDA...
20210414::231819: Head 2: Error: not receiving UDP ZDA...
20210414::231829: Head 2: Error: not receiving UDP ZDA...
20210414::231830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231839: Head 2: Error: not receiving UDP ZDA...
20210414::231850: Head 2: Error: not receiving UDP ZDA...
20210414::231900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231900: Head 2: Error: not receiving UDP ZDA...
20210414::231910: Head 2: Error: not receiving UDP ZDA...
20210414::231920: Head 2: Error: not receiving UDP ZDA...
20210414::231930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 22C, Laser 30.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210414::231930: Head 2: Error: not receiving UDP ZDA...
20210414::231941: Head 2: Error: not receiving UDP ZDA...
20210414::231942: GUI: OnBnClickedOk
20210414::231942: GUI: Exiting the WiSSL GUI..
20210414::231942: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210414::231942: GUI: Wrote configuration data.
