20210426::172731: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210426::172731: GUI: Live mode ON.
20210426::172731: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210426::172731: GUI: WiSSL GUI started at 2021_04_26_17:27:31
20210426::172731: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_26.txt
20210426::172731: GUI: Attempting Communications with Head 1...
20210426::172731: GUI: Attempting Communications with Head 2...
20210426::172735: GUI: Established Communications with Head 1.
20210426::172735: GUI: Established Communications with Head 2.
20210426::172736: Head 1: Initializing Communications with GUI ...
20210426::172736: Head 2: Initializing Communications with GUI ...
20210426::172737: Head 2: Communications Established.
20210426::172737: Head 1: Communications Established.
20210426::172738: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210426::172738: Head 2: Connection Established with the GUI.
20210426::172738: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210426::172738: Head 2: Initializing Subsystems, standby ...
20210426::172738: Head 1: Connection Established with the GUI.
20210426::172739: Head 2: Initializing Hardware, Stand by ...
20210426::172739: Head 1: Initializing Subsystems, standby ...
20210426::172739: Head 1: Initializing Hardware, Stand by ...
20210426::172748: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210426::172748: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210426::172748: Head 2: NtQuery - testing 1 ...
20210426::172749: Head 1: NtQuery - testing 1 ...
20210426::172749: Head 2: clock resolution: 10
20210426::172749: Head 1: clock resolution: 10
20210426::172749: Head 2: NtQuery - testing 2, after setting max res ...
20210426::172749: Head 1: NtQuery - testing 2, after setting max res ...
20210426::172749: Head 2: clock resolution: 10
20210426::172749: Head 1: clock resolution: 10
20210426::172750: Head 2: Initializing Optics Electronics ...
20210426::172750: Head 1: Initializing Optics Electronics ...
20210426::172750: Head 2: Power Laser Controller
20210426::172750: Head 1: Power Laser Controller
20210426::172754: Head 2: Power Scanner Controller
20210426::172754: Head 1: Power Scanner Controller
20210426::172756: Head 2: Power OPTO Sensor
20210426::172756: Head 1: Power OPTO Sensor
20210426::172800: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 44
20210426::172800: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172800: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172816: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::172816: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::172816: Head 2: Eye Safe Optical Filter check Passed
20210426::172816: Head 1: Eye Safe Optical Filter check Passed
20210426::172816: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210426::172817: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210426::172817: Head 2: Initializing Time Sync Subsystem.
20210426::172817: Head 1: Initializing Time Sync Subsystem.
20210426::172817: Head 2: Initializing CTD Subsystem.
20210426::172817: Head 1: Initializing CTD Subsystem.
20210426::172817: Head 2: CTD Initialization Successful
20210426::172817: Head 1: CTD Initialization Successful
20210426::172818: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210426::172818: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210426::172818: Head 2: Time Sync UDP started, waiting for sync...
20210426::172818: Head 1: Time Sync UDP started, waiting for sync...
20210426::172818: Head 2: Attempting CTD Ethernet connection with ROV...
20210426::172818: Head 1: Attempting CTD Ethernet connection with ROV...
20210426::172819: Head 2: Time Synchronization Achieved: 2021.04.26   17:28:19::0014
20210426::172819: Head 1: Time Synchronization Achieved: 2021.04.26   17:28:19::0014
20210426::172829: Head 1: CTD Ethernet connection established.
20210426::172829: Head 2: CTD Ethernet connection established.
20210426::172830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 15C, Laser 13.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172830: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.2C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 98
20210426::172830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 16C, Laser 15.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 16C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172900: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 151
20210426::172900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 16C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172930: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 204
20210426::172930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 17C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::172930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 16C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173000: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 258
20210426::173000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 17C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173030: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 311
20210426::173030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173100: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 364
20210426::173100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173130: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.5dbar, CTD 0.0psu, index 1.34, Packet 418
20210426::173130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173200: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 471
20210426::173200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173230: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 524
20210426::173230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173300: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 578
20210426::173300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173330: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 631
20210426::173330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173400: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 685
20210426::173400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173430: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 738
20210426::173430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173500: Head 1: Time Synchronization: 2021.04.26   17:35:00::0015
20210426::173500: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 791
20210426::173500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173530: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 845
20210426::173530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 19C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173600: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 898
20210426::173600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173630: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 951
20210426::173630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1005
20210426::173700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1058
20210426::173730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173800: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1111
20210426::173800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173830: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1165
20210426::173830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1218
20210426::173900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1271
20210426::173930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::173930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1325
20210426::174000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1378
20210426::174030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174100: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1432
20210426::174100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174130: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1485
20210426::174130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 1539
20210426::174200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174230: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1593
20210426::174230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174300: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1646
20210426::174300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174330: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1699
20210426::174330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174400: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1753
20210426::174400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174430: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.5C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1806
20210426::174430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174500: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1859
20210426::174500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174500: Head 1: Time Synchronization: 2021.04.26   17:45:00::0014
20210426::174500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174530: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1913
20210426::174530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174600: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1966
20210426::174600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174630: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2019
20210426::174630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174700: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2073
20210426::174700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174704: GUI: Live mode ON.
20210426::174704: GUI: Requesing START operation, Head 1
20210426::174704: GUI: Requesing START operation, Head 2
20210426::174704: Head 1: Received request: START
20210426::174704: Head 2: Received request: START
20210426::174704: Head 1: Starting Scan Operation
20210426::174704: Head 2: Starting Scan Operation
20210426::174706: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::174706: Head 2: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::174706: Head 1: Eye Safe Optical Filter check Passed
20210426::174706: Head 2: Eye Safe Optical Filter check Passed
20210426::174730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 1
20210426::174730: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2127
20210426::174730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 1
20210426::174734: Head 1: Configured for WATER Processing
20210426::174735: Head 1: Configured for WATER Processing
20210426::174735: Head 1: Configured for WATER Processing
20210426::174735: Head 1: Configured for WATER Processing
20210426::174736: Head 1: Configured for WATER Processing
20210426::174736: Head 1: Configured for WATER Processing
20210426::174736: Head 1: Configured for WATER Processing
20210426::174736: Head 1: Configured for WATER Processing
20210426::174737: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_174735_tank_dry.raa
20210426::174737: Head 2: Configured for WATER Processing
20210426::174737: Head 1: Configured for WATER Processing
20210426::174737: Head 2: Configured for WATER Processing
20210426::174737: Head 1: Configured for WATER Processing
20210426::174737: Head 2: Configured for WATER Processing
20210426::174737: Head 1: Configured for WATER Processing
20210426::174738: Head 2: Configured for WATER Processing
20210426::174738: Head 1: Configured for WATER Processing
20210426::174738: Head 2: Configured for WATER Processing
20210426::174738: Head 1: Configured for WATER Processing
20210426::174738: Head 2: Configured for WATER Processing
20210426::174738: Head 1: Configured for WATER Processing
20210426::174739: Head 2: Configured for WATER Processing
20210426::174739: Head 1: Configured for WATER Processing
20210426::174739: Head 2: Configured for WATER Processing
20210426::174739: Head 1: Configured for WATER Processing
20210426::174739: Head 2: Configured for WATER Processing
20210426::174739: Head 1: Configured for WATER Processing
20210426::174739: Head 2: Configured for WATER Processing
20210426::174740: Head 1: Configured for WATER Processing
20210426::174740: Head 2: Configured for WATER Processing
20210426::174740: Head 1: Configured for WATER Processing
20210426::174740: Head 2: Configured for WATER Processing
20210426::174740: Head 1: Configured for WATER Processing
20210426::174740: Head 2: Configured for WATER Processing
20210426::174741: Head 2: Configured for WATER Processing
20210426::174741: Head 2: Configured for WATER Processing
20210426::174741: Head 2: Configured for WATER Processing
20210426::174742: Head 2: Configured for WATER Processing
20210426::174742: Head 2: Configured for WATER Processing
20210426::174742: Head 2: Configured for WATER Processing
20210426::174743: Head 2: Configured for WATER Processing
20210426::174745: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_174745_tank_dry.raa
20210426::174748: GUI: Live mode ON.
20210426::174748: GUI: Requesing STOP operation, Head 1
20210426::174748: GUI: Requesing STOP operation, Head 2
20210426::174748: Head 1: Received request: STOP
20210426::174748: Head 2: Received request: STOP
20210426::174749: Head 1: Stopping Scan Operation
20210426::174749: Head 2: Stopping Scan Operation
20210426::174756: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::174756: Head 2: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::174757: Head 1: Eye Safe Optical Filter check Passed
20210426::174757: Head 2: Eye Safe Optical Filter check Passed
20210426::174800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174800: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2180
20210426::174800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174809: Head 1: ProcessingMgr stopped all worker threads.
20210426::174809: Head 1:       Stop finished, may now recover.
20210426::174812: Head 2: ProcessingMgr stopped all worker threads.
20210426::174812: Head 2:       Stop finished, may now recover.
20210426::174830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174830: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2233
20210426::174830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174900: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2287
20210426::174900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174930: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2340
20210426::174930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::174930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175000: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.4C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2394
20210426::175000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175030: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2447
20210426::175030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175100: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2500
20210426::175100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175130: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2554
20210426::175130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175137: Head 1: Warning, CTD not recieved within 2 minutes.
20210426::175137: Head 2: Warning, CTD not recieved within 2 minutes.
20210426::175200: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2607
20210426::175200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210426::175220: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210426::175221: GUI: ERROR: Received Invalid Packet ID: 0
20210426::175222: GUI: Lost Communications with Head 2.
20210426::175222: GUI: Requesing STOP operation, Head 1
20210426::175222: GUI: Attempting Communications with Head 2...
20210426::175223: Head 1: Received request: STOP
20210426::175228: GUI: OnBnClickedOk
20210426::175228: GUI: Exiting the WiSSL GUI..
20210426::175228: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210426::175228: GUI: Wrote configuration data.
20210426::204459: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210426::204459: GUI: Live mode ON.
20210426::204459: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210426::204459: GUI: WiSSL GUI started at 2021_04_26_20:44:59
20210426::204459: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_26.txt
20210426::204500: GUI: Attempting Communications with Head 1...
20210426::204500: GUI: Attempting Communications with Head 2...
20210426::204503: GUI: Established Communications with Head 2.
20210426::204503: GUI: Established Communications with Head 1.
20210426::204504: Head 2: Initializing Communications with GUI ...
20210426::204504: Head 1: Initializing Communications with GUI ...
20210426::204505: Head 2: Communications Established.
20210426::204505: Head 1: Communications Established.
20210426::204506: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210426::204506: Head 2: Connection Established with the GUI.
20210426::204506: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210426::204506: Head 2: Initializing Subsystems, standby ...
20210426::204506: Head 1: Connection Established with the GUI.
20210426::204507: Head 2: Initializing Hardware, Stand by ...
20210426::204507: Head 1: Initializing Subsystems, standby ...
20210426::204507: Head 1: Initializing Hardware, Stand by ...
20210426::204516: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210426::204516: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210426::204517: Head 2: NtQuery - testing 1 ...
20210426::204517: Head 1: NtQuery - testing 1 ...
20210426::204517: Head 2: clock resolution: 10
20210426::204517: Head 1: clock resolution: 10
20210426::204517: Head 2: NtQuery - testing 2, after setting max res ...
20210426::204517: Head 1: NtQuery - testing 2, after setting max res ...
20210426::204517: Head 2: clock resolution: 10
20210426::204518: Head 1: clock resolution: 10
20210426::204518: Head 2: Initializing Optics Electronics ...
20210426::204518: Head 1: Initializing Optics Electronics ...
20210426::204518: Head 2: Power Laser Controller
20210426::204518: Head 1: Power Laser Controller
20210426::204522: Head 2: Power Scanner Controller
20210426::204522: Head 1: Power Scanner Controller
20210426::204524: Head 2: Power OPTO Sensor
20210426::204524: Head 1: Power OPTO Sensor
20210426::204530: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204530: System NOT Initialized, Gain 0, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 48
20210426::204530: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204544: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::204544: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::204544: Head 2: Eye Safe Optical Filter check Passed
20210426::204544: Head 1: Eye Safe Optical Filter check Passed
20210426::204545: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210426::204545: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210426::204545: Head 2: Initializing Time Sync Subsystem.
20210426::204545: Head 1: Initializing Time Sync Subsystem.
20210426::204545: Head 2: Initializing CTD Subsystem.
20210426::204545: Head 1: Initializing CTD Subsystem.
20210426::204546: Head 2: CTD Initialization Successful
20210426::204546: Head 1: CTD Initialization Successful
20210426::204546: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210426::204546: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210426::204546: Head 2: Time Sync UDP started, waiting for sync...
20210426::204546: Head 1: Time Sync UDP started, waiting for sync...
20210426::204546: Head 2: Attempting CTD Ethernet connection with ROV...
20210426::204547: Head 1: Attempting CTD Ethernet connection with ROV...
20210426::204547: Head 2: Time Synchronization Achieved: 2021.04.26   20:45:47::0016
20210426::204548: Head 1: Time Synchronization Achieved: 2021.04.26   20:45:48::0014
20210426::204600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 15.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 101
20210426::204600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 16.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 16.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204630: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 154
20210426::204630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 17C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 17.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204700: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 208
20210426::204700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 18.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204730: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 261
20210426::204730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 18.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204800: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 314
20210426::204800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 19.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204830: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 368
20210426::204830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 19.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204900: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 421
20210426::204900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 20.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::204930: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 475
20210426::204930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 20.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205000: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 528
20210426::205000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205022: Head 1: CTD Ethernet connection established.
20210426::205022: Head 2: CTD Ethernet connection established.
20210426::205030: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 581
20210426::205030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205100: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 635
20210426::205100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205130: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 688
20210426::205130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205200: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 741
20210426::205200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205230: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 795
20210426::205230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205300: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 848
20210426::205300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205330: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 901
20210426::205330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205400: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 955
20210426::205400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205430: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1008
20210426::205430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205500: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1062
20210426::205500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205530: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1115
20210426::205530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205600: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1168
20210426::205600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205630: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1222
20210426::205630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205700: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1275
20210426::205700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205730: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1328
20210426::205730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205800: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1382
20210426::205800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205830: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1435
20210426::205830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205900: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.9C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1488
20210426::205900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1542
20210426::205930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::205943: GUI: Live mode ON.
20210426::205943: GUI: Requesing START operation, Head 1
20210426::205943: GUI: Requesing START operation, Head 2
20210426::205943: Head 1: Received request: START
20210426::205943: Head 2: Received request: START
20210426::205944: Head 1: Starting Scan Operation
20210426::205944: Head 2: Starting Scan Operation
20210426::205945: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210426::205945: Head 1: Eye Safe Optical Filter check Passed
20210426::205946: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::205946: Head 2: Eye Safe Optical Filter check Passed
20210426::205949: Head 1: Configured for WATER Processing
20210426::205950: Head 1: Configured for WATER Processing
20210426::205950: Head 1: Configured for WATER Processing
20210426::205950: Head 1: Configured for WATER Processing
20210426::205951: Head 1: Configured for WATER Processing
20210426::205951: Head 2: Configured for WATER Processing
20210426::205951: Head 1: Configured for WATER Processing
20210426::205951: Head 2: Configured for WATER Processing
20210426::205951: Head 1: Configured for WATER Processing
20210426::205951: Head 2: Configured for WATER Processing
20210426::205952: Head 1: Configured for WATER Processing
20210426::205952: Head 2: Configured for WATER Processing
20210426::205952: Head 1: Configured for WATER Processing
20210426::205952: Head 2: Configured for WATER Processing
20210426::205952: Head 1: Configured for WATER Processing
20210426::205952: Head 2: Configured for WATER Processing
20210426::205952: Head 1: Configured for WATER Processing
20210426::205953: Head 2: Configured for WATER Processing
20210426::205953: Head 1: Configured for WATER Processing
20210426::205953: Head 2: Configured for WATER Processing
20210426::205953: Head 1: Configured for WATER Processing
20210426::205953: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_205951_tank_dry.raa
20210426::205953: Head 2: Configured for WATER Processing
20210426::205953: Head 1: Configured for WATER Processing
20210426::205954: Head 2: Configured for WATER Processing
20210426::205954: Head 1: Configured for WATER Processing
20210426::205954: Head 2: Configured for WATER Processing
20210426::205954: Head 1: Configured for WATER Processing
20210426::205954: Head 2: Configured for WATER Processing
20210426::205954: Head 1: Configured for WATER Processing
20210426::205955: Head 2: Configured for WATER Processing
20210426::205955: Head 1: Configured for WATER Processing
20210426::205955: Head 2: Configured for WATER Processing
20210426::205955: Head 1: Configured for WATER Processing
20210426::205955: Head 1: Configured for WATER Processing
20210426::205955: Head 2: Configured for WATER Processing
20210426::205955: Head 2: Configured for WATER Processing
20210426::205956: Head 2: Configured for WATER Processing
20210426::205956: Head 2: Configured for WATER Processing
20210426::205956: Head 2: Configured for WATER Processing
20210426::205957: Head 2: Configured for WATER Processing
20210426::210000: Head 2: Time Synchronization: 2021.04.26   21:00:00::0015
20210426::210000: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1595
20210426::210000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210426::210000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210426::210001: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_210001_tank_dry.raa
20210426::210009: GUI: Live mode ON.
20210426::210009: GUI: Requesing STOP operation, Head 2
20210426::210009: GUI: Requesing STOP operation, Head 1
20210426::210009: Head 2: Received request: STOP
20210426::210009: Head 1: Received request: STOP
20210426::210010: Head 2: Stopping Scan Operation
20210426::210010: Head 1: Stopping Scan Operation
20210426::210012: Head 1: ProcessingMgr stopped all worker threads.
20210426::210012: Head 1:       Stop finished, may now recover.
20210426::210014: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210426::210014: Head 1: Eye Safe Optical Filter check Passed
20210426::210017: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::210018: Head 2: Eye Safe Optical Filter check Passed
20210426::210030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1649
20210426::210030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210039: Head 2: ProcessingMgr stopped all worker threads.
20210426::210039: Head 2:       Stop finished, may now recover.
20210426::210100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1702
20210426::210100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1755
20210426::210130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1809
20210426::210200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1862
20210426::210230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1916
20210426::210300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1969
20210426::210330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2023
20210426::210400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2076
20210426::210430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210500: Head 1: Time Synchronization: 2021.04.26   21:05:00::0015
20210426::210500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2130
20210426::210500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2183
20210426::210530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.0C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2237
20210426::210600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.7C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 2290
20210426::210630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.7C, CTD 4.4dbar, CTD -1.$psu, index -1.#J, Packet 2343
20210426::210700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.3C, CTD 3.8dbar, CTD -1.$psu, index -1.#J, Packet 2397
20210426::210730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 4.1dbar, CTD -1.$psu, index -1.#J, Packet 2450
20210426::210800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 3.7dbar, CTD 0.0psu, index 1.34, Packet 2504
20210426::210830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210900: Head 1: Time Synchronization: 2021.04.26   21:09:00::0015
20210426::210900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 4.1dbar, CTD 0.0psu, index 1.34, Packet 2557
20210426::210900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.0C, CTD 3.9dbar, CTD 0.0psu, index 1.34, Packet 2610
20210426::210930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::210930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.0C, CTD 3.8dbar, CTD 0.0psu, index 1.34, Packet 2664
20210426::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.0C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 2717
20210426::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 1.3dbar, CTD 0.0psu, index 1.34, Packet 2771
20210426::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.3dbar, CTD 0.0psu, index 1.34, Packet 2824
20210426::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.3dbar, CTD 0.0psu, index 1.34, Packet 2877
20210426::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 2931
20210426::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 2984
20210426::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 3038
20210426::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 3091
20210426::211400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3145
20210426::211430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3198
20210426::211500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 3252
20210426::211530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3305
20210426::211600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211607: Head 1: Comm CTD Error, disconnecting
20210426::211607: Head 2: Comm CTD Error, disconnecting
20210426::211607: Head 1: Warning, CTD not recieved within 2 minutes.
20210426::211607: Head 2: Warning, CTD not recieved within 2 minutes.
20210426::211607: Head 1: Restarting CTD Ethernet connection ...
20210426::211607: Head 2: Restarting CTD Ethernet connection ...
20210426::211630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3359
20210426::211630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3412
20210426::211700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3465
20210426::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3519
20210426::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3572
20210426::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3626
20210426::211900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3680
20210426::211930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::211947: Head 1: CTD Ethernet connection established.
20210426::211947: Head 2: CTD Ethernet connection established.
20210426::212000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3733
20210426::212000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3787
20210426::212030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3840
20210426::212100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 3893
20210426::212130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3947
20210426::212200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 4000
20210426::212230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 4054
20210426::212300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4107
20210426::212330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4160
20210426::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4214
20210426::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4267
20210426::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4321
20210426::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4374
20210426::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4428
20210426::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4481
20210426::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4534
20210426::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4588
20210426::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4641
20210426::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4694
20210426::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::212930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4748
20210426::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4801
20210426::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4854
20210426::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4908
20210426::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4961
20210426::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5014
20210426::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5068
20210426::213230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5121
20210426::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5175
20210426::213330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5228
20210426::213400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5281
20210426::213430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5335
20210426::213500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5388
20210426::213530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5441
20210426::213600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5495
20210426::213630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5549
20210426::213700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.9C, CTD 2.4dbar, CTD 0.0psu, index 1.34, Packet 5602
20210426::213730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.0C, CTD 4.5dbar, CTD 0.0psu, index 1.34, Packet 5656
20210426::213800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.0C, CTD 4.1dbar, CTD 0.0psu, index 1.34, Packet 5709
20210426::213830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.9C, CTD 13.8dbar, CTD 27.5psu, index 1.34, Packet 5763
20210426::213900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::213930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 18.1dbar, CTD 33.3psu, index 1.34, Packet 5816
20210426::213930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 22C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 18.0dbar, CTD 33.3psu, index 1.34, Packet 5869
20210426::214000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.5C, CTD 23.8dbar, CTD 33.6psu, index 1.34, Packet 5923
20210426::214030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.4C, CTD 26.4dbar, CTD 33.7psu, index 1.34, Packet 5977
20210426::214100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 21C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.4C, CTD 25.4dbar, CTD 31.4psu, index 1.34, Packet 6030
20210426::214130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 20C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 19C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.2C, CTD 28.4dbar, CTD 32.1psu, index 1.34, Packet 6083
20210426::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 20C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 19C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.1C, CTD 34.0dbar, CTD 33.4psu, index 1.34, Packet 6137
20210426::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 20C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.8C, CTD 36.9dbar, CTD 33.6psu, index 1.34, Packet 6190
20210426::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 20C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 18C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 35.5dbar, CTD 33.7psu, index 1.34, Packet 6243
20210426::214330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 19C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 18C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.8dbar, CTD 33.7psu, index 1.34, Packet 6297
20210426::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 19C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 18C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.2dbar, CTD 33.7psu, index 1.34, Packet 6350
20210426::214430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 19C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 18C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 18C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.2dbar, CTD 33.7psu, index 1.34, Packet 6404
20210426::214500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 25%, OPB 19C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.8dbar, CTD 33.7psu, index 1.34, Packet 6457
20210426::214530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 19C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 17C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.4dbar, CTD 33.7psu, index 1.34, Packet 6510
20210426::214600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 17C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 17C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 44.5dbar, CTD 33.8psu, index 1.34, Packet 6564
20210426::214630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.8C, CTD 51.1dbar, CTD 33.5psu, index 1.34, Packet 6617
20210426::214700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 17C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 50.5dbar, CTD 33.6psu, index 1.34, Packet 6670
20210426::214730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 17C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 51.4dbar, CTD 33.7psu, index 1.34, Packet 6724
20210426::214800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 17C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 51.8dbar, CTD 33.7psu, index 1.34, Packet 6777
20210426::214830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 17C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 17C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 53.1dbar, CTD 33.7psu, index 1.34, Packet 6831
20210426::214900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.5C, CTD 67.7dbar, CTD 33.7psu, index 1.34, Packet 6884
20210426::214930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 18C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::214930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.4C, CTD 89.9dbar, CTD 33.7psu, index 1.34, Packet 6937
20210426::215000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 110.0dbar, CTD 33.7psu, index 1.34, Packet 6991
20210426::215030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 126.2dbar, CTD 33.9psu, index 1.34, Packet 7044
20210426::215100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.9C, CTD 136.8dbar, CTD 34.0psu, index 1.34, Packet 7098
20210426::215130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 150.0dbar, CTD 34.0psu, index 1.34, Packet 7151
20210426::215200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 151.8dbar, CTD 34.0psu, index 1.34, Packet 7205
20210426::215230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 17C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 16C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.7C, CTD 164.9dbar, CTD 34.0psu, index 1.34, Packet 7258
20210426::215300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 17C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 15C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.6C, CTD 176.4dbar, CTD 34.1psu, index 1.34, Packet 7311
20210426::215330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.4C, CTD 183.8dbar, CTD 34.0psu, index 1.34, Packet 7365
20210426::215400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.3C, CTD 190.2dbar, CTD 34.0psu, index 1.34, Packet 7418
20210426::215430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 25.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 196.6dbar, CTD 34.1psu, index 1.34, Packet 7472
20210426::215500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 203.0dbar, CTD 34.1psu, index 1.34, Packet 7525
20210426::215530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.1C, CTD 215.5dbar, CTD 34.0psu, index 1.34, Packet 7578
20210426::215600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.1C, CTD 225.8dbar, CTD 34.1psu, index 1.34, Packet 7632
20210426::215630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 236.6dbar, CTD 34.1psu, index 1.34, Packet 7685
20210426::215700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 15C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 24.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 257.2dbar, CTD 34.1psu, index 1.34, Packet 7739
20210426::215730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 16C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.9C, CTD 279.7dbar, CTD 34.1psu, index 1.34, Packet 7792
20210426::215800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 16C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.8C, CTD 294.2dbar, CTD 34.0psu, index 1.34, Packet 7845
20210426::215830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.6C, CTD 307.5dbar, CTD 34.1psu, index 1.34, Packet 7899
20210426::215900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.6C, CTD 320.5dbar, CTD 34.1psu, index 1.34, Packet 7952
20210426::215930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::215930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.5C, CTD 336.1dbar, CTD 34.1psu, index 1.34, Packet 8006
20210426::220000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.4C, CTD 353.6dbar, CTD 34.1psu, index 1.34, Packet 8059
20210426::220030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.3C, CTD 371.6dbar, CTD 34.1psu, index 1.34, Packet 8113
20210426::220100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.2C, CTD 378.0dbar, CTD 34.2psu, index 1.34, Packet 8166
20210426::220130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 393.9dbar, CTD 34.2psu, index 1.34, Packet 8219
20210426::220200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 23.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 406.5dbar, CTD 34.2psu, index 1.34, Packet 8273
20210426::220230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 15C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 418.1dbar, CTD 34.1psu, index 1.34, Packet 8326
20210426::220300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 14C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 22.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 22.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.0C, CTD 436.6dbar, CTD 34.1psu, index 1.34, Packet 8380
20210426::220330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 14C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220334: GUI: Live mode ON.
20210426::220334: GUI: Requesing START operation, Head 2
20210426::220334: GUI: Requesing START operation, Head 1
20210426::220334: Head 1: Received request: START
20210426::220334: Head 2: Received request: START
20210426::220334: Head 1: Starting Scan Operation
20210426::220334: Head 2: Starting Scan Operation
20210426::220336: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::220336: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::220336: Head 1: Eye Safe Optical Filter check Passed
20210426::220336: Head 2: Eye Safe Optical Filter check Passed
20210426::220400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.9C, CTD 454.1dbar, CTD 34.2psu, index 1.34, Packet 8433
20210426::220400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 14C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220402: Head 1: Configured for WATER Processing
20210426::220402: Head 1: Configured for WATER Processing
20210426::220402: Head 1: Configured for WATER Processing
20210426::220403: Head 1: Configured for WATER Processing
20210426::220403: Head 1: Configured for WATER Processing
20210426::220403: Head 1: Configured for WATER Processing
20210426::220404: Head 1: Configured for WATER Processing
20210426::220404: Head 1: Configured for WATER Processing
20210426::220404: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220402_tank_dry.raa
20210426::220404: Head 1: Configured for WATER Processing
20210426::220405: Head 1: Configured for WATER Processing
20210426::220405: Head 1: Configured for WATER Processing
20210426::220405: Head 1: Configured for WATER Processing
20210426::220405: Head 1: Configured for WATER Processing
20210426::220406: Head 1: Configured for WATER Processing
20210426::220406: Head 2: Configured for WATER Processing
20210426::220406: Head 1: Configured for WATER Processing
20210426::220406: Head 2: Configured for WATER Processing
20210426::220406: Head 1: Configured for WATER Processing
20210426::220406: Head 2: Configured for WATER Processing
20210426::220407: Head 1: Configured for WATER Processing
20210426::220407: Head 2: Configured for WATER Processing
20210426::220407: Head 1: Configured for WATER Processing
20210426::220407: Head 2: Configured for WATER Processing
20210426::220407: Head 1: Configured for WATER Processing
20210426::220407: Head 2: Configured for WATER Processing
20210426::220408: Head 1: Configured for WATER Processing
20210426::220408: Head 2: Configured for WATER Processing
20210426::220408: Head 2: Configured for WATER Processing
20210426::220408: Head 2: Configured for WATER Processing
20210426::220408: Head 2: Configured for WATER Processing
20210426::220409: Head 2: Configured for WATER Processing
20210426::220409: Head 2: Configured for WATER Processing
20210426::220409: Head 2: Configured for WATER Processing
20210426::220410: Head 2: Configured for WATER Processing
20210426::220410: Head 2: Configured for WATER Processing
20210426::220410: Head 2: Configured for WATER Processing
20210426::220411: Head 2: Configured for WATER Processing
20210426::220411: Head 2: Configured for WATER Processing
20210426::220411: Head 2: Configured for WATER Processing
20210426::220412: Head 2: Configured for WATER Processing
20210426::220412: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220412_tank_dry.raa
20210426::220422: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220422_tank_dry.raa
20210426::220430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210426::220430: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.8C, CTD 474.3dbar, CTD 34.2psu, index 1.34, Packet 8487
20210426::220430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 14C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::220432: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220432_tank_dry.raa
20210426::220442: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220442_tank_dry.raa
20210426::220452: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220452_tank_dry.raa
20210426::220500: Head 1: Time Synchronization: 2021.04.26   22:05:00::0016
20210426::220500: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.7C, CTD 493.4dbar, CTD 34.2psu, index 1.34, Packet 8540
20210426::220500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 14C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::220500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::220502: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220502_tank_dry.raa
20210426::220512: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220512_tank_dry.raa
20210426::220522: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220522_tank_dry.raa
20210426::220524: GUI: Live mode ON.
20210426::220524: GUI: Requesing STOP operation, Head 2
20210426::220524: GUI: Requesing STOP operation, Head 1
20210426::220524: Head 1: Received request: STOP
20210426::220524: Head 2: Received request: STOP
20210426::220525: Head 1: Stopping Scan Operation
20210426::220525: Head 2: Stopping Scan Operation
20210426::220527: Head 2: ProcessingMgr stopped all worker threads.
20210426::220527: Head 1: ProcessingMgr stopped all worker threads.
20210426::220527: Head 2:       Stop finished, may now recover.
20210426::220527: Head 1:       Stop finished, may now recover.
20210426::220530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 0
20210426::220530: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::220530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.7C, CTD 512.3dbar, CTD 34.2psu, index 1.34, Packet 8594
20210426::220530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 14C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220530: Head 1: Eye Safe Optical Filter check Passed
20210426::220532: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::220532: Head 2: Eye Safe Optical Filter check Passed
20210426::220551: GUI: Live mode ON.
20210426::220551: GUI: Requesing START operation, Head 2
20210426::220551: GUI: Requesing START operation, Head 1
20210426::220551: Head 1: Received request: START
20210426::220551: Head 2: Received request: START
20210426::220552: Head 1: Starting Scan Operation
20210426::220552: Head 2: Starting Scan Operation
20210426::220553: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::220553: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::220553: Head 1: Eye Safe Optical Filter check Passed
20210426::220553: Head 2: Eye Safe Optical Filter check Passed
20210426::220557: Head 1: Configured for WATER Processing
20210426::220558: Head 2: Configured for WATER Processing
20210426::220558: Head 1: Configured for WATER Processing
20210426::220558: Head 2: Configured for WATER Processing
20210426::220558: Head 1: Configured for WATER Processing
20210426::220558: Head 2: Configured for WATER Processing
20210426::220558: Head 1: Configured for WATER Processing
20210426::220558: Head 2: Configured for WATER Processing
20210426::220559: Head 1: Configured for WATER Processing
20210426::220559: Head 2: Configured for WATER Processing
20210426::220559: Head 1: Configured for WATER Processing
20210426::220559: Head 2: Configured for WATER Processing
20210426::220559: Head 1: Configured for WATER Processing
20210426::220559: Head 2: Configured for WATER Processing
20210426::220600: Head 1: Configured for WATER Processing
20210426::220600: Head 2: Configured for WATER Processing
20210426::220600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.5C, CTD 529.2dbar, CTD 34.2psu, index 1.34, Packet 8647
20210426::220600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 14C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220600: Head 1: Configured for WATER Processing
20210426::220600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 20.5Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220600: Head 2: Configured for WATER Processing
20210426::220600: Head 1: Configured for WATER Processing
20210426::220600: Head 2: Configured for WATER Processing
20210426::220600: Head 1: Configured for WATER Processing
20210426::220601: Head 2: Configured for WATER Processing
20210426::220601: Head 1: Configured for WATER Processing
20210426::220601: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220559_tank_dry.raa
20210426::220601: Head 2: Configured for WATER Processing
20210426::220601: Head 1: Configured for WATER Processing
20210426::220601: Head 2: Configured for WATER Processing
20210426::220601: Head 1: Configured for WATER Processing
20210426::220601: Head 2: Configured for WATER Processing
20210426::220602: Head 1: Configured for WATER Processing
20210426::220602: Head 2: Configured for WATER Processing
20210426::220602: Head 1: Configured for WATER Processing
20210426::220602: Head 2: Configured for WATER Processing
20210426::220602: Head 1: Configured for WATER Processing
20210426::220602: Head 2: Configured for WATER Processing
20210426::220603: Head 1: Configured for WATER Processing
20210426::220603: Head 2: Configured for WATER Processing
20210426::220603: Head 1: Configured for WATER Processing
20210426::220603: Head 2: Configured for WATER Processing
20210426::220603: Head 1: Configured for WATER Processing
20210426::220603: Head 2: Configured for WATER Processing
20210426::220609: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220609_tank_dry.raa
20210426::220619: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220619_tank_dry.raa
20210426::220629: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220629_tank_dry.raa
20210426::220630: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.3C, CTD 546.5dbar, CTD 34.1psu, index 1.34, Packet 8700
20210426::220630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 14C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::220639: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220639_tank_dry.raa
20210426::220649: GUI: Archiving data to file --> C:\Data\20210412t1\20210426_220649_tank_dry.raa
20210426::220656: GUI: Live mode ON.
20210426::220656: GUI: Requesing STOP operation, Head 1
20210426::220656: GUI: Requesing STOP operation, Head 2
20210426::220656: Head 1: Received request: STOP
20210426::220656: Head 2: Received request: STOP
20210426::220656: Head 1: Stopping Scan Operation
20210426::220656: Head 2: Stopping Scan Operation
20210426::220658: Head 2: ProcessingMgr stopped all worker threads.
20210426::220658: Head 1: ProcessingMgr stopped all worker threads.
20210426::220659: Head 2:       Stop finished, may now recover.
20210426::220659: Head 1:       Stop finished, may now recover.
20210426::220700: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.1C, CTD 555.9dbar, CTD 34.2psu, index 1.34, Packet 8754
20210426::220700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 14C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220700: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::220700: Head 2: Eye Safe Optical Filter check Passed
20210426::220703: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::220703: Head 1: Eye Safe Optical Filter check Passed
20210426::220730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.9C, CTD 572.9dbar, CTD 34.2psu, index 1.34, Packet 8807
20210426::220730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 27%, OPB 14C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 13C, Laser 23.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.8C, CTD 591.5dbar, CTD 34.2psu, index 1.34, Packet 8861
20210426::220800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 26%, OPB 14C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 13C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.8C, CTD 606.1dbar, CTD 34.3psu, index 1.34, Packet 8914
20210426::220830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 26%, OPB 14C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.7C, CTD 617.6dbar, CTD 34.2psu, index 1.34, Packet 8968
20210426::220900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 26%, OPB 14C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.6C, CTD 633.4dbar, CTD 34.2psu, index 1.34, Packet 9021
20210426::220930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::220930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 650.5dbar, CTD 34.3psu, index 1.34, Packet 9074
20210426::221000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 663.9dbar, CTD 34.3psu, index 1.34, Packet 9128
20210426::221030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 677.1dbar, CTD 34.3psu, index 1.34, Packet 9181
20210426::221100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 690.3dbar, CTD 34.3psu, index 1.34, Packet 9235
20210426::221130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 703.7dbar, CTD 34.3psu, index 1.34, Packet 9288
20210426::221200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.2C, CTD 725.1dbar, CTD 34.3psu, index 1.34, Packet 9341
20210426::221230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 749.2dbar, CTD 34.3psu, index 1.34, Packet 9395
20210426::221300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 767.6dbar, CTD 34.3psu, index 1.34, Packet 9448
20210426::221330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 786.6dbar, CTD 34.3psu, index 1.34, Packet 9502
20210426::221400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 796.0dbar, CTD 34.3psu, index 1.34, Packet 9555
20210426::221430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 13C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 810.0dbar, CTD 34.4psu, index 1.34, Packet 9609
20210426::221500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 12C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 822.2dbar, CTD 34.4psu, index 1.34, Packet 9662
20210426::221530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 12C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 837.0dbar, CTD 34.4psu, index 1.34, Packet 9716
20210426::221600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 850.6dbar, CTD 34.4psu, index 1.34, Packet 9769
20210426::221630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 868.6dbar, CTD 34.4psu, index 1.34, Packet 9823
20210426::221700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 883.2dbar, CTD 34.3psu, index 1.34, Packet 9876
20210426::221730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 907.4dbar, CTD 34.4psu, index 1.34, Packet 9929
20210426::221800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 928.6dbar, CTD 34.4psu, index 1.34, Packet 9983
20210426::221830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 941.6dbar, CTD 34.4psu, index 1.34, Packet 10036
20210426::221900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::221930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 946.1dbar, CTD 34.4psu, index 1.34, Packet 10089
20210426::221930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 960.6dbar, CTD 34.4psu, index 1.34, Packet 10143
20210426::222000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 975.3dbar, CTD 34.4psu, index 1.34, Packet 10196
20210426::222030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.8dbar, CTD 34.4psu, index 1.34, Packet 10249
20210426::222100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 12C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1000.8dbar, CTD 34.4psu, index 1.34, Packet 10303
20210426::222130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1005.8dbar, CTD 34.4psu, index 1.34, Packet 10356
20210426::222200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1015.5dbar, CTD 34.4psu, index 1.34, Packet 10409
20210426::222230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.8dbar, CTD 34.4psu, index 1.34, Packet 10463
20210426::222300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.5dbar, CTD 34.4psu, index 1.34, Packet 10516
20210426::222330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1021.9dbar, CTD 34.4psu, index 1.34, Packet 10570
20210426::222400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1027.2dbar, CTD 34.4psu, index 1.34, Packet 10623
20210426::222430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1027.3dbar, CTD 34.4psu, index 1.34, Packet 10676
20210426::222500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 10730
20210426::222530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1026.7dbar, CTD 34.5psu, index 1.34, Packet 10783
20210426::222600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1026.9dbar, CTD 34.5psu, index 1.34, Packet 10836
20210426::222630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 1026.1dbar, CTD 34.4psu, index 1.34, Packet 10890
20210426::222700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.0dbar, CTD 34.5psu, index 1.34, Packet 10943
20210426::222730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.3dbar, CTD 34.4psu, index 1.34, Packet 10997
20210426::222800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.1dbar, CTD 34.5psu, index 1.34, Packet 11050
20210426::222830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1023.0dbar, CTD 34.4psu, index 1.34, Packet 11103
20210426::222900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::222930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1021.8dbar, CTD 34.4psu, index 1.34, Packet 11157
20210426::222930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.9dbar, CTD 34.4psu, index 1.34, Packet 11210
20210426::223000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.2dbar, CTD 34.4psu, index 1.34, Packet 11264
20210426::223030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.3dbar, CTD 34.4psu, index 1.34, Packet 11317
20210426::223100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.5dbar, CTD 34.4psu, index 1.34, Packet 11370
20210426::223130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223200: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.5dbar, CTD 34.4psu, index 1.34, Packet 11424
20210426::223200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223230: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.5psu, index 1.34, Packet 11477
20210426::223230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223300: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11530
20210426::223300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223330: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11584
20210426::223330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223400: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11637
20210426::223400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223430: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11690
20210426::223430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11744
20210426::223500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11797
20210426::223530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.6dbar, CTD 34.4psu, index 1.34, Packet 11850
20210426::223600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223630: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 11904
20210426::223630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223700: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.2dbar, CTD 34.4psu, index 1.34, Packet 11957
20210426::223700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210426::223716: GUI: Live mode ON.
20210426::223716: GUI: Requesing START operation, Head 1
20210426::223716: GUI: Requesing START operation, Head 2
20210426::223717: Head 2: Received request: START
20210426::223717: Head 1: Received request: START
20210426::223717: Head 2: Starting Scan Operation
20210426::223717: Head 1: Starting Scan Operation
20210426::223718: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::223718: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::223719: Head 2: Eye Safe Optical Filter check Passed
20210426::223719: Head 1: Eye Safe Optical Filter check Passed
20210426::223723: Head 2: Configured for WATER Processing
20210426::223723: Head 2: Configured for WATER Processing
20210426::223723: Head 2: Configured for WATER Processing
20210426::223724: Head 2: Configured for WATER Processing
20210426::223724: Head 2: Configured for WATER Processing
20210426::223724: Head 2: Configured for WATER Processing
20210426::223725: Head 2: Configured for WATER Processing
20210426::223725: Head 2: Configured for WATER Processing
20210426::223725: Head 2: Configured for WATER Processing
20210426::223726: Head 2: Configured for WATER Processing
20210426::223726: Head 2: Configured for WATER Processing
20210426::223726: Head 2: Configured for WATER Processing
20210426::223727: Head 2: Configured for WATER Processing
20210426::223727: Head 2: Configured for WATER Processing
20210426::223727: Head 2: Configured for WATER Processing
20210426::223727: Head 2: Configured for WATER Processing
20210426::223728: Head 2: Configured for WATER Processing
20210426::223728: Head 2: Configured for WATER Processing
20210426::223728: Head 2: Configured for WATER Processing
20210426::223729: Head 2: Configured for WATER Processing
20210426::223730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223730: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.2dbar, CTD 34.5psu, index 1.34, Packet 12011
20210426::223730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::223736: Head 1: Configured for WATER Processing
20210426::223737: Head 1: Configured for WATER Processing
20210426::223737: Head 1: Configured for WATER Processing
20210426::223737: Head 1: Configured for WATER Processing
20210426::223737: Head 1: Configured for WATER Processing
20210426::223738: Head 1: Configured for WATER Processing
20210426::223738: Head 1: Configured for WATER Processing
20210426::223738: Head 1: Configured for WATER Processing
20210426::223739: Head 1: Configured for WATER Processing
20210426::223739: Head 1: Configured for WATER Processing
20210426::223739: Head 1: Configured for WATER Processing
20210426::223740: Head 1: Configured for WATER Processing
20210426::223740: Head 1: Configured for WATER Processing
20210426::223740: Head 1: Configured for WATER Processing
20210426::223740: Head 1: Configured for WATER Processing
20210426::223741: Head 1: Configured for WATER Processing
20210426::223741: Head 1: Configured for WATER Processing
20210426::223741: Head 1: Configured for WATER Processing
20210426::223742: Head 1: Configured for WATER Processing
20210426::223742: Head 1: Configured for WATER Processing
20210426::223750: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223749_20210426d1_docr_lidar.raa
20210426::223759: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223759_20210426d1_docr_lidar.raa
20210426::223800: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.5psu, index 1.34, Packet 12064
20210426::223800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223809: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223809_20210426d1_docr_lidar.raa
20210426::223819: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223819_20210426d1_docr_lidar.raa
20210426::223829: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223829_20210426d1_docr_lidar.raa
20210426::223830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223830: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 12118
20210426::223830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223839: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223839_20210426d1_docr_lidar.raa
20210426::223849: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223849_20210426d1_docr_lidar.raa
20210426::223859: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223859_20210426d1_docr_lidar.raa
20210426::223859: Head 2: Time Synchronization: 2021.04.26   22:39:00::0014
20210426::223900: Head 1: Time Synchronization: 2021.04.26   22:39:00::0015
20210426::223900: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 12171
20210426::223900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 9C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223909: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223909_20210426d1_docr_lidar.raa
20210426::223919: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223919_20210426d1_docr_lidar.raa
20210426::223930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223930: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 12225
20210426::223930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20210426::223930: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223930_20210426d1_docr_lidar.raa
20210426::223940: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223940_20210426d1_docr_lidar.raa
20210426::223952: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_223952_20210426d1_docr_lidar.raa
20210426::224000: Head 1: Time Synchronization: 2021.04.26   22:40:00::0017
20210426::224000: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12278
20210426::224000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224002: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224002_20210426d1_docr_lidar.raa
20210426::224012: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224012_20210426d1_docr_lidar.raa
20210426::224022: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224022_20210426d1_docr_lidar.raa
20210426::224030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224030: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.5psu, index 1.34, Packet 12332
20210426::224030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224032: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224032_20210426d1_docr_lidar.raa
20210426::224042: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224042_20210426d1_docr_lidar.raa
20210426::224052: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224052_20210426d1_docr_lidar.raa
20210426::224100: Head 1: Time Synchronization: 2021.04.26   22:41:00::0013
20210426::224100: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12385
20210426::224100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224102: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224102_20210426d1_docr_lidar.raa
20210426::224112: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224112_20210426d1_docr_lidar.raa
20210426::224122: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224122_20210426d1_docr_lidar.raa
20210426::224130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224130: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12439
20210426::224130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224132: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224132_20210426d1_docr_lidar.raa
20210426::224142: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224142_20210426d1_docr_lidar.raa
20210426::224152: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224152_20210426d1_docr_lidar.raa
20210426::224200: Head 1: Time Synchronization: 2021.04.26   22:42:00::0014
20210426::224200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224200: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12492
20210426::224200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224202: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224202_20210426d1_docr_lidar.raa
20210426::224212: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224212_20210426d1_docr_lidar.raa
20210426::224222: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224222_20210426d1_docr_lidar.raa
20210426::224230: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.5psu, index 1.34, Packet 12546
20210426::224230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224232: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224232_20210426d1_docr_lidar.raa
20210426::224242: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224242_20210426d1_docr_lidar.raa
20210426::224252: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224252_20210426d1_docr_lidar.raa
20210426::224300: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12599
20210426::224300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224302: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224302_20210426d1_docr_lidar.raa
20210426::224312: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224312_20210426d1_docr_lidar.raa
20210426::224322: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224322_20210426d1_docr_lidar.raa
20210426::224330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224330: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12653
20210426::224330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224332: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224332_20210426d1_docr_lidar.raa
20210426::224342: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224342_20210426d1_docr_lidar.raa
20210426::224352: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224352_20210426d1_docr_lidar.raa
20210426::224400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224400: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12706
20210426::224400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224402: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224402_20210426d1_docr_lidar.raa
20210426::224412: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224412_20210426d1_docr_lidar.raa
20210426::224422: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224422_20210426d1_docr_lidar.raa
20210426::224430: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12760
20210426::224430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224432: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224432_20210426d1_docr_lidar.raa
20210426::224442: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224442_20210426d1_docr_lidar.raa
20210426::224452: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224452_20210426d1_docr_lidar.raa
20210426::224500: Head 1: Time Synchronization: 2021.04.26   22:45:00::0015
20210426::224500: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12813
20210426::224500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224502: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224502_20210426d1_docr_lidar.raa
20210426::224512: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224512_20210426d1_docr_lidar.raa
20210426::224522: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224522_20210426d1_docr_lidar.raa
20210426::224530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224530: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12867
20210426::224530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224531: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224532_20210426d1_docr_lidar.raa
20210426::224542: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224542_20210426d1_docr_lidar.raa
20210426::224552: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224552_20210426d1_docr_lidar.raa
20210426::224600: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 12920
20210426::224600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224602: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224602_20210426d1_docr_lidar.raa
20210426::224612: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224612_20210426d1_docr_lidar.raa
20210426::224622: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224622_20210426d1_docr_lidar.raa
20210426::224630: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1019.9dbar, CTD 34.4psu, index 1.34, Packet 12973
20210426::224630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224632: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224632_20210426d1_docr_lidar.raa
20210426::224642: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224642_20210426d1_docr_lidar.raa
20210426::224652: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224652_20210426d1_docr_lidar.raa
20210426::224700: Head 1: Time Synchronization: 2021.04.26   22:47:00::0015
20210426::224700: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.0dbar, CTD 34.4psu, index 1.34, Packet 13027
20210426::224700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224702: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224702_20210426d1_docr_lidar.raa
20210426::224712: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224712_20210426d1_docr_lidar.raa
20210426::224722: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224722_20210426d1_docr_lidar.raa
20210426::224730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224730: System  Initialized, Gain 7, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 13081
20210426::224730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20210426::224732: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224732_20210426d1_docr_lidar.raa
20210426::224734: Head 1: Setting Gain 8
20210426::224734: Head 2: Setting Gain 8
20210426::224742: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224742_20210426d1_docr_lidar.raa
20210426::224752: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224752_20210426d1_docr_lidar.raa
20210426::224800: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.1dbar, CTD 34.4psu, index 1.34, Packet 13134
20210426::224800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224802: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224802_20210426d1_docr_lidar.raa
20210426::224812: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224812_20210426d1_docr_lidar.raa
20210426::224812: Head 1: Setting Gain 5
20210426::224812: Head 2: Setting Gain 5
20210426::224822: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224822_20210426d1_docr_lidar.raa
20210426::224830: System  Initialized, Gain 5, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1020.8dbar, CTD 34.4psu, index 1.34, Packet 13187
20210426::224830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::224830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::224832: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224832_20210426d1_docr_lidar.raa
20210426::224842: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224842_20210426d1_docr_lidar.raa
20210426::224849: Head 1: Setting Gain 8
20210426::224849: Head 2: Setting Gain 8
20210426::224852: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224852_20210426d1_docr_lidar.raa
20210426::224900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224900: Head 2: Time Synchronization: 2021.04.26   22:49:00::0017
20210426::224900: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1021.4dbar, CTD 34.4psu, index 1.34, Packet 13241
20210426::224900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224902: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224902_20210426d1_docr_lidar.raa
20210426::224912: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224912_20210426d1_docr_lidar.raa
20210426::224922: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224922_20210426d1_docr_lidar.raa
20210426::224930: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1022.2dbar, CTD 34.4psu, index 1.34, Packet 13294
20210426::224930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::224932: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224932_20210426d1_docr_lidar.raa
20210426::224942: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224942_20210426d1_docr_lidar.raa
20210426::224952: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_224952_20210426d1_docr_lidar.raa
20210426::225000: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1022.9dbar, CTD 34.4psu, index 1.34, Packet 13348
20210426::225000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225002: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225002_20210426d1_docr_lidar.raa
20210426::225012: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225012_20210426d1_docr_lidar.raa
20210426::225022: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225022_20210426d1_docr_lidar.raa
20210426::225030: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1023.6dbar, CTD 34.4psu, index 1.34, Packet 13401
20210426::225030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225032: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225032_20210426d1_docr_lidar.raa
20210426::225042: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225042_20210426d1_docr_lidar.raa
20210426::225052: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225052_20210426d1_docr_lidar.raa
20210426::225100: Head 1: Time Synchronization: 2021.04.26   22:51:00::0015
20210426::225100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225100: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.6dbar, CTD 34.4psu, index 1.34, Packet 13455
20210426::225100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225102: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225102_20210426d1_docr_lidar.raa
20210426::225112: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225112_20210426d1_docr_lidar.raa
20210426::225122: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225122_20210426d1_docr_lidar.raa
20210426::225130: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.6dbar, CTD 34.5psu, index 1.34, Packet 13508
20210426::225130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225132: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225132_20210426d1_docr_lidar.raa
20210426::225142: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225142_20210426d1_docr_lidar.raa
20210426::225152: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225152_20210426d1_docr_lidar.raa
20210426::225200: Head 2: Time Synchronization: 2021.04.26   22:52:00::0016
20210426::225200: Head 1: Time Synchronization: 2021.04.26   22:52:00::0015
20210426::225200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225200: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13562
20210426::225200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225202: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225202_20210426d1_docr_lidar.raa
20210426::225212: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225212_20210426d1_docr_lidar.raa
20210426::225222: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225222_20210426d1_docr_lidar.raa
20210426::225230: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13615
20210426::225230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225232: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225232_20210426d1_docr_lidar.raa
20210426::225242: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225242_20210426d1_docr_lidar.raa
20210426::225252: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225252_20210426d1_docr_lidar.raa
20210426::225300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225300: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13669
20210426::225300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225302: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225302_20210426d1_docr_lidar.raa
20210426::225312: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225312_20210426d1_docr_lidar.raa
20210426::225322: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225322_20210426d1_docr_lidar.raa
20210426::225330: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13722
20210426::225330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225332: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225332_20210426d1_docr_lidar.raa
20210426::225341: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225342_20210426d1_docr_lidar.raa
20210426::225352: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225352_20210426d1_docr_lidar.raa
20210426::225400: Head 1: Time Synchronization: 2021.04.26   22:54:00::0015
20210426::225400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225400: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13776
20210426::225400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225402: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225402_20210426d1_docr_lidar.raa
20210426::225412: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225412_20210426d1_docr_lidar.raa
20210426::225422: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225422_20210426d1_docr_lidar.raa
20210426::225430: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13829
20210426::225430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225432: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225432_20210426d1_docr_lidar.raa
20210426::225442: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225442_20210426d1_docr_lidar.raa
20210426::225452: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225452_20210426d1_docr_lidar.raa
20210426::225500: Head 2: Time Synchronization: 2021.04.26   22:55:00::0015
20210426::225500: Head 1: Time Synchronization: 2021.04.26   22:55:00::0015
20210426::225500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225500: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 13883
20210426::225500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225502: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225502_20210426d1_docr_lidar.raa
20210426::225512: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225512_20210426d1_docr_lidar.raa
20210426::225522: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225522_20210426d1_docr_lidar.raa
20210426::225530: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 13936
20210426::225530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225532: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225532_20210426d1_docr_lidar.raa
20210426::225542: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225542_20210426d1_docr_lidar.raa
20210426::225552: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225552_20210426d1_docr_lidar.raa
20210426::225600: Head 2: Time Synchronization: 2021.04.26   22:56:00::0017
20210426::225600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225600: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 13990
20210426::225600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225602: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225602_20210426d1_docr_lidar.raa
20210426::225612: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225612_20210426d1_docr_lidar.raa
20210426::225622: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225622_20210426d1_docr_lidar.raa
20210426::225630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225630: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14043
20210426::225630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225632: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225632_20210426d1_docr_lidar.raa
20210426::225642: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225642_20210426d1_docr_lidar.raa
20210426::225652: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225652_20210426d1_docr_lidar.raa
20210426::225700: Head 2: Time Synchronization: 2021.04.26   22:57:00::0019
20210426::225700: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.5psu, index 1.34, Packet 14096
20210426::225700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225702: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225702_20210426d1_docr_lidar.raa
20210426::225712: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225712_20210426d1_docr_lidar.raa
20210426::225722: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225722_20210426d1_docr_lidar.raa
20210426::225730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225730: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14150
20210426::225730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225732: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225732_20210426d1_docr_lidar.raa
20210426::225742: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225742_20210426d1_docr_lidar.raa
20210426::225752: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225752_20210426d1_docr_lidar.raa
20210426::225800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225800: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14203
20210426::225800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225802: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225802_20210426d1_docr_lidar.raa
20210426::225812: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225812_20210426d1_docr_lidar.raa
20210426::225822: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225822_20210426d1_docr_lidar.raa
20210426::225830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225830: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14257
20210426::225830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225832: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225832_20210426d1_docr_lidar.raa
20210426::225842: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225842_20210426d1_docr_lidar.raa
20210426::225852: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225852_20210426d1_docr_lidar.raa
20210426::225900: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14310
20210426::225900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225902: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225902_20210426d1_docr_lidar.raa
20210426::225912: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225912_20210426d1_docr_lidar.raa
20210426::225922: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225922_20210426d1_docr_lidar.raa
20210426::225930: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14364
20210426::225930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::225932: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225932_20210426d1_docr_lidar.raa
20210426::225942: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225942_20210426d1_docr_lidar.raa
20210426::225952: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_225952_20210426d1_docr_lidar.raa
20210426::230000: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14417
20210426::230000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230002: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230002_20210426d1_docr_lidar.raa
20210426::230012: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230012_20210426d1_docr_lidar.raa
20210426::230022: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230022_20210426d1_docr_lidar.raa
20210426::230030: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14471
20210426::230030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230032: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230032_20210426d1_docr_lidar.raa
20210426::230042: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230042_20210426d1_docr_lidar.raa
20210426::230052: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230052_20210426d1_docr_lidar.raa
20210426::230100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230100: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14525
20210426::230100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230102: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230102_20210426d1_docr_lidar.raa
20210426::230112: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230112_20210426d1_docr_lidar.raa
20210426::230122: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230122_20210426d1_docr_lidar.raa
20210426::230130: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14578
20210426::230130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230132: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230132_20210426d1_docr_lidar.raa
20210426::230142: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230142_20210426d1_docr_lidar.raa
20210426::230152: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230152_20210426d1_docr_lidar.raa
20210426::230200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230200: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14632
20210426::230200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230202: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230202_20210426d1_docr_lidar.raa
20210426::230212: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230212_20210426d1_docr_lidar.raa
20210426::230222: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230222_20210426d1_docr_lidar.raa
20210426::230230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230230: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14686
20210426::230230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230232: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230232_20210426d1_docr_lidar.raa
20210426::230242: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230242_20210426d1_docr_lidar.raa
20210426::230252: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230252_20210426d1_docr_lidar.raa
20210426::230300: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14739
20210426::230300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230302: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230302_20210426d1_docr_lidar.raa
20210426::230312: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230312_20210426d1_docr_lidar.raa
20210426::230322: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230322_20210426d1_docr_lidar.raa
20210426::230330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230330: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 14793
20210426::230330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230332: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230332_20210426d1_docr_lidar.raa
20210426::230342: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230342_20210426d1_docr_lidar.raa
20210426::230352: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230352_20210426d1_docr_lidar.raa
20210426::230359: Head 1: Time Synchronization: 2021.04.26   23:04:00::0015
20210426::230400: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14846
20210426::230400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230402: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230402_20210426d1_docr_lidar.raa
20210426::230412: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230412_20210426d1_docr_lidar.raa
20210426::230422: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230422_20210426d1_docr_lidar.raa
20210426::230430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230430: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14900
20210426::230430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230432: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230432_20210426d1_docr_lidar.raa
20210426::230442: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230442_20210426d1_docr_lidar.raa
20210426::230451: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230452_20210426d1_docr_lidar.raa
20210426::230500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230500: Head 1: Time Synchronization: 2021.04.26   23:05:00::0015
20210426::230500: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 14953
20210426::230500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230502: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230502_20210426d1_docr_lidar.raa
20210426::230512: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230512_20210426d1_docr_lidar.raa
20210426::230522: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230522_20210426d1_docr_lidar.raa
20210426::230530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230530: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15007
20210426::230530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230532: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230532_20210426d1_docr_lidar.raa
20210426::230542: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230542_20210426d1_docr_lidar.raa
20210426::230552: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230552_20210426d1_docr_lidar.raa
20210426::230600: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15060
20210426::230600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230602: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230602_20210426d1_docr_lidar.raa
20210426::230612: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230612_20210426d1_docr_lidar.raa
20210426::230622: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230622_20210426d1_docr_lidar.raa
20210426::230630: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 15114
20210426::230630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230632: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230632_20210426d1_docr_lidar.raa
20210426::230642: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230642_20210426d1_docr_lidar.raa
20210426::230652: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230652_20210426d1_docr_lidar.raa
20210426::230700: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.8dbar, CTD 34.4psu, index 1.34, Packet 15167
20210426::230700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230702: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230702_20210426d1_docr_lidar.raa
20210426::230712: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230712_20210426d1_docr_lidar.raa
20210426::230722: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230722_20210426d1_docr_lidar.raa
20210426::230730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230730: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15221
20210426::230730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230732: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230732_20210426d1_docr_lidar.raa
20210426::230742: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230742_20210426d1_docr_lidar.raa
20210426::230752: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230752_20210426d1_docr_lidar.raa
20210426::230800: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.1dbar, CTD 34.4psu, index 1.34, Packet 15274
20210426::230800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230802: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230802_20210426d1_docr_lidar.raa
20210426::230812: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230812_20210426d1_docr_lidar.raa
20210426::230822: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230822_20210426d1_docr_lidar.raa
20210426::230830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230830: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15328
20210426::230830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230832: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230832_20210426d1_docr_lidar.raa
20210426::230842: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230842_20210426d1_docr_lidar.raa
20210426::230852: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230852_20210426d1_docr_lidar.raa
20210426::230900: Head 1: Time Synchronization: 2021.04.26   23:09:00::0020
20210426::230900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230900: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15381
20210426::230900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230902: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230902_20210426d1_docr_lidar.raa
20210426::230912: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230912_20210426d1_docr_lidar.raa
20210426::230922: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230922_20210426d1_docr_lidar.raa
20210426::230930: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1024.9dbar, CTD 34.4psu, index 1.34, Packet 15434
20210426::230930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::230932: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230932_20210426d1_docr_lidar.raa
20210426::230942: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230942_20210426d1_docr_lidar.raa
20210426::230952: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_230952_20210426d1_docr_lidar.raa
20210426::230959: Head 1: Time Synchronization: 2021.04.26   23:10:00::0015
20210426::231000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231000: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.0dbar, CTD 34.4psu, index 1.34, Packet 15488
20210426::231000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231002: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231002_20210426d1_docr_lidar.raa
20210426::231012: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231012_20210426d1_docr_lidar.raa
20210426::231022: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231022_20210426d1_docr_lidar.raa
20210426::231030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231030: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.0dbar, CTD 34.4psu, index 1.34, Packet 15541
20210426::231030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231032: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231032_20210426d1_docr_lidar.raa
20210426::231042: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231042_20210426d1_docr_lidar.raa
20210426::231052: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231052_20210426d1_docr_lidar.raa
20210426::231100: Head 2: Time Synchronization: 2021.04.26   23:11:00::0017
20210426::231100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231100: Head 1: Time Synchronization: 2021.04.26   23:11:00::0017
20210426::231100: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.0dbar, CTD 34.4psu, index 1.34, Packet 15594
20210426::231100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231102: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231102_20210426d1_docr_lidar.raa
20210426::231112: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231112_20210426d1_docr_lidar.raa
20210426::231122: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231122_20210426d1_docr_lidar.raa
20210426::231130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231130: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1025.1dbar, CTD 34.4psu, index 1.34, Packet 15648
20210426::231130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231132: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231132_20210426d1_docr_lidar.raa
20210426::231142: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231142_20210426d1_docr_lidar.raa
20210426::231152: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231152_20210426d1_docr_lidar.raa
20210426::231200: Head 2: Time Synchronization: 2021.04.26   23:12:00::0016
20210426::231200: Head 1: Time Synchronization: 2021.04.26   23:12:00::0015
20210426::231200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231200: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1026.2dbar, CTD 34.4psu, index 1.34, Packet 15701
20210426::231200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231202: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231202_20210426d1_docr_lidar.raa
20210426::231212: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231212_20210426d1_docr_lidar.raa
20210426::231222: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231222_20210426d1_docr_lidar.raa
20210426::231230: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 15754
20210426::231230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231232: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231232_20210426d1_docr_lidar.raa
20210426::231242: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231242_20210426d1_docr_lidar.raa
20210426::231252: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231252_20210426d1_docr_lidar.raa
20210426::231300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231300: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 15808
20210426::231300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231302: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231302_20210426d1_docr_lidar.raa
20210426::231312: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231312_20210426d1_docr_lidar.raa
20210426::231322: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231322_20210426d1_docr_lidar.raa
20210426::231330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231330: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 15861
20210426::231330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231332: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231332_20210426d1_docr_lidar.raa
20210426::231342: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231342_20210426d1_docr_lidar.raa
20210426::231352: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231352_20210426d1_docr_lidar.raa
20210426::231400: Head 1: Time Synchronization: 2021.04.26   23:14:00::0013
20210426::231400: Head 2: Time Synchronization: 2021.04.26   23:14:00::0014
20210426::231400: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 15914
20210426::231400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231402: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231402_20210426d1_docr_lidar.raa
20210426::231412: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231412_20210426d1_docr_lidar.raa
20210426::231422: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231422_20210426d1_docr_lidar.raa
20210426::231430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231430: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 15968
20210426::231430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231432: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231432_20210426d1_docr_lidar.raa
20210426::231442: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231442_20210426d1_docr_lidar.raa
20210426::231452: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231452_20210426d1_docr_lidar.raa
20210426::231500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231500: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16021
20210426::231500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231502: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231502_20210426d1_docr_lidar.raa
20210426::231512: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231512_20210426d1_docr_lidar.raa
20210426::231522: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231522_20210426d1_docr_lidar.raa
20210426::231530: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16074
20210426::231530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231532: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231532_20210426d1_docr_lidar.raa
20210426::231542: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231542_20210426d1_docr_lidar.raa
20210426::231552: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231552_20210426d1_docr_lidar.raa
20210426::231600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231600: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16128
20210426::231600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231602: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231602_20210426d1_docr_lidar.raa
20210426::231612: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231612_20210426d1_docr_lidar.raa
20210426::231622: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231622_20210426d1_docr_lidar.raa
20210426::231630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231630: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16181
20210426::231630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231632: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231632_20210426d1_docr_lidar.raa
20210426::231642: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231642_20210426d1_docr_lidar.raa
20210426::231652: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231652_20210426d1_docr_lidar.raa
20210426::231700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231700: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 16235
20210426::231700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231702: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231702_20210426d1_docr_lidar.raa
20210426::231712: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231712_20210426d1_docr_lidar.raa
20210426::231722: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231722_20210426d1_docr_lidar.raa
20210426::231730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231730: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 16288
20210426::231730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231732: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231732_20210426d1_docr_lidar.raa
20210426::231739: GUI: Live mode ON.
20210426::231739: GUI: Requesing STOP operation, Head 2
20210426::231739: GUI: Requesing STOP operation, Head 1
20210426::231740: Head 2: Received request: STOP
20210426::231740: Head 1: Received request: STOP
20210426::231740: Head 2: Stopping Scan Operation
20210426::231740: Head 1: Stopping Scan Operation
20210426::231742: Head 2: ProcessingMgr stopped all worker threads.
20210426::231742: Head 1: ProcessingMgr stopped all worker threads.
20210426::231742: GUI: Live mode ON.
20210426::231742: GUI: Requesing START operation, Head 2
20210426::231742: GUI: Requesing START operation, Head 1
20210426::231743: Head 2:       Stop finished, may now recover.
20210426::231743: Head 1:       Stop finished, may now recover.
20210426::231743: Head 2: Received request: START
20210426::231743: Head 1: Received request: START
20210426::231743: Head 2: Starting Scan Operation
20210426::231743: Head 1: Starting Scan Operation
20210426::231745: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231745: Head 2: Eye Safe Optical Filter check Passed
20210426::231746: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231746: Head 1: Eye Safe Optical Filter check Passed
20210426::231747: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231747: Head 2: Eye Safe Optical Filter check Passed
20210426::231748: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231749: Head 1: Eye Safe Optical Filter check Passed
20210426::231752: Head 2: Configured for WATER Processing
20210426::231752: Head 2: Configured for WATER Processing
20210426::231752: Head 2: Configured for WATER Processing
20210426::231752: Head 2: Configured for WATER Processing
20210426::231753: Head 2: Configured for WATER Processing
20210426::231753: Head 2: Configured for WATER Processing
20210426::231753: Head 2: Configured for WATER Processing
20210426::231754: Head 2: Configured for WATER Processing
20210426::231754: Head 2: Configured for WATER Processing
20210426::231754: Head 2: Configured for WATER Processing
20210426::231755: Head 2: Configured for WATER Processing
20210426::231755: Head 2: Configured for WATER Processing
20210426::231755: Head 2: Configured for WATER Processing
20210426::231756: Head 2: Configured for WATER Processing
20210426::231756: Head 2: Configured for WATER Processing
20210426::231757: Head 2: Configured for WATER Processing
20210426::231757: Head 2: Configured for WATER Processing
20210426::231757: Head 2: Configured for WATER Processing
20210426::231758: Head 2: Configured for WATER Processing
20210426::231758: Head 2: Configured for WATER Processing
20210426::231759: Head 1: Configured for WATER Processing
20210426::231759: Head 1: Configured for WATER Processing
20210426::231800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231800: Head 1: Configured for WATER Processing
20210426::231800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 16342
20210426::231800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::231800: Head 1: Configured for WATER Processing
20210426::231800: Head 1: Configured for WATER Processing
20210426::231801: Head 1: Configured for WATER Processing
20210426::231801: Head 1: Configured for WATER Processing
20210426::231801: Head 1: Configured for WATER Processing
20210426::231802: Head 1: Configured for WATER Processing
20210426::231802: Head 1: Configured for WATER Processing
20210426::231802: Head 1: Configured for WATER Processing
20210426::231803: Head 1: Configured for WATER Processing
20210426::231803: Head 1: Configured for WATER Processing
20210426::231803: Head 1: Configured for WATER Processing
20210426::231803: Head 1: Configured for WATER Processing
20210426::231804: Head 1: Configured for WATER Processing
20210426::231804: Head 1: Configured for WATER Processing
20210426::231804: Head 1: Configured for WATER Processing
20210426::231805: Head 1: Configured for WATER Processing
20210426::231805: Head 1: Configured for WATER Processing
20210426::231813: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231811_20210426d1_docr_lidar.raa
20210426::231821: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231821_20210426d1_docr_lidar.raa
20210426::231830: System  Initialized, Gain 8, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16395
20210426::231830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210426::231831: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231831_20210426d1_docr_lidar.raa
20210426::231841: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231841_20210426d1_docr_lidar.raa
20210426::231842: GUI: Live mode ON.
20210426::231842: GUI: Requesing STOP operation, Head 2
20210426::231842: GUI: Requesing STOP operation, Head 1
20210426::231842: Head 2: Received request: STOP
20210426::231842: Head 1: Received request: STOP
20210426::231842: Head 2: Stopping Scan Operation
20210426::231842: Head 1: Stopping Scan Operation
20210426::231845: Head 2: ProcessingMgr stopped all worker threads.
20210426::231845: Head 2:       Stop finished, may now recover.
20210426::231848: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231848: Head 2: Eye Safe Optical Filter check Passed
20210426::231850: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::231850: Head 1: Eye Safe Optical Filter check Passed
20210426::231851: Head 1: ProcessingMgr stopped all worker threads.
20210426::231852: Head 1:       Stop finished, may now recover.
20210426::231900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16449
20210426::231900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::231900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::231921: Head 1: Setting Gain 9
20210426::231921: Head 2: Setting Gain 9
20210426::231925: GUI: Live mode ON.
20210426::231925: GUI: Requesing START operation, Head 2
20210426::231925: GUI: Requesing START operation, Head 1
20210426::231925: Head 2: Received request: START
20210426::231925: Head 1: Received request: START
20210426::231925: Head 2: Starting Scan Operation
20210426::231925: Head 1: Starting Scan Operation
20210426::231927: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::231927: Head 2: Eye Safe Optical Filter check Passed
20210426::231928: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::231928: Head 1: Eye Safe Optical Filter check Passed
20210426::231930: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16502
20210426::231930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210426::231930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210426::231931: Head 2: Configured for WATER Processing
20210426::231932: Head 2: Configured for WATER Processing
20210426::231932: Head 2: Configured for WATER Processing
20210426::231932: Head 2: Configured for WATER Processing
20210426::231933: Head 2: Configured for WATER Processing
20210426::231933: Head 2: Configured for WATER Processing
20210426::231933: Head 2: Configured for WATER Processing
20210426::231933: Head 2: Configured for WATER Processing
20210426::231934: Head 2: Configured for WATER Processing
20210426::231934: Head 2: Configured for WATER Processing
20210426::231934: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::231934: Head 2: Configured for WATER Processing
20210426::231934: Head 1: Eye Safe Optical Filter check Passed
20210426::231935: Head 2: Configured for WATER Processing
20210426::231935: Head 2: Configured for WATER Processing
20210426::231935: Head 2: Configured for WATER Processing
20210426::231936: Head 2: Configured for WATER Processing
20210426::231936: Head 2: Configured for WATER Processing
20210426::231936: Head 2: Configured for WATER Processing
20210426::231936: Head 2: Configured for WATER Processing
20210426::231937: Head 2: Configured for WATER Processing
20210426::231937: Head 2: Configured for WATER Processing
20210426::231937: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::231938: Head 2: Eye Safe Optical Filter check Passed
20210426::231955: Head 1: Configured for WATER Processing
20210426::231955: Head 1: Configured for WATER Processing
20210426::231955: Head 1: Configured for WATER Processing
20210426::231955: Head 1: Configured for WATER Processing
20210426::231956: Head 1: Configured for WATER Processing
20210426::231956: Head 1: Configured for WATER Processing
20210426::231956: Head 1: Configured for WATER Processing
20210426::231956: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_231955_20210426d1_docr_lidar.raa
20210426::231957: Head 1: Configured for WATER Processing
20210426::231957: Head 1: Configured for WATER Processing
20210426::231957: Head 1: Configured for WATER Processing
20210426::231958: Head 1: Configured for WATER Processing
20210426::231958: Head 1: Configured for WATER Processing
20210426::231958: Head 1: Configured for WATER Processing
20210426::231958: Head 1: Configured for WATER Processing
20210426::231959: Head 1: Configured for WATER Processing
20210426::231959: Head 1: Configured for WATER Processing
20210426::231959: Head 1: Configured for WATER Processing
20210426::232000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232000: Head 1: Configured for WATER Processing
20210426::232000: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16556
20210426::232000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232000: Head 1: Configured for WATER Processing
20210426::232000: Head 1: Configured for WATER Processing
20210426::232000: GUI: Live mode ON.
20210426::232001: GUI: Requesing STOP operation, Head 2
20210426::232001: GUI: Requesing STOP operation, Head 1
20210426::232001: Head 1: Time Synchronization: 2021.04.26   23:20:00::0017
20210426::232001: Head 2: Received request: STOP
20210426::232001: Head 1: Received request: STOP
20210426::232001: Head 2: Stopping Scan Operation
20210426::232001: Head 1: Stopping Scan Operation
20210426::232003: Head 2: ProcessingMgr stopped all worker threads.
20210426::232004: Head 2:       Stop finished, may now recover.
20210426::232005: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::232006: Head 1: Eye Safe Optical Filter check Passed
20210426::232009: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210426::232009: Head 2: Eye Safe Optical Filter check Passed
20210426::232027: Head 1: ProcessingMgr stopped all worker threads.
20210426::232028: Head 1:       Stop finished, may now recover.
20210426::232030: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16609
20210426::232030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20210426::232030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::232100: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 16662
20210426::232100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20210426::232100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210426::232117: GUI: Live mode ON.
20210426::232117: GUI: Requesing START operation, Head 2
20210426::232117: GUI: Requesing START operation, Head 1
20210426::232117: Head 2: Received request: START
20210426::232117: Head 1: Received request: START
20210426::232117: Head 2: Starting Scan Operation
20210426::232117: Head 1: Starting Scan Operation
20210426::232119: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210426::232119: Head 1: Eye Safe Optical Filter check Passed
20210426::232122: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210426::232122: Head 2: Eye Safe Optical Filter check Passed
20210426::232127: Head 2: Configured for WATER Processing
20210426::232127: Head 2: Configured for WATER Processing
20210426::232127: Head 2: Configured for WATER Processing
20210426::232127: Head 2: Configured for WATER Processing
20210426::232128: Head 2: Configured for WATER Processing
20210426::232128: Head 2: Configured for WATER Processing
20210426::232128: Head 2: Configured for WATER Processing
20210426::232129: Head 2: Configured for WATER Processing
20210426::232129: Head 2: Configured for WATER Processing
20210426::232129: Head 2: Configured for WATER Processing
20210426::232130: Head 2: Configured for WATER Processing
20210426::232130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16716
20210426::232130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232130: Head 2: Configured for WATER Processing
20210426::232130: Head 2: Configured for WATER Processing
20210426::232130: Head 2: Configured for WATER Processing
20210426::232131: Head 2: Configured for WATER Processing
20210426::232131: Head 2: Configured for WATER Processing
20210426::232131: Head 2: Configured for WATER Processing
20210426::232132: Head 2: Configured for WATER Processing
20210426::232132: Head 2: Configured for WATER Processing
20210426::232132: Head 2: Configured for WATER Processing
20210426::232147: Head 1: Configured for WATER Processing
20210426::232147: Head 1: Configured for WATER Processing
20210426::232147: Head 1: Configured for WATER Processing
20210426::232148: Head 1: Configured for WATER Processing
20210426::232148: Head 1: Configured for WATER Processing
20210426::232148: Head 1: Configured for WATER Processing
20210426::232148: Head 1: Configured for WATER Processing
20210426::232149: Head 1: Configured for WATER Processing
20210426::232149: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232147_20210426d1_docr_lidar.raa
20210426::232149: Head 1: Configured for WATER Processing
20210426::232149: Head 1: Configured for WATER Processing
20210426::232150: Head 1: Configured for WATER Processing
20210426::232150: Head 1: Configured for WATER Processing
20210426::232150: Head 1: Configured for WATER Processing
20210426::232151: Head 1: Configured for WATER Processing
20210426::232151: Head 1: Configured for WATER Processing
20210426::232151: Head 1: Configured for WATER Processing
20210426::232151: Head 1: Configured for WATER Processing
20210426::232152: Head 1: Configured for WATER Processing
20210426::232152: Head 1: Configured for WATER Processing
20210426::232152: Head 1: Configured for WATER Processing
20210426::232157: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232157_20210426d1_docr_lidar.raa
20210426::232200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232200: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.4psu, index 1.34, Packet 16770
20210426::232200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 27%, OPB 11C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232207: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232207_20210426d1_docr_lidar.raa
20210426::232217: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232217_20210426d1_docr_lidar.raa
20210426::232227: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232227_20210426d1_docr_lidar.raa
20210426::232230: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.5psu, index 1.34, Packet 16823
20210426::232230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 27%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232237: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232237_20210426d1_docr_lidar.raa
20210426::232247: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232247_20210426d1_docr_lidar.raa
20210426::232257: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232257_20210426d1_docr_lidar.raa
20210426::232300: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.8dbar, CTD 34.4psu, index 1.34, Packet 16876
20210426::232300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232300: Head 1: Time Synchronization: 2021.04.26   23:23:00::0017
20210426::232300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 27%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232307: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232307_20210426d1_docr_lidar.raa
20210426::232317: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232317_20210426d1_docr_lidar.raa
20210426::232327: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232327_20210426d1_docr_lidar.raa
20210426::232330: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.9dbar, CTD 34.4psu, index 1.34, Packet 16930
20210426::232330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 29%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232337: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232337_20210426d1_docr_lidar.raa
20210426::232347: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232347_20210426d1_docr_lidar.raa
20210426::232357: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232357_20210426d1_docr_lidar.raa
20210426::232400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232400: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.0dbar, CTD 34.4psu, index 1.34, Packet 16984
20210426::232400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 29%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232407: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232407_20210426d1_docr_lidar.raa
20210426::232417: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232417_20210426d1_docr_lidar.raa
20210426::232427: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232427_20210426d1_docr_lidar.raa
20210426::232430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232430: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.1dbar, CTD 34.5psu, index 1.34, Packet 17037
20210426::232430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232437: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232437_20210426d1_docr_lidar.raa
20210426::232447: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232447_20210426d1_docr_lidar.raa
20210426::232457: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232457_20210426d1_docr_lidar.raa
20210426::232500: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.1dbar, CTD 34.4psu, index 1.34, Packet 17090
20210426::232500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 16C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 28%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232507: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232507_20210426d1_docr_lidar.raa
20210426::232517: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232517_20210426d1_docr_lidar.raa
20210426::232527: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232527_20210426d1_docr_lidar.raa
20210426::232530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232530: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.2dbar, CTD 34.4psu, index 1.34, Packet 17144
20210426::232530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232537: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232537_20210426d1_docr_lidar.raa
20210426::232547: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232547_20210426d1_docr_lidar.raa
20210426::232557: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232557_20210426d1_docr_lidar.raa
20210426::232600: Head 1: Time Synchronization: 2021.04.26   23:26:00::0016
20210426::232600: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.2dbar, CTD 34.4psu, index 1.34, Packet 17197
20210426::232600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232607: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232607_20210426d1_docr_lidar.raa
20210426::232617: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232617_20210426d1_docr_lidar.raa
20210426::232627: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232627_20210426d1_docr_lidar.raa
20210426::232630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232630: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.3dbar, CTD 34.4psu, index 1.34, Packet 17251
20210426::232630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232637: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232637_20210426d1_docr_lidar.raa
20210426::232647: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232647_20210426d1_docr_lidar.raa
20210426::232657: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232657_20210426d1_docr_lidar.raa
20210426::232700: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.2dbar, CTD 34.4psu, index 1.34, Packet 17304
20210426::232700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232707: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232707_20210426d1_docr_lidar.raa
20210426::232717: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232717_20210426d1_docr_lidar.raa
20210426::232727: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232727_20210426d1_docr_lidar.raa
20210426::232730: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.2dbar, CTD 34.4psu, index 1.34, Packet 17358
20210426::232730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232737: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232737_20210426d1_docr_lidar.raa
20210426::232747: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232747_20210426d1_docr_lidar.raa
20210426::232757: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232757_20210426d1_docr_lidar.raa
20210426::232759: Head 1: Time Synchronization: 2021.04.26   23:28:00::0016
20210426::232800: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.1dbar, CTD 34.4psu, index 1.34, Packet 17411
20210426::232800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232807: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232807_20210426d1_docr_lidar.raa
20210426::232817: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232817_20210426d1_docr_lidar.raa
20210426::232827: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232827_20210426d1_docr_lidar.raa
20210426::232830: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.9dbar, CTD 34.4psu, index 1.34, Packet 17465
20210426::232830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232837: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232837_20210426d1_docr_lidar.raa
20210426::232847: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232847_20210426d1_docr_lidar.raa
20210426::232857: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232857_20210426d1_docr_lidar.raa
20210426::232900: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.9dbar, CTD 34.4psu, index 1.34, Packet 17518
20210426::232900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232907: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232907_20210426d1_docr_lidar.raa
20210426::232917: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232917_20210426d1_docr_lidar.raa
20210426::232927: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232927_20210426d1_docr_lidar.raa
20210426::232930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232930: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.9dbar, CTD 34.4psu, index 1.34, Packet 17572
20210426::232930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::232937: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232937_20210426d1_docr_lidar.raa
20210426::232947: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232947_20210426d1_docr_lidar.raa
20210426::232957: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_232957_20210426d1_docr_lidar.raa
20210426::233000: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 17625
20210426::233000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233007: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233007_20210426d1_docr_lidar.raa
20210426::233017: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233017_20210426d1_docr_lidar.raa
20210426::233027: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233027_20210426d1_docr_lidar.raa
20210426::233030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233030: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.1dbar, CTD 34.5psu, index 1.34, Packet 17679
20210426::233030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233037: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233037_20210426d1_docr_lidar.raa
20210426::233047: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233047_20210426d1_docr_lidar.raa
20210426::233057: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233057_20210426d1_docr_lidar.raa
20210426::233100: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.1dbar, CTD 34.4psu, index 1.34, Packet 17732
20210426::233100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233107: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233107_20210426d1_docr_lidar.raa
20210426::233117: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233117_20210426d1_docr_lidar.raa
20210426::233127: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233127_20210426d1_docr_lidar.raa
20210426::233130: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.1dbar, CTD 34.4psu, index 1.34, Packet 17785
20210426::233130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233137: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233137_20210426d1_docr_lidar.raa
20210426::233147: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233147_20210426d1_docr_lidar.raa
20210426::233157: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233157_20210426d1_docr_lidar.raa
20210426::233200: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.2dbar, CTD 34.4psu, index 1.34, Packet 17839
20210426::233200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233207: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233207_20210426d1_docr_lidar.raa
20210426::233217: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233217_20210426d1_docr_lidar.raa
20210426::233227: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233227_20210426d1_docr_lidar.raa
20210426::233230: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.3dbar, CTD 34.4psu, index 1.34, Packet 17892
20210426::233230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233237: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233237_20210426d1_docr_lidar.raa
20210426::233247: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233247_20210426d1_docr_lidar.raa
20210426::233257: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233257_20210426d1_docr_lidar.raa
20210426::233300: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.5dbar, CTD 34.4psu, index 1.34, Packet 17946
20210426::233300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233307: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233307_20210426d1_docr_lidar.raa
20210426::233317: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233317_20210426d1_docr_lidar.raa
20210426::233327: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233327_20210426d1_docr_lidar.raa
20210426::233330: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 17999
20210426::233330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233337: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233337_20210426d1_docr_lidar.raa
20210426::233347: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233347_20210426d1_docr_lidar.raa
20210426::233357: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233357_20210426d1_docr_lidar.raa
20210426::233400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233400: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.7dbar, CTD 34.5psu, index 1.34, Packet 18053
20210426::233400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233407: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233407_20210426d1_docr_lidar.raa
20210426::233417: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233417_20210426d1_docr_lidar.raa
20210426::233427: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233427_20210426d1_docr_lidar.raa
20210426::233430: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 18106
20210426::233430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233437: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233437_20210426d1_docr_lidar.raa
20210426::233447: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233447_20210426d1_docr_lidar.raa
20210426::233457: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233457_20210426d1_docr_lidar.raa
20210426::233500: Head 2: Time Synchronization: 2021.04.26   23:35:00::0016
20210426::233500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233500: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.5dbar, CTD 34.4psu, index 1.34, Packet 18160
20210426::233500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233507: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233507_20210426d1_docr_lidar.raa
20210426::233517: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233517_20210426d1_docr_lidar.raa
20210426::233527: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233527_20210426d1_docr_lidar.raa
20210426::233530: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.5dbar, CTD 34.4psu, index 1.34, Packet 18213
20210426::233530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233537: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233537_20210426d1_docr_lidar.raa
20210426::233547: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233547_20210426d1_docr_lidar.raa
20210426::233557: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233557_20210426d1_docr_lidar.raa
20210426::233600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233600: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 18267
20210426::233600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233607: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233607_20210426d1_docr_lidar.raa
20210426::233617: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233617_20210426d1_docr_lidar.raa
20210426::233627: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233627_20210426d1_docr_lidar.raa
20210426::233630: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.3dbar, CTD 34.4psu, index 1.34, Packet 18320
20210426::233630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233637: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233637_20210426d1_docr_lidar.raa
20210426::233647: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233647_20210426d1_docr_lidar.raa
20210426::233657: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233657_20210426d1_docr_lidar.raa
20210426::233700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233700: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.2dbar, CTD 34.4psu, index 1.34, Packet 18374
20210426::233700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233707: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233707_20210426d1_docr_lidar.raa
20210426::233717: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233717_20210426d1_docr_lidar.raa
20210426::233727: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233727_20210426d1_docr_lidar.raa
20210426::233730: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1026.7dbar, CTD 34.4psu, index 1.34, Packet 18427
20210426::233730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233737: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233737_20210426d1_docr_lidar.raa
20210426::233747: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233747_20210426d1_docr_lidar.raa
20210426::233757: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233757_20210426d1_docr_lidar.raa
20210426::233759: Head 2: Time Synchronization: 2021.04.26   23:38:00::0015
20210426::233800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233800: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 18480
20210426::233800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233807: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233807_20210426d1_docr_lidar.raa
20210426::233817: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233817_20210426d1_docr_lidar.raa
20210426::233827: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233827_20210426d1_docr_lidar.raa
20210426::233830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233830: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.8dbar, CTD 34.4psu, index 1.34, Packet 18534
20210426::233830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233836: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233837_20210426d1_docr_lidar.raa
20210426::233847: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233847_20210426d1_docr_lidar.raa
20210426::233857: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233857_20210426d1_docr_lidar.raa
20210426::233900: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.5dbar, CTD 34.4psu, index 1.34, Packet 18587
20210426::233900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233907: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233907_20210426d1_docr_lidar.raa
20210426::233917: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233917_20210426d1_docr_lidar.raa
20210426::233927: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233927_20210426d1_docr_lidar.raa
20210426::233930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233930: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1029.3dbar, CTD 34.4psu, index 1.34, Packet 18641
20210426::233930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::233937: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233937_20210426d1_docr_lidar.raa
20210426::233947: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233947_20210426d1_docr_lidar.raa
20210426::233957: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_233957_20210426d1_docr_lidar.raa
20210426::234000: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.2dbar, CTD 34.4psu, index 1.34, Packet 18694
20210426::234000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234007: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234007_20210426d1_docr_lidar.raa
20210426::234017: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234017_20210426d1_docr_lidar.raa
20210426::234027: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234027_20210426d1_docr_lidar.raa
20210426::234030: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.1dbar, CTD 34.4psu, index 1.34, Packet 18747
20210426::234030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234037: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234037_20210426d1_docr_lidar.raa
20210426::234047: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234047_20210426d1_docr_lidar.raa
20210426::234057: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234057_20210426d1_docr_lidar.raa
20210426::234100: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.5dbar, CTD 34.4psu, index 1.34, Packet 18801
20210426::234100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234107: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234107_20210426d1_docr_lidar.raa
20210426::234117: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234117_20210426d1_docr_lidar.raa
20210426::234127: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234127_20210426d1_docr_lidar.raa
20210426::234130: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.2dbar, CTD 34.5psu, index 1.34, Packet 18854
20210426::234130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234137: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234137_20210426d1_docr_lidar.raa
20210426::234147: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234147_20210426d1_docr_lidar.raa
20210426::234157: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234157_20210426d1_docr_lidar.raa
20210426::234200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234200: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.0dbar, CTD 34.4psu, index 1.34, Packet 18908
20210426::234200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234207: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234207_20210426d1_docr_lidar.raa
20210426::234217: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234217_20210426d1_docr_lidar.raa
20210426::234227: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234227_20210426d1_docr_lidar.raa
20210426::234230: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.8dbar, CTD 34.4psu, index 1.34, Packet 18961
20210426::234230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234237: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234237_20210426d1_docr_lidar.raa
20210426::234247: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234247_20210426d1_docr_lidar.raa
20210426::234257: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234257_20210426d1_docr_lidar.raa
20210426::234300: Head 1: Time Synchronization: 2021.04.26   23:43:00::0015
20210426::234300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234300: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.4dbar, CTD 34.4psu, index 1.34, Packet 19015
20210426::234300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234307: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234307_20210426d1_docr_lidar.raa
20210426::234317: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234317_20210426d1_docr_lidar.raa
20210426::234327: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234327_20210426d1_docr_lidar.raa
20210426::234330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 29%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234330: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1026.0dbar, CTD 34.4psu, index 1.34, Packet 19068
20210426::234330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234337: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234337_20210426d1_docr_lidar.raa
20210426::234347: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234347_20210426d1_docr_lidar.raa
20210426::234357: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234357_20210426d1_docr_lidar.raa
20210426::234400: Head 2: Time Synchronization: 2021.04.26   23:44:00::0016
20210426::234400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234400: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1024.5dbar, CTD 34.4psu, index 1.34, Packet 19121
20210426::234400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234407: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234407_20210426d1_docr_lidar.raa
20210426::234417: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234417_20210426d1_docr_lidar.raa
20210426::234427: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234427_20210426d1_docr_lidar.raa
20210426::234430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234430: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1023.9dbar, CTD 34.4psu, index 1.34, Packet 19174
20210426::234430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234437: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234437_20210426d1_docr_lidar.raa
20210426::234447: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234447_20210426d1_docr_lidar.raa
20210426::234457: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234457_20210426d1_docr_lidar.raa
20210426::234500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234500: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1024.4dbar, CTD 34.4psu, index 1.34, Packet 19228
20210426::234500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234507: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234507_20210426d1_docr_lidar.raa
20210426::234517: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234517_20210426d1_docr_lidar.raa
20210426::234527: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234527_20210426d1_docr_lidar.raa
20210426::234530: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1025.3dbar, CTD 34.4psu, index 1.34, Packet 19281
20210426::234530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234537: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234537_20210426d1_docr_lidar.raa
20210426::234547: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234547_20210426d1_docr_lidar.raa
20210426::234557: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234557_20210426d1_docr_lidar.raa
20210426::234600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234600: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1026.4dbar, CTD 34.4psu, index 1.34, Packet 19335
20210426::234600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234607: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234607_20210426d1_docr_lidar.raa
20210426::234617: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234617_20210426d1_docr_lidar.raa
20210426::234627: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234627_20210426d1_docr_lidar.raa
20210426::234630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234630: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 19388
20210426::234630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234637: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234637_20210426d1_docr_lidar.raa
20210426::234647: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234647_20210426d1_docr_lidar.raa
20210426::234657: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234657_20210426d1_docr_lidar.raa
20210426::234700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234700: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.9dbar, CTD 34.4psu, index 1.34, Packet 19441
20210426::234700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234707: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234707_20210426d1_docr_lidar.raa
20210426::234717: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234717_20210426d1_docr_lidar.raa
20210426::234727: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234727_20210426d1_docr_lidar.raa
20210426::234730: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.1dbar, CTD 34.4psu, index 1.34, Packet 19494
20210426::234730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234737: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234737_20210426d1_docr_lidar.raa
20210426::234747: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234747_20210426d1_docr_lidar.raa
20210426::234756: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234757_20210426d1_docr_lidar.raa
20210426::234800: Head 1: Time Synchronization: 2021.04.26   23:48:00::0016
20210426::234800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234800: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.1dbar, CTD 34.4psu, index 1.34, Packet 19548
20210426::234800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234807: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234807_20210426d1_docr_lidar.raa
20210426::234817: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234817_20210426d1_docr_lidar.raa
20210426::234827: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234827_20210426d1_docr_lidar.raa
20210426::234830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234830: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.7dbar, CTD 34.4psu, index 1.34, Packet 19601
20210426::234830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234837: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234837_20210426d1_docr_lidar.raa
20210426::234847: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234847_20210426d1_docr_lidar.raa
20210426::234857: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234857_20210426d1_docr_lidar.raa
20210426::234900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234900: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.6dbar, CTD 34.4psu, index 1.34, Packet 19655
20210426::234900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234907: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234907_20210426d1_docr_lidar.raa
20210426::234917: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234917_20210426d1_docr_lidar.raa
20210426::234927: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234927_20210426d1_docr_lidar.raa
20210426::234930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234930: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.2dbar, CTD 34.4psu, index 1.34, Packet 19708
20210426::234930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::234937: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234937_20210426d1_docr_lidar.raa
20210426::234947: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234947_20210426d1_docr_lidar.raa
20210426::234957: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_234957_20210426d1_docr_lidar.raa
20210426::235000: Head 1: Time Synchronization: 2021.04.26   23:50:00::0014
20210426::235000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235000: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.1dbar, CTD 34.4psu, index 1.34, Packet 19762
20210426::235000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235007: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235007_20210426d1_docr_lidar.raa
20210426::235017: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235017_20210426d1_docr_lidar.raa
20210426::235027: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235027_20210426d1_docr_lidar.raa
20210426::235030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235030: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.9dbar, CTD 34.4psu, index 1.34, Packet 19815
20210426::235030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235037: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235037_20210426d1_docr_lidar.raa
20210426::235047: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235047_20210426d1_docr_lidar.raa
20210426::235057: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235057_20210426d1_docr_lidar.raa
20210426::235100: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 19869
20210426::235100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235107: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235107_20210426d1_docr_lidar.raa
20210426::235117: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235117_20210426d1_docr_lidar.raa
20210426::235127: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235127_20210426d1_docr_lidar.raa
20210426::235130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235130: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1026.2dbar, CTD 34.4psu, index 1.34, Packet 19922
20210426::235130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235137: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235137_20210426d1_docr_lidar.raa
20210426::235147: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235147_20210426d1_docr_lidar.raa
20210426::235157: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235157_20210426d1_docr_lidar.raa
20210426::235200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235200: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1024.7dbar, CTD 34.4psu, index 1.34, Packet 19976
20210426::235200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235207: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235207_20210426d1_docr_lidar.raa
20210426::235217: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235217_20210426d1_docr_lidar.raa
20210426::235227: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235227_20210426d1_docr_lidar.raa
20210426::235230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235230: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1024.0dbar, CTD 34.4psu, index 1.34, Packet 20029
20210426::235230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235237: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235237_20210426d1_docr_lidar.raa
20210426::235247: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235247_20210426d1_docr_lidar.raa
20210426::235257: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235257_20210426d1_docr_lidar.raa
20210426::235300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235300: Head 1: Time Synchronization: 2021.04.26   23:53:00::0015
20210426::235300: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1024.3dbar, CTD 34.4psu, index 1.34, Packet 20083
20210426::235300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235306: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235307_20210426d1_docr_lidar.raa
20210426::235317: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235317_20210426d1_docr_lidar.raa
20210426::235327: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235327_20210426d1_docr_lidar.raa
20210426::235330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235330: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1025.2dbar, CTD 34.4psu, index 1.34, Packet 20136
20210426::235330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235337: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235337_20210426d1_docr_lidar.raa
20210426::235347: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235347_20210426d1_docr_lidar.raa
20210426::235357: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235357_20210426d1_docr_lidar.raa
20210426::235400: Head 1: Time Synchronization: 2021.04.26   23:54:00::0016
20210426::235400: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1026.4dbar, CTD 34.4psu, index 1.34, Packet 20189
20210426::235400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235407: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235407_20210426d1_docr_lidar.raa
20210426::235417: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235417_20210426d1_docr_lidar.raa
20210426::235427: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235427_20210426d1_docr_lidar.raa
20210426::235430: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 1027.6dbar, CTD 34.4psu, index 1.34, Packet 20243
20210426::235430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235437: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235437_20210426d1_docr_lidar.raa
20210426::235447: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235447_20210426d1_docr_lidar.raa
20210426::235457: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235457_20210426d1_docr_lidar.raa
20210426::235500: Head 1: Time Synchronization: 2021.04.26   23:55:00::0016
20210426::235500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235500: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.8dbar, CTD 34.4psu, index 1.34, Packet 20297
20210426::235500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235507: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235507_20210426d1_docr_lidar.raa
20210426::235517: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235517_20210426d1_docr_lidar.raa
20210426::235527: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235527_20210426d1_docr_lidar.raa
20210426::235530: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.1dbar, CTD 34.4psu, index 1.34, Packet 20350
20210426::235530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235537: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235537_20210426d1_docr_lidar.raa
20210426::235547: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235547_20210426d1_docr_lidar.raa
20210426::235557: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235557_20210426d1_docr_lidar.raa
20210426::235600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235600: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.1dbar, CTD 34.4psu, index 1.34, Packet 20404
20210426::235600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235607: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235607_20210426d1_docr_lidar.raa
20210426::235617: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235617_20210426d1_docr_lidar.raa
20210426::235627: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235627_20210426d1_docr_lidar.raa
20210426::235630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235630: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.7dbar, CTD 34.4psu, index 1.34, Packet 20458
20210426::235630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235637: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235637_20210426d1_docr_lidar.raa
20210426::235647: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235647_20210426d1_docr_lidar.raa
20210426::235657: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235657_20210426d1_docr_lidar.raa
20210426::235700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235700: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.6dbar, CTD 34.4psu, index 1.34, Packet 20512
20210426::235700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235707: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235707_20210426d1_docr_lidar.raa
20210426::235717: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235717_20210426d1_docr_lidar.raa
20210426::235727: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235727_20210426d1_docr_lidar.raa
20210426::235730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235730: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.5dbar, CTD 34.4psu, index 1.34, Packet 20565
20210426::235730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235737: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235737_20210426d1_docr_lidar.raa
20210426::235747: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235747_20210426d1_docr_lidar.raa
20210426::235757: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235757_20210426d1_docr_lidar.raa
20210426::235800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235800: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.5dbar, CTD 34.4psu, index 1.34, Packet 20619
20210426::235800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235807: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235807_20210426d1_docr_lidar.raa
20210426::235817: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235817_20210426d1_docr_lidar.raa
20210426::235827: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235827_20210426d1_docr_lidar.raa
20210426::235830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235830: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1031.1dbar, CTD 34.4psu, index 1.34, Packet 20672
20210426::235830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235837: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235837_20210426d1_docr_lidar.raa
20210426::235847: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235847_20210426d1_docr_lidar.raa
20210426::235857: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235857_20210426d1_docr_lidar.raa
20210426::235900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235900: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1030.5dbar, CTD 34.4psu, index 1.34, Packet 20727
20210426::235900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235907: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235907_20210426d1_docr_lidar.raa
20210426::235917: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235917_20210426d1_docr_lidar.raa
20210426::235927: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235927_20210426d1_docr_lidar.raa
20210426::235930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 30%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235930: System  Initialized, Gain 9, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1029.7dbar, CTD 34.4psu, index 1.34, Packet 20782
20210426::235930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 31%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 1
20210426::235937: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235937_20210426d1_docr_lidar.raa
20210426::235947: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235947_20210426d1_docr_lidar.raa
20210426::235957: GUI: Archiving data to file --> C:\Data\20210426d1\20210426_235957_20210426d1_docr_lidar.raa
