20210818::210048: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210818::210048: GUI: Live mode ON.
20210818::210048: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210818::210048: GUI: WiSSL GUI started at 2021_08_18_21:00:48
20210818::210048: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_08_18.txt
20210818::210048: GUI: Attempting Communications with Head 1...
20210818::210048: GUI: Attempting Communications with Head 2...
20210818::210052: GUI: Established Communications with Head 1.
20210818::210052: GUI: Established Communications with Head 2.
20210818::210052: Head 1: Initializing Communications with GUI ...
20210818::210052: Head 2: Initializing Communications with GUI ...
20210818::210053: Head 1: Communications Established.
20210818::210053: Head 2: Communications Established.
20210818::210054: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210818::210055: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210818::210055: Head 2: Connection Established with the GUI.
20210818::210055: Head 1: Connection Established with the GUI.
20210818::210055: Head 2: Initializing Subsystems, standby ...
20210818::210055: Head 1: Initializing Subsystems, standby ...
20210818::210055: Head 2: Initializing Hardware, Stand by ...
20210818::210055: Head 1: Initializing Hardware, Stand by ...
20210818::210100: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210100: System NOT Initialized, Gain 0, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 20
20210818::210100: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210105: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210818::210105: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210818::210105: Head 1: NtQuery - testing 1 ...
20210818::210105: Head 2: NtQuery - testing 1 ...
20210818::210105: Head 1: clock resolution: 10
20210818::210106: Head 2: clock resolution: 10
20210818::210106: Head 1: NtQuery - testing 2, after setting max res ...
20210818::210106: Head 2: NtQuery - testing 2, after setting max res ...
20210818::210106: Head 1: clock resolution: 10
20210818::210106: Head 2: clock resolution: 10
20210818::210106: Head 1: Initializing Optics Electronics ...
20210818::210107: Head 2: Initializing Optics Electronics ...
20210818::210107: Head 1: Power Laser Controller
20210818::210107: Head 2: Power Laser Controller
20210818::210110: Head 1: Power Scanner Controller
20210818::210111: Head 2: Power Scanner Controller
20210818::210113: Head 1: Power OPTO Sensor
20210818::210113: Head 2: Power OPTO Sensor
20210818::210130: System NOT Initialized, Gain 0, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 73
20210818::210130: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210130: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210133: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::210133: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210818::210133: Head 1: Eye Safe Optical Filter check Passed
20210818::210133: Head 2: Eye Safe Optical Filter check Passed
20210818::210133: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210818::210134: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210818::210134: Head 1: Initializing Time Sync Subsystem.
20210818::210134: Head 2: Initializing Time Sync Subsystem.
20210818::210134: Head 1: Initializing CTD Subsystem.
20210818::210134: Head 2: Initializing CTD Subsystem.
20210818::210134: Head 1: CTD Initialization Successful
20210818::210134: Head 2: CTD Initialization Successful
20210818::210135: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210818::210135: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210818::210135: Head 1: Time Sync UDP started, waiting for sync...
20210818::210135: Head 2: Time Sync UDP started, waiting for sync...
20210818::210135: Head 1: Attempting CTD Ethernet connection with ROV...
20210818::210135: Head 2: Attempting CTD Ethernet connection with ROV...
20210818::210136: Head 1: Time Synchronization Achieved: 2021.08.18   21:01:36::0017
20210818::210136: Head 2: Time Synchronization Achieved: 2021.08.18   21:01:36::0017
20210818::210200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 26%, OPB 21C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210200: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 127
20210818::210200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 26%, OPB 21C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210208: Head 1: CTD Ethernet connection established.
20210818::210208: Head 2: CTD Ethernet connection established.
20210818::210230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 24%, OPB 21C, Laser 21.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210230: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.9C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 180
20210818::210230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 25%, OPB 21C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210300: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 233
20210818::210300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 24%, OPB 22C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 21C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 21C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210330: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 287
20210818::210330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 23%, OPB 22C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210400: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 340
20210818::210400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 21C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210430: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 394
20210818::210430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210500: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 447
20210818::210500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210530: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 500
20210818::210530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 22C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 24.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 554
20210818::210600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 24.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 607
20210818::210630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210700: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.5C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 660
20210818::210700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210730: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 714
20210818::210730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 26.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210800: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 767
20210818::210800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210830: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 820
20210818::210830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 26.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 26.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210900: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 874
20210818::210900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 27.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 26.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::210930: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 2.1dbar, CTD -1.$psu, index -1.#J, Packet 927
20210818::210930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 27.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211000: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 2.1dbar, CTD -1.$psu, index -1.#J, Packet 980
20210818::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 27.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 27.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211030: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1034
20210818::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211100: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1087
20210818::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 27.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211130: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1140
20210818::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 27.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 28.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211200: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1194
20210818::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211230: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1247
20210818::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 24C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 23C, Laser 28.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211300: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1300
20210818::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 24C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 28.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 28.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211330: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1354
20210818::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211400: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1407
20210818::211400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 28.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211430: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1460
20210818::211430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211500: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1514
20210818::211500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211530: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1567
20210818::211530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211600: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1620
20210818::211600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 24C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211630: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1674
20210818::211630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211700: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1727
20210818::211700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 25C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211730: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1780
20210818::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 25C, Laser 29.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 21%, OPB 25C, Laser 30.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211800: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1834
20210818::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 26C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211830: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 1887
20210818::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 26C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 30.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211900: Head 2: Time Synchronization: 2021.08.18   21:19:00::0018
20210818::211900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 30.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211900: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 1941
20210818::211900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 26C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211930: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.8dbar, CTD -1.$psu, index -1.#J, Packet 1994
20210818::211930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 26C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::211930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 30.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212000: Head 1: Time Synchronization: 2021.08.18   21:20:00::0015
20210818::212000: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.8dbar, CTD -1.$psu, index -1.#J, Packet 2047
20210818::212000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 26C, Laser 31.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212000: Head 2: Time Synchronization: 2021.08.18   21:20:00::0015
20210818::212000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 30.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 31.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212030: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.8dbar, CTD -1.$psu, index -1.#J, Packet 2101
20210818::212030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 32.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212100: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2154
20210818::212100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 32.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 31.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212130: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2207
20210818::212130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 32.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 31.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212133: GUI: Live mode ON.
20210818::212133: GUI: Requesing START operation, Head 1
20210818::212133: GUI: Requesing START operation, Head 2
20210818::212133: Head 1: Received request: START
20210818::212133: Head 2: Received request: START
20210818::212133: Head 1: Starting Scan Operation
20210818::212133: Head 2: Starting Scan Operation
20210818::212135: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::212135: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210818::212135: Head 2: Eye Safe Optical Filter check Passed
20210818::212135: Head 1: Eye Safe Optical Filter check Passed
20210818::212139: Head 2: Configured for WATER Processing
20210818::212139: Head 1: Configured for WATER Processing
20210818::212140: Head 2: Configured for WATER Processing
20210818::212140: Head 1: Configured for WATER Processing
20210818::212140: Head 2: Configured for WATER Processing
20210818::212140: Head 1: Configured for WATER Processing
20210818::212140: Head 2: Configured for WATER Processing
20210818::212140: Head 1: Configured for WATER Processing
20210818::212140: Head 2: Configured for WATER Processing
20210818::212141: Head 1: Configured for WATER Processing
20210818::212141: Head 2: Configured for WATER Processing
20210818::212141: Head 1: Configured for WATER Processing
20210818::212141: Head 2: Configured for WATER Processing
20210818::212141: Head 1: Configured for WATER Processing
20210818::212141: Head 2: Configured for WATER Processing
20210818::212141: Head 1: Configured for WATER Processing
20210818::212142: Head 2: Configured for WATER Processing
20210818::212142: Head 1: Configured for WATER Processing
20210818::212142: Head 2: Configured for WATER Processing
20210818::212142: Head 1: Configured for WATER Processing
20210818::212142: Head 2: Configured for WATER Processing
20210818::212142: Head 1: Configured for WATER Processing
20210818::212143: Head 2: Configured for WATER Processing
20210818::212143: Head 1: Configured for WATER Processing
20210818::212143: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212141_mbari_wissl_lidar.raa
20210818::212143: Head 2: Configured for WATER Processing
20210818::212143: Head 1: Configured for WATER Processing
20210818::212143: Head 2: Configured for WATER Processing
20210818::212143: Head 1: Configured for WATER Processing
20210818::212144: Head 2: Configured for WATER Processing
20210818::212144: Head 1: Configured for WATER Processing
20210818::212144: Head 2: Configured for WATER Processing
20210818::212144: Head 1: Configured for WATER Processing
20210818::212144: Head 2: Configured for WATER Processing
20210818::212144: Head 1: Configured for WATER Processing
20210818::212144: Head 2: Configured for WATER Processing
20210818::212144: Head 1: Configured for WATER Processing
20210818::212145: Head 2: Configured for WATER Processing
20210818::212145: Head 1: Configured for WATER Processing
20210818::212145: Head 2: Configured for WATER Processing
20210818::212145: Head 1: Configured for WATER Processing
20210818::212151: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212151_mbari_wissl_lidar.raa
20210818::212200: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2261
20210818::212200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 32.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 31.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212201: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212201_mbari_wissl_lidar.raa
20210818::212211: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212211_mbari_wissl_lidar.raa
20210818::212221: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212221_mbari_wissl_lidar.raa
20210818::212230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 32.0C, Dig 45.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212230: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2315
20210818::212230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 33.0C, Dig 40.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212231: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212231_mbari_wissl_lidar.raa
20210818::212241: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212241_mbari_wissl_lidar.raa
20210818::212251: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212251_mbari_wissl_lidar.raa
20210818::212300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 32.0C, Dig 47.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212300: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2368
20210818::212300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 34.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212301: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212301_mbari_wissl_lidar.raa
20210818::212311: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212311_mbari_wissl_lidar.raa
20210818::212321: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212321_mbari_wissl_lidar.raa
20210818::212330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 32.0C, Dig 47.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212330: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2421
20210818::212330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 33.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212331: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212331_mbari_wissl_lidar.raa
20210818::212341: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212341_mbari_wissl_lidar.raa
20210818::212351: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212351_mbari_wissl_lidar.raa
20210818::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212400: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2474
20210818::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 33.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212401: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212401_mbari_wissl_lidar.raa
20210818::212411: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212411_mbari_wissl_lidar.raa
20210818::212421: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212421_mbari_wissl_lidar.raa
20210818::212430: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2527
20210818::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 26C, Laser 34.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212431: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212431_mbari_wissl_lidar.raa
20210818::212439: GUI: Live mode ON.
20210818::212439: GUI: Requesing STOP operation, Head 1
20210818::212439: GUI: Requesing STOP operation, Head 2
20210818::212439: Head 2: Received request: STOP
20210818::212439: Head 1: Received request: STOP
20210818::212439: Head 2: Stopping Scan Operation
20210818::212440: Head 1: Stopping Scan Operation
20210818::212442: Head 2: ProcessingMgr stopped all worker threads.
20210818::212442: Head 2:       Stop finished, may now recover.
20210818::212442: GUI: Live mode ON.
20210818::212442: GUI: Requesing START operation, Head 1
20210818::212442: GUI: Requesing START operation, Head 2
20210818::212443: Head 2: Received request: START
20210818::212443: Head 1: Received request: START
20210818::212443: Head 2: Starting Scan Operation
20210818::212446: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::212446: Head 2: Eye Safe Optical Filter check Passed
20210818::212446: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210818::212447: Head 1: Eye Safe Optical Filter check Passed
20210818::212448: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::212448: Head 2: Eye Safe Optical Filter check Passed
20210818::212453: Head 2: Configured for WATER Processing
20210818::212453: Head 2: Configured for WATER Processing
20210818::212453: Head 2: Configured for WATER Processing
20210818::212454: Head 2: Configured for WATER Processing
20210818::212454: Head 2: Configured for WATER Processing
20210818::212454: Head 2: Configured for WATER Processing
20210818::212454: Head 2: Configured for WATER Processing
20210818::212455: Head 2: Configured for WATER Processing
20210818::212455: Head 2: Configured for WATER Processing
20210818::212455: Head 2: Configured for WATER Processing
20210818::212456: Head 2: Configured for WATER Processing
20210818::212456: Head 2: Configured for WATER Processing
20210818::212457: Head 2: Configured for WATER Processing
20210818::212457: Head 2: Configured for WATER Processing
20210818::212458: Head 2: Configured for WATER Processing
20210818::212458: Head 2: Configured for WATER Processing
20210818::212458: Head 2: Configured for WATER Processing
20210818::212458: Head 2: Configured for WATER Processing
20210818::212459: Head 2: Configured for WATER Processing
20210818::212459: Head 2: Configured for WATER Processing
20210818::212500: Head 2: Time Synchronization: 2021.08.18   21:25:00::0015
20210818::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212500: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2581
20210818::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 34.0C, Dig 43.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212502: Head 1: ProcessingMgr stopped all worker threads.
20210818::212502: Head 1:       Stop finished, may now recover.
20210818::212511: GUI: Live mode ON.
20210818::212511: GUI: Requesing STOP operation, Head 1
20210818::212511: GUI: Requesing STOP operation, Head 2
20210818::212511: Head 1: Received request: STOP
20210818::212511: Head 2: Received request: STOP
20210818::212511: Head 1: Stopping Scan Operation
20210818::212511: Head 2: Stopping Scan Operation
20210818::212513: Head 2: ProcessingMgr stopped all worker threads.
20210818::212514: Head 2:       Stop finished, may now recover.
20210818::212517: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::212517: Head 2: Eye Safe Optical Filter check Passed
20210818::212518: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210818::212518: Head 1: Eye Safe Optical Filter check Passed
20210818::212530: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2634
20210818::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 33.0C, Dig 43.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 32.0C, Dig 48.0C, Scan Az fault 0, gain 0, laser state 0
20210818::212534: Head 1:       Stop finished, may now recover.
20210818::212540: GUI: Live mode ON.
20210818::212541: GUI: Requesing START operation, Head 2
20210818::212541: GUI: Requesing START operation, Head 1
20210818::212541: Head 1: Received request: START
20210818::212541: Head 2: Received request: START
20210818::212541: Head 1: Starting Scan Operation
20210818::212541: Head 2: Starting Scan Operation
20210818::212545: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210818::212545: Head 2: Eye Safe Optical Filter check Passed
20210818::212546: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20210818::212546: Head 1: Eye Safe Optical Filter check Passed
20210818::212549: Head 2: Configured for WATER Processing
20210818::212550: Head 2: Configured for WATER Processing
20210818::212550: Head 2: Configured for WATER Processing
20210818::212550: Head 2: Configured for WATER Processing
20210818::212551: Head 2: Configured for WATER Processing
20210818::212551: Head 2: Configured for WATER Processing
20210818::212551: Head 2: Configured for WATER Processing
20210818::212552: Head 2: Configured for WATER Processing
20210818::212552: Head 2: Configured for WATER Processing
20210818::212552: Head 2: Configured for WATER Processing
20210818::212553: Head 2: Configured for WATER Processing
20210818::212553: Head 2: Configured for WATER Processing
20210818::212553: Head 2: Configured for WATER Processing
20210818::212553: Head 2: Configured for WATER Processing
20210818::212554: Head 2: Configured for WATER Processing
20210818::212554: Head 2: Configured for WATER Processing
20210818::212554: Head 2: Configured for WATER Processing
20210818::212555: Head 2: Configured for WATER Processing
20210818::212555: Head 2: Configured for WATER Processing
20210818::212555: Head 2: Configured for WATER Processing
20210818::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 32.0C, Dig 47.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212600: System  Initialized, Gain 1, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.7dbar, CTD -1.$psu, index -1.#J, Packet 2688
20210818::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 33.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 1
20210818::212621: Head 1: Configured for WATER Processing
20210818::212622: Head 1: Configured for WATER Processing
20210818::212622: Head 1: Configured for WATER Processing
20210818::212622: Head 1: Configured for WATER Processing
20210818::212623: Head 1: Configured for WATER Processing
20210818::212623: Head 1: Configured for WATER Processing
20210818::212623: Head 1: Configured for WATER Processing
20210818::212623: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212622_mbari_wissl_lidar.raa
20210818::212623: Head 1: Configured for WATER Processing
20210818::212624: Head 1: Configured for WATER Processing
20210818::212624: Head 1: Configured for WATER Processing
20210818::212625: Head 1: Configured for WATER Processing
20210818::212625: Head 1: Configured for WATER Processing
20210818::212625: Head 1: Configured for WATER Processing
20210818::212626: Head 1: Configured for WATER Processing
20210818::212626: Head 1: Configured for WATER Processing
20210818::212627: Head 1: Configured for WATER Processing
20210818::212627: Head 1: Configured for WATER Processing
20210818::212628: Head 1: Configured for WATER Processing
20210818::212628: Head 1: Configured for WATER Processing
20210818::212628: Head 1: Configured for WATER Processing
20210818::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 47.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212630: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 2.6dbar, CTD -1.$psu, index -1.#J, Packet 2741
20210818::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 34.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212632: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212632_mbari_wissl_lidar.raa
20210818::212643: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212643_mbari_wissl_lidar.raa
20210818::212653: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212653_mbari_wissl_lidar.raa
20210818::212700: Head 1: Time Synchronization: 2021.08.18   21:27:00::0017
20210818::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212700: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.7C, CTD 6.0dbar, CTD -1.$psu, index -1.#J, Packet 2794
20210818::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 34.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212703: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212703_mbari_wissl_lidar.raa
20210818::212713: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212713_mbari_wissl_lidar.raa
20210818::212723: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212723_mbari_wissl_lidar.raa
20210818::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212730: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 1.3psu, index 1.34, Packet 2847
20210818::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 34.0C, Dig 41.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212733: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212733_mbari_wissl_lidar.raa
20210818::212744: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212743_mbari_wissl_lidar.raa
20210818::212753: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212753_mbari_wissl_lidar.raa
20210818::212800: Head 1: Time Synchronization: 2021.08.18   21:28:00::0015
20210818::212800: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 2.2psu, index 1.34, Packet 2901
20210818::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 34.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212803: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212803_mbari_wissl_lidar.raa
20210818::212813: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212813_mbari_wissl_lidar.raa
20210818::212823: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212823_mbari_wissl_lidar.raa
20210818::212830: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 3.9psu, index 1.34, Packet 2954
20210818::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 35.0C, Dig 42.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 33.0C, Dig 48.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212833: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212833_mbari_wissl_lidar.raa
20210818::212843: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212843_mbari_wissl_lidar.raa
20210818::212853: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212853_mbari_wissl_lidar.raa
20210818::212900: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.5psu, index 1.34, Packet 3007
20210818::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212900: Head 1: Time Synchronization: 2021.08.18   21:29:00::0015
20210818::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 33.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212903: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212903_mbari_wissl_lidar.raa
20210818::212913: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212913_mbari_wissl_lidar.raa
20210818::212923: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212923_mbari_wissl_lidar.raa
20210818::212930: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.6psu, index 1.34, Packet 3061
20210818::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 33.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::212933: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212933_mbari_wissl_lidar.raa
20210818::212943: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212943_mbari_wissl_lidar.raa
20210818::212953: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_212953_mbari_wissl_lidar.raa
20210818::213000: Head 1: Time Synchronization: 2021.08.18   21:30:00::0014
20210818::213000: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.7psu, index 1.34, Packet 3114
20210818::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 33.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213003: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213003_mbari_wissl_lidar.raa
20210818::213013: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213013_mbari_wissl_lidar.raa
20210818::213023: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213023_mbari_wissl_lidar.raa
20210818::213030: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 12.4psu, index 1.34, Packet 3167
20210818::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213033: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213033_mbari_wissl_lidar.raa
20210818::213043: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213043_mbari_wissl_lidar.raa
20210818::213053: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213053_mbari_wissl_lidar.raa
20210818::213100: Head 2: Time Synchronization: 2021.08.18   21:31:00::0015
20210818::213100: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 12.8psu, index 1.34, Packet 3221
20210818::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213103: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213103_mbari_wissl_lidar.raa
20210818::213113: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213113_mbari_wissl_lidar.raa
20210818::213123: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213123_mbari_wissl_lidar.raa
20210818::213130: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.5psu, index 1.34, Packet 3273
20210818::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213133: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213133_mbari_wissl_lidar.raa
20210818::213136: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213136: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213139: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213139: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213142: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213142: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213143: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213143_mbari_wissl_lidar.raa
20210818::213145: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213145: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213148: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213148: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213151: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 889 msec
20210818::213151: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 889 msec
20210818::213153: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213153_mbari_wissl_lidar.raa
20210818::213156: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213156: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213159: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213159: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213200: Head 1: Time Synchronization: 2021.08.18   21:32:00::0014
20210818::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213200: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.5psu, index 1.34, Packet 3327
20210818::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213202: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213202: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213203: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213203_mbari_wissl_lidar.raa
20210818::213205: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213205: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213208: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213208: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213211: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 887 msec
20210818::213211: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 887 msec
20210818::213213: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213213_mbari_wissl_lidar.raa
20210818::213216: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213216: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 174 msec
20210818::213219: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213219: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213222: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213222: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 465 msec
20210818::213223: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213223_mbari_wissl_lidar.raa
20210818::213225: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213225: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213228: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 746 msec
20210818::213228: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 746 msec
20210818::213230: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.3psu, index 1.34, Packet 3380
20210818::213230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 35.0C, Dig 43.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213231: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 886 msec
20210818::213231: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 886 msec
20210818::213233: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213233_mbari_wissl_lidar.raa
20210818::213236: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213236: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213239: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213239: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 316 msec
20210818::213242: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 464 msec
20210818::213242: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 464 msec
20210818::213243: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213243_mbari_wissl_lidar.raa
20210818::213245: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213245: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213248: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213248: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213251: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 887 msec
20210818::213251: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 887 msec
20210818::213253: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213253_mbari_wissl_lidar.raa
20210818::213256: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213256: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213259: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213259: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213300: Head 1: Time Synchronization: 2021.08.18   21:33:00::0015
20210818::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 32C, OCB 23%, OPB 25C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213300: System  Initialized, Gain 4, Elec PB 35.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.6C, CTD 7.2dbar, CTD 13.2psu, index 1.34, Packet 3434
20210818::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 35.0C, Dig 44.0C, Scan Az fault 0, gain 3, laser state 1
20210818::213302: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 463 msec
20210818::213302: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 463 msec
20210818::213303: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213303_mbari_wissl_lidar.raa
20210818::213305: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 601 msec
20210818::213305: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 603 msec
20210818::213308: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 744 msec
20210818::213308: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 745 msec
20210818::213311: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 886 msec
20210818::213311: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 886 msec
20210818::213314: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213313_mbari_wissl_lidar.raa
20210818::213316: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213316: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 173 msec
20210818::213319: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213319: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 315 msec
20210818::213322: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 464 msec
20210818::213322: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 466 msec
20210818::213323: GUI: Archiving data to file --> C:\Data\20210428d1\20210818_213323_mbari_wissl_lidar.raa
20210818::213334: GUI: Lost Communications with Sensor 1.
20210818::213334: GUI: Lost Communications with Head 2.
20210818::213343: GUI: Attempting Communications with Head 2...
20210818::213344: GUI: Attempting Communications with Head 1...
20210818::220259: GUI: OnBnClickedOk
20210818::220259: GUI: Exiting the WiSSL GUI..
20210818::220259: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210818::220259: GUI: Wrote configuration data.
