20210912::000000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000000: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1315
20210912::000000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 33.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000030: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1369
20210912::000030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000100: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1422
20210912::000100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000130: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1475
20210912::000130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000130: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::000131: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000132: GUI: Lost Communications with Sensor 1.
20210912::000132: GUI: Attempting Communications with Head 1...
20210912::000132: GUI: Requesing STOP operation, Head 2
20210912::000133: Head 2: Received request: STOP
20210912::000133: GUI: Established Communications with Head 1.
20210912::000134: Head 1: Initializing Communications with GUI ...
20210912::000135: Head 1: Communications Established.
20210912::000136: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000136: Head 1: Connection Established with the GUI.
20210912::000136: Head 1: Initializing Subsystems, standby ...
20210912::000137: Head 1: Initializing Hardware, Stand by ...
20210912::000137: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000138: Head 1: NtQuery - testing 1 ...
20210912::000138: Head 1: clock resolution: 10
20210912::000138: Head 1: NtQuery - testing 2, after setting max res ...
20210912::000138: Head 1: clock resolution: 10
20210912::000139: Head 1: Initializing Optics Electronics ...
20210912::000139: Head 1: Power Laser Controller
20210912::000143: Head 1: Power Scanner Controller
20210912::000145: Head 1: Power OPTO Sensor
20210912::000146: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::000147: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000148: GUI: Lost Communications with Head 2.
20210912::000148: GUI: Attempting Communications with Head 2...
20210912::000149: GUI: Established Communications with Head 2.
20210912::000150: Head 2: Initializing Communications with GUI ...
20210912::000150: Head 2: Communications Established.
20210912::000152: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000152: Head 2: Connection Established with the GUI.
20210912::000152: Head 2: Initializing Subsystems, standby ...
20210912::000153: Head 2: Initializing Hardware, Stand by ...
20210912::000153: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000154: Head 2: NtQuery - testing 1 ...
20210912::000154: Head 2: clock resolution: 10
20210912::000154: Head 2: NtQuery - testing 2, after setting max res ...
20210912::000155: Head 2: clock resolution: 10
20210912::000155: Head 2: Initializing Optics Electronics ...
20210912::000155: Head 2: Power Laser Controller
20210912::000159: Head 2: Power Scanner Controller
20210912::000200: System NOT Initialized, Gain 0, Elec PB 38.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 48
20210912::000200: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000200: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000201: Head 2: Power OPTO Sensor
20210912::000203: Head 1: Eye Safe Optical Filter State there 15, not there 15, transition 1
20210912::000204: Head 1: Eye Safe Optical Filter check Passed
20210912::000204: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::000204: Head 1: Initializing Time Sync Subsystem.
20210912::000205: Head 1: Initializing CTD Subsystem.
20210912::000205: Head 1: CTD Initialization Successful
20210912::000205: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::000206: Head 1: Time Sync UDP started, waiting for sync...
20210912::000206: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::000206: Head 1: Time Synchronization Achieved: 2021.09.12   00:02:07::0014
20210912::000220: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::000220: Head 2: Eye Safe Optical Filter check Passed
20210912::000220: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::000220: Head 2: Initializing Time Sync Subsystem.
20210912::000221: Head 1: CTD Ethernet connection established.
20210912::000221: Head 2: Initializing CTD Subsystem.
20210912::000221: Head 2: CTD Initialization Successful
20210912::000221: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::000222: Head 1: Comm CTD: read error - invalid header received
20210912::000222: Head 2: Time Sync UDP started, waiting for sync...
20210912::000222: Head 1: Comm CTD: read error - invalid header received
20210912::000222: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::000222: Head 1: Comm CTD: read error - invalid header received
20210912::000222: Head 2: Time Synchronization Achieved: 2021.09.12   00:02:23::0014
20210912::000223: Head 1: Comm CTD: read error - invalid header received
20210912::000223: Head 1: Comm CTD: read error - invalid header received
20210912::000223: Head 1: Comm CTD: read error - invalid header received
20210912::000223: Head 1: Comm CTD: read error - invalid header received
20210912::000224: Head 1: Comm CTD: read error - invalid header received
20210912::000224: Head 1: Comm CTD: read error - invalid header received
20210912::000224: Head 1: Comm CTD: read error - invalid header received
20210912::000225: Head 1: Comm CTD: read error - invalid header received
20210912::000225: Head 1: Comm CTD: read error - invalid header received
20210912::000225: Head 1: Comm CTD: read error - invalid header received
20210912::000226: Head 1: Comm CTD: read error - invalid header received
20210912::000226: Head 1: Comm CTD: read error - invalid header received
20210912::000226: Head 1: Comm CTD: read error - invalid header received
20210912::000226: Head 1: Comm CTD: read error - invalid header received
20210912::000227: Head 1: Comm CTD: read error - invalid header received
20210912::000227: Head 1: Comm CTD: read error - invalid header received
20210912::000227: Head 1: Comm CTD: read error - invalid header received
20210912::000228: Head 1: Comm CTD: read error - invalid header received
20210912::000228: Head 1: Comm CTD: read error - invalid header received
20210912::000228: Head 1: Comm CTD: read error - invalid header received
20210912::000229: Head 1: Comm CTD: read error - invalid header received
20210912::000229: Head 1: Comm CTD: read error - invalid header received
20210912::000229: Head 1: Comm CTD: read error - invalid header received
20210912::000229: Head 1: Comm CTD: read error - invalid header received
20210912::000230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000230: Head 1: Comm CTD: read error - invalid header received
20210912::000230: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 102
20210912::000230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000230: Head 1: Comm CTD: read error - invalid header received
20210912::000230: Head 1: Comm CTD: read error - invalid header received
20210912::000231: Head 1: Comm CTD: read error - invalid header received
20210912::000231: Head 1: Comm CTD: read error - invalid header received
20210912::000231: Head 1: Comm CTD: read error - invalid header received
20210912::000232: Head 1: Comm CTD: read error - invalid header received
20210912::000232: Head 1: Comm CTD: read error - invalid header received
20210912::000232: Head 1: Comm CTD: read error - invalid header received
20210912::000232: Head 1: Comm CTD: read error - invalid header received
20210912::000233: Head 1: Comm CTD: read error - invalid header received
20210912::000233: Head 1: Comm CTD: read error - invalid header received
20210912::000233: Head 1: Comm CTD: read error - invalid header received
20210912::000234: Head 1: Comm CTD: read error - invalid header received
20210912::000234: Head 1: Comm CTD: read error - invalid header received
20210912::000234: Head 1: Comm CTD: read error - invalid header received
20210912::000235: Head 1: Comm CTD: read error - invalid header received
20210912::000235: Head 1: Comm CTD: read error - invalid header received
20210912::000235: Head 1: Comm CTD: read error - invalid header received
20210912::000236: Head 1: Comm CTD: read error - invalid header received
20210912::000236: Head 1: Comm CTD: read error - invalid header received
20210912::000236: Head 1: Comm CTD: read error - invalid header received
20210912::000236: Head 1: Comm CTD: read error - invalid header received
20210912::000237: Head 1: Comm CTD: read error - invalid header received
20210912::000237: Head 1: Comm CTD: read error - invalid header received
20210912::000237: Head 1: Comm CTD: read error - invalid header received
20210912::000238: Head 1: Comm CTD: read error - invalid header received
20210912::000238: Head 1: Comm CTD: read error - invalid header received
20210912::000238: Head 1: Comm CTD: read error - invalid header received
20210912::000239: Head 1: Comm CTD: read error - invalid header received
20210912::000239: Head 1: Comm CTD: read error - invalid header received
20210912::000239: Head 1: Comm CTD: read error - invalid header received
20210912::000239: Head 2: CTD Ethernet connection established.
20210912::000239: Head 1: Comm CTD: read error - invalid header received
20210912::000240: Head 1: Comm CTD: read error - invalid header received
20210912::000240: Head 1: Comm CTD: read error - invalid header received
20210912::000240: Head 2: Comm CTD: read error - invalid header received
20210912::000240: Head 1: Comm CTD: read error - invalid header received
20210912::000241: Head 2: Comm CTD: read error - invalid header received
20210912::000241: Head 1: Comm CTD: read error - invalid header received
20210912::000241: Head 2: Comm CTD: read error - invalid header received
20210912::000241: Head 1: Comm CTD: read error - invalid header received
20210912::000241: Head 2: Comm CTD: read error - invalid header received
20210912::000241: Head 1: Comm CTD: read error - invalid header received
20210912::000242: Head 2: Comm CTD: read error - invalid header received
20210912::000242: Head 1: Comm CTD: read error - invalid header received
20210912::000242: Head 2: Comm CTD: read error - invalid header received
20210912::000242: Head 1: Comm CTD: read error - invalid header received
20210912::000242: Head 2: Comm CTD: read error - invalid header received
20210912::000242: Head 1: Comm CTD: read error - invalid header received
20210912::000242: Head 2: Comm CTD: read error - invalid header received
20210912::000242: Head 1: Comm CTD: read error - invalid header received
20210912::000243: Head 1: Comm CTD: read error - invalid header received
20210912::000243: Head 2: Comm CTD: read error - invalid header received
20210912::000243: Head 1: Comm CTD: read error - invalid header received
20210912::000243: Head 2: Comm CTD: read error - invalid header received
20210912::000243: Head 2: Comm CTD: read error - invalid header received
20210912::000243: Head 1: Comm CTD: read error - invalid header received
20210912::000244: Head 2: Comm CTD: read error - invalid header received
20210912::000244: Head 1: Comm CTD: read error - invalid header received
20210912::000244: Head 1: Comm CTD: read error - invalid header received
20210912::000244: Head 2: Comm CTD: read error - invalid header received
20210912::000244: Head 1: Comm CTD: read error - invalid header received
20210912::000244: Head 2: Comm CTD: read error - invalid header received
20210912::000245: Head 2: Comm CTD: read error - invalid header received
20210912::000245: Head 1: Comm CTD: read error - invalid header received
20210912::000245: Head 1: Comm CTD: read error - invalid header received
20210912::000245: Head 2: Comm CTD: read error - invalid header received
20210912::000245: Head 1: Comm CTD: read error - invalid header received
20210912::000245: Head 2: Comm CTD: read error - invalid header received
20210912::000245: Head 2: Comm CTD: read error - invalid header received
20210912::000245: Head 1: Comm CTD: read error - invalid header received
20210912::000246: Head 2: Comm CTD: read error - invalid header received
20210912::000246: Head 1: Comm CTD: read error - invalid header received
20210912::000246: Head 1: Comm CTD: read error - invalid header received
20210912::000246: Head 2: Comm CTD: read error - invalid header received
20210912::000246: Head 1: Comm CTD: read error - invalid header received
20210912::000246: Head 2: Comm CTD: read error - invalid header received
20210912::000247: Head 2: Comm CTD: read error - invalid header received
20210912::000247: Head 1: Comm CTD: read error - invalid header received
20210912::000247: Head 1: Comm CTD: read error - invalid header received
20210912::000247: Head 2: Comm CTD: read error - invalid header received
20210912::000247: Head 2: Comm CTD: read error - invalid header received
20210912::000247: Head 1: Comm CTD: read error - invalid header received
20210912::000248: Head 2: Comm CTD: read error - invalid header received
20210912::000248: Head 1: Comm CTD: read error - invalid header received
20210912::000248: Head 2: Comm CTD: read error - invalid header received
20210912::000248: Head 1: Comm CTD: read error - invalid header received
20210912::000248: Head 1: Comm CTD: read error - invalid header received
20210912::000248: Head 2: Comm CTD: read error - invalid header received
20210912::000249: Head 2: Comm CTD: read error - invalid header received
20210912::000249: Head 1: Comm CTD: read error - invalid header received
20210912::000249: Head 2: Comm CTD: read error - invalid header received
20210912::000249: Head 1: Comm CTD: read error - invalid header received
20210912::000249: Head 2: Comm CTD: read error - invalid header received
20210912::000249: Head 1: Comm CTD: read error - invalid header received
20210912::000249: Head 2: Comm CTD: read error - invalid header received
20210912::000249: Head 1: Comm CTD: read error - invalid header received
20210912::000250: Head 2: Comm CTD: read error - invalid header received
20210912::000250: Head 1: Comm CTD: read error - invalid header received
20210912::000250: Head 2: Comm CTD: read error - invalid header received
20210912::000250: Head 1: Comm CTD: read error - invalid header received
20210912::000250: Head 2: Comm CTD: read error - invalid header received
20210912::000250: Head 1: Comm CTD: read error - invalid header received
20210912::000251: Head 1: Comm CTD: read error - invalid header received
20210912::000251: Head 2: Comm CTD: read error - invalid header received
20210912::000251: Head 1: Comm CTD: read error - invalid header received
20210912::000251: Head 2: Comm CTD: read error - invalid header received
20210912::000251: Head 2: Comm CTD: read error - invalid header received
20210912::000251: Head 1: Comm CTD: read error - invalid header received
20210912::000252: Head 1: Comm CTD: read error - invalid header received
20210912::000252: Head 2: Comm CTD: read error - invalid header received
20210912::000252: Head 1: Comm CTD: read error - invalid header received
20210912::000252: Head 2: Comm CTD: read error - invalid header received
20210912::000252: Head 1: Comm CTD: read error - invalid header received
20210912::000252: Head 2: Comm CTD: read error - invalid header received
20210912::000252: Head 1: Comm CTD: read error - invalid header received
20210912::000252: Head 2: Comm CTD: read error - invalid header received
20210912::000253: Head 1: Comm CTD: read error - invalid header received
20210912::000253: Head 2: Comm CTD: read error - invalid header received
20210912::000253: Head 1: Comm CTD: read error - invalid header received
20210912::000253: Head 2: Comm CTD: read error - invalid header received
20210912::000253: Head 1: Comm CTD: read error - invalid header received
20210912::000253: Head 2: Comm CTD: read error - invalid header received
20210912::000254: Head 1: Comm CTD: read error - invalid header received
20210912::000254: Head 2: Comm CTD: read error - invalid header received
20210912::000254: Head 1: Comm CTD: read error - invalid header received
20210912::000254: Head 2: Comm CTD: read error - invalid header received
20210912::000254: Head 1: Comm CTD: read error - invalid header received
20210912::000254: Head 2: Comm CTD: read error - invalid header received
20210912::000255: Head 1: Comm CTD: read error - invalid header received
20210912::000255: Head 2: Comm CTD: read error - invalid header received
20210912::000255: Head 1: Comm CTD: read error - invalid header received
20210912::000255: Head 2: Comm CTD: read error - invalid header received
20210912::000255: Head 1: Comm CTD: read error - invalid header received
20210912::000255: Head 2: Comm CTD: read error - invalid header received
20210912::000255: Head 1: Comm CTD: read error - invalid header received
20210912::000255: Head 2: Comm CTD: read error - invalid header received
20210912::000256: Head 1: Comm CTD: read error - invalid header received
20210912::000256: Head 2: Comm CTD: read error - invalid header received
20210912::000256: Head 1: Comm CTD: read error - invalid header received
20210912::000256: Head 2: Comm CTD: read error - invalid header received
20210912::000256: Head 1: Comm CTD: read error - invalid header received
20210912::000256: Head 2: Comm CTD: read error - invalid header received
20210912::000257: Head 1: Comm CTD: read error - invalid header received
20210912::000257: Head 2: Comm CTD: read error - invalid header received
20210912::000257: Head 1: Comm CTD: read error - invalid header received
20210912::000257: Head 2: Comm CTD: read error - invalid header received
20210912::000257: Head 1: Comm CTD: read error - invalid header received
20210912::000257: Head 2: Comm CTD: read error - invalid header received
20210912::000258: Head 1: Comm CTD: read error - invalid header received
20210912::000258: Head 2: Comm CTD: read error - invalid header received
20210912::000258: Head 1: Comm CTD: read error - invalid header received
20210912::000258: Head 2: Comm CTD: read error - invalid header received
20210912::000258: Head 1: Comm CTD: read error - invalid header received
20210912::000258: Head 2: Comm CTD: read error - invalid header received
20210912::000258: Head 1: Comm CTD: read error - invalid header received
20210912::000258: Head 2: Comm CTD: read error - invalid header received
20210912::000259: Head 1: Comm CTD: read error - invalid header received
20210912::000259: Head 2: Comm CTD: read error - invalid header received
20210912::000259: Head 1: Comm CTD: read error - invalid header received
20210912::000259: Head 2: Comm CTD: read error - invalid header received
20210912::000259: Head 1: Comm CTD: read error - invalid header received
20210912::000259: Head 2: Comm CTD: read error - invalid header received
20210912::000300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000300: Head 1: Comm CTD: read error - invalid header received
20210912::000300: Head 2: Comm CTD: read error - invalid header received
20210912::000300: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 155
20210912::000300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000300: Head 1: Comm CTD: read error - invalid header received
20210912::000300: Head 2: Comm CTD: read error - invalid header received
20210912::000300: Head 1: Comm CTD: read error - invalid header received
20210912::000300: Head 2: Comm CTD: read error - invalid header received
20210912::000301: Head 1: Comm CTD: read error - invalid header received
20210912::000301: Head 2: Comm CTD: read error - invalid header received
20210912::000301: Head 1: Comm CTD: read error - invalid header received
20210912::000301: Head 2: Comm CTD: read error - invalid header received
20210912::000301: Head 1: Comm CTD: read error - invalid header received
20210912::000301: Head 2: Comm CTD: read error - invalid header received
20210912::000301: Head 1: Comm CTD: read error - invalid header received
20210912::000302: Head 2: Comm CTD: read error - invalid header received
20210912::000302: Head 1: Comm CTD: read error - invalid header received
20210912::000302: Head 2: Comm CTD: read error - invalid header received
20210912::000302: Head 1: Comm CTD: read error - invalid header received
20210912::000302: Head 2: Comm CTD: read error - invalid header received
20210912::000302: Head 1: Comm CTD: read error - invalid header received
20210912::000302: Head 2: Comm CTD: read error - invalid header received
20210912::000303: Head 1: Comm CTD: read error - invalid header received
20210912::000303: Head 2: Comm CTD: read error - invalid header received
20210912::000303: Head 1: Comm CTD: read error - invalid header received
20210912::000303: Head 2: Comm CTD: read error - invalid header received
20210912::000303: Head 1: Comm CTD: read error - invalid header received
20210912::000303: Head 2: Comm CTD: read error - invalid header received
20210912::000304: Head 1: Comm CTD: read error - invalid header received
20210912::000304: Head 2: Comm CTD: read error - invalid header received
20210912::000304: Head 1: Comm CTD: read error - invalid header received
20210912::000304: Head 2: Comm CTD: read error - invalid header received
20210912::000304: Head 1: Comm CTD: read error - invalid header received
20210912::000304: Head 2: Comm CTD: read error - invalid header received
20210912::000305: Head 1: Comm CTD: read error - invalid header received
20210912::000305: Head 2: Comm CTD: read error - invalid header received
20210912::000305: Head 1: Comm CTD: read error - invalid header received
20210912::000305: Head 2: Comm CTD: read error - invalid header received
20210912::000305: Head 1: Comm CTD: read error - invalid header received
20210912::000305: Head 2: Comm CTD: read error - invalid header received
20210912::000305: Head 1: Comm CTD: read error - invalid header received
20210912::000305: Head 2: Comm CTD: read error - invalid header received
20210912::000306: Head 1: Comm CTD: read error - invalid header received
20210912::000306: Head 2: Comm CTD: read error - invalid header received
20210912::000306: Head 1: Comm CTD: read error - invalid header received
20210912::000306: Head 2: Comm CTD: read error - invalid header received
20210912::000306: Head 1: Comm CTD: read error - invalid header received
20210912::000306: Head 2: Comm CTD: read error - invalid header received
20210912::000307: Head 1: Comm CTD: read error - invalid header received
20210912::000307: Head 2: Comm CTD: read error - invalid header received
20210912::000307: Head 1: Comm CTD: read error - invalid header received
20210912::000307: Head 1: Comm CTD: read error - invalid header received
20210912::000308: Head 1: Comm CTD: read error - invalid header received
20210912::000308: Head 1: Comm CTD: read error - invalid header received
20210912::000308: Head 1: Comm CTD: read error - invalid header received
20210912::000308: Head 1: Comm CTD: read error - invalid header received
20210912::000309: Head 1: Comm CTD: read error - invalid header received
20210912::000309: Head 1: Comm CTD: read error - invalid header received
20210912::000309: Head 1: Comm CTD: read error - invalid header received
20210912::000310: Head 1: Comm CTD: read error - invalid header received
20210912::000310: Head 1: Comm CTD: read error - invalid header received
20210912::000310: Head 1: Comm CTD: read error - invalid header received
20210912::000311: Head 1: Comm CTD: read error - invalid header received
20210912::000311: Head 1: Comm CTD: read error - invalid header received
20210912::000330: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 208
20210912::000330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000400: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 262
20210912::000400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000430: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 315
20210912::000430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000500: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 368
20210912::000500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000530: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 422
20210912::000530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000600: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 475
20210912::000600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000630: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 529
20210912::000630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000700: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 582
20210912::000700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 35.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000729: GUI: OnBnClickedOk
20210912::000729: GUI: Exiting the WiSSL GUI..
20210912::000729: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210912::000729: GUI: Wrote configuration data.
20210912::000736: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210912::000736: GUI: Live mode ON.
20210912::000736: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210912::000737: GUI: WiSSL GUI started at 2021_09_12_00:07:37
20210912::000737: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_09_12.txt
20210912::000737: GUI: Attempting Communications with Head 1...
20210912::000737: GUI: Attempting Communications with Head 2...
20210912::000737: GUI: Established Communications with Head 2.
20210912::000737: GUI: Established Communications with Head 1.
20210912::000738: Head 2: Lost Communications with GUI
20210912::000738: Head 1: Lost Communications with GUI
20210912::000738: Head 1: Initializing Communications with GUI ...
20210912::000738: Head 2: Initializing Communications with GUI ...
20210912::000739: Head 2: Communications Established.
20210912::000739: Head 1: Communications Established.
20210912::000747: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::000748: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000748: GUI: Lost Communications with Sensor 1.
20210912::000749: GUI: Attempting Communications with Head 1...
20210912::000749: GUI: Requesing STOP operation, Head 2
20210912::000749: Head 2: Received request: STOP
20210912::000750: GUI: Established Communications with Head 1.
20210912::000750: Head 1: Initializing Communications with GUI ...
20210912::000751: Head 1: Communications Established.
20210912::000753: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000753: Head 1: Connection Established with the GUI.
20210912::000753: Head 1: Initializing Subsystems, standby ...
20210912::000753: Head 1: Initializing Hardware, Stand by ...
20210912::000754: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000755: Head 1: NtQuery - testing 1 ...
20210912::000755: Head 1: clock resolution: 10
20210912::000755: Head 1: NtQuery - testing 2, after setting max res ...
20210912::000755: Head 1: clock resolution: 10
20210912::000756: Head 1: Initializing Optics Electronics ...
20210912::000756: Head 1: Power Laser Controller
20210912::000758: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::000759: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000759: GUI: Lost Communications with Head 2.
20210912::000800: System NOT Initialized, Gain 0, Elec PB 43.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 18
20210912::000800: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 48.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000800: Head 1: Power Scanner Controller
20210912::000800: GUI: Attempting Communications with Head 2...
20210912::000800: GUI: Established Communications with Head 2.
20210912::000801: Head 2: Initializing Communications with GUI ...
20210912::000802: Head 1: Power OPTO Sensor
20210912::000802: Head 2: Communications Established.
20210912::000803: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000804: Head 2: Connection Established with the GUI.
20210912::000804: Head 2: Initializing Subsystems, standby ...
20210912::000804: Head 2: Initializing Hardware, Stand by ...
20210912::000805: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000805: Head 2: NtQuery - testing 1 ...
20210912::000806: Head 2: clock resolution: 10
20210912::000806: Head 2: NtQuery - testing 2, after setting max res ...
20210912::000806: Head 2: clock resolution: 10
20210912::000807: Head 2: Initializing Optics Electronics ...
20210912::000807: Head 2: Power Laser Controller
20210912::000811: Head 2: Power Scanner Controller
20210912::000813: Head 2: Power OPTO Sensor
20210912::000820: Head 1: Eye Safe Optical Filter State there 15, not there 15, transition 1
20210912::000821: Head 1: Eye Safe Optical Filter check Passed
20210912::000821: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::000821: Head 1: Initializing Time Sync Subsystem.
20210912::000822: Head 1: Initializing CTD Subsystem.
20210912::000822: Head 1: CTD Initialization Successful
20210912::000822: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::000823: Head 1: Time Sync UDP started, waiting for sync...
20210912::000823: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::000823: Head 1: Time Synchronization Achieved: 2021.09.12   00:08:24::0014
20210912::000830: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000830: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 72
20210912::000830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 35.0C, Dig 48.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000831: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::000832: Head 2: Eye Safe Optical Filter check Passed
20210912::000832: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::000832: Head 2: Initializing Time Sync Subsystem.
20210912::000832: Head 2: Initializing CTD Subsystem.
20210912::000833: Head 2: CTD Initialization Successful
20210912::000833: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::000833: Head 2: Time Sync UDP started, waiting for sync...
20210912::000834: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::000834: Head 2: Time Synchronization Achieved: 2021.09.12   00:08:35::0011
20210912::000847: Head 1: CTD Ethernet connection established.
20210912::000847: Head 2: CTD Ethernet connection established.
20210912::000848: Head 1: Comm CTD: read error - invalid header received
20210912::000848: Head 2: Comm CTD: read error - invalid header received
20210912::000849: Head 1: Comm CTD: read error - invalid header received
20210912::000849: Head 2: Comm CTD: read error - invalid header received
20210912::000849: Head 1: Comm CTD: read error - invalid header received
20210912::000849: Head 2: Comm CTD: read error - invalid header received
20210912::000849: Head 1: Comm CTD: read error - invalid header received
20210912::000849: Head 2: Comm CTD: read error - invalid header received
20210912::000849: Head 1: Comm CTD: read error - invalid header received
20210912::000849: Head 2: Comm CTD: read error - invalid header received
20210912::000850: Head 1: Comm CTD: read error - invalid header received
20210912::000850: Head 2: Comm CTD: read error - invalid header received
20210912::000850: Head 1: Comm CTD: read error - invalid header received
20210912::000850: Head 2: Comm CTD: read error - invalid header received
20210912::000850: Head 1: Comm CTD: read error - invalid header received
20210912::000850: Head 2: Comm CTD: read error - invalid header received
20210912::000851: Head 1: Comm CTD: read error - invalid header received
20210912::000851: Head 2: Comm CTD: read error - invalid header received
20210912::000851: Head 1: Comm CTD: read error - invalid header received
20210912::000851: Head 2: Comm CTD: read error - invalid header received
20210912::000851: Head 1: Comm CTD: read error - invalid header received
20210912::000851: Head 2: Comm CTD: read error - invalid header received
20210912::000852: Head 1: Comm CTD: read error - invalid header received
20210912::000852: Head 2: Comm CTD: read error - invalid header received
20210912::000852: Head 1: Comm CTD: read error - invalid header received
20210912::000852: Head 2: Comm CTD: read error - invalid header received
20210912::000852: Head 1: Comm CTD: read error - invalid header received
20210912::000852: Head 2: Comm CTD: read error - invalid header received
20210912::000852: Head 1: Comm CTD: read error - invalid header received
20210912::000852: Head 2: Comm CTD: read error - invalid header received
20210912::000853: Head 1: Comm CTD: read error - invalid header received
20210912::000853: Head 2: Comm CTD: read error - invalid header received
20210912::000853: Head 1: Comm CTD: read error - invalid header received
20210912::000853: Head 2: Comm CTD: read error - invalid header received
20210912::000853: Head 1: Comm CTD: read error - invalid header received
20210912::000853: Head 2: Comm CTD: read error - invalid header received
20210912::000854: Head 1: Comm CTD: read error - invalid header received
20210912::000854: Head 2: Comm CTD: read error - invalid header received
20210912::000854: Head 1: Comm CTD: read error - invalid header received
20210912::000854: Head 2: Comm CTD: read error - invalid header received
20210912::000854: Head 1: Comm CTD: read error - invalid header received
20210912::000854: Head 2: Comm CTD: read error - invalid header received
20210912::000855: Head 1: Comm CTD: read error - invalid header received
20210912::000855: Head 2: Comm CTD: read error - invalid header received
20210912::000855: Head 1: Comm CTD: read error - invalid header received
20210912::000855: Head 2: Comm CTD: read error - invalid header received
20210912::000855: Head 1: Comm CTD: read error - invalid header received
20210912::000855: Head 2: Comm CTD: read error - invalid header received
20210912::000855: Head 1: Comm CTD: read error - invalid header received
20210912::000855: Head 2: Comm CTD: read error - invalid header received
20210912::000856: Head 1: Comm CTD: read error - invalid header received
20210912::000856: Head 2: Comm CTD: read error - invalid header received
20210912::000856: Head 1: Comm CTD: read error - invalid header received
20210912::000856: Head 2: Comm CTD: read error - invalid header received
20210912::000856: Head 1: Comm CTD: read error - invalid header received
20210912::000856: Head 2: Comm CTD: read error - invalid header received
20210912::000857: Head 1: Comm CTD: read error - invalid header received
20210912::000857: Head 2: Comm CTD: read error - invalid header received
20210912::000857: Head 1: Comm CTD: read error - invalid header received
20210912::000857: Head 2: Comm CTD: read error - invalid header received
20210912::000857: Head 1: Comm CTD: read error - invalid header received
20210912::000857: Head 2: Comm CTD: read error - invalid header received
20210912::000858: Head 1: Comm CTD: read error - invalid header received
20210912::000858: Head 2: Comm CTD: read error - invalid header received
20210912::000858: Head 1: Comm CTD: read error - invalid header received
20210912::000858: Head 2: Comm CTD: read error - invalid header received
20210912::000858: Head 1: Comm CTD: read error - invalid header received
20210912::000858: Head 2: Comm CTD: read error - invalid header received
20210912::000858: Head 1: Comm CTD: read error - invalid header received
20210912::000859: Head 2: Comm CTD: read error - invalid header received
20210912::000859: Head 1: Comm CTD: read error - invalid header received
20210912::000859: Head 2: Comm CTD: read error - invalid header received
20210912::000859: Head 1: Comm CTD: read error - invalid header received
20210912::000859: Head 2: Comm CTD: read error - invalid header received
20210912::000859: Head 1: Comm CTD: read error - invalid header received
20210912::000859: Head 2: Comm CTD: read error - invalid header received
20210912::000900: Head 1: Comm CTD: read error - invalid header received
20210912::000900: Head 2: Comm CTD: read error - invalid header received
20210912::000900: System  Initialized, Gain 1, Elec PB 42.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 125
20210912::000900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 48.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000900: Head 1: Comm CTD: read error - invalid header received
20210912::000900: Head 2: Comm CTD: read error - invalid header received
20210912::000900: Head 1: Comm CTD: read error - invalid header received
20210912::000900: Head 2: Comm CTD: read error - invalid header received
20210912::000901: Head 1: Comm CTD: read error - invalid header received
20210912::000901: Head 2: Comm CTD: read error - invalid header received
20210912::000901: Head 1: Comm CTD: read error - invalid header received
20210912::000901: Head 2: Comm CTD: read error - invalid header received
20210912::000901: Head 1: Comm CTD: read error - invalid header received
20210912::000901: Head 2: Comm CTD: read error - invalid header received
20210912::000902: Head 1: Comm CTD: read error - invalid header received
20210912::000902: Head 2: Comm CTD: read error - invalid header received
20210912::000902: Head 1: Comm CTD: read error - invalid header received
20210912::000902: Head 2: Comm CTD: read error - invalid header received
20210912::000902: Head 1: Comm CTD: read error - invalid header received
20210912::000902: Head 2: Comm CTD: read error - invalid header received
20210912::000902: Head 1: Comm CTD: read error - invalid header received
20210912::000902: Head 2: Comm CTD: read error - invalid header received
20210912::000903: Head 1: Comm CTD: read error - invalid header received
20210912::000903: Head 2: Comm CTD: read error - invalid header received
20210912::000903: Head 1: Comm CTD: read error - invalid header received
20210912::000903: Head 2: Comm CTD: read error - invalid header received
20210912::000903: Head 1: Comm CTD: read error - invalid header received
20210912::000903: Head 2: Comm CTD: read error - invalid header received
20210912::000904: Head 1: Comm CTD: read error - invalid header received
20210912::000904: Head 2: Comm CTD: read error - invalid header received
20210912::000904: Head 1: Comm CTD: read error - invalid header received
20210912::000904: Head 2: Comm CTD: read error - invalid header received
20210912::000904: Head 1: Comm CTD: read error - invalid header received
20210912::000904: Head 2: Comm CTD: read error - invalid header received
20210912::000905: Head 1: Comm CTD: read error - invalid header received
20210912::000905: Head 2: Comm CTD: read error - invalid header received
20210912::000905: Head 1: Comm CTD: read error - invalid header received
20210912::000905: Head 2: Comm CTD: read error - invalid header received
20210912::000905: Head 1: Comm CTD: read error - invalid header received
20210912::000905: Head 2: Comm CTD: read error - invalid header received
20210912::000905: Head 1: Comm CTD: read error - invalid header received
20210912::000905: Head 2: Comm CTD: read error - invalid header received
20210912::000906: Head 1: Comm CTD: read error - invalid header received
20210912::000906: Head 2: Comm CTD: read error - invalid header received
20210912::000906: Head 1: Comm CTD: read error - invalid header received
20210912::000906: Head 2: Comm CTD: read error - invalid header received
20210912::000906: Head 1: Comm CTD: read error - invalid header received
20210912::000906: Head 2: Comm CTD: read error - invalid header received
20210912::000907: Head 1: Comm CTD: read error - invalid header received
20210912::000907: Head 2: Comm CTD: read error - invalid header received
20210912::000907: Head 1: Comm CTD: read error - invalid header received
20210912::000907: Head 2: Comm CTD: read error - invalid header received
20210912::000907: Head 1: Comm CTD: read error - invalid header received
20210912::000907: Head 2: Comm CTD: read error - invalid header received
20210912::000908: Head 1: Comm CTD: read error - invalid header received
20210912::000908: Head 2: Comm CTD: read error - invalid header received
20210912::000908: Head 1: Comm CTD: read error - invalid header received
20210912::000908: Head 2: Comm CTD: read error - invalid header received
20210912::000908: Head 1: Comm CTD: read error - invalid header received
20210912::000908: Head 2: Comm CTD: read error - invalid header received
20210912::000908: Head 1: Comm CTD: read error - invalid header received
20210912::000908: Head 2: Comm CTD: read error - invalid header received
20210912::000909: Head 1: Comm CTD: read error - invalid header received
20210912::000909: Head 2: Comm CTD: read error - invalid header received
20210912::000909: Head 1: Comm CTD: read error - invalid header received
20210912::000909: Head 2: Comm CTD: read error - invalid header received
20210912::000909: Head 1: Comm CTD: read error - invalid header received
20210912::000909: Head 2: Comm CTD: read error - invalid header received
20210912::000910: Head 1: Comm CTD: read error - invalid header received
20210912::000910: Head 2: Comm CTD: read error - invalid header received
20210912::000910: Head 1: Comm CTD: read error - invalid header received
20210912::000910: Head 2: Comm CTD: read error - invalid header received
20210912::000910: Head 1: Comm CTD: read error - invalid header received
20210912::000910: Head 2: Comm CTD: read error - invalid header received
20210912::000911: Head 1: Comm CTD: read error - invalid header received
20210912::000911: Head 2: Comm CTD: read error - invalid header received
20210912::000911: Head 1: Comm CTD: read error - invalid header received
20210912::000911: Head 2: Comm CTD: read error - invalid header received
20210912::000911: Head 1: Comm CTD: read error - invalid header received
20210912::000911: Head 2: Comm CTD: read error - invalid header received
20210912::000911: Head 1: Comm CTD: read error - invalid header received
20210912::000912: Head 2: Comm CTD: read error - invalid header received
20210912::000912: Head 1: Comm CTD: read error - invalid header received
20210912::000912: Head 2: Comm CTD: read error - invalid header received
20210912::000912: Head 1: Comm CTD: read error - invalid header received
20210912::000912: Head 2: Comm CTD: read error - invalid header received
20210912::000912: Head 1: Comm CTD: read error - invalid header received
20210912::000912: Head 2: Comm CTD: read error - invalid header received
20210912::000913: Head 1: Comm CTD: read error - invalid header received
20210912::000913: Head 2: Comm CTD: read error - invalid header received
20210912::000913: Head 1: Comm CTD: read error - invalid header received
20210912::000913: Head 2: Comm CTD: read error - invalid header received
20210912::000913: Head 1: Comm CTD: read error - invalid header received
20210912::000913: Head 2: Comm CTD: read error - invalid header received
20210912::000914: Head 1: Comm CTD: read error - invalid header received
20210912::000914: Head 2: Comm CTD: read error - invalid header received
20210912::000914: Head 1: Comm CTD: read error - invalid header received
20210912::000914: Head 2: Comm CTD: read error - invalid header received
20210912::000914: Head 1: Comm CTD: read error - invalid header received
20210912::000914: Head 2: Comm CTD: read error - invalid header received
20210912::000915: Head 1: Comm CTD: read error - invalid header received
20210912::000915: Head 2: Comm CTD: read error - invalid header received
20210912::000915: Head 1: Comm CTD: read error - invalid header received
20210912::000915: Head 2: Comm CTD: read error - invalid header received
20210912::000915: Head 1: Comm CTD: read error - invalid header received
20210912::000915: Head 2: Comm CTD: read error - invalid header received
20210912::000915: Head 1: Comm CTD: read error - invalid header received
20210912::000915: Head 2: Comm CTD: read error - invalid header received
20210912::000916: Head 1: Comm CTD: read error - invalid header received
20210912::000916: Head 2: Comm CTD: read error - invalid header received
20210912::000916: Head 1: Comm CTD: read error - invalid header received
20210912::000916: Head 2: Comm CTD: read error - invalid header received
20210912::000916: Head 1: Comm CTD: read error - invalid header received
20210912::000916: Head 2: Comm CTD: read error - invalid header received
20210912::000917: Head 1: Comm CTD: read error - invalid header received
20210912::000917: Head 2: Comm CTD: read error - invalid header received
20210912::000917: Head 1: Comm CTD: read error - invalid header received
20210912::000917: Head 2: Comm CTD: read error - invalid header received
20210912::000917: Head 1: Comm CTD: read error - invalid header received
20210912::000917: Head 2: Comm CTD: read error - invalid header received
20210912::000918: Head 1: Comm CTD: read error - invalid header received
20210912::000918: Head 2: Comm CTD: read error - invalid header received
20210912::000918: Head 1: Comm CTD: read error - invalid header received
20210912::000918: Head 2: Comm CTD: read error - invalid header received
20210912::000918: Head 1: Comm CTD: read error - invalid header received
20210912::000918: Head 2: Comm CTD: read error - invalid header received
20210912::000918: Head 1: Comm CTD: read error - invalid header received
20210912::000918: Head 2: Comm CTD: read error - invalid header received
20210912::000919: Head 1: Comm CTD: read error - invalid header received
20210912::000919: Head 2: Comm CTD: read error - invalid header received
20210912::000919: Head 1: Comm CTD: read error - invalid header received
20210912::000919: Head 2: Comm CTD: read error - invalid header received
20210912::000930: System  Initialized, Gain 1, Elec PB 42.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 178
20210912::000930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 48.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::000932: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::000933: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000933: GUI: Lost Communications with Sensor 1.
20210912::000933: GUI: Attempting Communications with Head 1...
20210912::000934: GUI: Established Communications with Head 1.
20210912::000934: GUI: Requesing STOP operation, Head 2
20210912::000934: Head 2: Received request: STOP
20210912::000934: GUI: Requesing STOP operation, Head 1
20210912::000935: Head 1: Initializing Communications with GUI ...
20210912::000935: Head 1: Communications Established.
20210912::000936: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000936: Head 1: Connection Established with the GUI.
20210912::000937: Head 1: Initializing Subsystems, standby ...
20210912::000937: Head 1: Initializing Hardware, Stand by ...
20210912::000938: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000938: Head 1: NtQuery - testing 1 ...
20210912::000938: Head 1: clock resolution: 10
20210912::000939: Head 1: NtQuery - testing 2, after setting max res ...
20210912::000939: Head 1: clock resolution: 10
20210912::000939: Head 1: Initializing Optics Electronics ...
20210912::000940: Head 1: Power Laser Controller
20210912::000943: Head 1: Power Scanner Controller
20210912::000944: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::000945: GUI: ERROR: Received Invalid Packet ID: 0
20210912::000945: GUI: Lost Communications with Head 2.
20210912::000945: Head 1: Power OPTO Sensor
20210912::000945: GUI: Attempting Communications with Head 2...
20210912::000946: GUI: Established Communications with Head 2.
20210912::000947: Head 2: Initializing Communications with GUI ...
20210912::000947: Head 2: Communications Established.
20210912::000948: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::000948: Head 2: Connection Established with the GUI.
20210912::000949: Head 2: Initializing Subsystems, standby ...
20210912::000949: Head 2: Initializing Hardware, Stand by ...
20210912::000950: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::000950: Head 2: NtQuery - testing 1 ...
20210912::000950: Head 2: clock resolution: 10
20210912::000951: Head 2: NtQuery - testing 2, after setting max res ...
20210912::000951: Head 2: clock resolution: 10
20210912::000951: Head 2: Initializing Optics Electronics ...
20210912::000952: Head 2: Power Laser Controller
20210912::000955: Head 2: Power Scanner Controller
20210912::000957: Head 2: Power OPTO Sensor
20210912::001000: System NOT Initialized, Gain 0, Elec PB 43.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 46
20210912::001000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001000: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001004: Head 1: Eye Safe Optical Filter State there 15, not there 15, transition 1
20210912::001004: Head 1: Eye Safe Optical Filter check Passed
20210912::001005: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::001005: Head 1: Initializing Time Sync Subsystem.
20210912::001005: Head 1: Initializing CTD Subsystem.
20210912::001005: Head 1: CTD Initialization Successful
20210912::001006: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::001006: Head 1: Time Sync UDP started, waiting for sync...
20210912::001006: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::001007: Head 1: Time Synchronization Achieved: 2021.09.12   00:10:08::0015
20210912::001016: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::001016: Head 2: Eye Safe Optical Filter check Passed
20210912::001017: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::001017: Head 2: Initializing Time Sync Subsystem.
20210912::001017: Head 2: Initializing CTD Subsystem.
20210912::001017: Head 2: CTD Initialization Successful
20210912::001018: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::001018: Head 2: Time Sync UDP started, waiting for sync...
20210912::001018: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::001019: Head 2: Time Synchronization Achieved: 2021.09.12   00:10:20::0014
20210912::001024: Head 2: CTD Ethernet connection established.
20210912::001024: Head 1: CTD Ethernet connection established.
20210912::001025: Head 2: Comm CTD: read error - invalid header received
20210912::001025: Head 1: Comm CTD: read error - invalid header received
20210912::001025: Head 2: Comm CTD: read error - invalid header received
20210912::001025: Head 1: Comm CTD: read error - invalid header received
20210912::001025: Head 2: Comm CTD: read error - invalid header received
20210912::001025: Head 1: Comm CTD: read error - invalid header received
20210912::001026: Head 2: Comm CTD: read error - invalid header received
20210912::001026: Head 1: Comm CTD: read error - invalid header received
20210912::001026: Head 2: Comm CTD: read error - invalid header received
20210912::001026: Head 1: Comm CTD: read error - invalid header received
20210912::001026: Head 2: Comm CTD: read error - invalid header received
20210912::001026: Head 1: Comm CTD: read error - invalid header received
20210912::001027: Head 2: Comm CTD: read error - invalid header received
20210912::001027: Head 1: Comm CTD: read error - invalid header received
20210912::001027: Head 2: Comm CTD: read error - invalid header received
20210912::001027: Head 1: Comm CTD: read error - invalid header received
20210912::001027: Head 2: Comm CTD: read error - invalid header received
20210912::001027: Head 1: Comm CTD: read error - invalid header received
20210912::001027: Head 2: Comm CTD: read error - invalid header received
20210912::001027: Head 1: Comm CTD: read error - invalid header received
20210912::001028: Head 2: Comm CTD: read error - invalid header received
20210912::001028: Head 1: Comm CTD: read error - invalid header received
20210912::001028: Head 2: Comm CTD: read error - invalid header received
20210912::001028: Head 1: Comm CTD: read error - invalid header received
20210912::001028: Head 2: Comm CTD: read error - invalid header received
20210912::001028: Head 1: Comm CTD: read error - invalid header received
20210912::001029: Head 2: Comm CTD: read error - invalid header received
20210912::001029: Head 1: Comm CTD: read error - invalid header received
20210912::001029: Head 2: Comm CTD: read error - invalid header received
20210912::001029: Head 1: Comm CTD: read error - invalid header received
20210912::001029: Head 2: Comm CTD: read error - invalid header received
20210912::001029: Head 1: Comm CTD: read error - invalid header received
20210912::001030: Head 2: Comm CTD: read error - invalid header received
20210912::001030: Head 1: Comm CTD: read error - invalid header received
20210912::001030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001030: Head 2: Comm CTD: read error - invalid header received
20210912::001030: Head 1: Comm CTD: read error - invalid header received
20210912::001030: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 100
20210912::001030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001030: Head 2: Comm CTD: read error - invalid header received
20210912::001030: Head 1: Comm CTD: read error - invalid header received
20210912::001030: Head 2: Comm CTD: read error - invalid header received
20210912::001030: Head 1: Comm CTD: read error - invalid header received
20210912::001031: Head 2: Comm CTD: read error - invalid header received
20210912::001031: Head 1: Comm CTD: read error - invalid header received
20210912::001031: Head 2: Comm CTD: read error - invalid header received
20210912::001031: Head 1: Comm CTD: read error - invalid header received
20210912::001031: Head 2: Comm CTD: read error - invalid header received
20210912::001031: Head 1: Comm CTD: read error - invalid header received
20210912::001032: Head 2: Comm CTD: read error - invalid header received
20210912::001032: Head 1: Comm CTD: read error - invalid header received
20210912::001032: Head 2: Comm CTD: read error - invalid header received
20210912::001032: Head 1: Comm CTD: read error - invalid header received
20210912::001032: Head 2: Comm CTD: read error - invalid header received
20210912::001032: Head 1: Comm CTD: read error - invalid header received
20210912::001033: Head 2: Comm CTD: read error - invalid header received
20210912::001033: Head 1: Comm CTD: read error - invalid header received
20210912::001033: Head 2: Comm CTD: read error - invalid header received
20210912::001033: Head 1: Comm CTD: read error - invalid header received
20210912::001033: Head 2: Comm CTD: read error - invalid header received
20210912::001033: Head 1: Comm CTD: read error - invalid header received
20210912::001033: Head 2: Comm CTD: read error - invalid header received
20210912::001033: Head 1: Comm CTD: read error - invalid header received
20210912::001034: Head 2: Comm CTD: read error - invalid header received
20210912::001034: Head 1: Comm CTD: read error - invalid header received
20210912::001034: Head 2: Comm CTD: read error - invalid header received
20210912::001034: Head 1: Comm CTD: read error - invalid header received
20210912::001034: Head 2: Comm CTD: read error - invalid header received
20210912::001034: Head 1: Comm CTD: read error - invalid header received
20210912::001035: Head 2: Comm CTD: read error - invalid header received
20210912::001035: Head 1: Comm CTD: read error - invalid header received
20210912::001035: Head 2: Comm CTD: read error - invalid header received
20210912::001035: Head 1: Comm CTD: read error - invalid header received
20210912::001035: Head 2: Comm CTD: read error - invalid header received
20210912::001035: Head 1: Comm CTD: read error - invalid header received
20210912::001036: Head 2: Comm CTD: read error - invalid header received
20210912::001036: Head 1: Comm CTD: read error - invalid header received
20210912::001036: Head 2: Comm CTD: read error - invalid header received
20210912::001036: Head 1: Comm CTD: read error - invalid header received
20210912::001036: Head 2: Comm CTD: read error - invalid header received
20210912::001036: Head 1: Comm CTD: read error - invalid header received
20210912::001036: Head 2: Comm CTD: read error - invalid header received
20210912::001036: Head 1: Comm CTD: read error - invalid header received
20210912::001037: Head 2: Comm CTD: read error - invalid header received
20210912::001037: Head 1: Comm CTD: read error - invalid header received
20210912::001037: Head 2: Comm CTD: read error - invalid header received
20210912::001037: Head 1: Comm CTD: read error - invalid header received
20210912::001037: Head 2: Comm CTD: read error - invalid header received
20210912::001037: Head 1: Comm CTD: read error - invalid header received
20210912::001038: Head 2: Comm CTD: read error - invalid header received
20210912::001038: Head 1: Comm CTD: read error - invalid header received
20210912::001038: Head 2: Comm CTD: read error - invalid header received
20210912::001038: Head 1: Comm CTD: read error - invalid header received
20210912::001038: Head 2: Comm CTD: read error - invalid header received
20210912::001038: Head 1: Comm CTD: read error - invalid header received
20210912::001039: Head 2: Comm CTD: read error - invalid header received
20210912::001039: Head 1: Comm CTD: read error - invalid header received
20210912::001039: Head 2: Comm CTD: read error - invalid header received
20210912::001039: Head 1: Comm CTD: read error - invalid header received
20210912::001039: Head 2: Comm CTD: read error - invalid header received
20210912::001039: Head 1: Comm CTD: read error - invalid header received
20210912::001040: Head 2: Comm CTD: read error - invalid header received
20210912::001040: Head 1: Comm CTD: read error - invalid header received
20210912::001040: Head 2: Comm CTD: read error - invalid header received
20210912::001040: Head 1: Comm CTD: read error - invalid header received
20210912::001040: Head 2: Comm CTD: read error - invalid header received
20210912::001040: Head 1: Comm CTD: read error - invalid header received
20210912::001040: Head 2: Comm CTD: read error - invalid header received
20210912::001040: Head 1: Comm CTD: read error - invalid header received
20210912::001041: Head 2: Comm CTD: read error - invalid header received
20210912::001041: Head 1: Comm CTD: read error - invalid header received
20210912::001041: Head 2: Comm CTD: read error - invalid header received
20210912::001041: Head 1: Comm CTD: read error - invalid header received
20210912::001041: Head 2: Comm CTD: read error - invalid header received
20210912::001041: Head 1: Comm CTD: read error - invalid header received
20210912::001042: Head 2: Comm CTD: read error - invalid header received
20210912::001042: Head 1: Comm CTD: read error - invalid header received
20210912::001042: Head 2: Comm CTD: read error - invalid header received
20210912::001042: Head 1: Comm CTD: read error - invalid header received
20210912::001042: Head 2: Comm CTD: read error - invalid header received
20210912::001042: Head 1: Comm CTD: read error - invalid header received
20210912::001043: Head 2: Comm CTD: read error - invalid header received
20210912::001043: Head 1: Comm CTD: read error - invalid header received
20210912::001043: Head 2: Comm CTD: read error - invalid header received
20210912::001043: Head 1: Comm CTD: read error - invalid header received
20210912::001043: Head 2: Comm CTD: read error - invalid header received
20210912::001043: Head 1: Comm CTD: read error - invalid header received
20210912::001043: Head 2: Comm CTD: read error - invalid header received
20210912::001043: Head 1: Comm CTD: read error - invalid header received
20210912::001044: Head 2: Comm CTD: read error - invalid header received
20210912::001044: Head 1: Comm CTD: read error - invalid header received
20210912::001044: Head 2: Comm CTD: read error - invalid header received
20210912::001044: Head 1: Comm CTD: read error - invalid header received
20210912::001044: Head 2: Comm CTD: read error - invalid header received
20210912::001044: Head 1: Comm CTD: read error - invalid header received
20210912::001045: Head 2: Comm CTD: read error - invalid header received
20210912::001045: Head 1: Comm CTD: read error - invalid header received
20210912::001045: Head 2: Comm CTD: read error - invalid header received
20210912::001045: Head 1: Comm CTD: read error - invalid header received
20210912::001045: Head 2: Comm CTD: read error - invalid header received
20210912::001045: Head 1: Comm CTD: read error - invalid header received
20210912::001046: Head 2: Comm CTD: read error - invalid header received
20210912::001046: Head 1: Comm CTD: read error - invalid header received
20210912::001046: Head 2: Comm CTD: read error - invalid header received
20210912::001046: Head 1: Comm CTD: read error - invalid header received
20210912::001046: Head 2: Comm CTD: read error - invalid header received
20210912::001046: Head 1: Comm CTD: read error - invalid header received
20210912::001046: Head 2: Comm CTD: read error - invalid header received
20210912::001046: Head 1: Comm CTD: read error - invalid header received
20210912::001047: Head 2: Comm CTD: read error - invalid header received
20210912::001047: Head 1: Comm CTD: read error - invalid header received
20210912::001047: Head 2: Comm CTD: read error - invalid header received
20210912::001047: Head 1: Comm CTD: read error - invalid header received
20210912::001047: Head 2: Comm CTD: read error - invalid header received
20210912::001047: Head 1: Comm CTD: read error - invalid header received
20210912::001048: Head 2: Comm CTD: read error - invalid header received
20210912::001048: Head 1: Comm CTD: read error - invalid header received
20210912::001048: Head 2: Comm CTD: read error - invalid header received
20210912::001048: Head 1: Comm CTD: read error - invalid header received
20210912::001048: Head 2: Comm CTD: read error - invalid header received
20210912::001048: Head 1: Comm CTD: read error - invalid header received
20210912::001049: Head 2: Comm CTD: read error - invalid header received
20210912::001049: Head 1: Comm CTD: read error - invalid header received
20210912::001049: Head 2: Comm CTD: read error - invalid header received
20210912::001049: Head 1: Comm CTD: read error - invalid header received
20210912::001049: Head 2: Comm CTD: read error - invalid header received
20210912::001049: Head 1: Comm CTD: read error - invalid header received
20210912::001049: Head 2: Comm CTD: read error - invalid header received
20210912::001049: Head 1: Comm CTD: read error - invalid header received
20210912::001050: Head 2: Comm CTD: read error - invalid header received
20210912::001050: Head 1: Comm CTD: read error - invalid header received
20210912::001050: Head 2: Comm CTD: read error - invalid header received
20210912::001050: Head 1: Comm CTD: read error - invalid header received
20210912::001050: Head 2: Comm CTD: read error - invalid header received
20210912::001050: Head 1: Comm CTD: read error - invalid header received
20210912::001051: Head 2: Comm CTD: read error - invalid header received
20210912::001051: Head 1: Comm CTD: read error - invalid header received
20210912::001051: Head 2: Comm CTD: read error - invalid header received
20210912::001051: Head 1: Comm CTD: read error - invalid header received
20210912::001100: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 152
20210912::001100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001130: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 206
20210912::001130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001200: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 260
20210912::001200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001230: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 312
20210912::001230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001300: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 366
20210912::001300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001330: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 419
20210912::001330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001400: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 472
20210912::001400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001430: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 526
20210912::001430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001500: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 579
20210912::001500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001530: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 632
20210912::001530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 36.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001600: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 685
20210912::001600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001630: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 739
20210912::001630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001700: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 18.7%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 792
20210912::001700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001730: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 18.7%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 845
20210912::001730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001800: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 899
20210912::001800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001830: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 952
20210912::001830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001900: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1005
20210912::001900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001930: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1059
20210912::001930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::001930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002000: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1112
20210912::002000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002030: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1165
20210912::002030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002100: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1219
20210912::002100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002130: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1272
20210912::002130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002200: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1325
20210912::002200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 32C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002230: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1379
20210912::002230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 32C, Laser 37.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002300: System  Initialized, Gain 1, Elec PB 47.4C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1432
20210912::002300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 32C, Laser 38.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002307: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::002308: GUI: ERROR: Received Invalid Packet ID: 0
20210912::002309: GUI: Lost Communications with Sensor 1.
20210912::002309: GUI: Requesing STOP operation, Head 2
20210912::002309: GUI: Attempting Communications with Head 1...
20210912::002309: Head 2: Received request: STOP
20210912::002310: GUI: Established Communications with Head 1.
20210912::002311: Head 1: Initializing Communications with GUI ...
20210912::002312: Head 1: Communications Established.
20210912::002313: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::002313: Head 1: Connection Established with the GUI.
20210912::002313: Head 1: Initializing Subsystems, standby ...
20210912::002314: Head 1: Initializing Hardware, Stand by ...
20210912::002314: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::002315: Head 1: NtQuery - testing 1 ...
20210912::002315: Head 1: clock resolution: 10
20210912::002315: Head 1: NtQuery - testing 2, after setting max res ...
20210912::002316: Head 1: clock resolution: 10
20210912::002316: Head 1: Initializing Optics Electronics ...
20210912::002316: Head 1: Power Laser Controller
20210912::002318: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::002319: GUI: ERROR: Received Invalid Packet ID: 0
20210912::002320: GUI: Lost Communications with Head 2.
20210912::002320: Head 1: Power Scanner Controller
20210912::002320: GUI: Attempting Communications with Head 2...
20210912::002321: GUI: Established Communications with Head 2.
20210912::002322: Head 2: Initializing Communications with GUI ...
20210912::002322: Head 1: Power OPTO Sensor
20210912::002323: Head 2: Communications Established.
20210912::002324: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::002324: Head 2: Connection Established with the GUI.
20210912::002324: Head 2: Initializing Subsystems, standby ...
20210912::002325: Head 2: Initializing Hardware, Stand by ...
20210912::002325: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::002326: Head 2: NtQuery - testing 1 ...
20210912::002326: Head 2: clock resolution: 10
20210912::002326: Head 2: NtQuery - testing 2, after setting max res ...
20210912::002327: Head 2: clock resolution: 10
20210912::002327: Head 2: Initializing Optics Electronics ...
20210912::002327: Head 2: Power Laser Controller
20210912::002330: System NOT Initialized, Gain 0, Elec PB 47.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 35
20210912::002330: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002330: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 59.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002331: Head 2: Power Scanner Controller
20210912::002333: Head 2: Power OPTO Sensor
20210912::002341: Head 1: Eye Safe Optical Filter State there 16, not there 14, transition 1
20210912::002341: Head 1: Eye Safe Optical Filter check Passed
20210912::002341: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::002341: Head 1: Initializing Time Sync Subsystem.
20210912::002342: Head 1: Initializing CTD Subsystem.
20210912::002342: Head 1: CTD Initialization Successful
20210912::002342: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::002343: Head 1: Time Sync UDP started, waiting for sync...
20210912::002343: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::002344: Head 1: Time Synchronization Achieved: 2021.09.12   00:23:45::0011
20210912::002352: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::002352: Head 2: Eye Safe Optical Filter check Passed
20210912::002352: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::002353: Head 2: Initializing Time Sync Subsystem.
20210912::002353: Head 2: Initializing CTD Subsystem.
20210912::002353: Head 2: CTD Initialization Successful
20210912::002354: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::002354: Head 2: Time Sync UDP started, waiting for sync...
20210912::002354: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::002355: Head 2: Time Synchronization Achieved: 2021.09.12   00:23:56::0014
20210912::002400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 0.0C, Dig 59.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002400: System  Initialized, Gain 1, Elec PB 47.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 89
20210912::002400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 25%, OPB 32C, Laser 38.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002409: Head 2: CTD Ethernet connection established.
20210912::002409: Head 1: CTD Ethernet connection established.
20210912::002410: Head 2: Comm CTD: read error - invalid header received
20210912::002410: Head 1: Comm CTD: read error - invalid header received
20210912::002410: Head 2: Comm CTD: read error - invalid header received
20210912::002410: Head 1: Comm CTD: read error - invalid header received
20210912::002410: Head 2: Comm CTD: read error - invalid header received
20210912::002410: Head 1: Comm CTD: read error - invalid header received
20210912::002410: Head 2: Comm CTD: read error - invalid header received
20210912::002411: Head 1: Comm CTD: read error - invalid header received
20210912::002411: Head 2: Comm CTD: read error - invalid header received
20210912::002411: Head 1: Comm CTD: read error - invalid header received
20210912::002411: Head 2: Comm CTD: read error - invalid header received
20210912::002411: Head 1: Comm CTD: read error - invalid header received
20210912::002411: Head 2: Comm CTD: read error - invalid header received
20210912::002411: Head 1: Comm CTD: read error - invalid header received
20210912::002412: Head 2: Comm CTD: read error - invalid header received
20210912::002412: Head 1: Comm CTD: read error - invalid header received
20210912::002412: Head 2: Comm CTD: read error - invalid header received
20210912::002412: Head 1: Comm CTD: read error - invalid header received
20210912::002412: Head 2: Comm CTD: read error - invalid header received
20210912::002412: Head 1: Comm CTD: read error - invalid header received
20210912::002413: Head 2: Comm CTD: read error - invalid header received
20210912::002413: Head 1: Comm CTD: read error - invalid header received
20210912::002413: Head 2: Comm CTD: read error - invalid header received
20210912::002413: Head 1: Comm CTD: read error - invalid header received
20210912::002413: Head 2: Comm CTD: read error - invalid header received
20210912::002413: Head 1: Comm CTD: read error - invalid header received
20210912::002414: Head 2: Comm CTD: read error - invalid header received
20210912::002414: Head 1: Comm CTD: read error - invalid header received
20210912::002414: Head 2: Comm CTD: read error - invalid header received
20210912::002414: Head 1: Comm CTD: read error - invalid header received
20210912::002414: Head 2: Comm CTD: read error - invalid header received
20210912::002414: Head 1: Comm CTD: read error - invalid header received
20210912::002414: Head 2: Comm CTD: read error - invalid header received
20210912::002414: Head 1: Comm CTD: read error - invalid header received
20210912::002415: Head 2: Comm CTD: read error - invalid header received
20210912::002415: Head 1: Comm CTD: read error - invalid header received
20210912::002415: Head 2: Comm CTD: read error - invalid header received
20210912::002415: Head 1: Comm CTD: read error - invalid header received
20210912::002415: Head 2: Comm CTD: read error - invalid header received
20210912::002415: Head 1: Comm CTD: read error - invalid header received
20210912::002416: Head 2: Comm CTD: read error - invalid header received
20210912::002416: Head 1: Comm CTD: read error - invalid header received
20210912::002416: Head 2: Comm CTD: read error - invalid header received
20210912::002416: Head 1: Comm CTD: read error - invalid header received
20210912::002416: Head 2: Comm CTD: read error - invalid header received
20210912::002416: Head 1: Comm CTD: read error - invalid header received
20210912::002417: Head 2: Comm CTD: read error - invalid header received
20210912::002417: Head 1: Comm CTD: read error - invalid header received
20210912::002417: Head 2: Comm CTD: read error - invalid header received
20210912::002417: Head 1: Comm CTD: read error - invalid header received
20210912::002417: Head 2: Comm CTD: read error - invalid header received
20210912::002417: Head 1: Comm CTD: read error - invalid header received
20210912::002417: Head 2: Comm CTD: read error - invalid header received
20210912::002417: Head 1: Comm CTD: read error - invalid header received
20210912::002418: Head 2: Comm CTD: read error - invalid header received
20210912::002418: Head 1: Comm CTD: read error - invalid header received
20210912::002418: Head 2: Comm CTD: read error - invalid header received
20210912::002418: Head 1: Comm CTD: read error - invalid header received
20210912::002418: Head 2: Comm CTD: read error - invalid header received
20210912::002418: Head 1: Comm CTD: read error - invalid header received
20210912::002419: Head 2: Comm CTD: read error - invalid header received
20210912::002419: Head 1: Comm CTD: read error - invalid header received
20210912::002419: Head 2: Comm CTD: read error - invalid header received
20210912::002419: Head 1: Comm CTD: read error - invalid header received
20210912::002419: Head 2: Comm CTD: read error - invalid header received
20210912::002419: Head 1: Comm CTD: read error - invalid header received
20210912::002420: Head 2: Comm CTD: read error - invalid header received
20210912::002420: Head 1: Comm CTD: read error - invalid header received
20210912::002420: Head 2: Comm CTD: read error - invalid header received
20210912::002420: Head 1: Comm CTD: read error - invalid header received
20210912::002420: Head 2: Comm CTD: read error - invalid header received
20210912::002420: Head 1: Comm CTD: read error - invalid header received
20210912::002420: Head 2: Comm CTD: read error - invalid header received
20210912::002420: Head 1: Comm CTD: read error - invalid header received
20210912::002421: Head 2: Comm CTD: read error - invalid header received
20210912::002421: Head 1: Comm CTD: read error - invalid header received
20210912::002421: Head 2: Comm CTD: read error - invalid header received
20210912::002421: Head 1: Comm CTD: read error - invalid header received
20210912::002421: Head 2: Comm CTD: read error - invalid header received
20210912::002421: Head 1: Comm CTD: read error - invalid header received
20210912::002422: Head 2: Comm CTD: read error - invalid header received
20210912::002422: Head 1: Comm CTD: read error - invalid header received
20210912::002422: Head 2: Comm CTD: read error - invalid header received
20210912::002422: Head 1: Comm CTD: read error - invalid header received
20210912::002422: Head 2: Comm CTD: read error - invalid header received
20210912::002422: Head 1: Comm CTD: read error - invalid header received
20210912::002423: Head 2: Comm CTD: read error - invalid header received
20210912::002423: Head 1: Comm CTD: read error - invalid header received
20210912::002423: Head 2: Comm CTD: read error - invalid header received
20210912::002423: Head 1: Comm CTD: read error - invalid header received
20210912::002423: Head 2: Comm CTD: read error - invalid header received
20210912::002423: Head 1: Comm CTD: read error - invalid header received
20210912::002423: Head 2: Comm CTD: read error - invalid header received
20210912::002424: Head 1: Comm CTD: read error - invalid header received
20210912::002424: Head 2: Comm CTD: read error - invalid header received
20210912::002424: Head 1: Comm CTD: read error - invalid header received
20210912::002424: Head 2: Comm CTD: read error - invalid header received
20210912::002424: Head 1: Comm CTD: read error - invalid header received
20210912::002424: Head 2: Comm CTD: read error - invalid header received
20210912::002424: Head 1: Comm CTD: read error - invalid header received
20210912::002425: Head 2: Comm CTD: read error - invalid header received
20210912::002425: Head 1: Comm CTD: read error - invalid header received
20210912::002425: Head 2: Comm CTD: read error - invalid header received
20210912::002425: GUI: ERROR: Received Invalid Packet ID: 0
20210912::002425: Head 2: Comm CTD: read error - invalid header received
20210912::002426: GUI: Lost Communications with Sensor 1.
20210912::002426: Head 2: Comm CTD: read error - invalid header received
20210912::002426: Head 2: Comm CTD: read error - invalid header received
20210912::002426: GUI: Attempting Communications with Head 1...
20210912::002426: Head 2: Comm CTD: read error - invalid header received
20210912::002426: GUI: Requesing STOP operation, Head 2
20210912::002426: Head 2: Comm CTD: read error - invalid header received
20210912::002427: Head 2: Comm CTD: read error - invalid header received
20210912::002427: Head 2: Comm CTD: read error - invalid header received
20210912::002427: Head 2: Comm CTD: read error - invalid header received
20210912::002428: Head 2: Comm CTD: read error - invalid header received
20210912::002428: Head 2: Comm CTD: read error - invalid header received
20210912::002428: Head 2: Comm CTD: read error - invalid header received
20210912::002429: Head 2: Comm CTD: read error - invalid header received
20210912::002429: Head 2: Comm CTD: read error - invalid header received
20210912::002429: Head 2: Comm CTD: read error - invalid header received
20210912::002430: Head 2: Comm CTD: read error - invalid header received
20210912::002430: Head 2: Received request: STOP
20210912::002430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 31C, Laser 36.0C, Dig 59.0C, Scan Az fault 0, gain 0, laser state 0
20210912::002435: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::002436: GUI: ERROR: Received Invalid Packet ID: 0
20210912::002436: GUI: Lost Communications with Head 2.
20210912::002437: GUI: Attempting Communications with Head 2...
20210912::010523: GUI: Established Communications with Head 1.
20210912::010524: Head 1: Initializing Communications with GUI ...
20210912::010525: Head 1: Communications Established.
20210912::010526: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::010526: Head 1: Connection Established with the GUI.
20210912::010526: Head 1: Initializing Subsystems, standby ...
20210912::010527: Head 1: Initializing Hardware, Stand by ...
20210912::010530: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 12
20210912::010530: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010534: GUI: Established Communications with Head 2.
20210912::010535: Head 2: Initializing Communications with GUI ...
20210912::010535: Head 2: Communications Established.
20210912::010536: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::010536: Head 2: Connection Established with the GUI.
20210912::010536: Head 2: Initializing Subsystems, standby ...
20210912::010537: Head 2: Initializing Hardware, Stand by ...
20210912::010545: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::010545: Head 1: NtQuery - testing 1 ...
20210912::010546: Head 1: clock resolution: 10
20210912::010546: Head 1: NtQuery - testing 2, after setting max res ...
20210912::010546: Head 1: clock resolution: 10
20210912::010547: Head 1: Initializing Optics Electronics ...
20210912::010547: Head 1: Power Laser Controller
20210912::010551: Head 1: Power Scanner Controller
20210912::010551: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::010552: Head 2: NtQuery - testing 1 ...
20210912::010552: Head 2: clock resolution: 10
20210912::010552: Head 2: NtQuery - testing 2, after setting max res ...
20210912::010552: Head 2: clock resolution: 10
20210912::010553: Head 1: Power OPTO Sensor
20210912::010553: Head 2: Initializing Optics Electronics ...
20210912::010553: Head 2: Power Laser Controller
20210912::010557: Head 2: Power Scanner Controller
20210912::010559: Head 2: Power OPTO Sensor
20210912::010600: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010600: System NOT Initialized, Gain 0, Elec PB 39.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 66
20210912::010600: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010613: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210912::010613: Head 1: Eye Safe Optical Filter check Passed
20210912::010613: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::010614: Head 1: Initializing Time Sync Subsystem.
20210912::010614: Head 1: Initializing CTD Subsystem.
20210912::010614: Head 1: CTD Initialization Successful
20210912::010615: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::010615: Head 1: Time Sync UDP started, waiting for sync...
20210912::010615: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::010616: Head 1: Time Synchronization Achieved: 2021.09.12   01:06:17::0014
20210912::010619: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::010619: Head 2: Eye Safe Optical Filter check Passed
20210912::010620: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::010620: Head 2: Initializing Time Sync Subsystem.
20210912::010620: Head 2: Initializing CTD Subsystem.
20210912::010621: Head 2: CTD Initialization Successful
20210912::010621: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::010621: Head 2: Time Sync UDP started, waiting for sync...
20210912::010621: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::010622: Head 2: Time Synchronization Achieved: 2021.09.12   01:06:23::0014
20210912::010625: Head 2: CTD Ethernet connection established.
20210912::010625: Head 1: CTD Ethernet connection established.
20210912::010626: Head 2: Comm CTD: read error - invalid header received
20210912::010626: Head 1: Comm CTD: read error - invalid header received
20210912::010627: Head 2: Comm CTD: read error - invalid header received
20210912::010627: Head 1: Comm CTD: read error - invalid header received
20210912::010627: Head 2: Comm CTD: read error - invalid header received
20210912::010627: Head 1: Comm CTD: read error - invalid header received
20210912::010627: Head 2: Comm CTD: read error - invalid header received
20210912::010627: Head 1: Comm CTD: read error - invalid header received
20210912::010628: Head 2: Comm CTD: read error - invalid header received
20210912::010628: Head 1: Comm CTD: read error - invalid header received
20210912::010628: Head 2: Comm CTD: read error - invalid header received
20210912::010628: Head 1: Comm CTD: read error - invalid header received
20210912::010628: Head 2: Comm CTD: read error - invalid header received
20210912::010628: Head 1: Comm CTD: read error - invalid header received
20210912::010629: Head 2: Comm CTD: read error - invalid header received
20210912::010629: Head 1: Comm CTD: read error - invalid header received
20210912::010629: Head 1: Comm CTD: read error - invalid header received
20210912::010629: Head 2: Comm CTD: read error - invalid header received
20210912::010629: Head 1: Comm CTD: read error - invalid header received
20210912::010629: Head 2: Comm CTD: read error - invalid header received
20210912::010630: Head 1: Comm CTD: read error - invalid header received
20210912::010630: Head 2: Comm CTD: read error - invalid header received
20210912::010630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 32%, OPB 26C, Laser 26.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010630: System  Initialized, Gain 1, Elec PB 39.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 119
20210912::010630: Head 1: Comm CTD: read error - invalid header received
20210912::010630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 33%, OPB 27C, Laser 26.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010630: Head 2: Comm CTD: read error - invalid header received
20210912::010630: Head 1: Comm CTD: read error - invalid header received
20210912::010630: Head 2: Comm CTD: read error - invalid header received
20210912::010630: Head 1: Comm CTD: read error - invalid header received
20210912::010630: Head 2: Comm CTD: read error - invalid header received
20210912::010631: Head 1: Comm CTD: read error - invalid header received
20210912::010631: Head 2: Comm CTD: read error - invalid header received
20210912::010631: Head 1: Comm CTD: read error - invalid header received
20210912::010631: Head 2: Comm CTD: read error - invalid header received
20210912::010631: Head 1: Comm CTD: read error - invalid header received
20210912::010631: Head 2: Comm CTD: read error - invalid header received
20210912::010632: Head 1: Comm CTD: read error - invalid header received
20210912::010632: Head 2: Comm CTD: read error - invalid header received
20210912::010632: Head 1: Comm CTD: read error - invalid header received
20210912::010632: Head 2: Comm CTD: read error - invalid header received
20210912::010632: Head 1: Comm CTD: read error - invalid header received
20210912::010632: Head 2: Comm CTD: read error - invalid header received
20210912::010633: Head 1: Comm CTD: read error - invalid header received
20210912::010633: Head 2: Comm CTD: read error - invalid header received
20210912::010633: Head 1: Comm CTD: read error - invalid header received
20210912::010633: Head 2: Comm CTD: read error - invalid header received
20210912::010633: Head 1: Comm CTD: read error - invalid header received
20210912::010633: Head 2: Comm CTD: read error - invalid header received
20210912::010633: Head 1: Comm CTD: read error - invalid header received
20210912::010633: Head 2: Comm CTD: read error - invalid header received
20210912::010634: Head 1: Comm CTD: read error - invalid header received
20210912::010634: Head 2: Comm CTD: read error - invalid header received
20210912::010634: Head 1: Comm CTD: read error - invalid header received
20210912::010634: Head 2: Comm CTD: read error - invalid header received
20210912::010634: Head 1: Comm CTD: read error - invalid header received
20210912::010634: Head 2: Comm CTD: read error - invalid header received
20210912::010635: Head 1: Comm CTD: read error - invalid header received
20210912::010635: Head 2: Comm CTD: read error - invalid header received
20210912::010635: Head 1: Comm CTD: read error - invalid header received
20210912::010635: Head 2: Comm CTD: read error - invalid header received
20210912::010635: Head 1: Comm CTD: read error - invalid header received
20210912::010635: Head 2: Comm CTD: read error - invalid header received
20210912::010636: Head 1: Comm CTD: read error - invalid header received
20210912::010636: Head 2: Comm CTD: read error - invalid header received
20210912::010636: Head 1: Comm CTD: read error - invalid header received
20210912::010636: Head 2: Comm CTD: read error - invalid header received
20210912::010636: Head 1: Comm CTD: read error - invalid header received
20210912::010636: Head 2: Comm CTD: read error - invalid header received
20210912::010636: Head 1: Comm CTD: read error - invalid header received
20210912::010637: Head 2: Comm CTD: read error - invalid header received
20210912::010637: Head 1: Comm CTD: read error - invalid header received
20210912::010637: Head 2: Comm CTD: read error - invalid header received
20210912::010637: Head 1: Comm CTD: read error - invalid header received
20210912::010637: Head 2: Comm CTD: read error - invalid header received
20210912::010637: Head 1: Comm CTD: read error - invalid header received
20210912::010637: Head 2: Comm CTD: read error - invalid header received
20210912::010638: Head 1: Comm CTD: read error - invalid header received
20210912::010638: Head 2: Comm CTD: read error - invalid header received
20210912::010638: Head 1: Comm CTD: read error - invalid header received
20210912::010638: Head 2: Comm CTD: read error - invalid header received
20210912::010638: Head 1: Comm CTD: read error - invalid header received
20210912::010638: Head 2: Comm CTD: read error - invalid header received
20210912::010639: Head 1: Comm CTD: read error - invalid header received
20210912::010639: Head 2: Comm CTD: read error - invalid header received
20210912::010639: Head 1: Comm CTD: read error - invalid header received
20210912::010639: Head 2: Comm CTD: read error - invalid header received
20210912::010639: Head 1: Comm CTD: read error - invalid header received
20210912::010639: Head 2: Comm CTD: read error - invalid header received
20210912::010639: Head 1: Comm CTD: read error - invalid header received
20210912::010640: Head 2: Comm CTD: read error - invalid header received
20210912::010640: Head 1: Comm CTD: read error - invalid header received
20210912::010640: Head 2: Comm CTD: read error - invalid header received
20210912::010640: Head 1: Comm CTD: read error - invalid header received
20210912::010640: Head 2: Comm CTD: read error - invalid header received
20210912::010640: Head 1: Comm CTD: read error - invalid header received
20210912::010640: Head 2: Comm CTD: read error - invalid header received
20210912::010641: Head 1: Comm CTD: read error - invalid header received
20210912::010641: Head 2: Comm CTD: read error - invalid header received
20210912::010641: Head 1: Comm CTD: read error - invalid header received
20210912::010641: Head 2: Comm CTD: read error - invalid header received
20210912::010641: Head 1: Comm CTD: read error - invalid header received
20210912::010641: Head 2: Comm CTD: read error - invalid header received
20210912::010642: Head 1: Comm CTD: read error - invalid header received
20210912::010642: Head 2: Comm CTD: read error - invalid header received
20210912::010642: Head 1: Comm CTD: read error - invalid header received
20210912::010642: Head 2: Comm CTD: read error - invalid header received
20210912::010642: Head 1: Comm CTD: read error - invalid header received
20210912::010642: Head 2: Comm CTD: read error - invalid header received
20210912::010643: Head 1: Comm CTD: read error - invalid header received
20210912::010643: Head 2: Comm CTD: read error - invalid header received
20210912::010643: Head 1: Comm CTD: read error - invalid header received
20210912::010643: Head 2: Comm CTD: read error - invalid header received
20210912::010643: Head 1: Comm CTD: read error - invalid header received
20210912::010643: Head 2: Comm CTD: read error - invalid header received
20210912::010643: Head 1: Comm CTD: read error - invalid header received
20210912::010643: Head 2: Comm CTD: read error - invalid header received
20210912::010644: Head 1: Comm CTD: read error - invalid header received
20210912::010644: Head 2: Comm CTD: read error - invalid header received
20210912::010644: Head 1: Comm CTD: read error - invalid header received
20210912::010644: Head 2: Comm CTD: read error - invalid header received
20210912::010644: Head 1: Comm CTD: read error - invalid header received
20210912::010644: Head 2: Comm CTD: read error - invalid header received
20210912::010645: Head 1: Comm CTD: read error - invalid header received
20210912::010645: Head 2: Comm CTD: read error - invalid header received
20210912::010645: Head 1: Comm CTD: read error - invalid header received
20210912::010645: Head 2: Comm CTD: read error - invalid header received
20210912::010645: Head 1: Comm CTD: read error - invalid header received
20210912::010645: Head 2: Comm CTD: read error - invalid header received
20210912::010646: Head 1: Comm CTD: read error - invalid header received
20210912::010646: Head 2: Comm CTD: read error - invalid header received
20210912::010646: Head 1: Comm CTD: read error - invalid header received
20210912::010646: Head 2: Comm CTD: read error - invalid header received
20210912::010646: Head 1: Comm CTD: read error - invalid header received
20210912::010646: Head 2: Comm CTD: read error - invalid header received
20210912::010646: Head 1: Comm CTD: read error - invalid header received
20210912::010646: Head 2: Comm CTD: read error - invalid header received
20210912::010647: Head 1: Comm CTD: read error - invalid header received
20210912::010647: Head 2: Comm CTD: read error - invalid header received
20210912::010647: Head 1: Comm CTD: read error - invalid header received
20210912::010647: Head 2: Comm CTD: read error - invalid header received
20210912::010647: Head 1: Comm CTD: read error - invalid header received
20210912::010647: Head 2: Comm CTD: read error - invalid header received
20210912::010648: Head 1: Comm CTD: read error - invalid header received
20210912::010648: Head 2: Comm CTD: read error - invalid header received
20210912::010700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 30%, OPB 27C, Laser 26.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010700: System  Initialized, Gain 1, Elec PB 42.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 172
20210912::010700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 30%, OPB 27C, Laser 27.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 28%, OPB 27C, Laser 27.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010730: System  Initialized, Gain 1, Elec PB 42.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 226
20210912::010730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 28%, OPB 28C, Laser 28.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010800: System  Initialized, Gain 1, Elec PB 42.1C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 280
20210912::010800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 27%, OPB 28C, Laser 29.0C, Dig 45.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 27%, OPB 27C, Laser 28.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010804: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::010805: GUI: ERROR: Received Invalid Packet ID: 0
20210912::010805: GUI: Lost Communications with Sensor 1.
20210912::010805: GUI: Requesing STOP operation, Head 2
20210912::010806: Head 2: Received request: STOP
20210912::010806: GUI: Attempting Communications with Head 1...
20210912::010806: GUI: Established Communications with Head 1.
20210912::010807: Head 1: Initializing Communications with GUI ...
20210912::010808: Head 1: Communications Established.
20210912::010809: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::010809: Head 1: Connection Established with the GUI.
20210912::010810: Head 1: Initializing Subsystems, standby ...
20210912::010810: Head 1: Initializing Hardware, Stand by ...
20210912::010811: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::010811: Head 1: NtQuery - testing 1 ...
20210912::010811: Head 1: clock resolution: 1
20210912::010812: Head 1: NtQuery - testing 2, after setting max res ...
20210912::010812: Head 1: clock resolution: 1
20210912::010812: Head 1: Initializing Optics Electronics ...
20210912::010813: Head 1: Power Laser Controller
20210912::010816: Head 1: Power Scanner Controller
20210912::010818: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::010819: Head 1: Power OPTO Sensor
20210912::010819: GUI: ERROR: Received Invalid Packet ID: 0
20210912::010819: GUI: Lost Communications with Head 2.
20210912::010820: GUI: Attempting Communications with Head 2...
20210912::010820: GUI: Established Communications with Head 2.
20210912::010821: Head 2: Initializing Communications with GUI ...
20210912::010822: Head 2: Communications Established.
20210912::010823: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::010824: Head 2: Connection Established with the GUI.
20210912::010824: Head 2: Initializing Subsystems, standby ...
20210912::010824: Head 2: Initializing Hardware, Stand by ...
20210912::010825: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::010825: Head 2: NtQuery - testing 1 ...
20210912::010826: Head 2: clock resolution: 1
20210912::010826: Head 2: NtQuery - testing 2, after setting max res ...
20210912::010826: Head 2: clock resolution: 1
20210912::010826: Head 2: Initializing Optics Electronics ...
20210912::010827: Head 2: Power Laser Controller
20210912::010830: System NOT Initialized, Gain 0, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 42
20210912::010830: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010830: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010831: Head 2: Power Scanner Controller
20210912::010833: Head 2: Power OPTO Sensor
20210912::010837: Head 1: Eye Safe Optical Filter State there 13, not there 17, transition 1
20210912::010837: Head 1: Eye Safe Optical Filter check Passed
20210912::010838: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::010838: Head 1: Initializing Time Sync Subsystem.
20210912::010838: Head 1: Initializing CTD Subsystem.
20210912::010839: Head 1: CTD Initialization Successful
20210912::010839: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::010839: Head 1: Time Sync UDP started, waiting for sync...
20210912::010839: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::010840: Head 1: Time Synchronization Achieved: 2021.09.12   01:08:41::0014
20210912::010851: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::010851: Head 2: Eye Safe Optical Filter check Passed
20210912::010852: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::010852: Head 2: Initializing Time Sync Subsystem.
20210912::010852: Head 2: Initializing CTD Subsystem.
20210912::010853: Head 2: CTD Initialization Successful
20210912::010853: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::010853: Head 2: Time Sync UDP started, waiting for sync...
20210912::010854: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::010854: Head 2: Time Synchronization Achieved: 2021.09.12   01:08:55::0013
20210912::010900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 26%, OPB 27C, Laser 0.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010900: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 96
20210912::010900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 26%, OPB 28C, Laser 30.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010906: Head 1: CTD Ethernet connection established.
20210912::010906: Head 2: CTD Ethernet connection established.
20210912::010907: Head 1: Comm CTD: read error - invalid header received
20210912::010907: Head 2: Comm CTD: read error - invalid header received
20210912::010907: Head 1: Comm CTD: read error - invalid header received
20210912::010907: Head 2: Comm CTD: read error - invalid header received
20210912::010908: Head 1: Comm CTD: read error - invalid header received
20210912::010908: Head 2: Comm CTD: read error - invalid header received
20210912::010908: Head 1: Comm CTD: read error - invalid header received
20210912::010908: Head 2: Comm CTD: read error - invalid header received
20210912::010908: Head 1: Comm CTD: read error - invalid header received
20210912::010908: Head 2: Comm CTD: read error - invalid header received
20210912::010909: Head 1: Comm CTD: read error - invalid header received
20210912::010909: Head 2: Comm CTD: read error - invalid header received
20210912::010909: Head 1: Comm CTD: read error - invalid header received
20210912::010909: Head 2: Comm CTD: read error - invalid header received
20210912::010909: Head 1: Comm CTD: read error - invalid header received
20210912::010909: Head 2: Comm CTD: read error - invalid header received
20210912::010909: Head 1: Comm CTD: read error - invalid header received
20210912::010909: Head 2: Comm CTD: read error - invalid header received
20210912::010910: Head 1: Comm CTD: read error - invalid header received
20210912::010910: Head 2: Comm CTD: read error - invalid header received
20210912::010910: Head 1: Comm CTD: read error - invalid header received
20210912::010910: Head 2: Comm CTD: read error - invalid header received
20210912::010910: Head 1: Comm CTD: read error - invalid header received
20210912::010910: Head 2: Comm CTD: read error - invalid header received
20210912::010911: Head 1: Comm CTD: read error - invalid header received
20210912::010911: Head 2: Comm CTD: read error - invalid header received
20210912::010911: Head 1: Comm CTD: read error - invalid header received
20210912::010911: Head 2: Comm CTD: read error - invalid header received
20210912::010911: Head 1: Comm CTD: read error - invalid header received
20210912::010911: Head 2: Comm CTD: read error - invalid header received
20210912::010912: Head 1: Comm CTD: read error - invalid header received
20210912::010912: Head 2: Comm CTD: read error - invalid header received
20210912::010912: Head 1: Comm CTD: read error - invalid header received
20210912::010912: Head 2: Comm CTD: read error - invalid header received
20210912::010912: Head 1: Comm CTD: read error - invalid header received
20210912::010912: Head 2: Comm CTD: read error - invalid header received
20210912::010912: Head 1: Comm CTD: read error - invalid header received
20210912::010913: Head 2: Comm CTD: read error - invalid header received
20210912::010913: Head 1: Comm CTD: read error - invalid header received
20210912::010913: Head 2: Comm CTD: read error - invalid header received
20210912::010913: Head 1: Comm CTD: read error - invalid header received
20210912::010913: Head 2: Comm CTD: read error - invalid header received
20210912::010913: Head 1: Comm CTD: read error - invalid header received
20210912::010913: Head 2: Comm CTD: read error - invalid header received
20210912::010914: Head 1: Comm CTD: read error - invalid header received
20210912::010914: Head 2: Comm CTD: read error - invalid header received
20210912::010914: Head 1: Comm CTD: read error - invalid header received
20210912::010914: Head 2: Comm CTD: read error - invalid header received
20210912::010914: Head 1: Comm CTD: read error - invalid header received
20210912::010914: Head 2: Comm CTD: read error - invalid header received
20210912::010915: Head 1: Comm CTD: read error - invalid header received
20210912::010915: Head 2: Comm CTD: read error - invalid header received
20210912::010915: Head 1: Comm CTD: read error - invalid header received
20210912::010915: Head 2: Comm CTD: read error - invalid header received
20210912::010915: Head 1: Comm CTD: read error - invalid header received
20210912::010915: Head 2: Comm CTD: read error - invalid header received
20210912::010915: Head 1: Comm CTD: read error - invalid header received
20210912::010916: Head 2: Comm CTD: read error - invalid header received
20210912::010916: Head 1: Comm CTD: read error - invalid header received
20210912::010916: Head 2: Comm CTD: read error - invalid header received
20210912::010916: Head 1: Comm CTD: read error - invalid header received
20210912::010916: Head 2: Comm CTD: read error - invalid header received
20210912::010916: Head 1: Comm CTD: read error - invalid header received
20210912::010916: Head 2: Comm CTD: read error - invalid header received
20210912::010917: Head 1: Comm CTD: read error - invalid header received
20210912::010917: Head 2: Comm CTD: read error - invalid header received
20210912::010917: Head 1: Comm CTD: read error - invalid header received
20210912::010917: Head 2: Comm CTD: read error - invalid header received
20210912::010917: Head 1: Comm CTD: read error - invalid header received
20210912::010917: Head 2: Comm CTD: read error - invalid header received
20210912::010918: Head 1: Comm CTD: read error - invalid header received
20210912::010918: Head 2: Comm CTD: read error - invalid header received
20210912::010918: Head 1: Comm CTD: read error - invalid header received
20210912::010918: Head 2: Comm CTD: read error - invalid header received
20210912::010918: Head 1: Comm CTD: read error - invalid header received
20210912::010918: Head 2: Comm CTD: read error - invalid header received
20210912::010918: Head 1: Comm CTD: read error - invalid header received
20210912::010919: Head 2: Comm CTD: read error - invalid header received
20210912::010919: Head 1: Comm CTD: read error - invalid header received
20210912::010919: Head 2: Comm CTD: read error - invalid header received
20210912::010919: Head 1: Comm CTD: read error - invalid header received
20210912::010919: Head 2: Comm CTD: read error - invalid header received
20210912::010919: Head 1: Comm CTD: read error - invalid header received
20210912::010919: Head 2: Comm CTD: read error - invalid header received
20210912::010920: Head 1: Comm CTD: read error - invalid header received
20210912::010920: Head 2: Comm CTD: read error - invalid header received
20210912::010920: Head 1: Comm CTD: read error - invalid header received
20210912::010920: Head 2: Comm CTD: read error - invalid header received
20210912::010920: Head 1: Comm CTD: read error - invalid header received
20210912::010920: Head 2: Comm CTD: read error - invalid header received
20210912::010921: Head 1: Comm CTD: read error - invalid header received
20210912::010921: Head 2: Comm CTD: read error - invalid header received
20210912::010921: Head 1: Comm CTD: read error - invalid header received
20210912::010921: Head 2: Comm CTD: read error - invalid header received
20210912::010921: Head 1: Comm CTD: read error - invalid header received
20210912::010921: Head 2: Comm CTD: read error - invalid header received
20210912::010922: Head 1: Comm CTD: read error - invalid header received
20210912::010922: Head 2: Comm CTD: read error - invalid header received
20210912::010922: Head 1: Comm CTD: read error - invalid header received
20210912::010922: Head 2: Comm CTD: read error - invalid header received
20210912::010922: Head 1: Comm CTD: read error - invalid header received
20210912::010922: Head 2: Comm CTD: read error - invalid header received
20210912::010922: Head 1: Comm CTD: read error - invalid header received
20210912::010922: Head 2: Comm CTD: read error - invalid header received
20210912::010923: Head 1: Comm CTD: read error - invalid header received
20210912::010923: Head 2: Comm CTD: read error - invalid header received
20210912::010923: Head 1: Comm CTD: read error - invalid header received
20210912::010923: Head 2: Comm CTD: read error - invalid header received
20210912::010923: Head 1: Comm CTD: read error - invalid header received
20210912::010923: Head 2: Comm CTD: read error - invalid header received
20210912::010924: Head 1: Comm CTD: read error - invalid header received
20210912::010924: Head 2: Comm CTD: read error - invalid header received
20210912::010924: Head 1: Comm CTD: read error - invalid header received
20210912::010924: Head 2: Comm CTD: read error - invalid header received
20210912::010930: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 149
20210912::010930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 25%, OPB 28C, Laser 31.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::010930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 25%, OPB 27C, Laser 29.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011000: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 202
20210912::011000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 25%, OPB 28C, Laser 31.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 25%, OPB 28C, Laser 30.0C, Dig 54.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011004: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::011005: GUI: ERROR: Received Invalid Packet ID: 0
20210912::011006: GUI: Lost Communications with Head 2.
20210912::011006: GUI: Attempting Communications with Head 2...
20210912::011006: GUI: Requesing STOP operation, Head 2
20210912::011006: GUI: Requesing STOP operation, Head 1
20210912::011007: Head 1: Received request: STOP
20210912::011007: GUI: Established Communications with Head 2.
20210912::011008: Head 2: Initializing Communications with GUI ...
20210912::011009: Head 2: Communications Established.
20210912::011010: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::011010: Head 2: Connection Established with the GUI.
20210912::011011: Head 2: Initializing Subsystems, standby ...
20210912::011011: Head 2: Initializing Hardware, Stand by ...
20210912::011012: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::011012: Head 2: NtQuery - testing 1 ...
20210912::011012: Head 2: clock resolution: 1
20210912::011013: Head 2: NtQuery - testing 2, after setting max res ...
20210912::011013: Head 2: clock resolution: 1
20210912::011013: Head 2: Initializing Optics Electronics ...
20210912::011013: Head 2: Power Laser Controller
20210912::011017: Head 2: Power Scanner Controller
20210912::011019: Head 2: Power OPTO Sensor
20210912::011023: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::011024: GUI: ERROR: Received Invalid Packet ID: 0
20210912::011024: GUI: Lost Communications with Sensor 1.
20210912::011025: GUI: Attempting Communications with Head 1...
20210912::011025: GUI: Established Communications with Head 1.
20210912::011026: Head 1: Initializing Communications with GUI ...
20210912::011027: Head 1: Communications Established.
20210912::011028: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::011029: Head 1: Connection Established with the GUI.
20210912::011029: Head 1: Initializing Subsystems, standby ...
20210912::011029: Head 1: Initializing Hardware, Stand by ...
20210912::011030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011030: System NOT Initialized, Gain 0, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 8
20210912::011030: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011030: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::011030: Head 1: NtQuery - testing 1 ...
20210912::011031: Head 1: clock resolution: 1
20210912::011031: Head 1: NtQuery - testing 2, after setting max res ...
20210912::011031: Head 1: clock resolution: 1
20210912::011032: Head 1: Initializing Optics Electronics ...
20210912::011032: Head 1: Power Laser Controller
20210912::011036: Head 1: Power Scanner Controller
20210912::011038: Head 1: Power OPTO Sensor
20210912::011038: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::011038: Head 2: Eye Safe Optical Filter check Passed
20210912::011038: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::011039: Head 2: Initializing Time Sync Subsystem.
20210912::011039: Head 2: Initializing CTD Subsystem.
20210912::011039: Head 2: CTD Initialization Successful
20210912::011040: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::011040: Head 2: Time Sync UDP started, waiting for sync...
20210912::011040: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::011041: Head 2: Time Synchronization Achieved: 2021.09.12   01:10:42::0019
20210912::011056: Head 1: Eye Safe Optical Filter State there 15, not there 15, transition 1
20210912::011057: Head 1: Eye Safe Optical Filter check Passed
20210912::011057: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::011057: Head 1: Initializing Time Sync Subsystem.
20210912::011058: Head 1: Initializing CTD Subsystem.
20210912::011058: Head 1: CTD Initialization Successful
20210912::011058: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::011058: Head 1: Time Sync UDP started, waiting for sync...
20210912::011059: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::011059: Head 1: Time Synchronization Achieved: 2021.09.12   01:11:00::0015
20210912::011100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 25%, OPB 28C, Laser 30.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011100: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 61
20210912::011100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 28C, Laser 0.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 25%, OPB 28C, Laser 31.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011130: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 115
20210912::011130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 29C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 25%, OPB 28C, Laser 31.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011200: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 168
20210912::011200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 28C, Laser 32.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011230: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 221
20210912::011230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 28C, Laser 31.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011300: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 275
20210912::011300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 28C, Laser 31.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011330: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 328
20210912::011330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 28C, Laser 32.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011400: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 381
20210912::011400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 28C, Laser 32.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011430: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 435
20210912::011430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011431: Head 2: CTD Ethernet connection established.
20210912::011431: Head 1: CTD Ethernet connection established.
20210912::011432: Head 2: Comm CTD: read error - invalid header received
20210912::011432: Head 1: Comm CTD: read error - invalid header received
20210912::011432: Head 2: Comm CTD: read error - invalid header received
20210912::011432: Head 1: Comm CTD: read error - invalid header received
20210912::011432: Head 2: Comm CTD: read error - invalid header received
20210912::011432: Head 1: Comm CTD: read error - invalid header received
20210912::011433: Head 2: Comm CTD: read error - invalid header received
20210912::011433: Head 1: Comm CTD: read error - invalid header received
20210912::011433: Head 2: Comm CTD: read error - invalid header received
20210912::011433: Head 1: Comm CTD: read error - invalid header received
20210912::011433: Head 2: Comm CTD: read error - invalid header received
20210912::011433: Head 1: Comm CTD: read error - invalid header received
20210912::011434: Head 2: Comm CTD: read error - invalid header received
20210912::011434: Head 1: Comm CTD: read error - invalid header received
20210912::011434: Head 2: Comm CTD: read error - invalid header received
20210912::011434: Head 1: Comm CTD: read error - invalid header received
20210912::011434: Head 2: Comm CTD: read error - invalid header received
20210912::011434: Head 1: Comm CTD: read error - invalid header received
20210912::011435: Head 2: Comm CTD: read error - invalid header received
20210912::011435: Head 1: Comm CTD: read error - invalid header received
20210912::011435: Head 2: Comm CTD: read error - invalid header received
20210912::011435: Head 1: Comm CTD: read error - invalid header received
20210912::011435: Head 2: Comm CTD: read error - invalid header received
20210912::011435: Head 1: Comm CTD: read error - invalid header received
20210912::011435: Head 2: Comm CTD: read error - invalid header received
20210912::011435: Head 1: Comm CTD: read error - invalid header received
20210912::011436: Head 2: Comm CTD: read error - invalid header received
20210912::011436: Head 1: Comm CTD: read error - invalid header received
20210912::011436: Head 2: Comm CTD: read error - invalid header received
20210912::011436: Head 1: Comm CTD: read error - invalid header received
20210912::011436: Head 2: Comm CTD: read error - invalid header received
20210912::011436: Head 1: Comm CTD: read error - invalid header received
20210912::011437: Head 2: Comm CTD: read error - invalid header received
20210912::011437: Head 1: Comm CTD: read error - invalid header received
20210912::011437: Head 2: Comm CTD: read error - invalid header received
20210912::011437: Head 1: Comm CTD: read error - invalid header received
20210912::011437: Head 2: Comm CTD: read error - invalid header received
20210912::011437: Head 1: Comm CTD: read error - invalid header received
20210912::011438: Head 2: Comm CTD: read error - invalid header received
20210912::011438: Head 1: Comm CTD: read error - invalid header received
20210912::011438: Head 2: Comm CTD: read error - invalid header received
20210912::011438: Head 1: Comm CTD: read error - invalid header received
20210912::011438: Head 2: Comm CTD: read error - invalid header received
20210912::011438: Head 1: Comm CTD: read error - invalid header received
20210912::011438: Head 2: Comm CTD: read error - invalid header received
20210912::011438: Head 1: Comm CTD: read error - invalid header received
20210912::011439: Head 2: Comm CTD: read error - invalid header received
20210912::011439: Head 1: Comm CTD: read error - invalid header received
20210912::011439: Head 2: Comm CTD: read error - invalid header received
20210912::011439: Head 1: Comm CTD: read error - invalid header received
20210912::011439: Head 2: Comm CTD: read error - invalid header received
20210912::011439: Head 1: Comm CTD: read error - invalid header received
20210912::011440: Head 2: Comm CTD: read error - invalid header received
20210912::011440: Head 1: Comm CTD: read error - invalid header received
20210912::011440: Head 2: Comm CTD: read error - invalid header received
20210912::011440: Head 1: Comm CTD: read error - invalid header received
20210912::011440: Head 2: Comm CTD: read error - invalid header received
20210912::011440: Head 1: Comm CTD: read error - invalid header received
20210912::011441: Head 2: Comm CTD: read error - invalid header received
20210912::011441: Head 1: Comm CTD: read error - invalid header received
20210912::011441: Head 2: Comm CTD: read error - invalid header received
20210912::011441: Head 1: Comm CTD: read error - invalid header received
20210912::011441: Head 2: Comm CTD: read error - invalid header received
20210912::011441: Head 1: Comm CTD: read error - invalid header received
20210912::011500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 32.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011500: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 488
20210912::011500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011530: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 541
20210912::011530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011600: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 595
20210912::011600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011630: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 648
20210912::011630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011700: System  Initialized, Gain 1, Elec PB 48.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 701
20210912::011700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011730: System  Initialized, Gain 1, Elec PB 48.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 755
20210912::011730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 30C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011800: System  Initialized, Gain 1, Elec PB 48.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 808
20210912::011800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 34.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011830: System  Initialized, Gain 1, Elec PB 48.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 861
20210912::011830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 35.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011844: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::011845: GUI: ERROR: Received Invalid Packet ID: 0
20210912::011846: GUI: Lost Communications with Head 2.
20210912::011846: GUI: Requesing STOP operation, Head 1
20210912::011846: Head 1: Received request: STOP
20210912::011846: GUI: Attempting Communications with Head 2...
20210912::011847: GUI: Established Communications with Head 2.
20210912::011848: Head 2: Initializing Communications with GUI ...
20210912::011849: Head 2: Communications Established.
20210912::011850: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::011850: Head 2: Connection Established with the GUI.
20210912::011850: Head 2: Initializing Subsystems, standby ...
20210912::011851: Head 2: Initializing Hardware, Stand by ...
20210912::011851: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::011852: Head 2: NtQuery - testing 1 ...
20210912::011852: Head 2: clock resolution: 10
20210912::011852: Head 2: NtQuery - testing 2, after setting max res ...
20210912::011853: Head 2: clock resolution: 10
20210912::011853: Head 2: Initializing Optics Electronics ...
20210912::011853: Head 2: Power Laser Controller
20210912::011857: Head 2: Power Scanner Controller
20210912::011859: Head 2: Power OPTO Sensor
20210912::011900: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 59.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011900: System  Initialized, Gain 1, Elec PB 49.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 915
20210912::011900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 35.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011918: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::011918: Head 2: Eye Safe Optical Filter check Passed
20210912::011918: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::011919: Head 2: Initializing Time Sync Subsystem.
20210912::011919: Head 2: Initializing CTD Subsystem.
20210912::011919: Head 2: CTD Initialization Successful
20210912::011919: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::011920: Head 2: Time Sync UDP started, waiting for sync...
20210912::011920: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::011921: Head 2: Time Synchronization Achieved: 2021.09.12   01:19:22::0020
20210912::011930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 29C, Laser 34.0C, Dig 59.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011930: System  Initialized, Gain 1, Elec PB 49.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 968
20210912::011930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 24%, OPB 30C, Laser 35.0C, Dig 50.0C, Scan Az fault 0, gain 0, laser state 0
20210912::011935: Head 2: CTD Ethernet connection established.
20210912::011936: Head 2: Comm CTD: read error - invalid header received
20210912::011936: Head 2: Comm CTD: read error - invalid header received
20210912::011936: Head 2: Comm CTD: read error - invalid header received
20210912::011937: Head 2: Comm CTD: read error - invalid header received
20210912::011937: Head 2: Comm CTD: read error - invalid header received
20210912::011937: Head 2: Comm CTD: read error - invalid header received
20210912::011938: Head 2: Comm CTD: read error - invalid header received
20210912::011938: Head 2: Comm CTD: read error - invalid header received
20210912::011938: Head 2: Comm CTD: read error - invalid header received
20210912::011938: Head 2: Comm CTD: read error - invalid header received
20210912::011939: Head 2: Comm CTD: read error - invalid header received
20210912::011939: Head 2: Comm CTD: read error - invalid header received
20210912::011939: Head 2: Comm CTD: read error - invalid header received
20210912::011940: Head 2: Comm CTD: read error - invalid header received
20210912::011940: Head 2: Comm CTD: read error - invalid header received
20210912::011940: Head 2: Comm CTD: read error - invalid header received
20210912::011941: Head 2: Comm CTD: read error - invalid header received
20210912::011941: Head 2: Comm CTD: read error - invalid header received
20210912::011941: Head 2: Comm CTD: read error - invalid header received
20210912::011941: Head 2: Comm CTD: read error - invalid header received
20210912::011942: Head 2: Comm CTD: read error - invalid header received
20210912::011942: Head 2: Comm CTD: read error - invalid header received
20210912::011942: Head 2: Comm CTD: read error - invalid header received
20210912::011943: Head 2: Comm CTD: read error - invalid header received
20210912::011943: Head 2: Comm CTD: read error - invalid header received
20210912::011943: Head 2: Comm CTD: read error - invalid header received
20210912::011944: Head 2: Comm CTD: read error - invalid header received
20210912::011944: Head 2: Comm CTD: read error - invalid header received
20210912::011944: Head 2: Comm CTD: read error - invalid header received
20210912::011945: Head 2: Comm CTD: read error - invalid header received
20210912::011945: Head 2: Comm CTD: read error - invalid header received
20210912::011945: Head 2: Comm CTD: read error - invalid header received
20210912::011945: Head 2: Comm CTD: read error - invalid header received
20210912::011946: Head 2: Comm CTD: read error - invalid header received
20210912::011946: Head 2: Comm CTD: read error - invalid header received
20210912::011946: Head 2: Comm CTD: read error - invalid header received
20210912::011947: Head 2: Comm CTD: read error - invalid header received
20210912::011947: Head 2: Comm CTD: read error - invalid header received
20210912::011947: Head 2: Comm CTD: read error - invalid header received
20210912::011948: Head 2: Comm CTD: read error - invalid header received
20210912::011948: Head 2: Comm CTD: read error - invalid header received
20210912::011948: Head 2: Comm CTD: read error - invalid header received
20210912::011949: Head 2: Comm CTD: read error - invalid header received
20210912::011949: Head 2: Comm CTD: read error - invalid header received
20210912::011949: Head 2: Comm CTD: read error - invalid header received
20210912::011949: Head 2: Comm CTD: read error - invalid header received
20210912::011950: Head 2: Comm CTD: read error - invalid header received
20210912::011950: Head 2: Comm CTD: read error - invalid header received
20210912::011950: Head 2: Comm CTD: read error - invalid header received
20210912::011951: Head 2: Comm CTD: read error - invalid header received
20210912::011951: Head 2: Comm CTD: read error - invalid header received
20210912::011951: Head 2: Comm CTD: read error - invalid header received
20210912::011952: Head 2: Comm CTD: read error - invalid header received
20210912::011952: Head 2: Comm CTD: read error - invalid header received
20210912::011952: GUI: ERROR: Received Invalid Packet ID: 0
20210912::011952: GUI: Requesing STOP operation, Head 2
20210912::011952: GUI: Error sending GUI CFG packet from sensor.
20210912::011953: GUI: Requesing STOP operation, Head 1
20210912::011953: GUI: Lost Communications with Head 2.
20210912::011953: Head 1: Received request: STOP
20210912::011953: GUI: Attempting Communications with Head 2...
20210912::011958: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::011959: GUI: ERROR: Received Invalid Packet ID: 0
20210912::011959: GUI: Lost Communications with Sensor 1.
20210912::012000: GUI: Attempting Communications with Head 1...
20210912::025058: GUI: Established Communications with Head 1.
20210912::025059: Head 1: Initializing Communications with GUI ...
20210912::025100: Head 1: Communications Established.
20210912::025100: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 0.00, Packet 3
20210912::025100: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210912::025101: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::025101: Head 1: Connection Established with the GUI.
20210912::025101: Head 1: Initializing Subsystems, standby ...
20210912::025102: Head 1: Initializing Hardware, Stand by ...
20210912::025112: GUI: Established Communications with Head 2.
20210912::025113: Head 2: Initializing Communications with GUI ...
20210912::025114: Head 2: Communications Established.
20210912::025115: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::025115: Head 2: Connection Established with the GUI.
20210912::025116: Head 2: Initializing Subsystems, standby ...
20210912::025116: Head 2: Initializing Hardware, Stand by ...
20210912::025122: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::025122: Head 1: NtQuery - testing 1 ...
20210912::025122: Head 1: clock resolution: 10
20210912::025123: Head 1: NtQuery - testing 2, after setting max res ...
20210912::025123: Head 1: clock resolution: 10
20210912::025123: Head 1: Initializing Optics Electronics ...
20210912::025124: Head 1: Power Laser Controller
20210912::025127: Head 1: Power Scanner Controller
20210912::025130: Head 1: Power OPTO Sensor
20210912::025130: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210912::025130: System NOT Initialized, Gain 0, Elec PB 34.6C, Elec PB 27.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 57
20210912::025130: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::025132: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::025132: Head 2: NtQuery - testing 1 ...
20210912::025133: Head 2: clock resolution: 10
20210912::025133: Head 2: NtQuery - testing 2, after setting max res ...
20210912::025133: Head 2: clock resolution: 10
20210912::025134: Head 2: Initializing Optics Electronics ...
20210912::025134: Head 2: Power Laser Controller
20210912::025138: Head 2: Power Scanner Controller
20210912::025140: Head 2: Power OPTO Sensor
20210912::025153: GUI: Lost Communications with Sensor 1.
20210912::025154: GUI: Lost Communications with Head 2.
20210912::025203: GUI: Attempting Communications with Head 2...
20210912::025206: GUI: OnBnClickedOk
20210912::025206: GUI: Exiting the WiSSL GUI..
20210912::025206: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210912::025206: GUI: Wrote configuration data.
20210912::025937: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210912::025937: GUI: Live mode ON.
20210912::025937: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210912::025937: GUI: WiSSL GUI started at 2021_09_12_02:59:37
20210912::025937: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_09_12.txt
20210912::025937: GUI: Attempting Communications with Head 1...
20210912::025937: GUI: Attempting Communications with Head 2...
20210912::025959: GUI: Established Communications with Head 1.
20210912::030000: Head #2, Init state OFF, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030000: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 0.00, Packet 1
20210912::030000: Head #1, Init state OFF, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030000: Head 1: Initializing Communications with GUI ...
20210912::030001: Head 1: Communications Established.
20210912::030002: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::030002: GUI: Established Communications with Head 2.
20210912::030002: Head 1: Connection Established with the GUI.
20210912::030002: Head 1: Initializing Subsystems, standby ...
20210912::030003: Head 1: Initializing Hardware, Stand by ...
20210912::030003: Head 2: Initializing Communications with GUI ...
20210912::030003: Head 2: Communications Established.
20210912::030004: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::030005: Head 2: Connection Established with the GUI.
20210912::030005: Head 2: Initializing Subsystems, standby ...
20210912::030005: Head 2: Initializing Hardware, Stand by ...
20210912::030015: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::030015: Head 1: NtQuery - testing 1 ...
20210912::030016: Head 1: clock resolution: 10
20210912::030016: Head 1: NtQuery - testing 2, after setting max res ...
20210912::030016: Head 1: clock resolution: 10
20210912::030017: Head 1: Initializing Optics Electronics ...
20210912::030017: Head 1: Power Laser Controller
20210912::030018: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::030018: Head 2: NtQuery - testing 1 ...
20210912::030018: Head 2: clock resolution: 10
20210912::030019: Head 2: NtQuery - testing 2, after setting max res ...
20210912::030019: Head 2: clock resolution: 10
20210912::030019: Head 2: Initializing Optics Electronics ...
20210912::030020: Head 2: Power Laser Controller
20210912::030021: Head 1: Power Scanner Controller
20210912::030023: Head 1: Power OPTO Sensor
20210912::030023: Head 2: Power Scanner Controller
20210912::030025: Head 2: Power OPTO Sensor
20210912::030030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030030: System NOT Initialized, Gain 0, Elec PB 36.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 54
20210912::030030: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030043: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210912::030043: Head 1: Eye Safe Optical Filter check Passed
20210912::030043: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::030044: Head 1: Initializing Time Sync Subsystem.
20210912::030044: Head 1: Initializing CTD Subsystem.
20210912::030044: Head 1: CTD Initialization Successful
20210912::030045: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::030045: Head 1: Time Sync UDP started, waiting for sync...
20210912::030045: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::030046: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::030046: Head 2: Eye Safe Optical Filter check Passed
20210912::030046: Head 1: Time Synchronization Achieved: 2021.09.12   03:00:47::0013
20210912::030046: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::030046: Head 2: Initializing Time Sync Subsystem.
20210912::030047: Head 2: Initializing CTD Subsystem.
20210912::030047: Head 2: CTD Initialization Successful
20210912::030047: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::030048: Head 2: Time Sync UDP started, waiting for sync...
20210912::030048: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::030048: Head 2: Time Synchronization Achieved: 2021.09.12   03:00:49::0014
20210912::030100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 30%, OPB 24C, Laser 23.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030100: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 108
20210912::030100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 31%, OPB 25C, Laser 24.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030121: Head 1: CTD Ethernet connection established.
20210912::030121: Head 2: CTD Ethernet connection established.
20210912::030130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 28%, OPB 24C, Laser 23.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030130: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.1dbar, CTD 0.0psu, index 1.33, Packet 161
20210912::030130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 29%, OPB 25C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 27%, OPB 24C, Laser 25.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030200: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 215
20210912::030200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 27%, OPB 25C, Laser 25.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 26%, OPB 24C, Laser 25.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030230: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 268
20210912::030230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 26%, OPB 25C, Laser 26.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030300: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 321
20210912::030300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 25%, OPB 25C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 25%, OPB 25C, Laser 26.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030330: System  Initialized, Gain 1, Elec PB 39.9C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 375
20210912::030330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 25%, OPB 26C, Laser 27.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 25%, OPB 25C, Laser 26.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030359: Head 1: Time Synchronization: 2021.09.12   03:04:00::0013
20210912::030400: System  Initialized, Gain 1, Elec PB 39.9C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 428
20210912::030400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 25C, Laser 27.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030430: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 481
20210912::030430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 26C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 24%, OPB 25C, Laser 27.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030459: Head 2: Time Synchronization: 2021.09.12   03:05:00::0014
20210912::030500: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 535
20210912::030500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 26C, Laser 28.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 25C, Laser 28.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030530: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.9C, CTD 0.2dbar, CTD 0.0psu, index 1.33, Packet 588
20210912::030530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 29.0C, Dig 40.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 25C, Laser 28.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030549: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::030550: GUI: ERROR: Received Invalid Packet ID: 0
20210912::030550: GUI: Lost Communications with Sensor 1.
20210912::030551: GUI: Attempting Communications with Head 1...
20210912::030551: GUI: Requesing STOP operation, Head 2
20210912::030551: GUI: Established Communications with Head 1.
20210912::030552: Head 2: Received request: STOP
20210912::030552: Head 1: Initializing Communications with GUI ...
20210912::030553: Head 1: Communications Established.
20210912::030554: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::030555: Head 1: Connection Established with the GUI.
20210912::030555: Head 1: Initializing Subsystems, standby ...
20210912::030555: Head 1: Initializing Hardware, Stand by ...
20210912::030556: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::030556: Head 1: NtQuery - testing 1 ...
20210912::030557: Head 1: clock resolution: 1
20210912::030557: Head 1: NtQuery - testing 2, after setting max res ...
20210912::030557: Head 1: clock resolution: 1
20210912::030557: Head 1: Initializing Optics Electronics ...
20210912::030558: Head 1: Power Laser Controller
20210912::030600: System NOT Initialized, Gain 0, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 15
20210912::030600: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 24%, OPB 25C, Laser 28.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030602: Head 1: Power Scanner Controller
20210912::030604: Head 1: Power OPTO Sensor
20210912::030622: Head 1: Eye Safe Optical Filter State there 15, not there 15, transition 1
20210912::030622: Head 1: Eye Safe Optical Filter check Passed
20210912::030623: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::030623: Head 1: Initializing Time Sync Subsystem.
20210912::030623: Head 1: Initializing CTD Subsystem.
20210912::030624: Head 1: CTD Initialization Successful
20210912::030624: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::030624: Head 1: Time Sync UDP started, waiting for sync...
20210912::030625: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::030625: Head 1: Time Synchronization Achieved: 2021.09.12   03:06:26::0014
20210912::030630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 25C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030630: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 69
20210912::030630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 0.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030700: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 122
20210912::030700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 30.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030702: Head 1: CTD Ethernet connection established.
20210912::030730: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 175
20210912::030730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 30.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030800: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 229
20210912::030800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030830: System  Initialized, Gain 1, Elec PB 41.0C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 282
20210912::030830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030900: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 335
20210912::030900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::030930: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 389
20210912::030930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031000: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 442
20210912::031000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031030: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 495
20210912::031030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 26C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031100: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 549
20210912::031100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031130: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 602
20210912::031130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031200: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 655
20210912::031200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031230: System  Initialized, Gain 1, Elec PB 43.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 709
20210912::031230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 32.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031300: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 762
20210912::031300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 31.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031330: System  Initialized, Gain 1, Elec PB 45.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 816
20210912::031330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031400: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 869
20210912::031400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031430: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 922
20210912::031430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031500: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 976
20210912::031500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031530: System  Initialized, Gain 1, Elec PB 44.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1029
20210912::031530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031600: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1083
20210912::031600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031630: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1136
20210912::031630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031700: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1189
20210912::031700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 32.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031730: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1243
20210912::031730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031800: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1296
20210912::031800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031830: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1349
20210912::031830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031900: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1403
20210912::031900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 29C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031928: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::031930: GUI: ERROR: Received Invalid Packet ID: 0
20210912::031930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 28C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031930: System  Initialized, Gain 1, Elec PB 46.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.8C, CTD 100.3dbar, CTD 1.0psu, index 1.34, Packet 1455
20210912::031930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 0, laser state 0
20210912::031930: GUI: Lost Communications with Sensor 1.
20210912::031930: GUI: Attempting Communications with Head 1...
20210912::031931: GUI: Requesing STOP operation, Head 2
20210912::031931: GUI: Established Communications with Head 1.
20210912::031931: Head 2: Received request: STOP
20210912::031932: Head 1: Initializing Communications with GUI ...
20210912::031932: Head 1: Communications Established.
20210912::031933: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::031933: Head 1: Connection Established with the GUI.
20210912::031933: Head 1: Initializing Subsystems, standby ...
20210912::031934: Head 1: Initializing Hardware, Stand by ...
20210912::031934: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210912::031935: Head 1: NtQuery - testing 1 ...
20210912::031935: Head 1: clock resolution: 10
20210912::031935: Head 1: NtQuery - testing 2, after setting max res ...
20210912::031936: Head 1: clock resolution: 10
20210912::031936: Head 1: Initializing Optics Electronics ...
20210912::031936: Head 1: Power Laser Controller
20210912::031940: Head 1: Power Scanner Controller
20210912::031942: Head 1: Power OPTO Sensor
20210912::032000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 23%, OPB 28C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032000: System NOT Initialized, Gain 0, Elec PB 47.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 52
20210912::032000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032001: Head 1: Eye Safe Optical Filter State there 16, not there 14, transition 1
20210912::032001: Head 1: Eye Safe Optical Filter check Passed
20210912::032001: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210912::032002: Head 1: Initializing Time Sync Subsystem.
20210912::032002: Head 1: Initializing CTD Subsystem.
20210912::032002: Head 1: CTD Initialization Successful
20210912::032002: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210912::032003: Head 1: Time Sync UDP started, waiting for sync...
20210912::032003: Head 1: Attempting CTD Ethernet connection with ROV...
20210912::032003: Head 1: CTD Ethernet connection established.
20210912::032004: Head 1: Time Synchronization Achieved: 2021.09.12   03:20:05::0013
20210912::032011: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::032012: GUI: ERROR: Received Invalid Packet ID: 0
20210912::032013: GUI: Lost Communications with Head 2.
20210912::032013: GUI: Attempting Communications with Head 2...
20210912::032013: GUI: Established Communications with Head 2.
20210912::032014: GUI: Requesing STOP operation, Head 1
20210912::032014: Head 1: Received request: STOP
20210912::032014: GUI: Requesing STOP operation, Head 2
20210912::032014: Head 2: Initializing Communications with GUI ...
20210912::032015: Head 2: Communications Established.
20210912::032016: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210912::032016: Head 2: Connection Established with the GUI.
20210912::032016: Head 2: Initializing Subsystems, standby ...
20210912::032017: Head 2: Initializing Hardware, Stand by ...
20210912::032017: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210912::032018: Head 2: NtQuery - testing 1 ...
20210912::032018: Head 2: clock resolution: 1
20210912::032018: Head 2: NtQuery - testing 2, after setting max res ...
20210912::032019: Head 2: clock resolution: 1
20210912::032019: Head 2: Initializing Optics Electronics ...
20210912::032019: Head 2: Power Laser Controller
20210912::032023: Head 2: Power Scanner Controller
20210912::032025: Head 2: Power OPTO Sensor
20210912::032030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 58.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032030: System  Initialized, Gain 1, Elec PB 47.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.6C, CTD 0.4dbar, CTD 0.0psu, index 1.33, Packet 106
20210912::032030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 34.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032044: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210912::032044: Head 2: Eye Safe Optical Filter check Passed
20210912::032044: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210912::032045: Head 2: Initializing Time Sync Subsystem.
20210912::032045: Head 2: Initializing CTD Subsystem.
20210912::032045: Head 2: CTD Initialization Successful
20210912::032046: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210912::032046: Head 2: Time Sync UDP started, waiting for sync...
20210912::032046: Head 2: Attempting CTD Ethernet connection with ROV...
20210912::032046: Head 2: CTD Ethernet connection established.
20210912::032047: Head 2: Time Synchronization Achieved: 2021.09.12   03:20:48::0013
20210912::032100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 35C, OCB 23%, OPB 28C, Laser 33.0C, Dig 58.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032100: System  Initialized, Gain 1, Elec PB 48.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 20.6C, CTD 0.7dbar, CTD 0.0psu, index 1.33, Packet 159
20210912::032100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 24%, OPB 29C, Laser 35.0C, Dig 53.0C, Scan Az fault 0, gain 0, laser state 0
20210912::032107: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210912::032108: GUI: ERROR: Received Invalid Packet ID: 0
20210912::032108: GUI: Lost Communications with Head 2.
20210912::032109: GUI: Attempting Communications with Head 2...
20210912::032109: GUI: Requesing STOP operation, Head 1
20210912::032109: Head 1: Received request: STOP
20210912::032115: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210912::032116: GUI: ERROR: Received Invalid Packet ID: 0
20210912::032116: GUI: Lost Communications with Sensor 1.
20210912::032117: GUI: Attempting Communications with Head 1...
20210912::035543: GUI: OnBnClickedOk
20210912::035543: GUI: Exiting the WiSSL GUI..
20210912::035543: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210912::035543: GUI: Wrote configuration data.
