20201012::182517: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20201012::182517: GUI: Live mode ON.
20201012::182517: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20201012::182517: GUI: WiSSL GUI started at 2020_10_12_18:25:17
20201012::182517: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2020_10_12.txt
20201012::182517: GUI: Attempting Communications with Head 1...
20201012::182517: GUI: Attempting Communications with Head 2...
20201012::182521: GUI: Established Communications with Head 2.
20201012::182521: GUI: Established Communications with Head 1.
20201012::182522: Head 1: Initializing Communications with GUI ...
20201012::182522: Head 2: Initializing Communications with GUI ...
20201012::182522: Head 1: Communications Established.
20201012::182523: Head 2: Communications Established.
20201012::182523: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::182524: Head 1: Connection Established with the GUI.
20201012::182524: Head 1: Initializing Subsystems, standby ...
20201012::182524: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::182524: Head 1: Initializing Hardware, Stand by ...
20201012::182524: Head 2: Connection Established with the GUI.
20201012::182525: Head 2: Initializing Subsystems, standby ...
20201012::182525: Head 2: Initializing Hardware, Stand by ...
20201012::182530: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182530: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 17
20201012::182530: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182543: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::182543: Head 1: NtQuery - testing 1 ...
20201012::182544: Head 1: clock resolution: 10
20201012::182544: Head 1: NtQuery - testing 2, after setting max res ...
20201012::182544: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::182544: Head 1: clock resolution: 10
20201012::182545: Head 2: NtQuery - testing 1 ...
20201012::182545: Head 1: Initializing Optics Electronics ...
20201012::182545: Head 2: clock resolution: 10
20201012::182545: Head 1: Power Laser Controller
20201012::182545: Head 2: NtQuery - testing 2, after setting max res ...
20201012::182545: Head 2: clock resolution: 10
20201012::182546: Head 2: Initializing Optics Electronics ...
20201012::182546: Head 2: Power Laser Controller
20201012::182549: Head 1: Power Scanner Controller
20201012::182550: Head 2: Power Scanner Controller
20201012::182551: Head 1: Power OPTO Sensor
20201012::182552: Head 2: Power OPTO Sensor
20201012::182600: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 71
20201012::182600: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182600: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182611: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::182611: Head 1: Eye Safe Optical Filter check Passed
20201012::182612: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201012::182612: Head 1: Initializing Time Sync Subsystem.
20201012::182612: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::182612: Head 1: Initializing CTD Subsystem.
20201012::182612: Head 2: Eye Safe Optical Filter check Passed
20201012::182612: Head 1: CTD Initialization Successful
20201012::182613: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201012::182613: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201012::182613: Head 2: Initializing Time Sync Subsystem.
20201012::182613: Head 1: Time Sync UDP started, waiting for sync...
20201012::182613: Head 2: Initializing CTD Subsystem.
20201012::182613: Head 1: Attempting CTD Ethernet connection with ROV...
20201012::182613: Head 2: CTD Initialization Successful
20201012::182614: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201012::182614: Head 1: Time Synchronization Achieved: 2020.10.12   18:26:15::0013
20201012::182614: Head 2: Time Sync UDP started, waiting for sync...
20201012::182614: Head 2: Attempting CTD Ethernet connection with ROV...
20201012::182615: Head 2: Time Synchronization Achieved: 2020.10.12   18:26:16::0015
20201012::182629: Head 2: CTD Ethernet connection established.
20201012::182629: Head 1: CTD Ethernet connection established.
20201012::182630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 19C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182630: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD -107374176.0C, CTD 2.0dbar, CTD -1.$psu, index 1.#J, Packet 127
20201012::182630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 20C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 19C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182700: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD -107374176.0C, CTD 2.0dbar, CTD -1.$psu, index 1.#J, Packet 182
20201012::182700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 26%, OPB 20C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182730: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.9C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 237
20201012::182730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 20C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201012::182806: GUI: Lost Communications with Sensor 1.
20201012::182806: GUI: Lost Communications with Head 2.
20201012::182813: GUI: Attempting Communications with Head 2...
20201012::182813: GUI: Attempting Communications with Head 1...
20201012::193329: GUI: Established Communications with Head 1.
20201012::193329: GUI: Established Communications with Head 2.
20201012::193330: Head #2, Init state OFF, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193330: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 0.00, Packet 1
20201012::193330: Head #1, Init state OFF, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193330: Head 1: Initializing Communications with GUI ...
20201012::193330: Head 2: Initializing Communications with GUI ...
20201012::193330: Head 1: Communications Established.
20201012::193331: Head 2: Communications Established.
20201012::193332: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::193332: Head 1: Connection Established with the GUI.
20201012::193332: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::193332: Head 1: Initializing Subsystems, standby ...
20201012::193332: Head 2: Connection Established with the GUI.
20201012::193333: Head 1: Initializing Hardware, Stand by ...
20201012::193333: Head 2: Initializing Subsystems, standby ...
20201012::193333: Head 2: Initializing Hardware, Stand by ...
20201012::193345: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::193345: Head 1: NtQuery - testing 1 ...
20201012::193345: Head 1: clock resolution: 10
20201012::193345: Head 1: NtQuery - testing 2, after setting max res ...
20201012::193346: Head 1: clock resolution: 10
20201012::193346: Head 1: Initializing Optics Electronics ...
20201012::193346: Head 1: Power Laser Controller
20201012::193350: Head 1: Power Scanner Controller
20201012::193351: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::193352: Head 2: NtQuery - testing 1 ...
20201012::193352: Head 2: clock resolution: 10
20201012::193352: Head 2: NtQuery - testing 2, after setting max res ...
20201012::193352: Head 1: Power OPTO Sensor
20201012::193352: Head 2: clock resolution: 10
20201012::193353: Head 2: Initializing Optics Electronics ...
20201012::193353: Head 2: Power Laser Controller
20201012::193357: Head 2: Power Scanner Controller
20201012::193359: Head 2: Power OPTO Sensor
20201012::193400: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193400: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 56
20201012::193400: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193412: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::193413: Head 1: Eye Safe Optical Filter check Passed
20201012::193413: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201012::193413: Head 1: Initializing Time Sync Subsystem.
20201012::193413: Head 1: Initializing CTD Subsystem.
20201012::193414: Head 1: CTD Initialization Successful
20201012::193414: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201012::193414: Head 1: Time Sync UDP started, waiting for sync...
20201012::193415: Head 1: Attempting CTD Ethernet connection with ROV...
20201012::193415: Head 1: Time Synchronization Achieved: 2020.10.12   19:34:16::0015
20201012::193419: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::193419: Head 2: Eye Safe Optical Filter check Passed
20201012::193420: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201012::193420: Head 2: Initializing Time Sync Subsystem.
20201012::193420: Head 2: Initializing CTD Subsystem.
20201012::193420: Head 2: CTD Initialization Successful
20201012::193421: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201012::193421: Head 2: Time Sync UDP started, waiting for sync...
20201012::193421: Head 2: Attempting CTD Ethernet connection with ROV...
20201012::193422: Head 2: Time Synchronization Achieved: 2020.10.12   19:34:23::0014
20201012::193430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 20C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193430: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 111
20201012::193430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 28%, OPB 20C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193433: Head 2: CTD Ethernet connection established.
20201012::193433: Head 1: CTD Ethernet connection established.
20201012::193500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 26%, OPB 20C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193500: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.8C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 166
20201012::193500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 26%, OPB 21C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193512: Head 2: Setting Gain 1
20201012::193512: Head 1: Setting Gain 1
20201012::193530: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.8C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 221
20201012::193530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 20C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 21C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193530: GUI: Live mode ON.
20201012::193530: GUI: Requesing START operation, Head 2
20201012::193530: GUI: Requesing START operation, Head 1
20201012::193531: Head 2: Received request: START
20201012::193531: Head 1: Received request: START
20201012::193531: Head 2: Starting Scan Operation
20201012::193531: Head 1: Starting Scan Operation
20201012::193532: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::193533: Head 2: Eye Safe Optical Filter check Passed
20201012::193535: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20201012::193536: Head 1: Eye Safe Optical Filter check Passed
20201012::193537: Head 2: Configured for WATER Processing
20201012::193537: Head 2: Configured for WATER Processing
20201012::193537: Head 2: Configured for WATER Processing
20201012::193538: Head 2: Configured for WATER Processing
20201012::193538: Head 2: Configured for WATER Processing
20201012::193538: Head 2: Configured for WATER Processing
20201012::193539: Head 2: Configured for WATER Processing
20201012::193539: Head 2: Configured for WATER Processing
20201012::193539: Head 2: Configured for WATER Processing
20201012::193540: Head 2: Configured for WATER Processing
20201012::193540: Head 2: Configured for WATER Processing
20201012::193540: Head 2: Configured for WATER Processing
20201012::193540: Head 1: Configured for WATER Processing
20201012::193540: Head 2: Configured for WATER Processing
20201012::193541: Head 1: Configured for WATER Processing
20201012::193541: Head 2: Configured for WATER Processing
20201012::193541: Head 1: Configured for WATER Processing
20201012::193541: Head 2: Configured for WATER Processing
20201012::193541: Head 1: Configured for WATER Processing
20201012::193541: Head 2: Configured for WATER Processing
20201012::193541: Head 1: Configured for WATER Processing
20201012::193542: Head 2: Configured for WATER Processing
20201012::193542: Head 1: Configured for WATER Processing
20201012::193542: Head 2: Configured for WATER Processing
20201012::193542: Head 1: Configured for WATER Processing
20201012::193542: Head 2: Configured for WATER Processing
20201012::193542: Head 1: Configured for WATER Processing
20201012::193543: Head 2: Configured for WATER Processing
20201012::193543: Head 1: Configured for WATER Processing
20201012::193543: Head 1: Configured for WATER Processing
20201012::193543: Head 1: Configured for WATER Processing
20201012::193544: Head 1: Configured for WATER Processing
20201012::193544: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201012_193542_1.raa
20201012::193544: Head 1: Configured for WATER Processing
20201012::193544: Head 1: Configured for WATER Processing
20201012::193544: Head 1: Configured for WATER Processing
20201012::193545: Head 1: Configured for WATER Processing
20201012::193545: Head 1: Configured for WATER Processing
20201012::193545: Head 1: Configured for WATER Processing
20201012::193546: Head 1: Configured for WATER Processing
20201012::193546: Head 1: Configured for WATER Processing
20201012::193551: GUI: Live mode ON.
20201012::193551: GUI: Requesing STOP operation, Head 1
20201012::193551: GUI: Requesing STOP operation, Head 2
20201012::193551: Head 2: Received request: STOP
20201012::193551: Head 1: Received request: STOP
20201012::193552: Head 2: Stopping Scan Operation
20201012::193552: Head 1: Stopping Scan Operation
20201012::193554: Head 2: ProcessingMgr stopped all worker threads.
20201012::193554: Head 1: ProcessingMgr stopped all worker threads.
20201012::193554: Head 2:       Stop finished, may now recover.
20201012::193554: Head 1:       Stop finished, may now recover.
20201012::193557: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::193557: Head 2: Eye Safe Optical Filter check Passed
20201012::193559: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20201012::193600: Head 1: Eye Safe Optical Filter check Passed
20201012::193600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 20C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193600: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.8C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 276
20201012::193600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 21C, Laser 22.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193630: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.9C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 331
20201012::193630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 22.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193700: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.9C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 385
20201012::193700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 22C, Laser 23.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193730: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.9C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 441
20201012::193730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 23.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193800: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.9C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 496
20201012::193800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 24.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193830: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 551
20201012::193830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 25.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193900: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 606
20201012::193900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 25.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::193930: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 661
20201012::193930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 25.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194000: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 715
20201012::194000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 25.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194030: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 770
20201012::194030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 26.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194100: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 826
20201012::194100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 26.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 22C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194130: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.1C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 881
20201012::194130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 26.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 22C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194200: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 935
20201012::194200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 27.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194230: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 990
20201012::194230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 23C, Laser 27.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 22C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194300: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 19.0C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 1045
20201012::194300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 23C, Laser 27.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 22C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 23C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194330: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 18.4C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 1100
20201012::194330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 23C, Laser 28.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 23C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194400: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 14.2C, CTD 4.8dbar, CTD 0.1psu, index 1.34, Packet 1155
20201012::194400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 24C, Laser 28.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20201012::194421: GUI: Lost Communications with Head 2.
20201012::194421: GUI: Lost Communications with Sensor 1.
20201012::194428: GUI: Attempting Communications with Head 1...
20201012::194438: GUI: Attempting Communications with Head 2...
20201012::201623: GUI: Established Communications with Head 1.
20201012::201624: Head 1: Initializing Communications with GUI ...
20201012::201625: Head 1: Communications Established.
20201012::201626: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::201627: Head 1: Connection Established with the GUI.
20201012::201627: Head 1: Initializing Subsystems, standby ...
20201012::201627: Head 1: Initializing Hardware, Stand by ...
20201012::201630: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 12
20201012::201630: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201634: GUI: Established Communications with Head 2.
20201012::201634: Head 2: Initializing Communications with GUI ...
20201012::201635: Head 2: Communications Established.
20201012::201636: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::201637: Head 2: Connection Established with the GUI.
20201012::201637: Head 2: Initializing Subsystems, standby ...
20201012::201637: Head 2: Initializing Hardware, Stand by ...
20201012::201641: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::201641: Head 1: NtQuery - testing 1 ...
20201012::201642: Head 1: clock resolution: 10
20201012::201642: Head 1: NtQuery - testing 2, after setting max res ...
20201012::201642: Head 1: clock resolution: 10
20201012::201643: Head 1: Initializing Optics Electronics ...
20201012::201643: Head 1: Power Laser Controller
20201012::201647: Head 1: Power Scanner Controller
20201012::201649: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::201649: Head 1: Power OPTO Sensor
20201012::201649: Head 2: NtQuery - testing 1 ...
20201012::201649: Head 2: clock resolution: 10
20201012::201650: Head 2: NtQuery - testing 2, after setting max res ...
20201012::201650: Head 2: clock resolution: 10
20201012::201650: Head 2: Initializing Optics Electronics ...
20201012::201651: Head 2: Power Laser Controller
20201012::201654: Head 2: Power Scanner Controller
20201012::201656: Head 2: Power OPTO Sensor
20201012::201700: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201700: System NOT Initialized, Gain 0, Elec PB 22.6C, Elec PB 28.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 67
20201012::201700: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201709: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::201709: Head 1: Eye Safe Optical Filter check Passed
20201012::201710: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201012::201710: Head 1: Initializing Time Sync Subsystem.
20201012::201710: Head 1: Initializing CTD Subsystem.
20201012::201710: Head 1: CTD Initialization Successful
20201012::201711: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201012::201711: Head 1: Time Sync UDP started, waiting for sync...
20201012::201711: Head 1: Attempting CTD Ethernet connection with ROV...
20201012::201712: Head 1: Time Synchronization Achieved: 2020.10.12   20:17:13::0013
20201012::201717: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::201717: Head 2: Eye Safe Optical Filter check Passed
20201012::201717: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201012::201717: Head 2: Initializing Time Sync Subsystem.
20201012::201718: Head 2: Initializing CTD Subsystem.
20201012::201718: Head 2: CTD Initialization Successful
20201012::201718: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201012::201719: Head 2: Time Sync UDP started, waiting for sync...
20201012::201719: Head 2: Attempting CTD Ethernet connection with ROV...
20201012::201720: Head 2: Time Synchronization Achieved: 2020.10.12   20:17:21::0014
20201012::201730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 29%, OPB 17C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201730: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 28.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 122
20201012::201730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 29%, OPB 18C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 27%, OPB 18C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201800: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 177
20201012::201800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 27%, OPB 19C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201830: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 231
20201012::201830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 19C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 18C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 286
20201012::201900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 19C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 18C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::201930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 342
20201012::201930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 397
20201012::202000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 451
20201012::202030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 507
20201012::202100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 562
20201012::202130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 616
20201012::202200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201012::202222: GUI: Lost Communications with Sensor 1.
20201012::202222: GUI: Lost Communications with Head 2.
20201012::202228: GUI: Attempting Communications with Head 1...
20201012::202228: GUI: Attempting Communications with Head 2...
20201012::210905: GUI: Established Communications with Head 1.
20201012::210905: GUI: Established Communications with Head 2.
20201012::210906: Head 1: Initializing Communications with GUI ...
20201012::210906: Head 2: Initializing Communications with GUI ...
20201012::210907: Head 2: Communications Established.
20201012::210907: Head 1: Communications Established.
20201012::210908: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::210908: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::210908: Head 2: Connection Established with the GUI.
20201012::210908: Head 1: Connection Established with the GUI.
20201012::210909: Head 2: Initializing Subsystems, standby ...
20201012::210909: Head 1: Initializing Subsystems, standby ...
20201012::210909: Head 2: Initializing Hardware, Stand by ...
20201012::210909: Head 1: Initializing Hardware, Stand by ...
20201012::210923: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::210924: Head 1: NtQuery - testing 1 ...
20201012::210924: Head 1: clock resolution: 10
20201012::210924: Head 1: NtQuery - testing 2, after setting max res ...
20201012::210925: Head 1: clock resolution: 10
20201012::210925: Head 1: Initializing Optics Electronics ...
20201012::210925: Head 1: Power Laser Controller
20201012::210929: Head 1: Power Scanner Controller
20201012::210930: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::210930: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::210930: System NOT Initialized, Gain 0, Elec PB 23.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 45
20201012::210930: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::210930: Head 2: NtQuery - testing 1 ...
20201012::210930: Head 2: clock resolution: 10
20201012::210930: Head 2: NtQuery - testing 2, after setting max res ...
20201012::210931: Head 2: clock resolution: 10
20201012::210931: Head 1: Power OPTO Sensor
20201012::210931: Head 2: Initializing Optics Electronics ...
20201012::210931: Head 2: Power Laser Controller
20201012::210935: Head 2: Power Scanner Controller
20201012::210937: Head 2: Power OPTO Sensor
20201012::210951: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::210951: Head 1: Eye Safe Optical Filter check Passed
20201012::210952: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201012::210952: Head 1: Initializing Time Sync Subsystem.
20201012::210952: Head 1: Initializing CTD Subsystem.
20201012::210953: Head 1: CTD Initialization Successful
20201012::210953: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201012::210953: Head 1: Time Sync UDP started, waiting for sync...
20201012::210954: Head 1: Attempting CTD Ethernet connection with ROV...
20201012::210954: Head 1: Time Synchronization Achieved: 2020.10.12   21:09:55::0015
20201012::210957: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::210958: Head 2: Eye Safe Optical Filter check Passed
20201012::210958: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201012::210958: Head 2: Initializing Time Sync Subsystem.
20201012::210959: Head 2: Initializing CTD Subsystem.
20201012::210959: Head 2: CTD Initialization Successful
20201012::210959: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201012::210959: Head 2: Time Sync UDP started, waiting for sync...
20201012::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 30%, OPB 17C, Laser 0.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211000: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 99
20201012::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 30%, OPB 18C, Laser 0.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211000: Head 2: Attempting CTD Ethernet connection with ROV...
20201012::211000: Head 2: Time Synchronization Achieved: 2020.10.12   21:10:01::0014
20201012::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 28%, OPB 18C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211030: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 155
20201012::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 28%, OPB 19C, Laser 18.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211100: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 209
20201012::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 26%, OPB 18C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 26%, OPB 19C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 18C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211130: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 264
20201012::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 19C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 319
20201012::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 18C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 374
20201012::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 21.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 429
20201012::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 21.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 484
20201012::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201012::211340: GUI: Lost Communications with Head 2.
20201012::211340: GUI: Lost Communications with Sensor 1.
20201012::211349: GUI: Attempting Communications with Head 1...
20201012::211349: GUI: Attempting Communications with Head 2...
20201012::233937: GUI: Established Communications with Head 1.
20201012::233938: Head 1: Initializing Communications with GUI ...
20201012::233938: Head 1: Communications Established.
20201012::233939: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::233940: Head 1: Connection Established with the GUI.
20201012::233940: Head 1: Initializing Subsystems, standby ...
20201012::233940: GUI: Established Communications with Head 2.
20201012::233940: Head 1: Initializing Hardware, Stand by ...
20201012::233941: Head 2: Initializing Communications with GUI ...
20201012::233941: Head 2: Communications Established.
20201012::233942: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201012::233943: Head 2: Connection Established with the GUI.
20201012::233943: Head 2: Initializing Subsystems, standby ...
20201012::233943: Head 2: Initializing Hardware, Stand by ...
20201012::233951: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20201012::233951: GUI: Live mode ON.
20201012::233951: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20201012::233951: GUI: WiSSL GUI started at 2020_10_12_23:39:51
20201012::233951: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2020_10_12.txt
20201012::233951: GUI: Attempting Communications with Head 1...
20201012::233951: GUI: Attempting Communications with Head 2...
20201012::233952: GUI: Established Communications with Head 1.
20201012::233952: GUI: Established Communications with Head 2.
20201012::233954: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::233955: Head 1: NtQuery - testing 1 ...
20201012::233955: Head 1: clock resolution: 10
20201012::233955: Head 1: NtQuery - testing 2, after setting max res ...
20201012::233956: Head 1: clock resolution: 10
20201012::233956: Head 1: Initializing Optics Electronics ...
20201012::233956: Head 1: Power Laser Controller
20201012::234000: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 41
20201012::234000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234000: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234000: Head 1: Power Scanner Controller
20201012::234001: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201012::234001: Head 2: NtQuery - testing 1 ...
20201012::234001: Head 2: clock resolution: 10
20201012::234002: Head 2: NtQuery - testing 2, after setting max res ...
20201012::234002: Head 1: Power OPTO Sensor
20201012::234002: Head 2: clock resolution: 10
20201012::234002: GUI: Lost Communications with Sensor 1.
20201012::234002: GUI: Lost Communications with Head 2.
20201012::234002: Head 2: Initializing Optics Electronics ...
20201012::234003: Head 2: Power Laser Controller
20201012::234006: Head 2: Power Scanner Controller
20201012::234009: Head 2: Power OPTO Sensor
20201012::234012: GUI: Attempting Communications with Head 2...
20201012::234012: GUI: Attempting Communications with Head 1...
20201012::234022: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201012::234022: Head 1: Eye Safe Optical Filter check Passed
20201012::234023: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201012::234023: Head 1: Initializing Time Sync Subsystem.
20201012::234023: Head 1: Initializing CTD Subsystem.
20201012::234024: Head 1: CTD Initialization Successful
20201012::234024: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201012::234024: Head 1: Time Sync UDP started, waiting for sync...
20201012::234024: Head 1: Attempting CTD Ethernet connection with ROV...
20201012::234025: Head 1: Time Synchronization Achieved: 2020.10.12   23:40:26::0015
20201012::234029: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201012::234029: Head 2: Eye Safe Optical Filter check Passed
20201012::234029: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201012::234030: Head 2: Initializing Time Sync Subsystem.
20201012::234030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 29%, OPB 16C, Laser 0.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234030: Head 2: Initializing CTD Subsystem.
20201012::234030: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 97
20201012::234030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 30%, OPB 17C, Laser 0.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234030: Head 2: CTD Initialization Successful
20201012::234030: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201012::234031: Head 2: Time Sync UDP started, waiting for sync...
20201012::234031: Head 2: Attempting CTD Ethernet connection with ROV...
20201012::234032: Head 2: Time Synchronization Achieved: 2020.10.12   23:40:33::0013
20201012::234100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 27%, OPB 17C, Laser 16.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 152
20201012::234100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 27%, OPB 17C, Laser 17.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 17C, Laser 16.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 207
20201012::234130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 18C, Laser 18.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234155: Head 2: CTD Ethernet connection established.
20201012::234155: Head 1: CTD Ethernet connection established.
20201012::234200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 17C, Laser 17.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 262
20201012::234200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 18C, Laser 19.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234205: GUI: OnBnClickedOk
20201012::234205: GUI: Exiting the WiSSL GUI..
20201012::234205: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20201012::234205: GUI: Wrote configuration data.
20201012::234230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 18.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.2C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 317
20201012::234230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 18C, Laser 19.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 17C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234300: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.3C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 372
20201012::234300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 18C, Laser 20.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201012::234313: Head 1: Comm CTD Error, disconnecting
20201012::234313: Head 2: Comm CTD Error, disconnecting
20201012::234313: Head 1: Restarting CTD Ethernet connection ...
20201012::234313: Head 2: Restarting CTD Ethernet connection ...
20201012::234334: GUI: Lost Communications with Sensor 1.
20201012::234335: GUI: Lost Communications with Head 2.
20201012::234350: GUI: Attempting Communications with Head 1...
20201012::234353: GUI: Attempting Communications with Head 2...
