20210430::161933: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210430::161933: GUI: Live mode ON.
20210430::161933: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210430::161933: GUI: WiSSL GUI started at 2021_04_30_16:19:33
20210430::161933: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_30.txt
20210430::161933: GUI: Attempting Communications with Head 1...
20210430::161933: GUI: Attempting Communications with Head 2...
20210430::161936: GUI: Established Communications with Head 2.
20210430::161936: GUI: Established Communications with Head 1.
20210430::161937: Head 1: Initializing Communications with GUI ...
20210430::161937: Head 2: Initializing Communications with GUI ...
20210430::161938: Head 2: Communications Established.
20210430::161938: Head 1: Communications Established.
20210430::161939: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210430::161939: Head 2: Connection Established with the GUI.
20210430::161940: Head 2: Initializing Subsystems, standby ...
20210430::161940: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210430::161940: Head 2: Initializing Hardware, Stand by ...
20210430::161940: Head 1: Connection Established with the GUI.
20210430::161940: Head 1: Initializing Subsystems, standby ...
20210430::161941: Head 1: Initializing Hardware, Stand by ...
20210430::161949: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210430::161950: Head 2: NtQuery - testing 1 ...
20210430::161950: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210430::161950: Head 2: clock resolution: 10
20210430::161950: Head 1: NtQuery - testing 1 ...
20210430::161950: Head 2: NtQuery - testing 2, after setting max res ...
20210430::161951: Head 1: clock resolution: 10
20210430::161951: Head 2: clock resolution: 10
20210430::161951: Head 1: NtQuery - testing 2, after setting max res ...
20210430::161951: Head 2: Initializing Optics Electronics ...
20210430::161951: Head 1: clock resolution: 10
20210430::161951: Head 2: Power Laser Controller
20210430::161951: Head 1: Initializing Optics Electronics ...
20210430::161952: Head 1: Power Laser Controller
20210430::161955: Head 2: Power Scanner Controller
20210430::161956: Head 1: Power Scanner Controller
20210430::161957: Head 2: Power OPTO Sensor
20210430::161958: Head 1: Power OPTO Sensor
20210430::162000: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162000: System NOT Initialized, Gain 0, Elec PB 17.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 42
20210430::162000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162017: Head 2: Eye Safe Optical Filter State there 4, not there 26, transition 1
20210430::162018: Head 2: Eye Safe Optical Filter check Passed
20210430::162018: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::162018: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210430::162018: Head 1: Eye Safe Optical Filter check Passed
20210430::162018: Head 2: Initializing Time Sync Subsystem.
20210430::162018: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210430::162019: Head 2: Initializing CTD Subsystem.
20210430::162019: Head 1: Initializing Time Sync Subsystem.
20210430::162019: Head 2: CTD Initialization Successful
20210430::162019: Head 1: Initializing CTD Subsystem.
20210430::162019: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210430::162019: Head 1: CTD Initialization Successful
20210430::162019: Head 2: Time Sync UDP started, waiting for sync...
20210430::162020: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210430::162020: Head 2: Attempting CTD Ethernet connection with ROV...
20210430::162020: Head 1: Time Sync UDP started, waiting for sync...
20210430::162020: Head 1: Attempting CTD Ethernet connection with ROV...
20210430::162020: Head 2: Time Synchronization Achieved: 2021.04.30   16:20:21::0015
20210430::162021: Head 1: Time Synchronization Achieved: 2021.04.30   16:20:22::0019
20210430::162028: Head 2: CTD Ethernet connection established.
20210430::162028: Head 1: CTD Ethernet connection established.
20210430::162030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 14C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162030: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 95
20210430::162030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 27%, OPB 14C, Laser 14.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162100: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 148
20210430::162100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 15C, Laser 14.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 14C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162130: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 202
20210430::162130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 15C, Laser 15.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162200: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 255
20210430::162200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 15C, Laser 16.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 15.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162230: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 308
20210430::162230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 15C, Laser 16.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 15C, Laser 15.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 362
20210430::162300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 16C, Laser 17.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 15C, Laser 16.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 15C, Laser 17.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 416
20210430::162330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 16C, Laser 17.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 15C, Laser 17.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162400: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 469
20210430::162400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 16C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162430: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 522
20210430::162430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 16C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 15C, Laser 17.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 15C, Laser 17.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162500: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 576
20210430::162500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 15C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162530: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 630
20210430::162530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162600: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 683
20210430::162600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 15C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162630: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.6dbar, CTD 0.0psu, index 1.34, Packet 736
20210430::162630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 16C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162700: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 790
20210430::162700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 16C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162730: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.3dbar, CTD 0.0psu, index 1.34, Packet 843
20210430::162730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 16C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162800: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.2dbar, CTD 0.0psu, index 1.34, Packet 896
20210430::162800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 20%, OPB 16C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162830: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 950
20210430::162830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162900: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 1003
20210430::162900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162930: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.7dbar, CTD 0.0psu, index 1.34, Packet 1057
20210430::162930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::162930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163000: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 1110
20210430::163000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163030: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1164
20210430::163030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163100: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 1217
20210430::163100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 18C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163130: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 1270
20210430::163130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163200: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 1324
20210430::163200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163230: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.4dbar, CTD 0.0psu, index 1.34, Packet 1377
20210430::163230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1430
20210430::163300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1484
20210430::163330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163352: GUI: Live mode ON.
20210430::163352: GUI: Requesing START operation, Head 1
20210430::163352: GUI: Requesing START operation, Head 2
20210430::163352: Head 1: Received request: START
20210430::163352: Head 2: Received request: START
20210430::163352: Head 1: Starting Scan Operation
20210430::163352: Head 2: Starting Scan Operation
20210430::163354: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20210430::163354: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::163354: Head 1: Eye Safe Optical Filter check Passed
20210430::163354: Head 2: Eye Safe Optical Filter check Passed
20210430::163400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1537
20210430::163400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210430::163400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 1
20210430::163430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1591
20210430::163430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 1
20210430::163430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 1
20210430::163430: Head 1: Configured for WATER Processing
20210430::163431: Head 1: Configured for WATER Processing
20210430::163431: Head 1: Configured for WATER Processing
20210430::163431: Head 1: Configured for WATER Processing
20210430::163432: Head 1: Configured for WATER Processing
20210430::163432: Head 1: Configured for WATER Processing
20210430::163432: Head 1: Configured for WATER Processing
20210430::163433: Head 2: Configured for WATER Processing
20210430::163433: Head 1: Configured for WATER Processing
20210430::163433: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_163431_20210428d1_docr_lidar.raa
20210430::163433: Head 2: Configured for WATER Processing
20210430::163433: Head 1: Configured for WATER Processing
20210430::163433: Head 2: Configured for WATER Processing
20210430::163433: Head 1: Configured for WATER Processing
20210430::163433: Head 2: Configured for WATER Processing
20210430::163433: Head 1: Configured for WATER Processing
20210430::163434: Head 2: Configured for WATER Processing
20210430::163434: Head 1: Configured for WATER Processing
20210430::163434: Head 2: Configured for WATER Processing
20210430::163434: Head 1: Configured for WATER Processing
20210430::163434: Head 2: Configured for WATER Processing
20210430::163434: Head 1: Configured for WATER Processing
20210430::163435: Head 2: Configured for WATER Processing
20210430::163435: Head 1: Configured for WATER Processing
20210430::163435: Head 2: Configured for WATER Processing
20210430::163435: Head 1: Configured for WATER Processing
20210430::163435: Head 2: Configured for WATER Processing
20210430::163435: Head 1: Configured for WATER Processing
20210430::163436: Head 2: Configured for WATER Processing
20210430::163436: Head 1: Configured for WATER Processing
20210430::163436: Head 2: Configured for WATER Processing
20210430::163436: Head 1: Configured for WATER Processing
20210430::163436: Head 2: Configured for WATER Processing
20210430::163436: Head 1: Configured for WATER Processing
20210430::163436: Head 2: Configured for WATER Processing
20210430::163437: Head 2: Configured for WATER Processing
20210430::163437: Head 2: Configured for WATER Processing
20210430::163437: Head 2: Configured for WATER Processing
20210430::163438: Head 2: Configured for WATER Processing
20210430::163438: Head 2: Configured for WATER Processing
20210430::163438: Head 2: Configured for WATER Processing
20210430::163440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_163441_20210428d1_docr_lidar.raa
20210430::163442: GUI: Live mode ON.
20210430::163442: GUI: Requesing STOP operation, Head 2
20210430::163442: GUI: Requesing STOP operation, Head 1
20210430::163442: Head 2: Received request: STOP
20210430::163442: Head 1: Received request: STOP
20210430::163442: Head 2: Stopping Scan Operation
20210430::163442: Head 1: Stopping Scan Operation
20210430::163448: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20210430::163448: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::163448: Head 1: Eye Safe Optical Filter check Passed
20210430::163448: Head 2: Eye Safe Optical Filter check Passed
20210430::163500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1644
20210430::163500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163506: Head 2: ProcessingMgr stopped all worker threads.
20210430::163507: Head 2:       Stop finished, may now recover.
20210430::163519: Head 1: ProcessingMgr stopped all worker threads.
20210430::163519: Head 1:       Stop finished, may now recover.
20210430::163530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1698
20210430::163530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 1751
20210430::163600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 1805
20210430::163630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1858
20210430::163700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1911
20210430::163730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163759: Head 1: Time Synchronization: 2021.04.30   16:38:00::0012
20210430::163800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 1965
20210430::163800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.1C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2018
20210430::163830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2071
20210430::163900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::163930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2125
20210430::163930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2178
20210430::164000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2231
20210430::164030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2285
20210430::164100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2338
20210430::164130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2392
20210430::164200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2445
20210430::164230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2498
20210430::164300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.2C, CTD 2.1dbar, CTD 0.0psu, index 1.34, Packet 2552
20210430::164330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.9C, CTD 3.4dbar, CTD 0.0psu, index 1.34, Packet 2605
20210430::164400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.1C, CTD 4.6dbar, CTD 0.0psu, index 1.34, Packet 2658
20210430::164430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.9C, CTD 4.2dbar, CTD 0.1psu, index 1.34, Packet 2712
20210430::164500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.9C, CTD 11.9dbar, CTD 16.4psu, index 1.34, Packet 2765
20210430::164530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.8C, CTD 12.7dbar, CTD 18.4psu, index 1.34, Packet 2818
20210430::164600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.8C, CTD 18.2dbar, CTD 34.2psu, index 1.34, Packet 2872
20210430::164630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 17.6dbar, CTD 34.1psu, index 1.34, Packet 2925
20210430::164700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 20.8dbar, CTD 34.1psu, index 1.34, Packet 2978
20210430::164730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 18C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 18C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 25.1dbar, CTD 34.0psu, index 1.34, Packet 3032
20210430::164800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 29.2dbar, CTD 33.8psu, index 1.34, Packet 3085
20210430::164830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.7C, CTD 35.7dbar, CTD 33.7psu, index 1.34, Packet 3139
20210430::164900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 35.1dbar, CTD 33.7psu, index 1.34, Packet 3192
20210430::164930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::164959: Head 1: Time Synchronization: 2021.04.30   16:50:00::0015
20210430::165000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 38.1dbar, CTD 33.7psu, index 1.34, Packet 3245
20210430::165000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 27.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.4C, CTD 45.4dbar, CTD 33.6psu, index 1.34, Packet 3299
20210430::165030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 60.4dbar, CTD 33.7psu, index 1.34, Packet 3352
20210430::165100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.4C, CTD 70.3dbar, CTD 33.8psu, index 1.34, Packet 3405
20210430::165130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 79.2dbar, CTD 33.9psu, index 1.34, Packet 3459
20210430::165200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 92.6dbar, CTD 33.9psu, index 1.34, Packet 3512
20210430::165230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.2C, CTD 100.5dbar, CTD 33.9psu, index 1.34, Packet 3565
20210430::165300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.2C, CTD 99.9dbar, CTD 33.9psu, index 1.34, Packet 3619
20210430::165330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 108.9dbar, CTD 33.9psu, index 1.34, Packet 3672
20210430::165400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.0C, CTD 118.6dbar, CTD 34.0psu, index 1.34, Packet 3725
20210430::165430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.0C, CTD 129.9dbar, CTD 34.0psu, index 1.34, Packet 3779
20210430::165500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.9C, CTD 139.6dbar, CTD 34.0psu, index 1.34, Packet 3832
20210430::165530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 17C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.9C, CTD 147.7dbar, CTD 34.0psu, index 1.34, Packet 3885
20210430::165600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 26.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 25.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.9C, CTD 150.6dbar, CTD 34.0psu, index 1.34, Packet 3939
20210430::165630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 155.8dbar, CTD 34.0psu, index 1.34, Packet 3992
20210430::165700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.7C, CTD 168.3dbar, CTD 34.0psu, index 1.34, Packet 4045
20210430::165730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.6C, CTD 181.0dbar, CTD 34.0psu, index 1.34, Packet 4099
20210430::165800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.5C, CTD 193.1dbar, CTD 34.0psu, index 1.34, Packet 4152
20210430::165830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.3C, CTD 204.8dbar, CTD 34.1psu, index 1.34, Packet 4205
20210430::165900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 24.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::165930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 217.6dbar, CTD 34.1psu, index 1.34, Packet 4259
20210430::165930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 230.0dbar, CTD 34.1psu, index 1.34, Packet 4312
20210430::170000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.1C, CTD 242.2dbar, CTD 34.0psu, index 1.34, Packet 4365
20210430::170030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.9C, CTD 254.7dbar, CTD 34.1psu, index 1.34, Packet 4419
20210430::170100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 16C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.8C, CTD 267.3dbar, CTD 34.0psu, index 1.34, Packet 4472
20210430::170130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.6C, CTD 279.9dbar, CTD 34.0psu, index 1.34, Packet 4526
20210430::170200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.3C, CTD 292.3dbar, CTD 34.1psu, index 1.34, Packet 4579
20210430::170230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.2C, CTD 304.7dbar, CTD 34.1psu, index 1.34, Packet 4632
20210430::170300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 317.9dbar, CTD 34.1psu, index 1.34, Packet 4686
20210430::170330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 336.2dbar, CTD 34.1psu, index 1.34, Packet 4739
20210430::170400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.0C, CTD 354.8dbar, CTD 34.1psu, index 1.34, Packet 4792
20210430::170430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 14C, Laser 23.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.9C, CTD 372.9dbar, CTD 34.2psu, index 1.34, Packet 4846
20210430::170500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 15C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.8C, CTD 389.2dbar, CTD 34.1psu, index 1.34, Packet 4899
20210430::170530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.7C, CTD 404.8dbar, CTD 34.2psu, index 1.34, Packet 4952
20210430::170600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.7C, CTD 420.6dbar, CTD 34.2psu, index 1.34, Packet 5006
20210430::170630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.6C, CTD 436.8dbar, CTD 34.2psu, index 1.34, Packet 5059
20210430::170700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.5C, CTD 453.2dbar, CTD 34.2psu, index 1.34, Packet 5113
20210430::170730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.4C, CTD 470.1dbar, CTD 34.2psu, index 1.34, Packet 5166
20210430::170800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.3C, CTD 486.8dbar, CTD 34.2psu, index 1.34, Packet 5219
20210430::170830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.2C, CTD 504.1dbar, CTD 34.2psu, index 1.34, Packet 5273
20210430::170900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.1C, CTD 521.0dbar, CTD 34.2psu, index 1.34, Packet 5326
20210430::170930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::170959: Head 2: Time Synchronization: 2021.04.30   17:10:00::0016
20210430::171000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.0C, CTD 537.6dbar, CTD 34.2psu, index 1.34, Packet 5380
20210430::171000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.9C, CTD 554.2dbar, CTD 34.2psu, index 1.34, Packet 5433
20210430::171030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.8C, CTD 570.0dbar, CTD 34.2psu, index 1.34, Packet 5486
20210430::171100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.7C, CTD 585.5dbar, CTD 34.3psu, index 1.34, Packet 5540
20210430::171130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.6C, CTD 600.8dbar, CTD 34.2psu, index 1.34, Packet 5593
20210430::171200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 616.1dbar, CTD 34.3psu, index 1.34, Packet 5646
20210430::171230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 631.7dbar, CTD 34.3psu, index 1.34, Packet 5700
20210430::171300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 647.8dbar, CTD 34.3psu, index 1.34, Packet 5753
20210430::171330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 22.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 663.8dbar, CTD 34.3psu, index 1.34, Packet 5806
20210430::171400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 12C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 680.0dbar, CTD 34.3psu, index 1.34, Packet 5860
20210430::171430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.2C, CTD 696.9dbar, CTD 34.3psu, index 1.34, Packet 5913
20210430::171500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 713.7dbar, CTD 34.3psu, index 1.34, Packet 5966
20210430::171530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 731.6dbar, CTD 34.3psu, index 1.34, Packet 6020
20210430::171600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 749.2dbar, CTD 34.3psu, index 1.34, Packet 6073
20210430::171630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 766.4dbar, CTD 34.3psu, index 1.34, Packet 6126
20210430::171700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 21.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 784.0dbar, CTD 34.3psu, index 1.34, Packet 6179
20210430::171730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 801.6dbar, CTD 34.4psu, index 1.34, Packet 6233
20210430::171800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 820.3dbar, CTD 34.4psu, index 1.34, Packet 6286
20210430::171830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 838.1dbar, CTD 34.3psu, index 1.34, Packet 6340
20210430::171900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 853.0dbar, CTD 34.4psu, index 1.34, Packet 6393
20210430::171930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::171930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 869.8dbar, CTD 34.4psu, index 1.34, Packet 6446
20210430::172000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 887.2dbar, CTD 34.4psu, index 1.34, Packet 6500
20210430::172030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 11C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 903.8dbar, CTD 34.4psu, index 1.34, Packet 6553
20210430::172100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 920.7dbar, CTD 34.4psu, index 1.34, Packet 6606
20210430::172130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 20.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 937.3dbar, CTD 34.4psu, index 1.34, Packet 6660
20210430::172200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 12C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 949.9dbar, CTD 34.4psu, index 1.34, Packet 6713
20210430::172230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 965.2dbar, CTD 34.4psu, index 1.34, Packet 6766
20210430::172300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.6dbar, CTD 34.4psu, index 1.34, Packet 6820
20210430::172330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 995.0dbar, CTD 34.4psu, index 1.34, Packet 6873
20210430::172400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 997.5dbar, CTD 34.4psu, index 1.34, Packet 6926
20210430::172430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 998.3dbar, CTD 34.4psu, index 1.34, Packet 6980
20210430::172500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 995.6dbar, CTD 34.4psu, index 1.34, Packet 7033
20210430::172530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.9dbar, CTD 34.4psu, index 1.34, Packet 7087
20210430::172600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 992.6dbar, CTD 34.4psu, index 1.34, Packet 7140
20210430::172630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.0dbar, CTD 34.4psu, index 1.34, Packet 7193
20210430::172700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 7247
20210430::172730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 7300
20210430::172800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 7353
20210430::172830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 19.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 7407
20210430::172900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.7dbar, CTD 34.4psu, index 1.34, Packet 7460
20210430::172930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::172930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.7dbar, CTD 34.4psu, index 1.34, Packet 7515
20210430::173000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 7568
20210430::173030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.7dbar, CTD 34.4psu, index 1.34, Packet 7621
20210430::173100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.7dbar, CTD 34.4psu, index 1.34, Packet 7675
20210430::173130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.7dbar, CTD 34.4psu, index 1.34, Packet 7728
20210430::173200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.1dbar, CTD 34.4psu, index 1.34, Packet 7782
20210430::173230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 7835
20210430::173300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 7888
20210430::173330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 36.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173344: GUI: Live mode ON.
20210430::173344: GUI: Requesing START operation, Head 2
20210430::173344: GUI: Requesing START operation, Head 1
20210430::173344: Head 2: Received request: START
20210430::173344: Head 1: Received request: START
20210430::173345: Head 2: Starting Scan Operation
20210430::173345: Head 1: Starting Scan Operation
20210430::173346: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::173346: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210430::173346: Head 2: Eye Safe Optical Filter check Passed
20210430::173346: Head 1: Eye Safe Optical Filter check Passed
20210430::173351: Head 2: Configured for WATER Processing
20210430::173351: Head 1: Configured for WATER Processing
20210430::173351: Head 2: Configured for WATER Processing
20210430::173351: Head 1: Configured for WATER Processing
20210430::173351: Head 2: Configured for WATER Processing
20210430::173351: Head 1: Configured for WATER Processing
20210430::173352: Head 2: Configured for WATER Processing
20210430::173352: Head 1: Configured for WATER Processing
20210430::173352: Head 2: Configured for WATER Processing
20210430::173352: Head 1: Configured for WATER Processing
20210430::173352: Head 2: Configured for WATER Processing
20210430::173352: Head 1: Configured for WATER Processing
20210430::173353: Head 2: Configured for WATER Processing
20210430::173353: Head 1: Configured for WATER Processing
20210430::173353: Head 2: Configured for WATER Processing
20210430::173353: Head 1: Configured for WATER Processing
20210430::173353: Head 1: Configured for WATER Processing
20210430::173353: Head 2: Configured for WATER Processing
20210430::173354: Head 1: Configured for WATER Processing
20210430::173354: Head 2: Configured for WATER Processing
20210430::173354: Head 1: Configured for WATER Processing
20210430::173354: Head 2: Configured for WATER Processing
20210430::173354: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173353_20210428d1_docr_lidar.raa
20210430::173354: Head 1: Configured for WATER Processing
20210430::173354: Head 2: Configured for WATER Processing
20210430::173354: Head 1: Configured for WATER Processing
20210430::173355: Head 2: Configured for WATER Processing
20210430::173355: Head 1: Configured for WATER Processing
20210430::173355: Head 2: Configured for WATER Processing
20210430::173355: Head 1: Configured for WATER Processing
20210430::173355: Head 2: Configured for WATER Processing
20210430::173355: Head 1: Configured for WATER Processing
20210430::173355: Head 2: Configured for WATER Processing
20210430::173356: Head 1: Configured for WATER Processing
20210430::173356: Head 2: Configured for WATER Processing
20210430::173356: Head 1: Configured for WATER Processing
20210430::173356: Head 2: Configured for WATER Processing
20210430::173356: Head 1: Configured for WATER Processing
20210430::173356: Head 2: Configured for WATER Processing
20210430::173357: Head 1: Configured for WATER Processing
20210430::173357: Head 2: Configured for WATER Processing
20210430::173359: Head 2: Time Synchronization: 2021.04.30   17:34:00::0013
20210430::173400: System  Initialized, Gain 9, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.1dbar, CTD 34.4psu, index 1.34, Packet 7942
20210430::173400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173403: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173403_20210428d1_docr_lidar.raa
20210430::173412: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173413_20210428d1_docr_lidar.raa
20210430::173422: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173423_20210428d1_docr_lidar.raa
20210430::173430: System  Initialized, Gain 9, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 7995
20210430::173430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173432: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173433_20210428d1_docr_lidar.raa
20210430::173442: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173443_20210428d1_docr_lidar.raa
20210430::173452: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173453_20210428d1_docr_lidar.raa
20210430::173500: System  Initialized, Gain 9, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8049
20210430::173500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173503: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173503_20210428d1_docr_lidar.raa
20210430::173512: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173513_20210428d1_docr_lidar.raa
20210430::173523: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173523_20210428d1_docr_lidar.raa
20210430::173526: GUI: Live mode ON.
20210430::173526: GUI: Requesing STOP operation, Head 1
20210430::173526: GUI: Requesing STOP operation, Head 2
20210430::173526: Head 1: Received request: STOP
20210430::173526: Head 2: Received request: STOP
20210430::173527: Head 1: Stopping Scan Operation
20210430::173527: Head 2: Stopping Scan Operation
20210430::173530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173530: System  Initialized, Gain 9, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8103
20210430::173530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 27%, OPB 11C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173531: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210430::173531: Head 2: Eye Safe Optical Filter check Passed
20210430::173533: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::173533: Head 1: Eye Safe Optical Filter check Passed
20210430::173537: GUI: Live mode ON.
20210430::173537: GUI: Requesing START operation, Head 1
20210430::173537: GUI: Requesing START operation, Head 2
20210430::173537: Head 1: Received request: START
20210430::173537: Head 2: Received request: START
20210430::173542: Head 2: ProcessingMgr stopped all worker threads.
20210430::173542: Head 2:       Stop finished, may now recover.
20210430::173554: Head 1: ProcessingMgr stopped all worker threads.
20210430::173555: Head 1:       Stop finished, may now recover.
20210430::173600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8156
20210430::173600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173609: GUI: Live mode ON.
20210430::173609: GUI: Requesing STOP operation, Head 2
20210430::173609: GUI: Requesing STOP operation, Head 1
20210430::173609: Head 2: Received request: STOP
20210430::173609: Head 1: Received request: STOP
20210430::173609: Head 2: Stopping Scan Operation
20210430::173609: Head 1: Stopping Scan Operation
20210430::173611: Head 2:       Stop finished, may now recover.
20210430::173614: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::173614: Head 2: Eye Safe Optical Filter check Passed
20210430::173615: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210430::173615: Head 1: Eye Safe Optical Filter check Passed
20210430::173630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.1dbar, CTD 34.4psu, index 1.34, Packet 8209
20210430::173630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210430::173642: Head 1:       Stop finished, may now recover.
20210430::173647: GUI: Live mode ON.
20210430::173647: GUI: Requesing START operation, Head 1
20210430::173647: GUI: Requesing START operation, Head 2
20210430::173648: Head 1: Received request: START
20210430::173648: Head 2: Received request: START
20210430::173648: Head 1: Starting Scan Operation
20210430::173648: Head 2: Starting Scan Operation
20210430::173649: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210430::173650: Head 1: Eye Safe Optical Filter check Passed
20210430::173652: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::173652: Head 2: Eye Safe Optical Filter check Passed
20210430::173656: Head 2: Configured for WATER Processing
20210430::173657: Head 2: Configured for WATER Processing
20210430::173657: Head 2: Configured for WATER Processing
20210430::173657: Head 2: Configured for WATER Processing
20210430::173658: Head 2: Configured for WATER Processing
20210430::173658: Head 2: Configured for WATER Processing
20210430::173658: Head 2: Configured for WATER Processing
20210430::173658: Head 2: Configured for WATER Processing
20210430::173659: Head 2: Configured for WATER Processing
20210430::173659: Head 2: Configured for WATER Processing
20210430::173659: Head 2: Configured for WATER Processing
20210430::173700: Head 2: Configured for WATER Processing
20210430::173700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8263
20210430::173700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 23.0C, Scan Az fault 0, gain 0, laser state 1
20210430::173700: Head 2: Configured for WATER Processing
20210430::173700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 12.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173700: Head 2: Configured for WATER Processing
20210430::173701: Head 2: Configured for WATER Processing
20210430::173701: Head 2: Configured for WATER Processing
20210430::173701: Head 2: Configured for WATER Processing
20210430::173701: Head 2: Configured for WATER Processing
20210430::173702: Head 2: Configured for WATER Processing
20210430::173702: Head 2: Configured for WATER Processing
20210430::173729: Head 1: Configured for WATER Processing
20210430::173730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8316
20210430::173730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 20.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173730: Head 1: Configured for WATER Processing
20210430::173730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173730: Head 1: Configured for WATER Processing
20210430::173730: Head 1: Configured for WATER Processing
20210430::173731: Head 1: Configured for WATER Processing
20210430::173731: Head 1: Configured for WATER Processing
20210430::173731: Head 1: Configured for WATER Processing
20210430::173731: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173730_20210428d1_docr_lidar.raa
20210430::173732: Head 1: Configured for WATER Processing
20210430::173732: Head 1: Configured for WATER Processing
20210430::173732: Head 1: Configured for WATER Processing
20210430::173732: Head 1: Configured for WATER Processing
20210430::173733: Head 1: Configured for WATER Processing
20210430::173733: Head 1: Configured for WATER Processing
20210430::173733: Head 1: Configured for WATER Processing
20210430::173734: Head 1: Configured for WATER Processing
20210430::173734: Head 1: Configured for WATER Processing
20210430::173734: Head 1: Configured for WATER Processing
20210430::173735: Head 1: Configured for WATER Processing
20210430::173735: Head 1: Configured for WATER Processing
20210430::173735: Head 1: Configured for WATER Processing
20210430::173739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173740_20210428d1_docr_lidar.raa
20210430::173750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173750_20210428d1_docr_lidar.raa
20210430::173759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173800_20210428d1_docr_lidar.raa
20210430::173800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8370
20210430::173800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173810_20210428d1_docr_lidar.raa
20210430::173819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173820_20210428d1_docr_lidar.raa
20210430::173829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173830_20210428d1_docr_lidar.raa
20210430::173830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 8423
20210430::173830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173840_20210428d1_docr_lidar.raa
20210430::173849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173850_20210428d1_docr_lidar.raa
20210430::173900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173900_20210428d1_docr_lidar.raa
20210430::173900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.5dbar, CTD 34.4psu, index 1.34, Packet 8477
20210430::173900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173910_20210428d1_docr_lidar.raa
20210430::173919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173920_20210428d1_docr_lidar.raa
20210430::173930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173930_20210428d1_docr_lidar.raa
20210430::173930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 992.2dbar, CTD 34.4psu, index 1.34, Packet 8530
20210430::173930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20210430::173939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173940_20210428d1_docr_lidar.raa
20210430::173950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_173950_20210428d1_docr_lidar.raa
20210430::174000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174000_20210428d1_docr_lidar.raa
20210430::174000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.8dbar, CTD 34.4psu, index 1.34, Packet 8584
20210430::174000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174010_20210428d1_docr_lidar.raa
20210430::174020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174020_20210428d1_docr_lidar.raa
20210430::174029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174030_20210428d1_docr_lidar.raa
20210430::174030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 989.6dbar, CTD 34.4psu, index 1.34, Packet 8637
20210430::174030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174040_20210428d1_docr_lidar.raa
20210430::174050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174050_20210428d1_docr_lidar.raa
20210430::174059: Head 1: Time Synchronization: 2021.04.30   17:41:00::0015
20210430::174059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174100_20210428d1_docr_lidar.raa
20210430::174100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.4dbar, CTD 34.4psu, index 1.34, Packet 8690
20210430::174100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174110_20210428d1_docr_lidar.raa
20210430::174120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174120_20210428d1_docr_lidar.raa
20210430::174129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174130_20210428d1_docr_lidar.raa
20210430::174130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.1dbar, CTD 34.4psu, index 1.34, Packet 8744
20210430::174130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174140_20210428d1_docr_lidar.raa
20210430::174149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174150_20210428d1_docr_lidar.raa
20210430::174159: Head 1: Time Synchronization: 2021.04.30   17:42:00::0014
20210430::174200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174200_20210428d1_docr_lidar.raa
20210430::174200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 985.9dbar, CTD 34.4psu, index 1.34, Packet 8797
20210430::174200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174210_20210428d1_docr_lidar.raa
20210430::174219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174220_20210428d1_docr_lidar.raa
20210430::174230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174230_20210428d1_docr_lidar.raa
20210430::174230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.6dbar, CTD 34.4psu, index 1.34, Packet 8851
20210430::174230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174240_20210428d1_docr_lidar.raa
20210430::174250: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174250_20210428d1_docr_lidar.raa
20210430::174259: Head 1: Time Synchronization: 2021.04.30   17:43:00::0013
20210430::174259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174300_20210428d1_docr_lidar.raa
20210430::174300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 983.3dbar, CTD 34.4psu, index 1.34, Packet 8904
20210430::174300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174310_20210428d1_docr_lidar.raa
20210430::174320: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174320_20210428d1_docr_lidar.raa
20210430::174329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174330_20210428d1_docr_lidar.raa
20210430::174330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.7dbar, CTD 34.4psu, index 1.34, Packet 8957
20210430::174330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174340_20210428d1_docr_lidar.raa
20210430::174349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174350_20210428d1_docr_lidar.raa
20210430::174359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174400_20210428d1_docr_lidar.raa
20210430::174400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 980.1dbar, CTD 34.4psu, index 1.34, Packet 9010
20210430::174400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174410_20210428d1_docr_lidar.raa
20210430::174419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174420_20210428d1_docr_lidar.raa
20210430::174429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174430_20210428d1_docr_lidar.raa
20210430::174430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.5dbar, CTD 34.4psu, index 1.34, Packet 9064
20210430::174430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174440_20210428d1_docr_lidar.raa
20210430::174449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174450_20210428d1_docr_lidar.raa
20210430::174459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174500_20210428d1_docr_lidar.raa
20210430::174500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 977.2dbar, CTD 34.4psu, index 1.34, Packet 9117
20210430::174500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174510_20210428d1_docr_lidar.raa
20210430::174519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174520_20210428d1_docr_lidar.raa
20210430::174529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174530_20210428d1_docr_lidar.raa
20210430::174530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 975.9dbar, CTD 34.4psu, index 1.34, Packet 9170
20210430::174530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174540_20210428d1_docr_lidar.raa
20210430::174549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174550_20210428d1_docr_lidar.raa
20210430::174559: Head 1: Time Synchronization: 2021.04.30   17:46:00::0013
20210430::174600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174600_20210428d1_docr_lidar.raa
20210430::174600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.4dbar, CTD 34.4psu, index 1.34, Packet 9224
20210430::174600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174610_20210428d1_docr_lidar.raa
20210430::174619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174620_20210428d1_docr_lidar.raa
20210430::174630: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174630_20210428d1_docr_lidar.raa
20210430::174630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.0dbar, CTD 34.4psu, index 1.34, Packet 9277
20210430::174630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174640_20210428d1_docr_lidar.raa
20210430::174650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174650_20210428d1_docr_lidar.raa
20210430::174659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174700_20210428d1_docr_lidar.raa
20210430::174700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 972.7dbar, CTD 34.4psu, index 1.34, Packet 9330
20210430::174700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174710_20210428d1_docr_lidar.raa
20210430::174720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174720_20210428d1_docr_lidar.raa
20210430::174729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174730_20210428d1_docr_lidar.raa
20210430::174730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.8dbar, CTD 34.4psu, index 1.34, Packet 9384
20210430::174730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174740_20210428d1_docr_lidar.raa
20210430::174750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174750_20210428d1_docr_lidar.raa
20210430::174759: Head 1: Time Synchronization: 2021.04.30   17:48:00::0016
20210430::174800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174800_20210428d1_docr_lidar.raa
20210430::174800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.3dbar, CTD 34.4psu, index 1.34, Packet 9438
20210430::174800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174810_20210428d1_docr_lidar.raa
20210430::174820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174820_20210428d1_docr_lidar.raa
20210430::174829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174830_20210428d1_docr_lidar.raa
20210430::174830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.6dbar, CTD 34.4psu, index 1.34, Packet 9491
20210430::174830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174840_20210428d1_docr_lidar.raa
20210430::174849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174850_20210428d1_docr_lidar.raa
20210430::174859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174900_20210428d1_docr_lidar.raa
20210430::174900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.0dbar, CTD 34.4psu, index 1.34, Packet 9545
20210430::174900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174910_20210428d1_docr_lidar.raa
20210430::174919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174920_20210428d1_docr_lidar.raa
20210430::174929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174930_20210428d1_docr_lidar.raa
20210430::174930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.4dbar, CTD 34.4psu, index 1.34, Packet 9598
20210430::174930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::174940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174940_20210428d1_docr_lidar.raa
20210430::174949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_174950_20210428d1_docr_lidar.raa
20210430::174959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175000_20210428d1_docr_lidar.raa
20210430::175000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.0dbar, CTD 34.4psu, index 1.34, Packet 9652
20210430::175000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175010_20210428d1_docr_lidar.raa
20210430::175019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175020_20210428d1_docr_lidar.raa
20210430::175029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175030_20210428d1_docr_lidar.raa
20210430::175030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 982.7dbar, CTD 34.4psu, index 1.34, Packet 9705
20210430::175030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175040_20210428d1_docr_lidar.raa
20210430::175050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175050_20210428d1_docr_lidar.raa
20210430::175059: Head 1: Time Synchronization: 2021.04.30   17:51:00::0014
20210430::175100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175100_20210428d1_docr_lidar.raa
20210430::175100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.1dbar, CTD 34.4psu, index 1.34, Packet 9759
20210430::175100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175110_20210428d1_docr_lidar.raa
20210430::175120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175120_20210428d1_docr_lidar.raa
20210430::175129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175130_20210428d1_docr_lidar.raa
20210430::175130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 985.4dbar, CTD 34.4psu, index 1.34, Packet 9812
20210430::175130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175140_20210428d1_docr_lidar.raa
20210430::175150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175150_20210428d1_docr_lidar.raa
20210430::175159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175200_20210428d1_docr_lidar.raa
20210430::175200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 986.6dbar, CTD 34.4psu, index 1.34, Packet 9865
20210430::175200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175210_20210428d1_docr_lidar.raa
20210430::175219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175220_20210428d1_docr_lidar.raa
20210430::175229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175230_20210428d1_docr_lidar.raa
20210430::175230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.8dbar, CTD 34.4psu, index 1.34, Packet 9919
20210430::175230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175240_20210428d1_docr_lidar.raa
20210430::175249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175250_20210428d1_docr_lidar.raa
20210430::175300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175300_20210428d1_docr_lidar.raa
20210430::175300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 989.1dbar, CTD 34.4psu, index 1.34, Packet 9972
20210430::175300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175310_20210428d1_docr_lidar.raa
20210430::175319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175320_20210428d1_docr_lidar.raa
20210430::175329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175330_20210428d1_docr_lidar.raa
20210430::175330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.4dbar, CTD 34.4psu, index 1.34, Packet 10025
20210430::175330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175340_20210428d1_docr_lidar.raa
20210430::175349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175350_20210428d1_docr_lidar.raa
20210430::175359: Head 1: Time Synchronization: 2021.04.30   17:54:00::0014
20210430::175359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175400_20210428d1_docr_lidar.raa
20210430::175400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 991.7dbar, CTD 34.4psu, index 1.34, Packet 10079
20210430::175400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175410_20210428d1_docr_lidar.raa
20210430::175420: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175420_20210428d1_docr_lidar.raa
20210430::175430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175430_20210428d1_docr_lidar.raa
20210430::175430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.1dbar, CTD 34.4psu, index 1.34, Packet 10132
20210430::175430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175440_20210428d1_docr_lidar.raa
20210430::175450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175450_20210428d1_docr_lidar.raa
20210430::175459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175500_20210428d1_docr_lidar.raa
20210430::175500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 10185
20210430::175500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175510_20210428d1_docr_lidar.raa
20210430::175520: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175520_20210428d1_docr_lidar.raa
20210430::175529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175530_20210428d1_docr_lidar.raa
20210430::175530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 10239
20210430::175530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175540_20210428d1_docr_lidar.raa
20210430::175549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175550_20210428d1_docr_lidar.raa
20210430::175559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175600_20210428d1_docr_lidar.raa
20210430::175600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 992.8dbar, CTD 34.4psu, index 1.34, Packet 10292
20210430::175600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175610: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175610_20210428d1_docr_lidar.raa
20210430::175619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175620_20210428d1_docr_lidar.raa
20210430::175629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175630_20210428d1_docr_lidar.raa
20210430::175630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 991.3dbar, CTD 34.4psu, index 1.34, Packet 10346
20210430::175630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175640: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175640_20210428d1_docr_lidar.raa
20210430::175649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175650_20210428d1_docr_lidar.raa
20210430::175659: Head 2: Time Synchronization: 2021.04.30   17:57:00::0018
20210430::175700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175700_20210428d1_docr_lidar.raa
20210430::175700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.0dbar, CTD 34.4psu, index 1.34, Packet 10399
20210430::175700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175710_20210428d1_docr_lidar.raa
20210430::175719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175720_20210428d1_docr_lidar.raa
20210430::175730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175730_20210428d1_docr_lidar.raa
20210430::175730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.7dbar, CTD 34.4psu, index 1.34, Packet 10452
20210430::175730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175740_20210428d1_docr_lidar.raa
20210430::175749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175750_20210428d1_docr_lidar.raa
20210430::175759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175800_20210428d1_docr_lidar.raa
20210430::175800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.4dbar, CTD 34.4psu, index 1.34, Packet 10505
20210430::175800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175810_20210428d1_docr_lidar.raa
20210430::175819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175820_20210428d1_docr_lidar.raa
20210430::175830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175830_20210428d1_docr_lidar.raa
20210430::175830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 986.3dbar, CTD 34.4psu, index 1.34, Packet 10559
20210430::175830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175840_20210428d1_docr_lidar.raa
20210430::175850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175850_20210428d1_docr_lidar.raa
20210430::175859: Head 1: Time Synchronization: 2021.04.30   17:59:00::0015
20210430::175859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175900_20210428d1_docr_lidar.raa
20210430::175900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 985.1dbar, CTD 34.4psu, index 1.34, Packet 10613
20210430::175900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175910_20210428d1_docr_lidar.raa
20210430::175920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175920_20210428d1_docr_lidar.raa
20210430::175929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175930_20210428d1_docr_lidar.raa
20210430::175930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 983.8dbar, CTD 34.4psu, index 1.34, Packet 10666
20210430::175930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::175940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175940_20210428d1_docr_lidar.raa
20210430::175950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_175950_20210428d1_docr_lidar.raa
20210430::175959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180000_20210428d1_docr_lidar.raa
20210430::180000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 982.3dbar, CTD 34.4psu, index 1.34, Packet 10719
20210430::180000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180010_20210428d1_docr_lidar.raa
20210430::180020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180020_20210428d1_docr_lidar.raa
20210430::180029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180030_20210428d1_docr_lidar.raa
20210430::180030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 980.6dbar, CTD 34.4psu, index 1.34, Packet 10773
20210430::180030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180040_20210428d1_docr_lidar.raa
20210430::180050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180050_20210428d1_docr_lidar.raa
20210430::180059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180100_20210428d1_docr_lidar.raa
20210430::180100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.1dbar, CTD 34.4psu, index 1.34, Packet 10826
20210430::180100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180110_20210428d1_docr_lidar.raa
20210430::180119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180120_20210428d1_docr_lidar.raa
20210430::180129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180130_20210428d1_docr_lidar.raa
20210430::180130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 977.7dbar, CTD 34.4psu, index 1.34, Packet 10880
20210430::180130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180140_20210428d1_docr_lidar.raa
20210430::180150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180150_20210428d1_docr_lidar.raa
20210430::180159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180200_20210428d1_docr_lidar.raa
20210430::180200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 976.3dbar, CTD 34.4psu, index 1.34, Packet 10933
20210430::180200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180210_20210428d1_docr_lidar.raa
20210430::180220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180220_20210428d1_docr_lidar.raa
20210430::180229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180230_20210428d1_docr_lidar.raa
20210430::180230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 974.9dbar, CTD 34.4psu, index 1.34, Packet 10987
20210430::180230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180240_20210428d1_docr_lidar.raa
20210430::180250: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180250_20210428d1_docr_lidar.raa
20210430::180259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180300_20210428d1_docr_lidar.raa
20210430::180300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.4dbar, CTD 34.4psu, index 1.34, Packet 11040
20210430::180300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180310_20210428d1_docr_lidar.raa
20210430::180319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180320_20210428d1_docr_lidar.raa
20210430::180329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180330_20210428d1_docr_lidar.raa
20210430::180330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 972.7dbar, CTD 34.4psu, index 1.34, Packet 11093
20210430::180330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180340_20210428d1_docr_lidar.raa
20210430::180349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180350_20210428d1_docr_lidar.raa
20210430::180359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180400_20210428d1_docr_lidar.raa
20210430::180400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.3dbar, CTD 34.4psu, index 1.34, Packet 11147
20210430::180400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180410_20210428d1_docr_lidar.raa
20210430::180419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180420_20210428d1_docr_lidar.raa
20210430::180430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180430_20210428d1_docr_lidar.raa
20210430::180430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.8dbar, CTD 34.4psu, index 1.34, Packet 11201
20210430::180430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180440_20210428d1_docr_lidar.raa
20210430::180449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180450_20210428d1_docr_lidar.raa
20210430::180500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180500_20210428d1_docr_lidar.raa
20210430::180500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.2dbar, CTD 34.4psu, index 1.34, Packet 11254
20210430::180500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180510_20210428d1_docr_lidar.raa
20210430::180519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180520_20210428d1_docr_lidar.raa
20210430::180530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180530_20210428d1_docr_lidar.raa
20210430::180530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 977.5dbar, CTD 34.4psu, index 1.34, Packet 11307
20210430::180530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180540_20210428d1_docr_lidar.raa
20210430::180549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180550_20210428d1_docr_lidar.raa
20210430::180600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 978.9dbar, CTD 34.4psu, index 1.34, Packet 11360
20210430::180600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180600_20210428d1_docr_lidar.raa
20210430::180600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180610_20210428d1_docr_lidar.raa
20210430::180619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180620_20210428d1_docr_lidar.raa
20210430::180630: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180630_20210428d1_docr_lidar.raa
20210430::180630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.3dbar, CTD 34.4psu, index 1.34, Packet 11414
20210430::180630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180640_20210428d1_docr_lidar.raa
20210430::180649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180650_20210428d1_docr_lidar.raa
20210430::180659: Head 1: Time Synchronization: 2021.04.30   18:07:00::0015
20210430::180700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180700_20210428d1_docr_lidar.raa
20210430::180700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.0dbar, CTD 34.4psu, index 1.34, Packet 11467
20210430::180700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180710_20210428d1_docr_lidar.raa
20210430::180720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180720_20210428d1_docr_lidar.raa
20210430::180730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.7dbar, CTD 34.4psu, index 1.34, Packet 11520
20210430::180730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180730_20210428d1_docr_lidar.raa
20210430::180730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180740_20210428d1_docr_lidar.raa
20210430::180750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180750_20210428d1_docr_lidar.raa
20210430::180759: Head 1: Time Synchronization: 2021.04.30   18:08:00::0014
20210430::180759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180800_20210428d1_docr_lidar.raa
20210430::180800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.0dbar, CTD 34.4psu, index 1.34, Packet 11574
20210430::180800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180810_20210428d1_docr_lidar.raa
20210430::180820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180820_20210428d1_docr_lidar.raa
20210430::180830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.3dbar, CTD 34.4psu, index 1.34, Packet 11627
20210430::180830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180830_20210428d1_docr_lidar.raa
20210430::180830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180840_20210428d1_docr_lidar.raa
20210430::180850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180850_20210428d1_docr_lidar.raa
20210430::180859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180900_20210428d1_docr_lidar.raa
20210430::180900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.3dbar, CTD 34.4psu, index 1.34, Packet 11681
20210430::180900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180910_20210428d1_docr_lidar.raa
20210430::180920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180920_20210428d1_docr_lidar.raa
20210430::180930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.5dbar, CTD 34.4psu, index 1.34, Packet 11734
20210430::180930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180930_20210428d1_docr_lidar.raa
20210430::180930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::180939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180940_20210428d1_docr_lidar.raa
20210430::180950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_180950_20210428d1_docr_lidar.raa
20210430::180959: Head 1: Time Synchronization: 2021.04.30   18:10:00::0015
20210430::181000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181000_20210428d1_docr_lidar.raa
20210430::181000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.9dbar, CTD 34.4psu, index 1.34, Packet 11788
20210430::181000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181010_20210428d1_docr_lidar.raa
20210430::181019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181020_20210428d1_docr_lidar.raa
20210430::181029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181030_20210428d1_docr_lidar.raa
20210430::181030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.2dbar, CTD 34.4psu, index 1.34, Packet 11841
20210430::181030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181040_20210428d1_docr_lidar.raa
20210430::181050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181050_20210428d1_docr_lidar.raa
20210430::181059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181100_20210428d1_docr_lidar.raa
20210430::181100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.7dbar, CTD 34.4psu, index 1.34, Packet 11895
20210430::181100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181110_20210428d1_docr_lidar.raa
20210430::181120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181120_20210428d1_docr_lidar.raa
20210430::181129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181130_20210428d1_docr_lidar.raa
20210430::181130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.2dbar, CTD 34.4psu, index 1.34, Packet 11948
20210430::181130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181140_20210428d1_docr_lidar.raa
20210430::181149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181150_20210428d1_docr_lidar.raa
20210430::181159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181200_20210428d1_docr_lidar.raa
20210430::181200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 12002
20210430::181200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181210_20210428d1_docr_lidar.raa
20210430::181219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181220_20210428d1_docr_lidar.raa
20210430::181230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181230_20210428d1_docr_lidar.raa
20210430::181230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.5dbar, CTD 34.4psu, index 1.34, Packet 12055
20210430::181230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181240_20210428d1_docr_lidar.raa
20210430::181249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181250_20210428d1_docr_lidar.raa
20210430::181300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181300_20210428d1_docr_lidar.raa
20210430::181300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.9dbar, CTD 34.4psu, index 1.34, Packet 12109
20210430::181300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181310_20210428d1_docr_lidar.raa
20210430::181319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181320_20210428d1_docr_lidar.raa
20210430::181330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181330_20210428d1_docr_lidar.raa
20210430::181330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.5dbar, CTD 34.4psu, index 1.34, Packet 12162
20210430::181330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181340_20210428d1_docr_lidar.raa
20210430::181349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181350_20210428d1_docr_lidar.raa
20210430::181359: Head 1: Time Synchronization: 2021.04.30   18:14:00::0012
20210430::181400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181400: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181400_20210428d1_docr_lidar.raa
20210430::181400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.2dbar, CTD 34.4psu, index 1.34, Packet 12215
20210430::181400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181410_20210428d1_docr_lidar.raa
20210430::181419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181420_20210428d1_docr_lidar.raa
20210430::181430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181430_20210428d1_docr_lidar.raa
20210430::181430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.9dbar, CTD 34.4psu, index 1.34, Packet 12269
20210430::181430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181440_20210428d1_docr_lidar.raa
20210430::181449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181450_20210428d1_docr_lidar.raa
20210430::181459: Head 1: Time Synchronization: 2021.04.30   18:15:00::0013
20210430::181459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181500_20210428d1_docr_lidar.raa
20210430::181500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.9dbar, CTD 34.4psu, index 1.34, Packet 12322
20210430::181500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181510_20210428d1_docr_lidar.raa
20210430::181519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181520_20210428d1_docr_lidar.raa
20210430::181530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181530_20210428d1_docr_lidar.raa
20210430::181530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.7dbar, CTD 34.4psu, index 1.34, Packet 12376
20210430::181530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181540_20210428d1_docr_lidar.raa
20210430::181549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181550_20210428d1_docr_lidar.raa
20210430::181559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181600_20210428d1_docr_lidar.raa
20210430::181559: Head 1: Time Synchronization: 2021.04.30   18:16:00::0016
20210430::181600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.4dbar, CTD 34.4psu, index 1.34, Packet 12429
20210430::181600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181610: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181610_20210428d1_docr_lidar.raa
20210430::181619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181620_20210428d1_docr_lidar.raa
20210430::181629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181630_20210428d1_docr_lidar.raa
20210430::181630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.9dbar, CTD 34.4psu, index 1.34, Packet 12483
20210430::181630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181640: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181640_20210428d1_docr_lidar.raa
20210430::181649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181650_20210428d1_docr_lidar.raa
20210430::181700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181700_20210428d1_docr_lidar.raa
20210430::181700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.2dbar, CTD 34.4psu, index 1.34, Packet 12536
20210430::181700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181710: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181710_20210428d1_docr_lidar.raa
20210430::181719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181720_20210428d1_docr_lidar.raa
20210430::181729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181730_20210428d1_docr_lidar.raa
20210430::181730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.7dbar, CTD 34.4psu, index 1.34, Packet 12590
20210430::181730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181740_20210428d1_docr_lidar.raa
20210430::181749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181750_20210428d1_docr_lidar.raa
20210430::181759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181800_20210428d1_docr_lidar.raa
20210430::181800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.4dbar, CTD 34.4psu, index 1.34, Packet 12643
20210430::181800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181810_20210428d1_docr_lidar.raa
20210430::181819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181820_20210428d1_docr_lidar.raa
20210430::181830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181830_20210428d1_docr_lidar.raa
20210430::181830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.0dbar, CTD 34.4psu, index 1.34, Packet 12697
20210430::181830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181840_20210428d1_docr_lidar.raa
20210430::181849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181850_20210428d1_docr_lidar.raa
20210430::181859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181900_20210428d1_docr_lidar.raa
20210430::181900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.6dbar, CTD 34.4psu, index 1.34, Packet 12750
20210430::181900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181910_20210428d1_docr_lidar.raa
20210430::181920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181920_20210428d1_docr_lidar.raa
20210430::181929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181930_20210428d1_docr_lidar.raa
20210430::181930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.2dbar, CTD 34.4psu, index 1.34, Packet 12804
20210430::181930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::181940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181940_20210428d1_docr_lidar.raa
20210430::181949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_181950_20210428d1_docr_lidar.raa
20210430::181959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182000_20210428d1_docr_lidar.raa
20210430::182000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 972.9dbar, CTD 34.4psu, index 1.34, Packet 12857
20210430::182000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182010_20210428d1_docr_lidar.raa
20210430::182019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182020_20210428d1_docr_lidar.raa
20210430::182029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182030_20210428d1_docr_lidar.raa
20210430::182030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 972.9dbar, CTD 34.4psu, index 1.34, Packet 12910
20210430::182030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182040_20210428d1_docr_lidar.raa
20210430::182049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182050_20210428d1_docr_lidar.raa
20210430::182059: Head 1: Time Synchronization: 2021.04.30   18:21:00::0016
20210430::182100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182100_20210428d1_docr_lidar.raa
20210430::182100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.3dbar, CTD 34.4psu, index 1.34, Packet 12964
20210430::182100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182110_20210428d1_docr_lidar.raa
20210430::182119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182120_20210428d1_docr_lidar.raa
20210430::182129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182130_20210428d1_docr_lidar.raa
20210430::182130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.7dbar, CTD 34.4psu, index 1.34, Packet 13017
20210430::182130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182140_20210428d1_docr_lidar.raa
20210430::182150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182150_20210428d1_docr_lidar.raa
20210430::182159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182200_20210428d1_docr_lidar.raa
20210430::182200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.1dbar, CTD 34.4psu, index 1.34, Packet 13071
20210430::182200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182210_20210428d1_docr_lidar.raa
20210430::182220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182220_20210428d1_docr_lidar.raa
20210430::182229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182230_20210428d1_docr_lidar.raa
20210430::182230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.4dbar, CTD 34.4psu, index 1.34, Packet 13124
20210430::182230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182240_20210428d1_docr_lidar.raa
20210430::182249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182250_20210428d1_docr_lidar.raa
20210430::182259: Head 2: Time Synchronization: 2021.04.30   18:23:00::0015
20210430::182259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182300_20210428d1_docr_lidar.raa
20210430::182300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.7dbar, CTD 34.4psu, index 1.34, Packet 13178
20210430::182300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182310_20210428d1_docr_lidar.raa
20210430::182319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182320_20210428d1_docr_lidar.raa
20210430::182329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182330_20210428d1_docr_lidar.raa
20210430::182330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.2dbar, CTD 34.4psu, index 1.34, Packet 13231
20210430::182330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182340_20210428d1_docr_lidar.raa
20210430::182349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182350_20210428d1_docr_lidar.raa
20210430::182359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182400_20210428d1_docr_lidar.raa
20210430::182359: Head 1: Time Synchronization: 2021.04.30   18:24:00::0013
20210430::182400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.9dbar, CTD 34.4psu, index 1.34, Packet 13285
20210430::182400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182410_20210428d1_docr_lidar.raa
20210430::182419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182420_20210428d1_docr_lidar.raa
20210430::182429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182430_20210428d1_docr_lidar.raa
20210430::182430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.4dbar, CTD 34.4psu, index 1.34, Packet 13338
20210430::182430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182440_20210428d1_docr_lidar.raa
20210430::182449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182450_20210428d1_docr_lidar.raa
20210430::182459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182500_20210428d1_docr_lidar.raa
20210430::182500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.8dbar, CTD 34.4psu, index 1.34, Packet 13392
20210430::182500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182510_20210428d1_docr_lidar.raa
20210430::182519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182520_20210428d1_docr_lidar.raa
20210430::182529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182530_20210428d1_docr_lidar.raa
20210430::182530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.1dbar, CTD 34.4psu, index 1.34, Packet 13445
20210430::182530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182540_20210428d1_docr_lidar.raa
20210430::182549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182550_20210428d1_docr_lidar.raa
20210430::182559: Head 1: Time Synchronization: 2021.04.30   18:26:00::0016
20210430::182559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182600_20210428d1_docr_lidar.raa
20210430::182600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.9dbar, CTD 34.4psu, index 1.34, Packet 13499
20210430::182600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182610: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182610_20210428d1_docr_lidar.raa
20210430::182619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182620_20210428d1_docr_lidar.raa
20210430::182629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182630_20210428d1_docr_lidar.raa
20210430::182630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.3dbar, CTD 34.4psu, index 1.34, Packet 13552
20210430::182630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182640_20210428d1_docr_lidar.raa
20210430::182649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182650_20210428d1_docr_lidar.raa
20210430::182659: Head 1: Time Synchronization: 2021.04.30   18:27:00::0013
20210430::182700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182700_20210428d1_docr_lidar.raa
20210430::182700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.6dbar, CTD 34.4psu, index 1.34, Packet 13606
20210430::182700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182710_20210428d1_docr_lidar.raa
20210430::182719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182720_20210428d1_docr_lidar.raa
20210430::182730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.0dbar, CTD 34.4psu, index 1.34, Packet 13659
20210430::182730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182730_20210428d1_docr_lidar.raa
20210430::182730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182740_20210428d1_docr_lidar.raa
20210430::182749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182750_20210428d1_docr_lidar.raa
20210430::182759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182800_20210428d1_docr_lidar.raa
20210430::182800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 13713
20210430::182800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182810_20210428d1_docr_lidar.raa
20210430::182819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182820_20210428d1_docr_lidar.raa
20210430::182830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182830_20210428d1_docr_lidar.raa
20210430::182830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 13767
20210430::182830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182840_20210428d1_docr_lidar.raa
20210430::182849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182850_20210428d1_docr_lidar.raa
20210430::182859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182900_20210428d1_docr_lidar.raa
20210430::182900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.1dbar, CTD 34.4psu, index 1.34, Packet 13820
20210430::182900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182910_20210428d1_docr_lidar.raa
20210430::182920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182920_20210428d1_docr_lidar.raa
20210430::182929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182930_20210428d1_docr_lidar.raa
20210430::182930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.5dbar, CTD 34.4psu, index 1.34, Packet 13874
20210430::182930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::182939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182940_20210428d1_docr_lidar.raa
20210430::182950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_182950_20210428d1_docr_lidar.raa
20210430::182959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183000_20210428d1_docr_lidar.raa
20210430::183000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.1dbar, CTD 34.4psu, index 1.34, Packet 13927
20210430::183000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183010_20210428d1_docr_lidar.raa
20210430::183019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183020_20210428d1_docr_lidar.raa
20210430::183029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183030_20210428d1_docr_lidar.raa
20210430::183030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.7dbar, CTD 34.4psu, index 1.34, Packet 13981
20210430::183030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183040_20210428d1_docr_lidar.raa
20210430::183049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183050_20210428d1_docr_lidar.raa
20210430::183059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183100_20210428d1_docr_lidar.raa
20210430::183059: Head 1: Time Synchronization: 2021.04.30   18:31:00::0014
20210430::183100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.4dbar, CTD 34.4psu, index 1.34, Packet 14034
20210430::183100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183110_20210428d1_docr_lidar.raa
20210430::183119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183120_20210428d1_docr_lidar.raa
20210430::183130: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183130_20210428d1_docr_lidar.raa
20210430::183130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.3dbar, CTD 34.4psu, index 1.34, Packet 14088
20210430::183130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183140_20210428d1_docr_lidar.raa
20210430::183149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183150_20210428d1_docr_lidar.raa
20210430::183159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183200_20210428d1_docr_lidar.raa
20210430::183200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.2dbar, CTD 34.4psu, index 1.34, Packet 14141
20210430::183200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183210_20210428d1_docr_lidar.raa
20210430::183220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183220_20210428d1_docr_lidar.raa
20210430::183229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183230_20210428d1_docr_lidar.raa
20210430::183230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.8dbar, CTD 34.4psu, index 1.34, Packet 14194
20210430::183230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183240_20210428d1_docr_lidar.raa
20210430::183249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183250_20210428d1_docr_lidar.raa
20210430::183259: Head 1: Time Synchronization: 2021.04.30   18:33:00::0014
20210430::183259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183300_20210428d1_docr_lidar.raa
20210430::183300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.3dbar, CTD 34.4psu, index 1.34, Packet 14248
20210430::183300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183310_20210428d1_docr_lidar.raa
20210430::183319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183320_20210428d1_docr_lidar.raa
20210430::183330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183330_20210428d1_docr_lidar.raa
20210430::183330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.7dbar, CTD 34.4psu, index 1.34, Packet 14301
20210430::183330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183340_20210428d1_docr_lidar.raa
20210430::183349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183350_20210428d1_docr_lidar.raa
20210430::183400: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183400_20210428d1_docr_lidar.raa
20210430::183400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.2dbar, CTD 34.4psu, index 1.34, Packet 14354
20210430::183400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183410_20210428d1_docr_lidar.raa
20210430::183419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183420_20210428d1_docr_lidar.raa
20210430::183429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183430_20210428d1_docr_lidar.raa
20210430::183430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.0dbar, CTD 34.4psu, index 1.34, Packet 14408
20210430::183430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183440_20210428d1_docr_lidar.raa
20210430::183450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183450_20210428d1_docr_lidar.raa
20210430::183459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183500_20210428d1_docr_lidar.raa
20210430::183500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.7dbar, CTD 34.4psu, index 1.34, Packet 14461
20210430::183500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183510_20210428d1_docr_lidar.raa
20210430::183520: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183520_20210428d1_docr_lidar.raa
20210430::183529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183530_20210428d1_docr_lidar.raa
20210430::183530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.3dbar, CTD 34.4psu, index 1.34, Packet 14515
20210430::183530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183540_20210428d1_docr_lidar.raa
20210430::183550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183550_20210428d1_docr_lidar.raa
20210430::183600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183600_20210428d1_docr_lidar.raa
20210430::183600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.9dbar, CTD 34.4psu, index 1.34, Packet 14568
20210430::183600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183610_20210428d1_docr_lidar.raa
20210430::183619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183620_20210428d1_docr_lidar.raa
20210430::183629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183630_20210428d1_docr_lidar.raa
20210430::183630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.4dbar, CTD 34.4psu, index 1.34, Packet 14622
20210430::183630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183640: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183640_20210428d1_docr_lidar.raa
20210430::183649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183650_20210428d1_docr_lidar.raa
20210430::183659: Head 1: Time Synchronization: 2021.04.30   18:37:00::0013
20210430::183659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183700_20210428d1_docr_lidar.raa
20210430::183700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.0dbar, CTD 34.4psu, index 1.34, Packet 14675
20210430::183700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183710: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183710_20210428d1_docr_lidar.raa
20210430::183719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183720_20210428d1_docr_lidar.raa
20210430::183729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183730_20210428d1_docr_lidar.raa
20210430::183730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.8dbar, CTD 34.4psu, index 1.34, Packet 14729
20210430::183730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183740_20210428d1_docr_lidar.raa
20210430::183749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183750_20210428d1_docr_lidar.raa
20210430::183759: Head 2: Time Synchronization: 2021.04.30   18:38:00::0016
20210430::183800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183800_20210428d1_docr_lidar.raa
20210430::183800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.2dbar, CTD 34.4psu, index 1.34, Packet 14782
20210430::183800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183810_20210428d1_docr_lidar.raa
20210430::183819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183820_20210428d1_docr_lidar.raa
20210430::183829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183830_20210428d1_docr_lidar.raa
20210430::183830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.6dbar, CTD 34.4psu, index 1.34, Packet 14836
20210430::183830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183840_20210428d1_docr_lidar.raa
20210430::183849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183850_20210428d1_docr_lidar.raa
20210430::183859: Head 1: Time Synchronization: 2021.04.30   18:39:00::0013
20210430::183900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183900_20210428d1_docr_lidar.raa
20210430::183900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.0dbar, CTD 34.4psu, index 1.34, Packet 14889
20210430::183900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183910_20210428d1_docr_lidar.raa
20210430::183919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183920_20210428d1_docr_lidar.raa
20210430::183930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183930_20210428d1_docr_lidar.raa
20210430::183930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.3dbar, CTD 34.4psu, index 1.34, Packet 14943
20210430::183930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::183939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183940_20210428d1_docr_lidar.raa
20210430::183949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_183950_20210428d1_docr_lidar.raa
20210430::183959: Head 1: Time Synchronization: 2021.04.30   18:40:00::0015
20210430::184000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184000_20210428d1_docr_lidar.raa
20210430::184000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.5dbar, CTD 34.4psu, index 1.34, Packet 14996
20210430::184000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184010_20210428d1_docr_lidar.raa
20210430::184019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184020_20210428d1_docr_lidar.raa
20210430::184030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184030: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184030_20210428d1_docr_lidar.raa
20210430::184030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.0dbar, CTD 34.4psu, index 1.34, Packet 15050
20210430::184030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184040_20210428d1_docr_lidar.raa
20210430::184049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184050_20210428d1_docr_lidar.raa
20210430::184100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184100_20210428d1_docr_lidar.raa
20210430::184100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.5dbar, CTD 34.4psu, index 1.34, Packet 15103
20210430::184100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184110_20210428d1_docr_lidar.raa
20210430::184119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184120_20210428d1_docr_lidar.raa
20210430::184130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184130: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184130_20210428d1_docr_lidar.raa
20210430::184130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.0dbar, CTD 34.4psu, index 1.34, Packet 15156
20210430::184130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184140_20210428d1_docr_lidar.raa
20210430::184149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184150_20210428d1_docr_lidar.raa
20210430::184159: Head 1: Time Synchronization: 2021.04.30   18:42:00::0013
20210430::184159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184200_20210428d1_docr_lidar.raa
20210430::184200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.4dbar, CTD 34.4psu, index 1.34, Packet 15210
20210430::184200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184210_20210428d1_docr_lidar.raa
20210430::184219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184220_20210428d1_docr_lidar.raa
20210430::184230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184230_20210428d1_docr_lidar.raa
20210430::184230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.5dbar, CTD 34.4psu, index 1.34, Packet 15263
20210430::184230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184240_20210428d1_docr_lidar.raa
20210430::184249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184250_20210428d1_docr_lidar.raa
20210430::184300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184300_20210428d1_docr_lidar.raa
20210430::184300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.7dbar, CTD 34.4psu, index 1.34, Packet 15317
20210430::184300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184310_20210428d1_docr_lidar.raa
20210430::184319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184320_20210428d1_docr_lidar.raa
20210430::184330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184330_20210428d1_docr_lidar.raa
20210430::184330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.1dbar, CTD 34.4psu, index 1.34, Packet 15370
20210430::184330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184340_20210428d1_docr_lidar.raa
20210430::184349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184350_20210428d1_docr_lidar.raa
20210430::184359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184400_20210428d1_docr_lidar.raa
20210430::184400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.4dbar, CTD 34.4psu, index 1.34, Packet 15423
20210430::184400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184410_20210428d1_docr_lidar.raa
20210430::184419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184420_20210428d1_docr_lidar.raa
20210430::184430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184430_20210428d1_docr_lidar.raa
20210430::184430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.9dbar, CTD 34.4psu, index 1.34, Packet 15477
20210430::184430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184440_20210428d1_docr_lidar.raa
20210430::184449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184450_20210428d1_docr_lidar.raa
20210430::184500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184500_20210428d1_docr_lidar.raa
20210430::184500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.4dbar, CTD 34.4psu, index 1.34, Packet 15531
20210430::184500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184510_20210428d1_docr_lidar.raa
20210430::184519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184520_20210428d1_docr_lidar.raa
20210430::184530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184530_20210428d1_docr_lidar.raa
20210430::184530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.5dbar, CTD 34.4psu, index 1.34, Packet 15584
20210430::184530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184540_20210428d1_docr_lidar.raa
20210430::184550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184550_20210428d1_docr_lidar.raa
20210430::184559: Head 1: Time Synchronization: 2021.04.30   18:46:00::0015
20210430::184600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.2dbar, CTD 34.4psu, index 1.34, Packet 15637
20210430::184600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184600_20210428d1_docr_lidar.raa
20210430::184600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184610_20210428d1_docr_lidar.raa
20210430::184620: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184620_20210428d1_docr_lidar.raa
20210430::184629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184630_20210428d1_docr_lidar.raa
20210430::184630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.7dbar, CTD 34.4psu, index 1.34, Packet 15691
20210430::184630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184640_20210428d1_docr_lidar.raa
20210430::184650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184650_20210428d1_docr_lidar.raa
20210430::184659: Head 1: Time Synchronization: 2021.04.30   18:47:00::0015
20210430::184659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184700_20210428d1_docr_lidar.raa
20210430::184700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.3dbar, CTD 34.4psu, index 1.34, Packet 15745
20210430::184700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184710_20210428d1_docr_lidar.raa
20210430::184720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184720_20210428d1_docr_lidar.raa
20210430::184729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184730_20210428d1_docr_lidar.raa
20210430::184730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.0dbar, CTD 34.4psu, index 1.34, Packet 15798
20210430::184730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184740_20210428d1_docr_lidar.raa
20210430::184750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184750_20210428d1_docr_lidar.raa
20210430::184759: Head 1: Time Synchronization: 2021.04.30   18:48:00::0016
20210430::184759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184800_20210428d1_docr_lidar.raa
20210430::184800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.8dbar, CTD 34.4psu, index 1.34, Packet 15852
20210430::184800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184810_20210428d1_docr_lidar.raa
20210430::184820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184820_20210428d1_docr_lidar.raa
20210430::184829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184830_20210428d1_docr_lidar.raa
20210430::184830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.6dbar, CTD 34.4psu, index 1.34, Packet 15905
20210430::184830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184840_20210428d1_docr_lidar.raa
20210430::184850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184850_20210428d1_docr_lidar.raa
20210430::184859: Head 1: Time Synchronization: 2021.04.30   18:49:00::0016
20210430::184859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184900_20210428d1_docr_lidar.raa
20210430::184900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.2dbar, CTD 34.4psu, index 1.34, Packet 15959
20210430::184900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184910_20210428d1_docr_lidar.raa
20210430::184919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184920_20210428d1_docr_lidar.raa
20210430::184929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184930_20210428d1_docr_lidar.raa
20210430::184930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.8dbar, CTD 34.4psu, index 1.34, Packet 16012
20210430::184930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::184940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184940_20210428d1_docr_lidar.raa
20210430::184949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_184950_20210428d1_docr_lidar.raa
20210430::184959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185000_20210428d1_docr_lidar.raa
20210430::185000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.2dbar, CTD 34.4psu, index 1.34, Packet 16066
20210430::185000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185010_20210428d1_docr_lidar.raa
20210430::185019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185020_20210428d1_docr_lidar.raa
20210430::185030: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185030_20210428d1_docr_lidar.raa
20210430::185030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.8dbar, CTD 34.4psu, index 1.34, Packet 16119
20210430::185030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185040_20210428d1_docr_lidar.raa
20210430::185049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185050_20210428d1_docr_lidar.raa
20210430::185059: Head 1: Time Synchronization: 2021.04.30   18:51:00::0014
20210430::185059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185100_20210428d1_docr_lidar.raa
20210430::185100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.6dbar, CTD 34.4psu, index 1.34, Packet 16173
20210430::185100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185110_20210428d1_docr_lidar.raa
20210430::185120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185120_20210428d1_docr_lidar.raa
20210430::185129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185130_20210428d1_docr_lidar.raa
20210430::185130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.3dbar, CTD 34.4psu, index 1.34, Packet 16226
20210430::185130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185140_20210428d1_docr_lidar.raa
20210430::185150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185150_20210428d1_docr_lidar.raa
20210430::185159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185200_20210428d1_docr_lidar.raa
20210430::185200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.0dbar, CTD 34.4psu, index 1.34, Packet 16280
20210430::185200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185210_20210428d1_docr_lidar.raa
20210430::185219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185220_20210428d1_docr_lidar.raa
20210430::185230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185230_20210428d1_docr_lidar.raa
20210430::185230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.6dbar, CTD 34.4psu, index 1.34, Packet 16333
20210430::185230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185240_20210428d1_docr_lidar.raa
20210430::185249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185250_20210428d1_docr_lidar.raa
20210430::185259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185300_20210428d1_docr_lidar.raa
20210430::185300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.2dbar, CTD 34.4psu, index 1.34, Packet 16387
20210430::185300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185310_20210428d1_docr_lidar.raa
20210430::185320: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185320_20210428d1_docr_lidar.raa
20210430::185329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185330_20210428d1_docr_lidar.raa
20210430::185330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.1dbar, CTD 34.4psu, index 1.34, Packet 16440
20210430::185330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185340_20210428d1_docr_lidar.raa
20210430::185350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185350_20210428d1_docr_lidar.raa
20210430::185359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185400_20210428d1_docr_lidar.raa
20210430::185400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.4dbar, CTD 34.4psu, index 1.34, Packet 16493
20210430::185400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185410_20210428d1_docr_lidar.raa
20210430::185420: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185420_20210428d1_docr_lidar.raa
20210430::185429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185430_20210428d1_docr_lidar.raa
20210430::185430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.8dbar, CTD 34.4psu, index 1.34, Packet 16547
20210430::185430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185440_20210428d1_docr_lidar.raa
20210430::185449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185450_20210428d1_docr_lidar.raa
20210430::185459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185500_20210428d1_docr_lidar.raa
20210430::185500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.1dbar, CTD 34.4psu, index 1.34, Packet 16600
20210430::185500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185510_20210428d1_docr_lidar.raa
20210430::185519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185520_20210428d1_docr_lidar.raa
20210430::185529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185530_20210428d1_docr_lidar.raa
20210430::185530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.5dbar, CTD 34.4psu, index 1.34, Packet 16654
20210430::185530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185540_20210428d1_docr_lidar.raa
20210430::185549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185550_20210428d1_docr_lidar.raa
20210430::185600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.8dbar, CTD 34.4psu, index 1.34, Packet 16707
20210430::185600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185600_20210428d1_docr_lidar.raa
20210430::185600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185610_20210428d1_docr_lidar.raa
20210430::185619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185620_20210428d1_docr_lidar.raa
20210430::185630: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185630_20210428d1_docr_lidar.raa
20210430::185630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.0dbar, CTD 34.4psu, index 1.34, Packet 16761
20210430::185630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185640_20210428d1_docr_lidar.raa
20210430::185650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185650_20210428d1_docr_lidar.raa
20210430::185700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185700_20210428d1_docr_lidar.raa
20210430::185700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.3dbar, CTD 34.4psu, index 1.34, Packet 16815
20210430::185700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185710_20210428d1_docr_lidar.raa
20210430::185719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185720_20210428d1_docr_lidar.raa
20210430::185729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185730_20210428d1_docr_lidar.raa
20210430::185730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.7dbar, CTD 34.4psu, index 1.34, Packet 16868
20210430::185730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185740_20210428d1_docr_lidar.raa
20210430::185750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185750_20210428d1_docr_lidar.raa
20210430::185759: Head 2: Time Synchronization: 2021.04.30   18:58:00::0014
20210430::185759: Head 1: Time Synchronization: 2021.04.30   18:58:00::0014
20210430::185759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185800_20210428d1_docr_lidar.raa
20210430::185800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.2dbar, CTD 34.4psu, index 1.34, Packet 16921
20210430::185800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185810_20210428d1_docr_lidar.raa
20210430::185819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185820_20210428d1_docr_lidar.raa
20210430::185829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185830_20210428d1_docr_lidar.raa
20210430::185830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.6dbar, CTD 34.4psu, index 1.34, Packet 16975
20210430::185830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185840_20210428d1_docr_lidar.raa
20210430::185849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185850_20210428d1_docr_lidar.raa
20210430::185859: Head 1: Time Synchronization: 2021.04.30   18:59:00::0013
20210430::185900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.0dbar, CTD 34.4psu, index 1.34, Packet 17028
20210430::185900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185900_20210428d1_docr_lidar.raa
20210430::185900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185910_20210428d1_docr_lidar.raa
20210430::185919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185920_20210428d1_docr_lidar.raa
20210430::185930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185930_20210428d1_docr_lidar.raa
20210430::185930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.2dbar, CTD 34.4psu, index 1.34, Packet 17082
20210430::185930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::185939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185940_20210428d1_docr_lidar.raa
20210430::185949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_185950_20210428d1_docr_lidar.raa
20210430::185959: Head 1: Time Synchronization: 2021.04.30   19:00:00::0016
20210430::190000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.6dbar, CTD 34.4psu, index 1.34, Packet 17135
20210430::190000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190000_20210428d1_docr_lidar.raa
20210430::190000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190010_20210428d1_docr_lidar.raa
20210430::190019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190020_20210428d1_docr_lidar.raa
20210430::190030: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190030_20210428d1_docr_lidar.raa
20210430::190030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.0dbar, CTD 34.4psu, index 1.34, Packet 17189
20210430::190030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190040_20210428d1_docr_lidar.raa
20210430::190050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190050_20210428d1_docr_lidar.raa
20210430::190059: Head 1: Time Synchronization: 2021.04.30   19:01:00::0014
20210430::190059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190100_20210428d1_docr_lidar.raa
20210430::190100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.4dbar, CTD 34.4psu, index 1.34, Packet 17242
20210430::190100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190110_20210428d1_docr_lidar.raa
20210430::190119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190120_20210428d1_docr_lidar.raa
20210430::190130: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190130_20210428d1_docr_lidar.raa
20210430::190130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.8dbar, CTD 34.4psu, index 1.34, Packet 17296
20210430::190130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190140_20210428d1_docr_lidar.raa
20210430::190149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190150_20210428d1_docr_lidar.raa
20210430::190159: Head 1: Time Synchronization: 2021.04.30   19:02:00::0014
20210430::190159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190200_20210428d1_docr_lidar.raa
20210430::190200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 17349
20210430::190200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190210_20210428d1_docr_lidar.raa
20210430::190219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190220_20210428d1_docr_lidar.raa
20210430::190229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190230_20210428d1_docr_lidar.raa
20210430::190230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 17403
20210430::190230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190240_20210428d1_docr_lidar.raa
20210430::190249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190250_20210428d1_docr_lidar.raa
20210430::190259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190300_20210428d1_docr_lidar.raa
20210430::190300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.6dbar, CTD 34.4psu, index 1.34, Packet 17456
20210430::190300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190310_20210428d1_docr_lidar.raa
20210430::190320: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190320_20210428d1_docr_lidar.raa
20210430::190329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190330_20210428d1_docr_lidar.raa
20210430::190330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.1dbar, CTD 34.4psu, index 1.34, Packet 17510
20210430::190330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190340_20210428d1_docr_lidar.raa
20210430::190350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190350_20210428d1_docr_lidar.raa
20210430::190359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190400_20210428d1_docr_lidar.raa
20210430::190400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.7dbar, CTD 34.4psu, index 1.34, Packet 17563
20210430::190400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190410_20210428d1_docr_lidar.raa
20210430::190419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190420_20210428d1_docr_lidar.raa
20210430::190429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190430_20210428d1_docr_lidar.raa
20210430::190430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.4dbar, CTD 34.4psu, index 1.34, Packet 17617
20210430::190430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190440_20210428d1_docr_lidar.raa
20210430::190449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190450_20210428d1_docr_lidar.raa
20210430::190459: Head 1: Time Synchronization: 2021.04.30   19:05:00::0015
20210430::190500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190500_20210428d1_docr_lidar.raa
20210430::190500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.0dbar, CTD 34.4psu, index 1.34, Packet 17671
20210430::190500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190510_20210428d1_docr_lidar.raa
20210430::190519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190520_20210428d1_docr_lidar.raa
20210430::190530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190530_20210428d1_docr_lidar.raa
20210430::190530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.7dbar, CTD 34.4psu, index 1.34, Packet 17724
20210430::190530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190540_20210428d1_docr_lidar.raa
20210430::190549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190550_20210428d1_docr_lidar.raa
20210430::190559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190600_20210428d1_docr_lidar.raa
20210430::190600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.3dbar, CTD 34.4psu, index 1.34, Packet 17777
20210430::190600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190610_20210428d1_docr_lidar.raa
20210430::190619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190620_20210428d1_docr_lidar.raa
20210430::190629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190630_20210428d1_docr_lidar.raa
20210430::190630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.8dbar, CTD 34.4psu, index 1.34, Packet 17831
20210430::190630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190640_20210428d1_docr_lidar.raa
20210430::190649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190650_20210428d1_docr_lidar.raa
20210430::190659: Head 1: Time Synchronization: 2021.04.30   19:07:00::0016
20210430::190700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.5dbar, CTD 34.4psu, index 1.34, Packet 17884
20210430::190700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190700_20210428d1_docr_lidar.raa
20210430::190710: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190710_20210428d1_docr_lidar.raa
20210430::190719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190720_20210428d1_docr_lidar.raa
20210430::190730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190730_20210428d1_docr_lidar.raa
20210430::190730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.2dbar, CTD 34.4psu, index 1.34, Packet 17938
20210430::190730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190740_20210428d1_docr_lidar.raa
20210430::190750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190750_20210428d1_docr_lidar.raa
20210430::190759: Head 1: Time Synchronization: 2021.04.30   19:08:00::0015
20210430::190800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190800_20210428d1_docr_lidar.raa
20210430::190800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.0dbar, CTD 34.4psu, index 1.34, Packet 17991
20210430::190800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190810_20210428d1_docr_lidar.raa
20210430::190820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190820_20210428d1_docr_lidar.raa
20210430::190829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190830_20210428d1_docr_lidar.raa
20210430::190830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.8dbar, CTD 34.4psu, index 1.34, Packet 18045
20210430::190830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190840_20210428d1_docr_lidar.raa
20210430::190850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190850_20210428d1_docr_lidar.raa
20210430::190859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190900_20210428d1_docr_lidar.raa
20210430::190900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.4dbar, CTD 34.4psu, index 1.34, Packet 18098
20210430::190900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190910_20210428d1_docr_lidar.raa
20210430::190920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190920_20210428d1_docr_lidar.raa
20210430::190929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190930_20210428d1_docr_lidar.raa
20210430::190930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.1dbar, CTD 34.4psu, index 1.34, Packet 18152
20210430::190930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::190939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190940_20210428d1_docr_lidar.raa
20210430::190950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_190950_20210428d1_docr_lidar.raa
20210430::190959: Head 1: Time Synchronization: 2021.04.30   19:10:00::0016
20210430::190959: Head 2: Time Synchronization: 2021.04.30   19:10:00::0017
20210430::190959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191000_20210428d1_docr_lidar.raa
20210430::191000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.7dbar, CTD 34.4psu, index 1.34, Packet 18206
20210430::191000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191010_20210428d1_docr_lidar.raa
20210430::191020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191020_20210428d1_docr_lidar.raa
20210430::191029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191030_20210428d1_docr_lidar.raa
20210430::191030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.5dbar, CTD 34.4psu, index 1.34, Packet 18259
20210430::191030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191040_20210428d1_docr_lidar.raa
20210430::191049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191050_20210428d1_docr_lidar.raa
20210430::191059: Head 1: Time Synchronization: 2021.04.30   19:11:00::0014
20210430::191100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.5dbar, CTD 34.4psu, index 1.34, Packet 18312
20210430::191100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191100_20210428d1_docr_lidar.raa
20210430::191100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191110_20210428d1_docr_lidar.raa
20210430::191120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191120_20210428d1_docr_lidar.raa
20210430::191129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191130_20210428d1_docr_lidar.raa
20210430::191130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.9dbar, CTD 34.4psu, index 1.34, Packet 18366
20210430::191130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191140_20210428d1_docr_lidar.raa
20210430::191149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191150_20210428d1_docr_lidar.raa
20210430::191159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191200_20210428d1_docr_lidar.raa
20210430::191200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.2dbar, CTD 34.4psu, index 1.34, Packet 18420
20210430::191200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191210_20210428d1_docr_lidar.raa
20210430::191219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191220_20210428d1_docr_lidar.raa
20210430::191229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191230_20210428d1_docr_lidar.raa
20210430::191230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.5dbar, CTD 34.4psu, index 1.34, Packet 18473
20210430::191230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191240_20210428d1_docr_lidar.raa
20210430::191249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191250_20210428d1_docr_lidar.raa
20210430::191300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191300_20210428d1_docr_lidar.raa
20210430::191300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.7dbar, CTD 34.4psu, index 1.34, Packet 18527
20210430::191300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191310_20210428d1_docr_lidar.raa
20210430::191319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191320_20210428d1_docr_lidar.raa
20210430::191330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191330_20210428d1_docr_lidar.raa
20210430::191330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.9dbar, CTD 34.4psu, index 1.34, Packet 18580
20210430::191330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191340_20210428d1_docr_lidar.raa
20210430::191349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191350_20210428d1_docr_lidar.raa
20210430::191359: Head 2: Time Synchronization: 2021.04.30   19:14:00::0015
20210430::191400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.3dbar, CTD 34.4psu, index 1.34, Packet 18633
20210430::191400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191400: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191400_20210428d1_docr_lidar.raa
20210430::191409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191410_20210428d1_docr_lidar.raa
20210430::191420: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191420_20210428d1_docr_lidar.raa
20210430::191429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191430_20210428d1_docr_lidar.raa
20210430::191430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.7dbar, CTD 34.4psu, index 1.34, Packet 18687
20210430::191430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191440_20210428d1_docr_lidar.raa
20210430::191450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191450_20210428d1_docr_lidar.raa
20210430::191459: Head 1: Time Synchronization: 2021.04.30   19:15:00::0015
20210430::191459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191500_20210428d1_docr_lidar.raa
20210430::191500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.1dbar, CTD 34.4psu, index 1.34, Packet 18741
20210430::191500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191510_20210428d1_docr_lidar.raa
20210430::191520: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191520_20210428d1_docr_lidar.raa
20210430::191530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191530_20210428d1_docr_lidar.raa
20210430::191530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.4dbar, CTD 34.4psu, index 1.34, Packet 18794
20210430::191530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191540_20210428d1_docr_lidar.raa
20210430::191550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191550_20210428d1_docr_lidar.raa
20210430::191559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191600_20210428d1_docr_lidar.raa
20210430::191600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.9dbar, CTD 34.4psu, index 1.34, Packet 18848
20210430::191600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191610_20210428d1_docr_lidar.raa
20210430::191619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191620_20210428d1_docr_lidar.raa
20210430::191629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191630_20210428d1_docr_lidar.raa
20210430::191630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.3dbar, CTD 34.4psu, index 1.34, Packet 18901
20210430::191630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191640: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191640_20210428d1_docr_lidar.raa
20210430::191649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191650_20210428d1_docr_lidar.raa
20210430::191659: Head 1: Time Synchronization: 2021.04.30   19:17:00::0014
20210430::191659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191700_20210428d1_docr_lidar.raa
20210430::191700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.7dbar, CTD 34.4psu, index 1.34, Packet 18955
20210430::191700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191710: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191710_20210428d1_docr_lidar.raa
20210430::191720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191720_20210428d1_docr_lidar.raa
20210430::191729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191730_20210428d1_docr_lidar.raa
20210430::191730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.1dbar, CTD 34.4psu, index 1.34, Packet 19008
20210430::191730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191740_20210428d1_docr_lidar.raa
20210430::191749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191750_20210428d1_docr_lidar.raa
20210430::191759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191800_20210428d1_docr_lidar.raa
20210430::191800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.6dbar, CTD 34.3psu, index 1.34, Packet 19062
20210430::191800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191810_20210428d1_docr_lidar.raa
20210430::191820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191820_20210428d1_docr_lidar.raa
20210430::191829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191830_20210428d1_docr_lidar.raa
20210430::191830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.7dbar, CTD 34.4psu, index 1.34, Packet 19115
20210430::191830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191840_20210428d1_docr_lidar.raa
20210430::191850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191850_20210428d1_docr_lidar.raa
20210430::191859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191900_20210428d1_docr_lidar.raa
20210430::191900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 19169
20210430::191900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191910_20210428d1_docr_lidar.raa
20210430::191920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191920_20210428d1_docr_lidar.raa
20210430::191929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191930_20210428d1_docr_lidar.raa
20210430::191930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.3dbar, CTD 34.4psu, index 1.34, Packet 19222
20210430::191930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::191939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191940_20210428d1_docr_lidar.raa
20210430::191950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_191950_20210428d1_docr_lidar.raa
20210430::191959: Head 1: Time Synchronization: 2021.04.30   19:20:00::0014
20210430::191959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192000_20210428d1_docr_lidar.raa
20210430::192000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.8dbar, CTD 34.4psu, index 1.34, Packet 19276
20210430::192000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192010_20210428d1_docr_lidar.raa
20210430::192020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192020_20210428d1_docr_lidar.raa
20210430::192029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192030_20210428d1_docr_lidar.raa
20210430::192030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.5dbar, CTD 34.5psu, index 1.34, Packet 19330
20210430::192030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192040_20210428d1_docr_lidar.raa
20210430::192050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192050_20210428d1_docr_lidar.raa
20210430::192059: Head 2: Time Synchronization: 2021.04.30   19:21:00::0015
20210430::192059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192100_20210428d1_docr_lidar.raa
20210430::192100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.0dbar, CTD 34.4psu, index 1.34, Packet 19383
20210430::192100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192110_20210428d1_docr_lidar.raa
20210430::192120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192120_20210428d1_docr_lidar.raa
20210430::192129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192130_20210428d1_docr_lidar.raa
20210430::192130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.5dbar, CTD 34.4psu, index 1.34, Packet 19436
20210430::192130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192140_20210428d1_docr_lidar.raa
20210430::192150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192150_20210428d1_docr_lidar.raa
20210430::192159: Head 2: Time Synchronization: 2021.04.30   19:22:00::0016
20210430::192159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192200_20210428d1_docr_lidar.raa
20210430::192200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.2dbar, CTD 34.4psu, index 1.34, Packet 19490
20210430::192200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192210_20210428d1_docr_lidar.raa
20210430::192219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192220_20210428d1_docr_lidar.raa
20210430::192230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.9dbar, CTD 34.4psu, index 1.34, Packet 19543
20210430::192230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192230_20210428d1_docr_lidar.raa
20210430::192239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192240_20210428d1_docr_lidar.raa
20210430::192249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192250_20210428d1_docr_lidar.raa
20210430::192300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192300_20210428d1_docr_lidar.raa
20210430::192300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.5dbar, CTD 34.4psu, index 1.34, Packet 19597
20210430::192300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192310_20210428d1_docr_lidar.raa
20210430::192319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192320_20210428d1_docr_lidar.raa
20210430::192329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192330_20210428d1_docr_lidar.raa
20210430::192330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.2dbar, CTD 34.4psu, index 1.34, Packet 19650
20210430::192330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192340_20210428d1_docr_lidar.raa
20210430::192349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192350_20210428d1_docr_lidar.raa
20210430::192359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192400_20210428d1_docr_lidar.raa
20210430::192400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.8dbar, CTD 34.4psu, index 1.34, Packet 19704
20210430::192400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192410_20210428d1_docr_lidar.raa
20210430::192419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192420_20210428d1_docr_lidar.raa
20210430::192430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192430_20210428d1_docr_lidar.raa
20210430::192430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.6dbar, CTD 34.4psu, index 1.34, Packet 19757
20210430::192430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192440_20210428d1_docr_lidar.raa
20210430::192449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192450_20210428d1_docr_lidar.raa
20210430::192500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.4dbar, CTD 34.4psu, index 1.34, Packet 19810
20210430::192500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192500_20210428d1_docr_lidar.raa
20210430::192500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192510_20210428d1_docr_lidar.raa
20210430::192519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192520_20210428d1_docr_lidar.raa
20210430::192529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192530_20210428d1_docr_lidar.raa
20210430::192530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.2dbar, CTD 34.4psu, index 1.34, Packet 19864
20210430::192530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192540_20210428d1_docr_lidar.raa
20210430::192550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192550_20210428d1_docr_lidar.raa
20210430::192559: Head 1: Time Synchronization: 2021.04.30   19:26:00::0013
20210430::192559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192600_20210428d1_docr_lidar.raa
20210430::192600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.9dbar, CTD 34.4psu, index 1.34, Packet 19917
20210430::192600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192610_20210428d1_docr_lidar.raa
20210430::192620: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192620_20210428d1_docr_lidar.raa
20210430::192629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192630_20210428d1_docr_lidar.raa
20210430::192630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.6dbar, CTD 34.4psu, index 1.34, Packet 19970
20210430::192630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192640_20210428d1_docr_lidar.raa
20210430::192650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192650_20210428d1_docr_lidar.raa
20210430::192659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192700_20210428d1_docr_lidar.raa
20210430::192700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.7dbar, CTD 34.4psu, index 1.34, Packet 20024
20210430::192700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192710_20210428d1_docr_lidar.raa
20210430::192720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192720_20210428d1_docr_lidar.raa
20210430::192729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192730_20210428d1_docr_lidar.raa
20210430::192730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.2dbar, CTD 34.4psu, index 1.34, Packet 20077
20210430::192730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192740_20210428d1_docr_lidar.raa
20210430::192749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192750_20210428d1_docr_lidar.raa
20210430::192759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192800_20210428d1_docr_lidar.raa
20210430::192800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.7dbar, CTD 34.4psu, index 1.34, Packet 20131
20210430::192800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192810_20210428d1_docr_lidar.raa
20210430::192819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192820_20210428d1_docr_lidar.raa
20210430::192829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192830_20210428d1_docr_lidar.raa
20210430::192830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.0dbar, CTD 34.4psu, index 1.34, Packet 20184
20210430::192830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192840_20210428d1_docr_lidar.raa
20210430::192849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192850_20210428d1_docr_lidar.raa
20210430::192859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192900_20210428d1_docr_lidar.raa
20210430::192900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.2dbar, CTD 34.4psu, index 1.34, Packet 20238
20210430::192900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192910_20210428d1_docr_lidar.raa
20210430::192919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192920_20210428d1_docr_lidar.raa
20210430::192929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192930_20210428d1_docr_lidar.raa
20210430::192930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.5dbar, CTD 34.4psu, index 1.34, Packet 20291
20210430::192930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::192940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192940_20210428d1_docr_lidar.raa
20210430::192949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_192950_20210428d1_docr_lidar.raa
20210430::192959: Head 1: Time Synchronization: 2021.04.30   19:30:00::0015
20210430::192959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193000_20210428d1_docr_lidar.raa
20210430::193000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.7dbar, CTD 34.4psu, index 1.34, Packet 20345
20210430::193000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193010_20210428d1_docr_lidar.raa
20210430::193019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193020_20210428d1_docr_lidar.raa
20210430::193029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193030_20210428d1_docr_lidar.raa
20210430::193030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.0dbar, CTD 34.4psu, index 1.34, Packet 20398
20210430::193030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193040_20210428d1_docr_lidar.raa
20210430::193049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193050_20210428d1_docr_lidar.raa
20210430::193059: Head 1: Time Synchronization: 2021.04.30   19:31:00::0014
20210430::193059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193100_20210428d1_docr_lidar.raa
20210430::193100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.4dbar, CTD 34.4psu, index 1.34, Packet 20452
20210430::193100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193110_20210428d1_docr_lidar.raa
20210430::193119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193120_20210428d1_docr_lidar.raa
20210430::193130: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193130_20210428d1_docr_lidar.raa
20210430::193130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.8dbar, CTD 34.4psu, index 1.34, Packet 20505
20210430::193130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193140_20210428d1_docr_lidar.raa
20210430::193150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193150_20210428d1_docr_lidar.raa
20210430::193159: Head 1: Time Synchronization: 2021.04.30   19:32:00::0014
20210430::193159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193200_20210428d1_docr_lidar.raa
20210430::193200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.1dbar, CTD 34.4psu, index 1.34, Packet 20559
20210430::193200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193210_20210428d1_docr_lidar.raa
20210430::193219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193220_20210428d1_docr_lidar.raa
20210430::193230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193230_20210428d1_docr_lidar.raa
20210430::193230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.4dbar, CTD 34.4psu, index 1.34, Packet 20612
20210430::193230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193240_20210428d1_docr_lidar.raa
20210430::193249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193250_20210428d1_docr_lidar.raa
20210430::193259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193300_20210428d1_docr_lidar.raa
20210430::193300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.9dbar, CTD 34.4psu, index 1.34, Packet 20666
20210430::193300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193310_20210428d1_docr_lidar.raa
20210430::193320: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193320_20210428d1_docr_lidar.raa
20210430::193330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 990.3dbar, CTD 34.4psu, index 1.34, Packet 20719
20210430::193330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193330_20210428d1_docr_lidar.raa
20210430::193330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193340_20210428d1_docr_lidar.raa
20210430::193350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193350_20210428d1_docr_lidar.raa
20210430::193359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193400_20210428d1_docr_lidar.raa
20210430::193400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.8dbar, CTD 34.5psu, index 1.34, Packet 20773
20210430::193400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193410_20210428d1_docr_lidar.raa
20210430::193420: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193420_20210428d1_docr_lidar.raa
20210430::193429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193430_20210428d1_docr_lidar.raa
20210430::193430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.3dbar, CTD 34.5psu, index 1.34, Packet 20826
20210430::193430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193440_20210428d1_docr_lidar.raa
20210430::193449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193450_20210428d1_docr_lidar.raa
20210430::193459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193500_20210428d1_docr_lidar.raa
20210430::193500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.7dbar, CTD 34.4psu, index 1.34, Packet 20880
20210430::193500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193510_20210428d1_docr_lidar.raa
20210430::193520: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193520_20210428d1_docr_lidar.raa
20210430::193529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193530_20210428d1_docr_lidar.raa
20210430::193530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 995.0dbar, CTD 34.4psu, index 1.34, Packet 20933
20210430::193530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193540_20210428d1_docr_lidar.raa
20210430::193550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193550_20210428d1_docr_lidar.raa
20210430::193559: Head 2: Time Synchronization: 2021.04.30   19:36:00::0015
20210430::193559: Head 1: Time Synchronization: 2021.04.30   19:36:00::0015
20210430::193559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193600_20210428d1_docr_lidar.raa
20210430::193600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 20987
20210430::193600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193610_20210428d1_docr_lidar.raa
20210430::193619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193620_20210428d1_docr_lidar.raa
20210430::193629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193630_20210428d1_docr_lidar.raa
20210430::193630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 992.5dbar, CTD 34.4psu, index 1.34, Packet 21040
20210430::193630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193640_20210428d1_docr_lidar.raa
20210430::193650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193650_20210428d1_docr_lidar.raa
20210430::193659: Head 1: Time Synchronization: 2021.04.30   19:37:00::0013
20210430::193700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193700_20210428d1_docr_lidar.raa
20210430::193700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.2dbar, CTD 34.5psu, index 1.34, Packet 21093
20210430::193700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193710_20210428d1_docr_lidar.raa
20210430::193720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193720_20210428d1_docr_lidar.raa
20210430::193729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193730_20210428d1_docr_lidar.raa
20210430::193730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 989.6dbar, CTD 34.4psu, index 1.34, Packet 21147
20210430::193730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193740_20210428d1_docr_lidar.raa
20210430::193750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193750_20210428d1_docr_lidar.raa
20210430::193759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193800_20210428d1_docr_lidar.raa
20210430::193800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 988.2dbar, CTD 34.4psu, index 1.34, Packet 21200
20210430::193800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193810_20210428d1_docr_lidar.raa
20210430::193819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193820_20210428d1_docr_lidar.raa
20210430::193830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193830_20210428d1_docr_lidar.raa
20210430::193830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 986.8dbar, CTD 34.5psu, index 1.34, Packet 21254
20210430::193830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193840_20210428d1_docr_lidar.raa
20210430::193849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193850_20210428d1_docr_lidar.raa
20210430::193859: Head 2: Time Synchronization: 2021.04.30   19:39:00::0016
20210430::193900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193900_20210428d1_docr_lidar.raa
20210430::193900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 985.5dbar, CTD 34.5psu, index 1.34, Packet 21307
20210430::193900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193910_20210428d1_docr_lidar.raa
20210430::193920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193920_20210428d1_docr_lidar.raa
20210430::193929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193930_20210428d1_docr_lidar.raa
20210430::193930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 984.2dbar, CTD 34.5psu, index 1.34, Packet 21361
20210430::193930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::193939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193940_20210428d1_docr_lidar.raa
20210430::193949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_193950_20210428d1_docr_lidar.raa
20210430::193959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194000_20210428d1_docr_lidar.raa
20210430::194000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 982.8dbar, CTD 34.4psu, index 1.34, Packet 21414
20210430::194000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194010_20210428d1_docr_lidar.raa
20210430::194020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194020_20210428d1_docr_lidar.raa
20210430::194029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194030_20210428d1_docr_lidar.raa
20210430::194030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.5dbar, CTD 34.3psu, index 1.34, Packet 21467
20210430::194030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194040_20210428d1_docr_lidar.raa
20210430::194050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194050_20210428d1_docr_lidar.raa
20210430::194059: Head 1: Time Synchronization: 2021.04.30   19:41:00::0015
20210430::194059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194100_20210428d1_docr_lidar.raa
20210430::194100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.2dbar, CTD 34.2psu, index 1.34, Packet 21521
20210430::194100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194110_20210428d1_docr_lidar.raa
20210430::194120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194120_20210428d1_docr_lidar.raa
20210430::194129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194130_20210428d1_docr_lidar.raa
20210430::194130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.0dbar, CTD 34.4psu, index 1.34, Packet 21574
20210430::194130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194140_20210428d1_docr_lidar.raa
20210430::194150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194150_20210428d1_docr_lidar.raa
20210430::194200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.8dbar, CTD 34.4psu, index 1.34, Packet 21627
20210430::194200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194200_20210428d1_docr_lidar.raa
20210430::194200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194210_20210428d1_docr_lidar.raa
20210430::194219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194220_20210428d1_docr_lidar.raa
20210430::194229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194230_20210428d1_docr_lidar.raa
20210430::194230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.4dbar, CTD 34.4psu, index 1.34, Packet 21681
20210430::194230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194240_20210428d1_docr_lidar.raa
20210430::194250: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194250_20210428d1_docr_lidar.raa
20210430::194259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194300_20210428d1_docr_lidar.raa
20210430::194300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.1dbar, CTD 34.4psu, index 1.34, Packet 21734
20210430::194300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194310_20210428d1_docr_lidar.raa
20210430::194319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194320_20210428d1_docr_lidar.raa
20210430::194329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194330_20210428d1_docr_lidar.raa
20210430::194330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.8dbar, CTD 34.4psu, index 1.34, Packet 21788
20210430::194330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194340_20210428d1_docr_lidar.raa
20210430::194350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194350_20210428d1_docr_lidar.raa
20210430::194359: Head 1: Time Synchronization: 2021.04.30   19:44:00::0015
20210430::194359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194400_20210428d1_docr_lidar.raa
20210430::194400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.8dbar, CTD 34.4psu, index 1.34, Packet 21841
20210430::194400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194410_20210428d1_docr_lidar.raa
20210430::194419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194420_20210428d1_docr_lidar.raa
20210430::194429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194430_20210428d1_docr_lidar.raa
20210430::194430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.2dbar, CTD 34.4psu, index 1.34, Packet 21895
20210430::194430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194440_20210428d1_docr_lidar.raa
20210430::194449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194450_20210428d1_docr_lidar.raa
20210430::194459: Head 1: Time Synchronization: 2021.04.30   19:45:00::0011
20210430::194459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194500_20210428d1_docr_lidar.raa
20210430::194500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.6dbar, CTD 34.4psu, index 1.34, Packet 21948
20210430::194500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194510_20210428d1_docr_lidar.raa
20210430::194519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194520_20210428d1_docr_lidar.raa
20210430::194529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194530_20210428d1_docr_lidar.raa
20210430::194530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.9dbar, CTD 34.4psu, index 1.34, Packet 22002
20210430::194530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194540_20210428d1_docr_lidar.raa
20210430::194549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194550_20210428d1_docr_lidar.raa
20210430::194559: Head 1: Time Synchronization: 2021.04.30   19:46:00::0014
20210430::194600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194600_20210428d1_docr_lidar.raa
20210430::194600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.2dbar, CTD 34.3psu, index 1.34, Packet 22055
20210430::194600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194610_20210428d1_docr_lidar.raa
20210430::194619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194620_20210428d1_docr_lidar.raa
20210430::194629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194630_20210428d1_docr_lidar.raa
20210430::194630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 980.4dbar, CTD 34.4psu, index 1.34, Packet 22108
20210430::194630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194640_20210428d1_docr_lidar.raa
20210430::194649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194650_20210428d1_docr_lidar.raa
20210430::194659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194700_20210428d1_docr_lidar.raa
20210430::194700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.7dbar, CTD 34.4psu, index 1.34, Packet 22162
20210430::194700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194710_20210428d1_docr_lidar.raa
20210430::194720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194720_20210428d1_docr_lidar.raa
20210430::194729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194730_20210428d1_docr_lidar.raa
20210430::194730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 983.1dbar, CTD 34.4psu, index 1.34, Packet 22216
20210430::194730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194740_20210428d1_docr_lidar.raa
20210430::194750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194750_20210428d1_docr_lidar.raa
20210430::194759: Head 1: Time Synchronization: 2021.04.30   19:48:00::0011
20210430::194759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194800_20210428d1_docr_lidar.raa
20210430::194800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.5dbar, CTD 34.4psu, index 1.34, Packet 22269
20210430::194800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194810_20210428d1_docr_lidar.raa
20210430::194819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194820_20210428d1_docr_lidar.raa
20210430::194829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194830_20210428d1_docr_lidar.raa
20210430::194830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 985.9dbar, CTD 34.4psu, index 1.34, Packet 22323
20210430::194830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194840_20210428d1_docr_lidar.raa
20210430::194849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194850_20210428d1_docr_lidar.raa
20210430::194859: Head 1: Time Synchronization: 2021.04.30   19:49:00::0014
20210430::194859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194900_20210428d1_docr_lidar.raa
20210430::194900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.1dbar, CTD 34.4psu, index 1.34, Packet 22376
20210430::194900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194910_20210428d1_docr_lidar.raa
20210430::194919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194920_20210428d1_docr_lidar.raa
20210430::194930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194930_20210428d1_docr_lidar.raa
20210430::194930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.6dbar, CTD 34.4psu, index 1.34, Packet 22430
20210430::194930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::194939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194940_20210428d1_docr_lidar.raa
20210430::194949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_194950_20210428d1_docr_lidar.raa
20210430::194959: Head 1: Time Synchronization: 2021.04.30   19:50:00::0015
20210430::195000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195000_20210428d1_docr_lidar.raa
20210430::195000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 990.1dbar, CTD 34.4psu, index 1.34, Packet 22483
20210430::195000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195010_20210428d1_docr_lidar.raa
20210430::195020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195020_20210428d1_docr_lidar.raa
20210430::195029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195030_20210428d1_docr_lidar.raa
20210430::195030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.6dbar, CTD 34.5psu, index 1.34, Packet 22537
20210430::195030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195040_20210428d1_docr_lidar.raa
20210430::195049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195050_20210428d1_docr_lidar.raa
20210430::195059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195100_20210428d1_docr_lidar.raa
20210430::195100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.0dbar, CTD 34.4psu, index 1.34, Packet 22590
20210430::195100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195110: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195110_20210428d1_docr_lidar.raa
20210430::195119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195120_20210428d1_docr_lidar.raa
20210430::195129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195130_20210428d1_docr_lidar.raa
20210430::195130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.4dbar, CTD 34.4psu, index 1.34, Packet 22643
20210430::195130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195140_20210428d1_docr_lidar.raa
20210430::195149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195150_20210428d1_docr_lidar.raa
20210430::195159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195200_20210428d1_docr_lidar.raa
20210430::195200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 995.1dbar, CTD 34.4psu, index 1.34, Packet 22697
20210430::195200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195210_20210428d1_docr_lidar.raa
20210430::195219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195220_20210428d1_docr_lidar.raa
20210430::195229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195230_20210428d1_docr_lidar.raa
20210430::195230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.4dbar, CTD 34.4psu, index 1.34, Packet 22751
20210430::195230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195240_20210428d1_docr_lidar.raa
20210430::195249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195250_20210428d1_docr_lidar.raa
20210430::195259: Head 1: Time Synchronization: 2021.04.30   19:53:00::0015
20210430::195259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195300_20210428d1_docr_lidar.raa
20210430::195300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.0dbar, CTD 34.5psu, index 1.34, Packet 22804
20210430::195300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195310_20210428d1_docr_lidar.raa
20210430::195319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195320_20210428d1_docr_lidar.raa
20210430::195330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.5dbar, CTD 34.5psu, index 1.34, Packet 22857
20210430::195330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195330_20210428d1_docr_lidar.raa
20210430::195330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195340_20210428d1_docr_lidar.raa
20210430::195349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195350_20210428d1_docr_lidar.raa
20210430::195400: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195400_20210428d1_docr_lidar.raa
20210430::195400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 990.0dbar, CTD 34.4psu, index 1.34, Packet 22911
20210430::195400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195410_20210428d1_docr_lidar.raa
20210430::195419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195420_20210428d1_docr_lidar.raa
20210430::195429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195430_20210428d1_docr_lidar.raa
20210430::195430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 988.5dbar, CTD 34.5psu, index 1.34, Packet 22965
20210430::195430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195440_20210428d1_docr_lidar.raa
20210430::195450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195450_20210428d1_docr_lidar.raa
20210430::195459: Head 1: Time Synchronization: 2021.04.30   19:55:00::0016
20210430::195459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195500_20210428d1_docr_lidar.raa
20210430::195500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 987.1dbar, CTD 34.5psu, index 1.34, Packet 23019
20210430::195500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195510_20210428d1_docr_lidar.raa
20210430::195519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195520_20210428d1_docr_lidar.raa
20210430::195529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195530_20210428d1_docr_lidar.raa
20210430::195530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 985.8dbar, CTD 34.5psu, index 1.34, Packet 23072
20210430::195530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195540_20210428d1_docr_lidar.raa
20210430::195549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195550_20210428d1_docr_lidar.raa
20210430::195559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195600_20210428d1_docr_lidar.raa
20210430::195600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.4dbar, CTD 34.5psu, index 1.34, Packet 23125
20210430::195600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195610_20210428d1_docr_lidar.raa
20210430::195619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195620_20210428d1_docr_lidar.raa
20210430::195630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195630: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195630_20210428d1_docr_lidar.raa
20210430::195630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 983.1dbar, CTD 34.4psu, index 1.34, Packet 23179
20210430::195630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195640_20210428d1_docr_lidar.raa
20210430::195649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195650_20210428d1_docr_lidar.raa
20210430::195659: Head 1: Time Synchronization: 2021.04.30   19:57:00::0014
20210430::195700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195700_20210428d1_docr_lidar.raa
20210430::195700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.7dbar, CTD 34.4psu, index 1.34, Packet 23232
20210430::195700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195710_20210428d1_docr_lidar.raa
20210430::195719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195720_20210428d1_docr_lidar.raa
20210430::195730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195730_20210428d1_docr_lidar.raa
20210430::195730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 980.4dbar, CTD 34.4psu, index 1.34, Packet 23286
20210430::195730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195740_20210428d1_docr_lidar.raa
20210430::195749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195750_20210428d1_docr_lidar.raa
20210430::195800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195800_20210428d1_docr_lidar.raa
20210430::195800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 979.1dbar, CTD 34.5psu, index 1.34, Packet 23339
20210430::195800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195810_20210428d1_docr_lidar.raa
20210430::195820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195820_20210428d1_docr_lidar.raa
20210430::195830: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195830_20210428d1_docr_lidar.raa
20210430::195830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 977.8dbar, CTD 34.4psu, index 1.34, Packet 23392
20210430::195830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195840_20210428d1_docr_lidar.raa
20210430::195850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195850_20210428d1_docr_lidar.raa
20210430::195859: Head 1: Time Synchronization: 2021.04.30   19:59:00::0015
20210430::195859: Head 2: Time Synchronization: 2021.04.30   19:59:00::0015
20210430::195859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195900_20210428d1_docr_lidar.raa
20210430::195900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.5dbar, CTD 34.5psu, index 1.34, Packet 23446
20210430::195900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195910_20210428d1_docr_lidar.raa
20210430::195920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195920_20210428d1_docr_lidar.raa
20210430::195929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195930_20210428d1_docr_lidar.raa
20210430::195930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.2dbar, CTD 34.4psu, index 1.34, Packet 23499
20210430::195930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::195940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195940_20210428d1_docr_lidar.raa
20210430::195949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_195950_20210428d1_docr_lidar.raa
20210430::195959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200000_20210428d1_docr_lidar.raa
20210430::200000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.9dbar, CTD 34.4psu, index 1.34, Packet 23553
20210430::200000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200010_20210428d1_docr_lidar.raa
20210430::200019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200020_20210428d1_docr_lidar.raa
20210430::200029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200030_20210428d1_docr_lidar.raa
20210430::200030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.6dbar, CTD 34.4psu, index 1.34, Packet 23606
20210430::200030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200040_20210428d1_docr_lidar.raa
20210430::200049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200050_20210428d1_docr_lidar.raa
20210430::200059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200100_20210428d1_docr_lidar.raa
20210430::200100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.8dbar, CTD 34.4psu, index 1.34, Packet 23660
20210430::200100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200110_20210428d1_docr_lidar.raa
20210430::200119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200120_20210428d1_docr_lidar.raa
20210430::200130: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200130_20210428d1_docr_lidar.raa
20210430::200130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.1dbar, CTD 34.4psu, index 1.34, Packet 23713
20210430::200130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200140_20210428d1_docr_lidar.raa
20210430::200149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200150_20210428d1_docr_lidar.raa
20210430::200200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200200_20210428d1_docr_lidar.raa
20210430::200200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.3dbar, CTD 34.4psu, index 1.34, Packet 23766
20210430::200200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200210_20210428d1_docr_lidar.raa
20210430::200219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200220_20210428d1_docr_lidar.raa
20210430::200230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200230_20210428d1_docr_lidar.raa
20210430::200230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.7dbar, CTD 34.4psu, index 1.34, Packet 23820
20210430::200230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200240_20210428d1_docr_lidar.raa
20210430::200249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200250_20210428d1_docr_lidar.raa
20210430::200300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200300_20210428d1_docr_lidar.raa
20210430::200300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.0dbar, CTD 34.4psu, index 1.34, Packet 23873
20210430::200300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200310_20210428d1_docr_lidar.raa
20210430::200319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200320_20210428d1_docr_lidar.raa
20210430::200330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.2dbar, CTD 34.4psu, index 1.34, Packet 23926
20210430::200330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200330_20210428d1_docr_lidar.raa
20210430::200330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200340_20210428d1_docr_lidar.raa
20210430::200350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200350_20210428d1_docr_lidar.raa
20210430::200359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200400_20210428d1_docr_lidar.raa
20210430::200400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 982.6dbar, CTD 34.5psu, index 1.34, Packet 23980
20210430::200400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200410_20210428d1_docr_lidar.raa
20210430::200419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200420_20210428d1_docr_lidar.raa
20210430::200429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200430_20210428d1_docr_lidar.raa
20210430::200430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.0dbar, CTD 34.4psu, index 1.34, Packet 24033
20210430::200430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200440_20210428d1_docr_lidar.raa
20210430::200449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200450_20210428d1_docr_lidar.raa
20210430::200459: Head 1: Time Synchronization: 2021.04.30   20:05:00::0015
20210430::200459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200500_20210428d1_docr_lidar.raa
20210430::200500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 985.4dbar, CTD 34.4psu, index 1.34, Packet 24087
20210430::200500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200510_20210428d1_docr_lidar.raa
20210430::200519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200520_20210428d1_docr_lidar.raa
20210430::200529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200530_20210428d1_docr_lidar.raa
20210430::200530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 986.7dbar, CTD 34.4psu, index 1.34, Packet 24140
20210430::200530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200540_20210428d1_docr_lidar.raa
20210430::200549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200550_20210428d1_docr_lidar.raa
20210430::200559: Head 2: Time Synchronization: 2021.04.30   20:06:00::0016
20210430::200600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.1dbar, CTD 34.4psu, index 1.34, Packet 24193
20210430::200600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200600_20210428d1_docr_lidar.raa
20210430::200600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200610: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200610_20210428d1_docr_lidar.raa
20210430::200619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200620_20210428d1_docr_lidar.raa
20210430::200629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200630_20210428d1_docr_lidar.raa
20210430::200630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 989.5dbar, CTD 34.4psu, index 1.34, Packet 24247
20210430::200630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200640_20210428d1_docr_lidar.raa
20210430::200650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200650_20210428d1_docr_lidar.raa
20210430::200659: Head 1: Time Synchronization: 2021.04.30   20:07:00::0014
20210430::200659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200700_20210428d1_docr_lidar.raa
20210430::200700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 991.1dbar, CTD 34.4psu, index 1.34, Packet 24300
20210430::200700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200710_20210428d1_docr_lidar.raa
20210430::200720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200720_20210428d1_docr_lidar.raa
20210430::200729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200730_20210428d1_docr_lidar.raa
20210430::200730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 992.6dbar, CTD 34.4psu, index 1.34, Packet 24354
20210430::200730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200740_20210428d1_docr_lidar.raa
20210430::200750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200750_20210428d1_docr_lidar.raa
20210430::200759: Head 1: Time Synchronization: 2021.04.30   20:08:00::0013
20210430::200759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200800_20210428d1_docr_lidar.raa
20210430::200800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.0dbar, CTD 34.4psu, index 1.34, Packet 24407
20210430::200800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200810_20210428d1_docr_lidar.raa
20210430::200820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200820_20210428d1_docr_lidar.raa
20210430::200829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200830_20210428d1_docr_lidar.raa
20210430::200830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 995.0dbar, CTD 34.4psu, index 1.34, Packet 24461
20210430::200830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200840_20210428d1_docr_lidar.raa
20210430::200849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200850_20210428d1_docr_lidar.raa
20210430::200859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200900_20210428d1_docr_lidar.raa
20210430::200900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 24514
20210430::200900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200910_20210428d1_docr_lidar.raa
20210430::200919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200920_20210428d1_docr_lidar.raa
20210430::200929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200930_20210428d1_docr_lidar.raa
20210430::200930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.2dbar, CTD 34.5psu, index 1.34, Packet 24568
20210430::200930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::200940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200940_20210428d1_docr_lidar.raa
20210430::200949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_200950_20210428d1_docr_lidar.raa
20210430::201000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201000_20210428d1_docr_lidar.raa
20210430::201000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 991.8dbar, CTD 34.5psu, index 1.34, Packet 24621
20210430::201000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201010_20210428d1_docr_lidar.raa
20210430::201019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201020_20210428d1_docr_lidar.raa
20210430::201030: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201030_20210428d1_docr_lidar.raa
20210430::201030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.2dbar, CTD 34.5psu, index 1.34, Packet 24674
20210430::201030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201040_20210428d1_docr_lidar.raa
20210430::201050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201050_20210428d1_docr_lidar.raa
20210430::201059: Head 2: Time Synchronization: 2021.04.30   20:11:00::0011
20210430::201059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201100_20210428d1_docr_lidar.raa
20210430::201100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 988.7dbar, CTD 34.5psu, index 1.34, Packet 24728
20210430::201100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201110_20210428d1_docr_lidar.raa
20210430::201120: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201120_20210428d1_docr_lidar.raa
20210430::201129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201130_20210428d1_docr_lidar.raa
20210430::201130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.4dbar, CTD 34.4psu, index 1.34, Packet 24781
20210430::201130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201140_20210428d1_docr_lidar.raa
20210430::201150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201150_20210428d1_docr_lidar.raa
20210430::201159: Head 1: Time Synchronization: 2021.04.30   20:12:00::0015
20210430::201159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201200_20210428d1_docr_lidar.raa
20210430::201200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 986.0dbar, CTD 34.4psu, index 1.34, Packet 24835
20210430::201200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201210_20210428d1_docr_lidar.raa
20210430::201220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201220_20210428d1_docr_lidar.raa
20210430::201229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201230_20210428d1_docr_lidar.raa
20210430::201230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 984.7dbar, CTD 34.4psu, index 1.34, Packet 24888
20210430::201230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201240_20210428d1_docr_lidar.raa
20210430::201249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201250_20210428d1_docr_lidar.raa
20210430::201259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201300_20210428d1_docr_lidar.raa
20210430::201300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.2dbar, CTD 34.4psu, index 1.34, Packet 24942
20210430::201300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201310_20210428d1_docr_lidar.raa
20210430::201319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201320_20210428d1_docr_lidar.raa
20210430::201329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201330_20210428d1_docr_lidar.raa
20210430::201330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 981.8dbar, CTD 34.4psu, index 1.34, Packet 24995
20210430::201330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201340_20210428d1_docr_lidar.raa
20210430::201349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201350_20210428d1_docr_lidar.raa
20210430::201359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201400_20210428d1_docr_lidar.raa
20210430::201400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 980.5dbar, CTD 34.5psu, index 1.34, Packet 25049
20210430::201400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201410_20210428d1_docr_lidar.raa
20210430::201419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201420_20210428d1_docr_lidar.raa
20210430::201429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201430_20210428d1_docr_lidar.raa
20210430::201430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.2dbar, CTD 34.4psu, index 1.34, Packet 25103
20210430::201430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201440_20210428d1_docr_lidar.raa
20210430::201449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201450_20210428d1_docr_lidar.raa
20210430::201459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201500_20210428d1_docr_lidar.raa
20210430::201500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.9dbar, CTD 34.4psu, index 1.34, Packet 25156
20210430::201500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201510_20210428d1_docr_lidar.raa
20210430::201519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201520_20210428d1_docr_lidar.raa
20210430::201529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201530_20210428d1_docr_lidar.raa
20210430::201530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.6dbar, CTD 34.4psu, index 1.34, Packet 25210
20210430::201530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201540_20210428d1_docr_lidar.raa
20210430::201549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201550_20210428d1_docr_lidar.raa
20210430::201559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201600_20210428d1_docr_lidar.raa
20210430::201600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.4dbar, CTD 34.4psu, index 1.34, Packet 25263
20210430::201600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201610_20210428d1_docr_lidar.raa
20210430::201620: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201620_20210428d1_docr_lidar.raa
20210430::201629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201630_20210428d1_docr_lidar.raa
20210430::201630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.1dbar, CTD 34.4psu, index 1.34, Packet 25317
20210430::201630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201640_20210428d1_docr_lidar.raa
20210430::201650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201650_20210428d1_docr_lidar.raa
20210430::201659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201700_20210428d1_docr_lidar.raa
20210430::201700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.5dbar, CTD 34.4psu, index 1.34, Packet 25370
20210430::201700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201710_20210428d1_docr_lidar.raa
20210430::201720: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201720_20210428d1_docr_lidar.raa
20210430::201729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201730_20210428d1_docr_lidar.raa
20210430::201730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.4dbar, CTD 34.4psu, index 1.34, Packet 25423
20210430::201730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201740_20210428d1_docr_lidar.raa
20210430::201749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201750_20210428d1_docr_lidar.raa
20210430::201759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201800_20210428d1_docr_lidar.raa
20210430::201800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.7dbar, CTD 34.4psu, index 1.34, Packet 25477
20210430::201800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201810: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201810_20210428d1_docr_lidar.raa
20210430::201820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201820_20210428d1_docr_lidar.raa
20210430::201829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201830_20210428d1_docr_lidar.raa
20210430::201830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.9dbar, CTD 34.4psu, index 1.34, Packet 25531
20210430::201830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201840_20210428d1_docr_lidar.raa
20210430::201849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201850_20210428d1_docr_lidar.raa
20210430::201900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201900_20210428d1_docr_lidar.raa
20210430::201900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.1dbar, CTD 34.4psu, index 1.34, Packet 25584
20210430::201900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201910: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201910_20210428d1_docr_lidar.raa
20210430::201919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201920_20210428d1_docr_lidar.raa
20210430::201929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201930_20210428d1_docr_lidar.raa
20210430::201930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.5dbar, CTD 34.4psu, index 1.34, Packet 25638
20210430::201930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::201939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201940_20210428d1_docr_lidar.raa
20210430::201949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_201950_20210428d1_docr_lidar.raa
20210430::201959: Head 1: Time Synchronization: 2021.04.30   20:20:00::0015
20210430::202000: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202000_20210428d1_docr_lidar.raa
20210430::202000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.8dbar, CTD 34.4psu, index 1.34, Packet 25691
20210430::202000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202010_20210428d1_docr_lidar.raa
20210430::202019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202020_20210428d1_docr_lidar.raa
20210430::202029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202030_20210428d1_docr_lidar.raa
20210430::202030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.1dbar, CTD 34.4psu, index 1.34, Packet 25744
20210430::202030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202040_20210428d1_docr_lidar.raa
20210430::202049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202050_20210428d1_docr_lidar.raa
20210430::202059: Head 1: Time Synchronization: 2021.04.30   20:21:00::0014
20210430::202100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202100_20210428d1_docr_lidar.raa
20210430::202100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.5dbar, CTD 34.4psu, index 1.34, Packet 25798
20210430::202100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202109: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202110_20210428d1_docr_lidar.raa
20210430::202119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202120_20210428d1_docr_lidar.raa
20210430::202129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202130_20210428d1_docr_lidar.raa
20210430::202130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.0dbar, CTD 34.4psu, index 1.34, Packet 25851
20210430::202130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202140_20210428d1_docr_lidar.raa
20210430::202150: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202150_20210428d1_docr_lidar.raa
20210430::202159: Head 2: Time Synchronization: 2021.04.30   20:22:00::0015
20210430::202159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202200_20210428d1_docr_lidar.raa
20210430::202200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 986.4dbar, CTD 34.4psu, index 1.34, Packet 25905
20210430::202200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202210_20210428d1_docr_lidar.raa
20210430::202220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202220_20210428d1_docr_lidar.raa
20210430::202229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202230_20210428d1_docr_lidar.raa
20210430::202230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 987.7dbar, CTD 34.4psu, index 1.34, Packet 25959
20210430::202230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202240_20210428d1_docr_lidar.raa
20210430::202249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202250_20210428d1_docr_lidar.raa
20210430::202259: Head 1: Time Synchronization: 2021.04.30   20:23:00::0015
20210430::202259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202300_20210428d1_docr_lidar.raa
20210430::202300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.1dbar, CTD 34.4psu, index 1.34, Packet 26012
20210430::202300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202310: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202310_20210428d1_docr_lidar.raa
20210430::202319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202320_20210428d1_docr_lidar.raa
20210430::202329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202330_20210428d1_docr_lidar.raa
20210430::202330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.6dbar, CTD 34.4psu, index 1.34, Packet 26066
20210430::202330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202340_20210428d1_docr_lidar.raa
20210430::202350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202350_20210428d1_docr_lidar.raa
20210430::202359: Head 1: Time Synchronization: 2021.04.30   20:24:00::0014
20210430::202359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202400_20210428d1_docr_lidar.raa
20210430::202400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 992.1dbar, CTD 34.4psu, index 1.34, Packet 26119
20210430::202400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202410_20210428d1_docr_lidar.raa
20210430::202419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202420_20210428d1_docr_lidar.raa
20210430::202429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202430_20210428d1_docr_lidar.raa
20210430::202430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 26173
20210430::202430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202440_20210428d1_docr_lidar.raa
20210430::202449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202450_20210428d1_docr_lidar.raa
20210430::202459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202500_20210428d1_docr_lidar.raa
20210430::202500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.8dbar, CTD 34.4psu, index 1.34, Packet 26226
20210430::202500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202510_20210428d1_docr_lidar.raa
20210430::202519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202520_20210428d1_docr_lidar.raa
20210430::202530: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202530_20210428d1_docr_lidar.raa
20210430::202530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 994.8dbar, CTD 34.4psu, index 1.34, Packet 26280
20210430::202530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202540_20210428d1_docr_lidar.raa
20210430::202549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202550_20210428d1_docr_lidar.raa
20210430::202559: Head 1: Time Synchronization: 2021.04.30   20:26:00::0015
20210430::202600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202600_20210428d1_docr_lidar.raa
20210430::202600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 26333
20210430::202600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202610_20210428d1_docr_lidar.raa
20210430::202619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202620_20210428d1_docr_lidar.raa
20210430::202630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202630: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202630_20210428d1_docr_lidar.raa
20210430::202630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 992.1dbar, CTD 34.4psu, index 1.34, Packet 26387
20210430::202630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202640_20210428d1_docr_lidar.raa
20210430::202649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202650_20210428d1_docr_lidar.raa
20210430::202659: Head 1: Time Synchronization: 2021.04.30   20:27:00::0016
20210430::202700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202700_20210428d1_docr_lidar.raa
20210430::202700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 990.6dbar, CTD 34.5psu, index 1.34, Packet 26440
20210430::202700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202710_20210428d1_docr_lidar.raa
20210430::202719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202720_20210428d1_docr_lidar.raa
20210430::202730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202730_20210428d1_docr_lidar.raa
20210430::202730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.1dbar, CTD 34.4psu, index 1.34, Packet 26493
20210430::202730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202740_20210428d1_docr_lidar.raa
20210430::202749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202750_20210428d1_docr_lidar.raa
20210430::202759: Head 2: Time Synchronization: 2021.04.30   20:28:00::0014
20210430::202800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202800_20210428d1_docr_lidar.raa
20210430::202800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.7dbar, CTD 34.4psu, index 1.34, Packet 26547
20210430::202800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202810_20210428d1_docr_lidar.raa
20210430::202820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202820_20210428d1_docr_lidar.raa
20210430::202829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202830_20210428d1_docr_lidar.raa
20210430::202830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.3dbar, CTD 34.4psu, index 1.34, Packet 26600
20210430::202830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202840_20210428d1_docr_lidar.raa
20210430::202849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202850_20210428d1_docr_lidar.raa
20210430::202859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202900_20210428d1_docr_lidar.raa
20210430::202900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.9dbar, CTD 34.4psu, index 1.34, Packet 26654
20210430::202900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202910_20210428d1_docr_lidar.raa
20210430::202919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202920_20210428d1_docr_lidar.raa
20210430::202929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202930_20210428d1_docr_lidar.raa
20210430::202930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.5dbar, CTD 34.4psu, index 1.34, Packet 26707
20210430::202930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::202940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202940_20210428d1_docr_lidar.raa
20210430::202949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_202950_20210428d1_docr_lidar.raa
20210430::202959: Head 2: Time Synchronization: 2021.04.30   20:30:00::0014
20210430::202959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203000_20210428d1_docr_lidar.raa
20210430::203000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.2dbar, CTD 34.4psu, index 1.34, Packet 26761
20210430::203000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203010_20210428d1_docr_lidar.raa
20210430::203019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203020_20210428d1_docr_lidar.raa
20210430::203029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203030_20210428d1_docr_lidar.raa
20210430::203030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.9dbar, CTD 34.4psu, index 1.34, Packet 26814
20210430::203030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203040_20210428d1_docr_lidar.raa
20210430::203049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203050_20210428d1_docr_lidar.raa
20210430::203100: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203100_20210428d1_docr_lidar.raa
20210430::203100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.6dbar, CTD 34.4psu, index 1.34, Packet 26867
20210430::203100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203110: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203110_20210428d1_docr_lidar.raa
20210430::203119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203120_20210428d1_docr_lidar.raa
20210430::203129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203130_20210428d1_docr_lidar.raa
20210430::203130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.3dbar, CTD 34.4psu, index 1.34, Packet 26921
20210430::203130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203140_20210428d1_docr_lidar.raa
20210430::203149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203150_20210428d1_docr_lidar.raa
20210430::203159: Head 2: Time Synchronization: 2021.04.30   20:32:00::0015
20210430::203159: Head 1: Time Synchronization: 2021.04.30   20:32:00::0018
20210430::203159: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203200_20210428d1_docr_lidar.raa
20210430::203200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.1dbar, CTD 34.4psu, index 1.34, Packet 26974
20210430::203200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203210: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203210_20210428d1_docr_lidar.raa
20210430::203219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203220_20210428d1_docr_lidar.raa
20210430::203229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203230_20210428d1_docr_lidar.raa
20210430::203230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.9dbar, CTD 34.4psu, index 1.34, Packet 27028
20210430::203230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203240: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203240_20210428d1_docr_lidar.raa
20210430::203249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203250_20210428d1_docr_lidar.raa
20210430::203259: Head 1: Time Synchronization: 2021.04.30   20:33:00::0014
20210430::203300: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203300_20210428d1_docr_lidar.raa
20210430::203300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.6dbar, CTD 34.4psu, index 1.34, Packet 27081
20210430::203300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203310_20210428d1_docr_lidar.raa
20210430::203319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203320_20210428d1_docr_lidar.raa
20210430::203330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203330_20210428d1_docr_lidar.raa
20210430::203330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.6dbar, CTD 34.4psu, index 1.34, Packet 27135
20210430::203330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203340_20210428d1_docr_lidar.raa
20210430::203349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203350_20210428d1_docr_lidar.raa
20210430::203359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203400_20210428d1_docr_lidar.raa
20210430::203400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.1dbar, CTD 34.4psu, index 1.34, Packet 27188
20210430::203400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203410_20210428d1_docr_lidar.raa
20210430::203419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203420_20210428d1_docr_lidar.raa
20210430::203429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203430_20210428d1_docr_lidar.raa
20210430::203430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.5dbar, CTD 34.4psu, index 1.34, Packet 27242
20210430::203430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203440_20210428d1_docr_lidar.raa
20210430::203450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203450_20210428d1_docr_lidar.raa
20210430::203459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203500_20210428d1_docr_lidar.raa
20210430::203500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.7dbar, CTD 34.4psu, index 1.34, Packet 27295
20210430::203500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203510_20210428d1_docr_lidar.raa
20210430::203519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203520_20210428d1_docr_lidar.raa
20210430::203529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203530_20210428d1_docr_lidar.raa
20210430::203530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.9dbar, CTD 34.4psu, index 1.34, Packet 27348
20210430::203530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203540_20210428d1_docr_lidar.raa
20210430::203549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203550_20210428d1_docr_lidar.raa
20210430::203600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203600_20210428d1_docr_lidar.raa
20210430::203600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.1dbar, CTD 34.4psu, index 1.34, Packet 27402
20210430::203600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203610_20210428d1_docr_lidar.raa
20210430::203619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203620_20210428d1_docr_lidar.raa
20210430::203629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203630_20210428d1_docr_lidar.raa
20210430::203630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.4dbar, CTD 34.4psu, index 1.34, Packet 27455
20210430::203630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203640_20210428d1_docr_lidar.raa
20210430::203650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203650_20210428d1_docr_lidar.raa
20210430::203700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203700_20210428d1_docr_lidar.raa
20210430::203700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.7dbar, CTD 34.4psu, index 1.34, Packet 27509
20210430::203700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203710_20210428d1_docr_lidar.raa
20210430::203719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203720_20210428d1_docr_lidar.raa
20210430::203729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203730_20210428d1_docr_lidar.raa
20210430::203730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.0dbar, CTD 34.4psu, index 1.34, Packet 27562
20210430::203730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203740: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203740_20210428d1_docr_lidar.raa
20210430::203749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203750_20210428d1_docr_lidar.raa
20210430::203759: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203800_20210428d1_docr_lidar.raa
20210430::203800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.5dbar, CTD 34.4psu, index 1.34, Packet 27615
20210430::203800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203810_20210428d1_docr_lidar.raa
20210430::203819: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203820_20210428d1_docr_lidar.raa
20210430::203829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203830_20210428d1_docr_lidar.raa
20210430::203830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.9dbar, CTD 34.4psu, index 1.34, Packet 27669
20210430::203830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203840_20210428d1_docr_lidar.raa
20210430::203849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203850_20210428d1_docr_lidar.raa
20210430::203859: Head 1: Time Synchronization: 2021.04.30   20:39:00::0014
20210430::203900: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203900_20210428d1_docr_lidar.raa
20210430::203900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.3dbar, CTD 34.4psu, index 1.34, Packet 27722
20210430::203900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203910_20210428d1_docr_lidar.raa
20210430::203919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203920_20210428d1_docr_lidar.raa
20210430::203930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203930_20210428d1_docr_lidar.raa
20210430::203930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.7dbar, CTD 34.4psu, index 1.34, Packet 27776
20210430::203930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::203939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203940_20210428d1_docr_lidar.raa
20210430::203949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_203950_20210428d1_docr_lidar.raa
20210430::203959: Head 1: Time Synchronization: 2021.04.30   20:40:00::0013
20210430::203959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204000_20210428d1_docr_lidar.raa
20210430::204000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.1dbar, CTD 34.4psu, index 1.34, Packet 27829
20210430::204000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204010_20210428d1_docr_lidar.raa
20210430::204020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204020_20210428d1_docr_lidar.raa
20210430::204029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204030_20210428d1_docr_lidar.raa
20210430::204030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.6dbar, CTD 34.4psu, index 1.34, Packet 27883
20210430::204030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204040_20210428d1_docr_lidar.raa
20210430::204049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204050_20210428d1_docr_lidar.raa
20210430::204059: Head 1: Time Synchronization: 2021.04.30   20:41:00::0013
20210430::204059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204100_20210428d1_docr_lidar.raa
20210430::204100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.1dbar, CTD 34.4psu, index 1.34, Packet 27937
20210430::204100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204110: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204110_20210428d1_docr_lidar.raa
20210430::204119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204120_20210428d1_docr_lidar.raa
20210430::204129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204130_20210428d1_docr_lidar.raa
20210430::204130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.4dbar, CTD 34.4psu, index 1.34, Packet 27990
20210430::204130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204139: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204140_20210428d1_docr_lidar.raa
20210430::204149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204150_20210428d1_docr_lidar.raa
20210430::204200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204200_20210428d1_docr_lidar.raa
20210430::204200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 994.6dbar, CTD 34.4psu, index 1.34, Packet 28044
20210430::204200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204210_20210428d1_docr_lidar.raa
20210430::204220: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204220_20210428d1_docr_lidar.raa
20210430::204229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204230_20210428d1_docr_lidar.raa
20210430::204230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.5dbar, CTD 34.4psu, index 1.34, Packet 28097
20210430::204230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204240_20210428d1_docr_lidar.raa
20210430::204249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204250_20210428d1_docr_lidar.raa
20210430::204259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204300_20210428d1_docr_lidar.raa
20210430::204300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.0dbar, CTD 34.4psu, index 1.34, Packet 28151
20210430::204300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204310_20210428d1_docr_lidar.raa
20210430::204319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204320_20210428d1_docr_lidar.raa
20210430::204329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204330_20210428d1_docr_lidar.raa
20210430::204330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.6dbar, CTD 34.4psu, index 1.34, Packet 28204
20210430::204330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204340_20210428d1_docr_lidar.raa
20210430::204349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204350_20210428d1_docr_lidar.raa
20210430::204359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204400_20210428d1_docr_lidar.raa
20210430::204400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.2dbar, CTD 34.4psu, index 1.34, Packet 28258
20210430::204400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204410_20210428d1_docr_lidar.raa
20210430::204419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204420_20210428d1_docr_lidar.raa
20210430::204430: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204430_20210428d1_docr_lidar.raa
20210430::204430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.9dbar, CTD 34.4psu, index 1.34, Packet 28311
20210430::204430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204439: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204440_20210428d1_docr_lidar.raa
20210430::204449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204450_20210428d1_docr_lidar.raa
20210430::204500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204500_20210428d1_docr_lidar.raa
20210430::204500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.5dbar, CTD 34.4psu, index 1.34, Packet 28365
20210430::204500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204510_20210428d1_docr_lidar.raa
20210430::204520: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204520_20210428d1_docr_lidar.raa
20210430::204529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204530_20210428d1_docr_lidar.raa
20210430::204530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.1dbar, CTD 34.4psu, index 1.34, Packet 28418
20210430::204530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204540_20210428d1_docr_lidar.raa
20210430::204550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204550_20210428d1_docr_lidar.raa
20210430::204559: Head 1: Time Synchronization: 2021.04.30   20:46:00::0014
20210430::204559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204600_20210428d1_docr_lidar.raa
20210430::204600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.6dbar, CTD 34.4psu, index 1.34, Packet 28471
20210430::204600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204610_20210428d1_docr_lidar.raa
20210430::204620: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204620_20210428d1_docr_lidar.raa
20210430::204629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204630_20210428d1_docr_lidar.raa
20210430::204630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.3dbar, CTD 34.4psu, index 1.34, Packet 28525
20210430::204630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204640_20210428d1_docr_lidar.raa
20210430::204650: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204650_20210428d1_docr_lidar.raa
20210430::204659: Head 1: Time Synchronization: 2021.04.30   20:47:00::0013
20210430::204659: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204700_20210428d1_docr_lidar.raa
20210430::204700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.1dbar, CTD 34.4psu, index 1.34, Packet 28579
20210430::204700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204710: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204710_20210428d1_docr_lidar.raa
20210430::204719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204720_20210428d1_docr_lidar.raa
20210430::204729: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204730_20210428d1_docr_lidar.raa
20210430::204730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.8dbar, CTD 34.4psu, index 1.34, Packet 28632
20210430::204730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204740_20210428d1_docr_lidar.raa
20210430::204749: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204750_20210428d1_docr_lidar.raa
20210430::204800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.6dbar, CTD 34.4psu, index 1.34, Packet 28685
20210430::204800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204800_20210428d1_docr_lidar.raa
20210430::204809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204810_20210428d1_docr_lidar.raa
20210430::204820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204820_20210428d1_docr_lidar.raa
20210430::204829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204830_20210428d1_docr_lidar.raa
20210430::204830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.4dbar, CTD 34.4psu, index 1.34, Packet 28739
20210430::204830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204840: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204840_20210428d1_docr_lidar.raa
20210430::204849: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204850_20210428d1_docr_lidar.raa
20210430::204859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204900_20210428d1_docr_lidar.raa
20210430::204900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.3dbar, CTD 34.4psu, index 1.34, Packet 28793
20210430::204900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204910_20210428d1_docr_lidar.raa
20210430::204919: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204920_20210428d1_docr_lidar.raa
20210430::204930: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204930_20210428d1_docr_lidar.raa
20210430::204930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 974.9dbar, CTD 34.4psu, index 1.34, Packet 28846
20210430::204930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::204939: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204940_20210428d1_docr_lidar.raa
20210430::204949: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_204950_20210428d1_docr_lidar.raa
20210430::204959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205000_20210428d1_docr_lidar.raa
20210430::205000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.5dbar, CTD 34.4psu, index 1.34, Packet 28899
20210430::205000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205009: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205010_20210428d1_docr_lidar.raa
20210430::205020: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205020_20210428d1_docr_lidar.raa
20210430::205029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205030_20210428d1_docr_lidar.raa
20210430::205030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 973.3dbar, CTD 34.4psu, index 1.34, Packet 28953
20210430::205030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 34.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205039: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205040_20210428d1_docr_lidar.raa
20210430::205050: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205050_20210428d1_docr_lidar.raa
20210430::205059: Head 1: Time Synchronization: 2021.04.30   20:51:00::0015
20210430::205059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205100_20210428d1_docr_lidar.raa
20210430::205100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.1dbar, CTD 34.4psu, index 1.34, Packet 29006
20210430::205100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205110: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205110_20210428d1_docr_lidar.raa
20210430::205119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205120_20210428d1_docr_lidar.raa
20210430::205129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205130_20210428d1_docr_lidar.raa
20210430::205130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.5dbar, CTD 34.4psu, index 1.34, Packet 29060
20210430::205130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205140_20210428d1_docr_lidar.raa
20210430::205149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205150_20210428d1_docr_lidar.raa
20210430::205159: Head 1: Time Synchronization: 2021.04.30   20:52:00::0015
20210430::205200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205200_20210428d1_docr_lidar.raa
20210430::205200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.6dbar, CTD 34.4psu, index 1.34, Packet 29113
20210430::205200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205210_20210428d1_docr_lidar.raa
20210430::205219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205220_20210428d1_docr_lidar.raa
20210430::205230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.9dbar, CTD 34.4psu, index 1.34, Packet 29166
20210430::205230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205230: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205230_20210428d1_docr_lidar.raa
20210430::205230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205240_20210428d1_docr_lidar.raa
20210430::205249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205250_20210428d1_docr_lidar.raa
20210430::205259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205300_20210428d1_docr_lidar.raa
20210430::205300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.2dbar, CTD 34.4psu, index 1.34, Packet 29220
20210430::205300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205310_20210428d1_docr_lidar.raa
20210430::205319: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205320_20210428d1_docr_lidar.raa
20210430::205329: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205330_20210428d1_docr_lidar.raa
20210430::205330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 981.5dbar, CTD 34.4psu, index 1.34, Packet 29274
20210430::205330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205340: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205340_20210428d1_docr_lidar.raa
20210430::205349: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205350_20210428d1_docr_lidar.raa
20210430::205359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205400_20210428d1_docr_lidar.raa
20210430::205400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.7dbar, CTD 34.4psu, index 1.34, Packet 29327
20210430::205400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205410: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205410_20210428d1_docr_lidar.raa
20210430::205419: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205420_20210428d1_docr_lidar.raa
20210430::205429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205430_20210428d1_docr_lidar.raa
20210430::205430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.0dbar, CTD 34.4psu, index 1.34, Packet 29381
20210430::205430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205440_20210428d1_docr_lidar.raa
20210430::205449: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205450_20210428d1_docr_lidar.raa
20210430::205459: Head 1: Time Synchronization: 2021.04.30   20:55:00::0015
20210430::205500: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205500_20210428d1_docr_lidar.raa
20210430::205500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.4dbar, CTD 34.4psu, index 1.34, Packet 29435
20210430::205500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205509: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205510_20210428d1_docr_lidar.raa
20210430::205519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205520_20210428d1_docr_lidar.raa
20210430::205529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205530_20210428d1_docr_lidar.raa
20210430::205530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 986.8dbar, CTD 34.4psu, index 1.34, Packet 29488
20210430::205530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205539: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205540_20210428d1_docr_lidar.raa
20210430::205550: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205550_20210428d1_docr_lidar.raa
20210430::205559: Head 1: Time Synchronization: 2021.04.30   20:56:00::0014
20210430::205559: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205600_20210428d1_docr_lidar.raa
20210430::205600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.1dbar, CTD 34.4psu, index 1.34, Packet 29541
20210430::205600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205610: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205610_20210428d1_docr_lidar.raa
20210430::205619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205620_20210428d1_docr_lidar.raa
20210430::205629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205630_20210428d1_docr_lidar.raa
20210430::205630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 989.6dbar, CTD 34.4psu, index 1.34, Packet 29595
20210430::205630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205640_20210428d1_docr_lidar.raa
20210430::205649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205650_20210428d1_docr_lidar.raa
20210430::205659: Head 1: Time Synchronization: 2021.04.30   20:57:00::0015
20210430::205700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.9dbar, CTD 34.4psu, index 1.34, Packet 29648
20210430::205700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205700: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205700_20210428d1_docr_lidar.raa
20210430::205709: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205710_20210428d1_docr_lidar.raa
20210430::205719: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205720_20210428d1_docr_lidar.raa
20210430::205730: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205730_20210428d1_docr_lidar.raa
20210430::205730: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.4dbar, CTD 34.4psu, index 1.34, Packet 29702
20210430::205730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205739: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205740_20210428d1_docr_lidar.raa
20210430::205750: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205750_20210428d1_docr_lidar.raa
20210430::205800: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205800_20210428d1_docr_lidar.raa
20210430::205800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205800: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.6dbar, CTD 34.4psu, index 1.34, Packet 29756
20210430::205800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205809: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205810_20210428d1_docr_lidar.raa
20210430::205820: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205820_20210428d1_docr_lidar.raa
20210430::205829: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205830_20210428d1_docr_lidar.raa
20210430::205830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205830: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.4dbar, CTD 34.4psu, index 1.34, Packet 29810
20210430::205830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205839: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205840_20210428d1_docr_lidar.raa
20210430::205850: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205850_20210428d1_docr_lidar.raa
20210430::205859: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205900_20210428d1_docr_lidar.raa
20210430::205900: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 992.4dbar, CTD 34.4psu, index 1.34, Packet 29863
20210430::205900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205909: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205910_20210428d1_docr_lidar.raa
20210430::205920: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205920_20210428d1_docr_lidar.raa
20210430::205929: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205930_20210428d1_docr_lidar.raa
20210430::205930: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 991.3dbar, CTD 34.4psu, index 1.34, Packet 29916
20210430::205930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::205940: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205940_20210428d1_docr_lidar.raa
20210430::205950: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_205950_20210428d1_docr_lidar.raa
20210430::205959: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210000_20210428d1_docr_lidar.raa
20210430::210000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210000: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 990.0dbar, CTD 34.4psu, index 1.34, Packet 29970
20210430::210000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210010: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210010_20210428d1_docr_lidar.raa
20210430::210019: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210020_20210428d1_docr_lidar.raa
20210430::210029: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210030_20210428d1_docr_lidar.raa
20210430::210030: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 988.7dbar, CTD 34.4psu, index 1.34, Packet 30023
20210430::210030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210040: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210040_20210428d1_docr_lidar.raa
20210430::210049: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210050_20210428d1_docr_lidar.raa
20210430::210059: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210100_20210428d1_docr_lidar.raa
20210430::210100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210100: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 987.2dbar, CTD 34.4psu, index 1.34, Packet 30077
20210430::210100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210110: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210110_20210428d1_docr_lidar.raa
20210430::210119: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210120_20210428d1_docr_lidar.raa
20210430::210129: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210130_20210428d1_docr_lidar.raa
20210430::210130: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 985.9dbar, CTD 34.4psu, index 1.34, Packet 30130
20210430::210130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210140: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210140_20210428d1_docr_lidar.raa
20210430::210149: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210150_20210428d1_docr_lidar.raa
20210430::210159: Head 1: Time Synchronization: 2021.04.30   21:02:00::0014
20210430::210200: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 984.7dbar, CTD 34.4psu, index 1.34, Packet 30183
20210430::210200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210200: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210200_20210428d1_docr_lidar.raa
20210430::210200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210209: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210210_20210428d1_docr_lidar.raa
20210430::210219: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210220_20210428d1_docr_lidar.raa
20210430::210229: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210230_20210428d1_docr_lidar.raa
20210430::210230: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 983.4dbar, CTD 34.4psu, index 1.34, Packet 30237
20210430::210230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210239: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210240_20210428d1_docr_lidar.raa
20210430::210249: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210250_20210428d1_docr_lidar.raa
20210430::210259: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210300_20210428d1_docr_lidar.raa
20210430::210300: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 982.2dbar, CTD 34.4psu, index 1.34, Packet 30290
20210430::210300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210309: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210310_20210428d1_docr_lidar.raa
20210430::210320: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210320_20210428d1_docr_lidar.raa
20210430::210330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210330: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210330_20210428d1_docr_lidar.raa
20210430::210330: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 980.9dbar, CTD 34.4psu, index 1.34, Packet 30344
20210430::210330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210339: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210340_20210428d1_docr_lidar.raa
20210430::210350: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210350_20210428d1_docr_lidar.raa
20210430::210359: Head 1: Time Synchronization: 2021.04.30   21:04:00::0015
20210430::210359: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210400_20210428d1_docr_lidar.raa
20210430::210400: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 979.5dbar, CTD 34.4psu, index 1.34, Packet 30397
20210430::210400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210409: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210410_20210428d1_docr_lidar.raa
20210430::210420: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210420_20210428d1_docr_lidar.raa
20210430::210429: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210430_20210428d1_docr_lidar.raa
20210430::210430: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 978.2dbar, CTD 34.4psu, index 1.34, Packet 30450
20210430::210430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210440: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210440_20210428d1_docr_lidar.raa
20210430::210450: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210450_20210428d1_docr_lidar.raa
20210430::210459: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210500_20210428d1_docr_lidar.raa
20210430::210500: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 977.1dbar, CTD 34.4psu, index 1.34, Packet 30504
20210430::210500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210510: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210510_20210428d1_docr_lidar.raa
20210430::210519: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210520_20210428d1_docr_lidar.raa
20210430::210529: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210530_20210428d1_docr_lidar.raa
20210430::210530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210530: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 975.9dbar, CTD 34.4psu, index 1.34, Packet 30557
20210430::210530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210540: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210540_20210428d1_docr_lidar.raa
20210430::210549: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210550_20210428d1_docr_lidar.raa
20210430::210559: Head 1: Time Synchronization: 2021.04.30   21:06:00::0013
20210430::210600: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210600_20210428d1_docr_lidar.raa
20210430::210600: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 974.3dbar, CTD 34.4psu, index 1.34, Packet 30610
20210430::210600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 22.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210609: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210610_20210428d1_docr_lidar.raa
20210430::210619: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210620_20210428d1_docr_lidar.raa
20210430::210629: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210630_20210428d1_docr_lidar.raa
20210430::210630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210630: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 972.4dbar, CTD 34.4psu, index 1.34, Packet 30664
20210430::210630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20210430::210639: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210640_20210428d1_docr_lidar.raa
20210430::210649: GUI: Archiving data to file --> C:\Data\20210428d1\20210430_210650_20210428d1_docr_lidar.raa
20210430::210658: GUI: Live mode ON.
20210430::210658: GUI: Requesing STOP operation, Head 1
20210430::210658: GUI: Requesing STOP operation, Head 2
20210430::210659: Head 1: Received request: STOP
20210430::210659: Head 2: Received request: STOP
20210430::210659: Head 1: Stopping Scan Operation
20210430::210659: Head 2: Stopping Scan Operation
20210430::210700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 0
20210430::210700: System  Initialized, Gain 8, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 972.3dbar, CTD 34.4psu, index 1.34, Packet 30718
20210430::210700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20210430::210701: Head 1: ProcessingMgr stopped all worker threads.
20210430::210701: Head 2: ProcessingMgr stopped all worker threads.
20210430::210701: Head 1:       Stop finished, may now recover.
20210430::210702: Head 2:       Stop finished, may now recover.
20210430::210703: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210430::210704: Head 2: Eye Safe Optical Filter check Passed
20210430::210704: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210430::210704: Head 1: Eye Safe Optical Filter check Passed
20210430::210730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 968.9dbar, CTD 34.4psu, index 1.34, Packet 30771
20210430::210730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 954.3dbar, CTD 34.4psu, index 1.34, Packet 30824
20210430::210800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 945.8dbar, CTD 34.4psu, index 1.34, Packet 30878
20210430::210830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 932.4dbar, CTD 34.4psu, index 1.34, Packet 30931
20210430::210900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 918.1dbar, CTD 34.4psu, index 1.34, Packet 30985
20210430::210930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::210930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 900.6dbar, CTD 34.4psu, index 1.34, Packet 31038
20210430::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 882.0dbar, CTD 34.4psu, index 1.34, Packet 31092
20210430::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211059: Head 1: Time Synchronization: 2021.04.30   21:11:00::0015
20210430::211100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 863.1dbar, CTD 34.4psu, index 1.34, Packet 31145
20210430::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 845.1dbar, CTD 34.4psu, index 1.34, Packet 31198
20210430::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 826.4dbar, CTD 34.4psu, index 1.34, Packet 31252
20210430::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 807.0dbar, CTD 34.4psu, index 1.34, Packet 31305
20210430::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 786.2dbar, CTD 34.4psu, index 1.34, Packet 31359
20210430::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 766.1dbar, CTD 34.4psu, index 1.34, Packet 31413
20210430::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 19.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 747.4dbar, CTD 34.4psu, index 1.34, Packet 31466
20210430::211400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211425: Head 1: Comm CTD Error, disconnecting
20210430::211425: Head 2: Comm CTD Error, disconnecting
20210430::211426: Head 1: Warning, CTD not recieved within 2 minutes.
20210430::211426: Head 2: Warning, CTD not recieved within 2 minutes.
20210430::211426: Head 1: Restarting CTD Ethernet connection ...
20210430::211426: Head 2: Restarting CTD Ethernet connection ...
20210430::211430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31520
20210430::211430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31573
20210430::211500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31627
20210430::211530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31680
20210430::211600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31733
20210430::211630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31787
20210430::211700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31840
20210430::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31893
20210430::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 31947
20210430::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::211845: GUI: OnBnClickedOk
20210430::211845: GUI: Exiting the WiSSL GUI..
20210430::211845: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210430::211845: GUI: Wrote configuration data.
20210430::212334: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210430::212334: GUI: Live mode ON.
20210430::212334: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210430::212334: GUI: WiSSL GUI started at 2021_04_30_21:23:34
20210430::212334: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_30.txt
20210430::212334: GUI: Attempting Communications with Head 1...
20210430::212334: GUI: Attempting Communications with Head 2...
20210430::212338: GUI: Established Communications with Head 1.
20210430::212338: GUI: Established Communications with Head 2.
20210430::212339: Head 2: Lost Communications with GUI
20210430::212339: Head 1: Lost Communications with GUI
20210430::212339: Head 2: Initializing Communications with GUI ...
20210430::212339: Head 1: Initializing Communications with GUI ...
20210430::212339: Head 2: Communications Established.
20210430::212340: Head 1: Communications Established.
20210430::212400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 32013
20210430::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 11C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 32066
20210430::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 18.0C, Dig 33.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 730.8dbar, CTD 34.4psu, index 1.34, Packet 32120
20210430::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 27%, OPB 12C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20210430::212500: GUI: OnBnClickedOk
20210430::212500: GUI: Exiting the WiSSL GUI..
20210430::212500: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210430::212500: GUI: Wrote configuration data.
