20201008::170459: GUI: OnBnClickedOk
20201008::170459: GUI: Exiting the WiSSL GUI..
20201008::170459: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20201008::170459: GUI: Wrote configuration data.
20201008::173854: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20201008::173854: GUI: Live mode ON.
20201008::173854: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20201008::173854: GUI: WiSSL GUI started at 2020_10_08_17:38:54
20201008::173854: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2020_10_08.txt
20201008::173854: GUI: Attempting Communications with Head 1...
20201008::173854: GUI: Attempting Communications with Head 2...
20201008::174020: GUI: Established Communications with Head 1.
20201008::174021: Head 1: Initializing Communications with GUI ...
20201008::174022: Head 1: Communications Established.
20201008::174023: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201008::174023: GUI: Established Communications with Head 2.
20201008::174023: Head 1: Connection Established with the GUI.
20201008::174023: Head 1: Initializing Subsystems, standby ...
20201008::174024: Head 1: Initializing Hardware, Stand by ...
20201008::174024: Head 2: Initializing Communications with GUI ...
20201008::174025: Head 2: Communications Established.
20201008::174026: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201008::174026: Head 2: Connection Established with the GUI.
20201008::174027: Head 2: Initializing Subsystems, standby ...
20201008::174027: Head 2: Initializing Hardware, Stand by ...
20201008::174030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174030: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 18
20201008::174030: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174037: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201008::174037: Head 1: NtQuery - testing 1 ...
20201008::174038: Head 1: clock resolution: 10
20201008::174038: Head 1: NtQuery - testing 2, after setting max res ...
20201008::174038: Head 1: clock resolution: 10
20201008::174038: Head 1: Initializing Optics Electronics ...
20201008::174039: Head 1: Power Laser Controller
20201008::174043: Head 1: Power Scanner Controller
20201008::174045: Head 1: Power OPTO Sensor
20201008::174045: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201008::174046: Head 2: NtQuery - testing 1 ...
20201008::174046: Head 2: clock resolution: 10
20201008::174046: Head 2: NtQuery - testing 2, after setting max res ...
20201008::174047: Head 2: clock resolution: 10
20201008::174047: Head 2: Initializing Optics Electronics ...
20201008::174047: Head 2: Power Laser Controller
20201008::174051: Head 2: Power Scanner Controller
20201008::174053: Head 2: Power OPTO Sensor
20201008::174100: System NOT Initialized, Gain 0, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 71
20201008::174100: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174100: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174105: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201008::174105: Head 1: Eye Safe Optical Filter check Passed
20201008::174105: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201008::174106: Head 1: Initializing Time Sync Subsystem.
20201008::174106: Head 1: Initializing CTD Subsystem.
20201008::174106: Head 1: CTD Initialization Successful
20201008::174107: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201008::174107: Head 1: Time Sync UDP started, waiting for sync...
20201008::174107: Head 1: Attempting CTD Ethernet connection with ROV...
20201008::174108: Head 1: Time Synchronization Achieved: 2020.10.08   17:41:09::0014
20201008::174113: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201008::174113: Head 2: Eye Safe Optical Filter check Passed
20201008::174114: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201008::174114: Head 2: Initializing Time Sync Subsystem.
20201008::174114: Head 2: Initializing CTD Subsystem.
20201008::174115: Head 2: CTD Initialization Successful
20201008::174115: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201008::174115: Head 2: Time Sync UDP started, waiting for sync...
20201008::174116: Head 2: Attempting CTD Ethernet connection with ROV...
20201008::174117: Head 2: Time Synchronization Achieved: 2020.10.08   17:41:18::0015
20201008::174130: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 124
20201008::174130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 27%, OPB 19C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 28%, OPB 18C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 18C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174200: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 178
20201008::174200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 19C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174227: Head 2: CTD Ethernet connection established.
20201008::174227: Head 1: CTD Ethernet connection established.
20201008::174230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 231
20201008::174230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 20C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 19C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174300: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 1.8dbar, CTD 0.0psu, index 1.34, Packet 285
20201008::174300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174330: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 339
20201008::174330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174400: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 394
20201008::174400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174430: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 450
20201008::174430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174500: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 505
20201008::174500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174530: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 559
20201008::174530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 21C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174600: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 612
20201008::174600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 666
20201008::174630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 719
20201008::174700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 19%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174730: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 773
20201008::174730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174800: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 826
20201008::174800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 19%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 879
20201008::174830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 19%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 19%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 933
20201008::174900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174930: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 986
20201008::174930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::174930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 19%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175000: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1039
20201008::175000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 19%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175030: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1093
20201008::175030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 19%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175100: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1146
20201008::175100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 19%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 19%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175130: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1200
20201008::175130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175200: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1253
20201008::175200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175230: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1306
20201008::175230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175300: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1360
20201008::175300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175315: Head 2: Comm CTD Error, disconnecting
20201008::175315: Head 1: Comm CTD Error, disconnecting
20201008::175316: Head 2: Warning, CTD not recieved within 2 minutes.
20201008::175316: Head 1: Warning, CTD not recieved within 2 minutes.
20201008::175316: Head 2: Restarting CTD Ethernet connection ...
20201008::175316: Head 1: Restarting CTD Ethernet connection ...
20201008::175330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175330: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1413
20201008::175330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175400: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1467
20201008::175400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175430: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1520
20201008::175430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175500: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1574
20201008::175500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175530: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1627
20201008::175530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175600: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1681
20201008::175600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175630: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1734
20201008::175630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175700: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1788
20201008::175700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175730: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1841
20201008::175730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175759: Head 1: Time Synchronization: 2020.10.08   17:58:00::0017
20201008::175759: Head 2: Time Synchronization: 2020.10.08   17:58:00::0017
20201008::175800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175800: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1895
20201008::175800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175830: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 1948
20201008::175830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175900: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2002
20201008::175900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175930: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2055
20201008::175930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::175930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180000: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2108
20201008::180000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 29.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180030: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2162
20201008::180030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 30.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180059: Head 1: Time Synchronization: 2020.10.08   18:01:00::0015
20201008::180100: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2215
20201008::180100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 30.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 23C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180130: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 19.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2269
20201008::180130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 30.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180200: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 1.9dbar, CTD 0.0psu, index 1.34, Packet 2323
20201008::180200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 30.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20201008::180205: Head 2: CTD Ethernet connection established.
20201008::180205: Head 1: CTD Ethernet connection established.
20201008::180214: GUI: Live mode ON.
20201008::180214: GUI: Requesing START operation, Head 1
20201008::180214: GUI: Requesing START operation, Head 2
20201008::180215: Head 2: Received request: START
20201008::180215: Head 1: Received request: START
20201008::180215: Head 2: Starting Scan Operation
20201008::180215: Head 1: Starting Scan Operation
20201008::180216: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201008::180217: Head 2: Eye Safe Optical Filter check Passed
20201008::180218: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20201008::180218: Head 1: Eye Safe Optical Filter check Passed
20201008::180227: Head 2: Configured for WATER Processing
20201008::180227: Head 2: Configured for WATER Processing
20201008::180228: Head 2: Configured for WATER Processing
20201008::180228: Head 2: Configured for WATER Processing
20201008::180228: Head 2: Configured for WATER Processing
20201008::180229: Head 2: Configured for WATER Processing
20201008::180229: Head 2: Configured for WATER Processing
20201008::180229: Head 2: Configured for WATER Processing
20201008::180230: Head 2: Configured for WATER Processing
20201008::180230: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2376
20201008::180230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 24C, Laser 30.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 1
20201008::180230: Head 2: Configured for WATER Processing
20201008::180230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 4.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 23C, Laser 29.0C, Dig 44.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180230: Head 2: Configured for WATER Processing
20201008::180230: Head 2: Configured for WATER Processing
20201008::180231: Head 2: Configured for WATER Processing
20201008::180231: Head 2: Configured for WATER Processing
20201008::180231: Head 2: Configured for WATER Processing
20201008::180232: Head 2: Configured for WATER Processing
20201008::180232: Head 2: Configured for WATER Processing
20201008::180232: Head 2: Configured for WATER Processing
20201008::180233: Head 2: Configured for WATER Processing
20201008::180233: Head 2: Configured for WATER Processing
20201008::180252: Head 1: Configured for WATER Processing
20201008::180252: Head 1: Configured for WATER Processing
20201008::180252: Head 1: Configured for WATER Processing
20201008::180252: Head 1: Configured for WATER Processing
20201008::180253: Head 1: Configured for WATER Processing
20201008::180253: Head 1: Configured for WATER Processing
20201008::180253: Head 1: Configured for WATER Processing
20201008::180254: Head 1: Configured for WATER Processing
20201008::180254: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180253_1.raa
20201008::180254: Head 1: Configured for WATER Processing
20201008::180254: Head 1: Configured for WATER Processing
20201008::180255: Head 1: Configured for WATER Processing
20201008::180255: Head 1: Configured for WATER Processing
20201008::180255: Head 1: Configured for WATER Processing
20201008::180256: Head 1: Configured for WATER Processing
20201008::180256: Head 1: Configured for WATER Processing
20201008::180256: Head 1: Configured for WATER Processing
20201008::180257: Head 1: Configured for WATER Processing
20201008::180257: Head 1: Configured for WATER Processing
20201008::180258: Head 1: Configured for WATER Processing
20201008::180258: Head 1: Configured for WATER Processing
20201008::180259: Head 1: Time Synchronization: 2020.10.08   18:03:00::0016
20201008::180300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 30.0C, Dig 44.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180300: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2430
20201008::180300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 25C, Laser 31.0C, Dig 39.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180302: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180303_1.raa
20201008::180312: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180313_1.raa
20201008::180322: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180323_1.raa
20201008::180330: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2483
20201008::180330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 25C, Laser 32.0C, Dig 41.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 30.0C, Dig 46.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180332: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180333_1.raa
20201008::180342: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180343_1.raa
20201008::180352: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180353_1.raa
20201008::180358: Head 2: Time Synchronization: 2020.10.08   18:04:00::0016
20201008::180359: Head 1: Time Synchronization: 2020.10.08   18:04:00::0016
20201008::180400: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2537
20201008::180400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 25C, Laser 32.0C, Dig 41.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 31.0C, Dig 46.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180402: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180403_1.raa
20201008::180412: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180413_1.raa
20201008::180422: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180423_1.raa
20201008::180430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 31.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180430: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2590
20201008::180430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 25C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180432: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180433_1.raa
20201008::180442: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180443_1.raa
20201008::180452: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180453_1.raa
20201008::180459: Head 1: Time Synchronization: 2020.10.08   18:05:00::0016
20201008::180500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 31.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180500: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2644
20201008::180500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 25C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180502: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180503_1.raa
20201008::180512: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180513_1.raa
20201008::180522: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180523_1.raa
20201008::180530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 31.0C, Dig 49.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180530: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2697
20201008::180530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 25C, Laser 33.0C, Dig 43.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180532: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180533_1.raa
20201008::180542: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180543_1.raa
20201008::180553: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180554_1.raa
20201008::180559: Head 1: Time Synchronization: 2020.10.08   18:06:00::0016
20201008::180600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 31.0C, Dig 49.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180600: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2750
20201008::180600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 29C, OCB 22%, OPB 25C, Laser 33.0C, Dig 43.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180603: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180604_1.raa
20201008::180613: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180614_1.raa
20201008::180623: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180624_1.raa
20201008::180630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180630: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2804
20201008::180630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 25C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180633: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180634_1.raa
20201008::180643: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180644_1.raa
20201008::180653: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180654_1.raa
20201008::180659: Head 1: Time Synchronization: 2020.10.08   18:07:00::0016
20201008::180700: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2857
20201008::180700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 44.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 24C, Laser 32.0C, Dig 50.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180703: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180704_1.raa
20201008::180713: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180714_1.raa
20201008::180723: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180724_1.raa
20201008::180730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 32.0C, Dig 51.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180730: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2911
20201008::180730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 45.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180733: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180734_1.raa
20201008::180743: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180744_1.raa
20201008::180753: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180754_1.raa
20201008::180759: Head 1: Time Synchronization: 2020.10.08   18:08:00::0016
20201008::180800: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 2964
20201008::180800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 45.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 32.0C, Dig 51.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180803: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180804_1.raa
20201008::180813: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180814_1.raa
20201008::180823: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180824_1.raa
20201008::180830: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3017
20201008::180830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 45.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 33.0C, Dig 51.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180833: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180834_1.raa
20201008::180843: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180844_1.raa
20201008::180853: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180854_1.raa
20201008::180859: Head 2: Time Synchronization: 2020.10.08   18:09:00::0015
20201008::180859: Head 1: Time Synchronization: 2020.10.08   18:09:00::0018
20201008::180900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 33.0C, Dig 51.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180900: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3071
20201008::180900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 45.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180903: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180904_1.raa
20201008::180913: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180914_1.raa
20201008::180923: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180924_1.raa
20201008::180930: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.7C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3124
20201008::180930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 33.0C, Dig 52.0C, Scan Az fault 0, gain 2, laser state 1
20201008::180933: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180934_1.raa
20201008::180943: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180944_1.raa
20201008::180953: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_180954_1.raa
20201008::180959: Head 1: Time Synchronization: 2020.10.08   18:10:00::0018
20201008::181000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 25C, Laser 33.0C, Dig 52.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181000: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3178
20201008::181000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 46.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181003: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181004_1.raa
20201008::181013: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181014_1.raa
20201008::181023: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181024_1.raa
20201008::181030: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3231
20201008::181030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 47.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 25C, Laser 33.0C, Dig 53.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181033: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181034_1.raa
20201008::181043: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181044_1.raa
20201008::181053: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181054_1.raa
20201008::181059: Head 1: Time Synchronization: 2020.10.08   18:11:00::0017
20201008::181100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 25C, Laser 33.0C, Dig 53.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181100: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3285
20201008::181100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 18.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 35.0C, Dig 47.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181103: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181104_1.raa
20201008::181113: Head 2: Comm CTD Error, disconnecting
20201008::181113: Head 1: Comm CTD Error, disconnecting
20201008::181113: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181114_1.raa
20201008::181113: Head 2: Warning, CTD not recieved within 2 minutes.
20201008::181114: Head 1: Warning, CTD not recieved within 2 minutes.
20201008::181114: Head 2: Restarting CTD Ethernet connection ...
20201008::181114: Head 1: Restarting CTD Ethernet connection ...
20201008::181123: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181124_1.raa
20201008::181130: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3338
20201008::181130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 35.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 25C, Laser 33.0C, Dig 53.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181133: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181134_1.raa
20201008::181143: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181144_1.raa
20201008::181153: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181154_1.raa
20201008::181159: Head 1: Time Synchronization: 2020.10.08   18:12:00::0016
20201008::181200: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3392
20201008::181200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 35.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 53.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181203: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181204_1.raa
20201008::181203: Head 2: CTD Ethernet connection established.
20201008::181204: Head 1: CTD Ethernet connection established.
20201008::181207: Head 2: Comm CTD Error, disconnecting
20201008::181207: Head 1: Comm CTD Error, disconnecting
20201008::181208: Head 2: Restarting CTD Ethernet connection ...
20201008::181208: Head 1: Restarting CTD Ethernet connection ...
20201008::181213: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181214_1.raa
20201008::181221: Head 2: CTD Ethernet connection established.
20201008::181221: Head 1: CTD Ethernet connection established.
20201008::181223: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181224_1.raa
20201008::181230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 54.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181230: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3446
20201008::181230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 35.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181233: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181234_1.raa
20201008::181244: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181245_1.raa
20201008::181254: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181255_1.raa
20201008::181300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 54.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181300: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3499
20201008::181300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 35.0C, Dig 48.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181304: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181305_1.raa
20201008::181314: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181315_1.raa
20201008::181324: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181325_1.raa
20201008::181330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181330: System  Initialized, Gain 3, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3552
20201008::181330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 2, laser state 1
20201008::181334: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181335_1.raa
20201008::181344: GUI: Archiving data to file --> C:\Data\Global Wall Scan 20200811\20201008_181345_1.raa
20201008::181353: GUI: Live mode ON.
20201008::181353: GUI: Requesing STOP operation, Head 1
20201008::181353: GUI: Requesing STOP operation, Head 2
20201008::181353: Head 1: Received request: STOP
20201008::181353: Head 2: Received request: STOP
20201008::181354: Head 1: Stopping Scan Operation
20201008::181354: Head 2: Stopping Scan Operation
20201008::181356: Head 1: ProcessingMgr stopped all worker threads.
20201008::181356: Head 1:       Stop finished, may now recover.
20201008::181400: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3606
20201008::181400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 2, laser state 0
20201008::181400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 2, laser state 0
20201008::181401: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20201008::181401: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201008::181402: Head 1: Eye Safe Optical Filter check Passed
20201008::181402: Head 2: Eye Safe Optical Filter check Passed
20201008::181425: Head 2: ProcessingMgr stopped all worker threads.
20201008::181426: Head 2:       Stop finished, may now recover.
20201008::181430: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3659
20201008::181430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181500: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3713
20201008::181500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181530: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3766
20201008::181530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181600: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3820
20201008::181600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181630: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3873
20201008::181630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181700: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3926
20201008::181700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 27C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 26C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181730: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 3980
20201008::181730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181800: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4033
20201008::181800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181830: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4087
20201008::181830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181900: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4141
20201008::181900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181930: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4194
20201008::181930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::181930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182000: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4248
20201008::182000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182030: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4301
20201008::182030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 34.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182100: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4355
20201008::182100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182130: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4408
20201008::182130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182200: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4461
20201008::182200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182230: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4515
20201008::182230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182300: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4568
20201008::182300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182330: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4621
20201008::182330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182400: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.9C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4675
20201008::182400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182430: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4728
20201008::182430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182430: Head 2: Comm CTD Error, disconnecting
20201008::182430: Head 1: Comm CTD Error, disconnecting
20201008::182430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 27C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182430: Head 2: Warning, CTD not recieved within 2 minutes.
20201008::182430: Head 1: Warning, CTD not recieved within 2 minutes.
20201008::182431: Head 2: Restarting CTD Ethernet connection ...
20201008::182431: Head 1: Restarting CTD Ethernet connection ...
20201008::182500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182500: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4782
20201008::182500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182530: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4836
20201008::182530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182600: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4889
20201008::182600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 33.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182630: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4942
20201008::182630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182700: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 4996
20201008::182700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182730: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5049
20201008::182730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182800: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5103
20201008::182800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182830: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5156
20201008::182830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182900: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5210
20201008::182900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182930: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.8C, CTD 2.0dbar, CTD 0.0psu, index 1.34, Packet 5263
20201008::182930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 29C, Laser 35.0C, Dig 49.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 28C, Laser 34.0C, Dig 55.0C, Scan Az fault 0, gain 0, laser state 0
20201008::182946: GUI: Lost Communications with Sensor 1.
20201008::182947: GUI: Lost Communications with Head 2.
20201008::182955: GUI: Attempting Communications with Head 1...
20201008::182955: GUI: Attempting Communications with Head 2...
20201008::183801: GUI: OnBnClickedOk
20201008::183801: GUI: Exiting the WiSSL GUI..
20201008::183801: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20201008::183801: GUI: Wrote configuration data.
