20210429::000000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000000: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3131.3dbar, CTD 34.7psu, index 1.35, Packet 63767
20210429::000000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000030: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3114.9dbar, CTD 34.7psu, index 1.35, Packet 63820
20210429::000030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000100: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3096.7dbar, CTD 34.7psu, index 1.35, Packet 63874
20210429::000100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000130: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3077.1dbar, CTD 34.7psu, index 1.35, Packet 63927
20210429::000130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 19.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000200: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3058.3dbar, CTD 34.7psu, index 1.35, Packet 63981
20210429::000200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000230: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3039.5dbar, CTD 34.7psu, index 1.35, Packet 64034
20210429::000230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000300: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3020.6dbar, CTD 34.7psu, index 1.35, Packet 64087
20210429::000300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 16.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 26%, OPB 7C, Laser 17.0C, Dig 31.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000330: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.6C, CTD 3002.3dbar, CTD 34.7psu, index 1.35, Packet 64141
20210429::000330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 28%, OPB 9C, Laser 18.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20210429::000358: GUI: OnBnClickedOk
20210429::000358: GUI: Exiting the WiSSL GUI..
20210429::000358: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210429::000358: GUI: Wrote configuration data.
20210429::131943: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210429::131943: GUI: Live mode ON.
20210429::131943: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210429::131943: GUI: WiSSL GUI started at 2021_04_29_13:19:43
20210429::131943: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_29.txt
20210429::131943: GUI: Attempting Communications with Head 1...
20210429::131943: GUI: Attempting Communications with Head 2...
20210429::131947: GUI: Established Communications with Head 1.
20210429::131947: GUI: Established Communications with Head 2.
20210429::131948: Head 1: Initializing Communications with GUI ...
20210429::131948: Head 2: Initializing Communications with GUI ...
20210429::131948: Head 2: Communications Established.
20210429::131949: Head 1: Communications Established.
20210429::131949: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210429::131950: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210429::131950: Head 2: Connection Established with the GUI.
20210429::131950: Head 1: Connection Established with the GUI.
20210429::131950: Head 2: Initializing Subsystems, standby ...
20210429::131950: Head 1: Initializing Subsystems, standby ...
20210429::131950: Head 2: Initializing Hardware, Stand by ...
20210429::131951: Head 1: Initializing Hardware, Stand by ...
20210429::132000: System NOT Initialized, Gain 0, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 28
20210429::132000: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132000: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210429::132000: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210429::132000: Head 2: NtQuery - testing 1 ...
20210429::132000: Head 1: NtQuery - testing 1 ...
20210429::132001: Head 2: clock resolution: 10
20210429::132001: Head 1: clock resolution: 10
20210429::132001: Head 2: NtQuery - testing 2, after setting max res ...
20210429::132001: Head 1: NtQuery - testing 2, after setting max res ...
20210429::132001: Head 2: clock resolution: 10
20210429::132001: Head 1: clock resolution: 10
20210429::132002: Head 2: Initializing Optics Electronics ...
20210429::132002: Head 1: Initializing Optics Electronics ...
20210429::132002: Head 2: Power Laser Controller
20210429::132002: Head 1: Power Laser Controller
20210429::132006: Head 2: Power Scanner Controller
20210429::132006: Head 1: Power Scanner Controller
20210429::132008: Head 2: Power OPTO Sensor
20210429::132008: Head 1: Power OPTO Sensor
20210429::132028: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210429::132028: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210429::132028: Head 2: Eye Safe Optical Filter check Passed
20210429::132028: Head 1: Eye Safe Optical Filter check Passed
20210429::132028: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210429::132028: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210429::132029: Head 2: Initializing Time Sync Subsystem.
20210429::132029: Head 1: Initializing Time Sync Subsystem.
20210429::132029: Head 2: Initializing CTD Subsystem.
20210429::132029: Head 1: Initializing CTD Subsystem.
20210429::132029: Head 2: CTD Initialization Successful
20210429::132029: Head 1: CTD Initialization Successful
20210429::132030: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210429::132030: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210429::132030: Head 2: Time Sync UDP started, waiting for sync...
20210429::132030: Head 1: Time Sync UDP started, waiting for sync...
20210429::132030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 15C, Laser 0.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132030: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 82
20210429::132030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 15C, Laser 0.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132030: Head 2: Attempting CTD Ethernet connection with ROV...
20210429::132030: Head 1: Attempting CTD Ethernet connection with ROV...
20210429::132031: Head 1: Time Synchronization Achieved: 2021.04.29   13:20:32::0020
20210429::132031: Head 2: Time Synchronization Achieved: 2021.04.29   13:20:32::0020
20210429::132048: Head 1: CTD Ethernet connection established.
20210429::132048: Head 2: CTD Ethernet connection established.
20210429::132100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 14.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132100: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 135
20210429::132100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 16C, Laser 15.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132130: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 1.9dbar, CTD 0.1psu, index 1.34, Packet 188
20210429::132130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 16.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 15C, Laser 15.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132200: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.2dbar, CTD 0.1psu, index 1.34, Packet 242
20210429::132200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 16C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 15C, Laser 16.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132230: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 295
20210429::132230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 16C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 16C, Laser 17.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132300: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 348
20210429::132300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 16C, Laser 17.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 16C, Laser 18.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132330: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 402
20210429::132330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 1.9dbar, CTD 0.1psu, index 1.34, Packet 455
20210429::132400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 19.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 18.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 19.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 509
20210429::132430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 20.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 16C, Laser 19.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 562
20210429::132500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 20.0C, Dig 29.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132517: GUI: Live mode ON.
20210429::132517: GUI: Requesing START operation, Head 1
20210429::132517: GUI: Requesing START operation, Head 2
20210429::132518: Head 1: Received request: START
20210429::132518: Head 2: Received request: START
20210429::132518: Head 1: Starting Scan Operation
20210429::132518: Head 2: Starting Scan Operation
20210429::132519: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20210429::132519: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210429::132520: Head 1: Eye Safe Optical Filter check Passed
20210429::132520: Head 2: Eye Safe Optical Filter check Passed
20210429::132524: Head 1: Configured for WATER Processing
20210429::132524: Head 1: Configured for WATER Processing
20210429::132525: Head 1: Configured for WATER Processing
20210429::132525: Head 1: Configured for WATER Processing
20210429::132525: Head 1: Configured for WATER Processing
20210429::132526: Head 1: Configured for WATER Processing
20210429::132526: Head 1: Configured for WATER Processing
20210429::132526: Head 1: Configured for WATER Processing
20210429::132526: Head 1: Configured for WATER Processing
20210429::132527: Head 1: Configured for WATER Processing
20210429::132527: Head 1: Configured for WATER Processing
20210429::132527: Head 1: Configured for WATER Processing
20210429::132528: GUI: Archiving data to file --> C:\Data\20210428d1\20210429_132526_20210428d1_docr_lidar.raa
20210429::132528: Head 1: Configured for WATER Processing
20210429::132528: Head 1: Configured for WATER Processing
20210429::132528: Head 1: Configured for WATER Processing
20210429::132529: Head 1: Configured for WATER Processing
20210429::132529: Head 1: Configured for WATER Processing
20210429::132529: Head 1: Configured for WATER Processing
20210429::132530: Head 1: Configured for WATER Processing
20210429::132530: Head 1: Configured for WATER Processing
20210429::132530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 19.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 1
20210429::132530: System  Initialized, Gain 4, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 616
20210429::132530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210429::132536: GUI: Archiving data to file --> C:\Data\20210428d1\20210429_132536_20210428d1_docr_lidar.raa
20210429::132545: GUI: Archiving data to file --> C:\Data\20210428d1\20210429_132546_20210428d1_docr_lidar.raa
20210429::132553: Head 2: Configured for WATER Processing
20210429::132553: Head 2: Configured for WATER Processing
20210429::132553: Head 2: Configured for WATER Processing
20210429::132554: Head 2: Configured for WATER Processing
20210429::132554: Head 2: Configured for WATER Processing
20210429::132554: Head 2: Configured for WATER Processing
20210429::132554: Head 2: Configured for WATER Processing
20210429::132555: Head 2: Configured for WATER Processing
20210429::132555: Head 2: Configured for WATER Processing
20210429::132555: GUI: Archiving data to file --> C:\Data\20210428d1\20210429_132556_20210428d1_docr_lidar.raa
20210429::132555: Head 2: Configured for WATER Processing
20210429::132556: Head 2: Configured for WATER Processing
20210429::132556: Head 2: Configured for WATER Processing
20210429::132556: Head 2: Configured for WATER Processing
20210429::132557: Head 2: Configured for WATER Processing
20210429::132557: Head 2: Configured for WATER Processing
20210429::132557: Head 2: Configured for WATER Processing
20210429::132558: Head 2: Configured for WATER Processing
20210429::132558: Head 2: Configured for WATER Processing
20210429::132558: Head 2: Configured for WATER Processing
20210429::132558: Head 2: Configured for WATER Processing
20210429::132600: System  Initialized, Gain 4, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 668
20210429::132600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20210429::132600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 20.0C, Dig 37.0C, Scan Az fault 0, gain 3, laser state 1
20210429::132604: GUI: Live mode ON.
20210429::132604: GUI: Requesing STOP operation, Head 1
20210429::132604: GUI: Requesing STOP operation, Head 2
20210429::132604: Head 1: Received request: STOP
20210429::132604: Head 2: Received request: STOP
20210429::132604: Head 1: Stopping Scan Operation
20210429::132604: Head 2: Stopping Scan Operation
20210429::132607: Head 1: ProcessingMgr stopped all worker threads.
20210429::132607: Head 1:       Stop finished, may now recover.
20210429::132610: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20210429::132610: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210429::132610: Head 1: Eye Safe Optical Filter check Passed
20210429::132610: Head 2: Eye Safe Optical Filter check Passed
20210429::132630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.3C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 723
20210429::132630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132641: Head 2: ProcessingMgr stopped all worker threads.
20210429::132642: Head 2:       Stop finished, may now recover.
20210429::132700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 776
20210429::132700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 830
20210429::132730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 883
20210429::132800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 936
20210429::132830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 17C, Laser 21.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 990
20210429::132900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::132930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1043
20210429::132930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1096
20210429::133000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1150
20210429::133030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1203
20210429::133100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1257
20210429::133130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.9C, CTD 2.9dbar, CTD 0.7psu, index 1.34, Packet 1310
20210429::133200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133230: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.4C, CTD 4.8dbar, CTD 0.9psu, index 1.34, Packet 1363
20210429::133230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.3C, CTD 4.1dbar, CTD 0.5psu, index 1.34, Packet 1417
20210429::133300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.2C, CTD 4.9dbar, CTD 0.4psu, index 1.34, Packet 1470
20210429::133330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133400: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.2C, CTD 14.5dbar, CTD 26.1psu, index 1.34, Packet 1524
20210429::133400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 24.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133430: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 13.8dbar, CTD 30.8psu, index 1.34, Packet 1577
20210429::133430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133500: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 11.8dbar, CTD 17.0psu, index 1.34, Packet 1630
20210429::133500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 23.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133530: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 10.8dbar, CTD 16.6psu, index 1.34, Packet 1684
20210429::133530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133600: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 11.2dbar, CTD 16.6psu, index 1.34, Packet 1737
20210429::133600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133630: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 10.7dbar, CTD 16.2psu, index 1.34, Packet 1791
20210429::133630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133700: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 11.7dbar, CTD 16.4psu, index 1.34, Packet 1844
20210429::133700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133730: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 11.8dbar, CTD 16.2psu, index 1.34, Packet 1897
20210429::133730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133800: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 4.3dbar, CTD 0.3psu, index 1.34, Packet 1951
20210429::133800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133830: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 3.8dbar, CTD 0.2psu, index 1.34, Packet 2004
20210429::133830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133859: Head 1: Time Synchronization: 2021.04.29   13:39:00::0013
20210429::133900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 3.1dbar, CTD 0.1psu, index 1.34, Packet 2058
20210429::133900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133915: Head 2: Comm CTD Error, disconnecting
20210429::133915: Head 1: Comm CTD Error, disconnecting
20210429::133915: Head 2: Warning, CTD not recieved within 2 minutes.
20210429::133915: Head 1: Warning, CTD not recieved within 2 minutes.
20210429::133915: Head 2: Restarting CTD Ethernet connection ...
20210429::133915: Head 1: Restarting CTD Ethernet connection ...
20210429::133930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 24.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 1.3dbar, CTD 0.1psu, index 1.34, Packet 2111
20210429::133930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 18C, Laser 25.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20210429::133941: GUI: OnBnClickedOk
20210429::133941: GUI: Exiting the WiSSL GUI..
20210429::133941: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210429::133941: GUI: Wrote configuration data.
