20210419::153312: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210419::153312: GUI: Live mode ON.
20210419::153312: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210419::153312: GUI: WiSSL GUI started at 2021_04_19_15:33:12
20210419::153312: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_04_19.txt
20210419::153312: GUI: Attempting Communications with Head 1...
20210419::153312: GUI: Attempting Communications with Head 2...
20210419::153330: System NOT Initialized, Gain 0, Elec PB 0.0C, Elec PB 0.0%, Elec PB 5V 0.0V, Elec PB 3V 0.0V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 0.00, Packet 14
20210419::153330: Head #1, Init state OFF, comm ctrl 0, comm data 0, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153333: GUI: Established Communications with Head 1.
20210419::153334: Head 1: Initializing Communications with GUI ...
20210419::153335: Head 1: Communications Established.
20210419::153336: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210419::153337: Head 1: Connection Established with the GUI.
20210419::153337: GUI: Established Communications with Head 2.
20210419::153337: Head 1: Initializing Subsystems, standby ...
20210419::153337: Head 1: Initializing Hardware, Stand by ...
20210419::153337: Head 2: Initializing Communications with GUI ...
20210419::153338: Head 2: Communications Established.
20210419::153339: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210419::153339: Head 2: Connection Established with the GUI.
20210419::153339: Head 2: Initializing Subsystems, standby ...
20210419::153340: Head 2: Initializing Hardware, Stand by ...
20210419::153348: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210419::153348: Head 1: NtQuery - testing 1 ...
20210419::153349: Head 1: clock resolution: 10
20210419::153349: Head 1: NtQuery - testing 2, after setting max res ...
20210419::153349: Head 1: clock resolution: 10
20210419::153350: Head 1: Initializing Optics Electronics ...
20210419::153350: Head 1: Power Laser Controller
20210419::153352: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210419::153353: Head 2: NtQuery - testing 1 ...
20210419::153353: Head 2: clock resolution: 10
20210419::153353: Head 2: NtQuery - testing 2, after setting max res ...
20210419::153354: Head 2: clock resolution: 10
20210419::153354: Head 1: Power Scanner Controller
20210419::153354: Head 2: Initializing Optics Electronics ...
20210419::153354: Head 2: Power Laser Controller
20210419::153356: Head 1: Power OPTO Sensor
20210419::153358: Head 2: Power Scanner Controller
20210419::153400: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153400: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 67
20210419::153400: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153400: Head 2: Power OPTO Sensor
20210419::153416: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210419::153416: Head 1: Eye Safe Optical Filter check Passed
20210419::153417: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210419::153417: Head 1: Initializing Time Sync Subsystem.
20210419::153417: Head 1: Initializing CTD Subsystem.
20210419::153417: Head 1: CTD Initialization Successful
20210419::153418: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210419::153418: Head 1: Time Sync UDP started, waiting for sync...
20210419::153418: Head 1: Attempting CTD Ethernet connection with ROV...
20210419::153419: Head 1: Time Synchronization Achieved: 2021.04.19   15:34:20::0018
20210419::153420: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210419::153420: Head 2: Eye Safe Optical Filter check Passed
20210419::153421: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210419::153421: Head 2: Initializing Time Sync Subsystem.
20210419::153421: Head 2: Initializing CTD Subsystem.
20210419::153422: Head 2: CTD Initialization Successful
20210419::153422: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210419::153422: Head 2: Time Sync UDP started, waiting for sync...
20210419::153423: Head 2: Attempting CTD Ethernet connection with ROV...
20210419::153423: Head 2: Time Synchronization Achieved: 2021.04.19   15:34:24::0018
20210419::153430: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 120
20210419::153430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 29%, OPB 19C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 29%, OPB 18C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 27%, OPB 18C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153500: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 174
20210419::153500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 27%, OPB 19C, Laser 19.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 19C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153530: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 227
20210419::153530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 25%, OPB 20C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153600: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 280
20210419::153600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 24%, OPB 20C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 24%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153630: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 334
20210419::153630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153700: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 387
20210419::153700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 21.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153730: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 440
20210419::153730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 22.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153800: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 493
20210419::153800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 20C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153830: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 547
20210419::153830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 23.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153900: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 600
20210419::153900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::153930: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 654
20210419::153930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154000: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 707
20210419::154000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 24.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154007: Head 1: CTD Ethernet connection established.
20210419::154007: Head 2: CTD Ethernet connection established.
20210419::154030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154030: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.1C, CTD 2.2dbar, CTD 1.2psu, index 1.34, Packet 761
20210419::154030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154100: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.2C, CTD 2.2dbar, CTD 1.2psu, index 1.34, Packet 814
20210419::154100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154130: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.2C, CTD 2.2dbar, CTD 1.0psu, index 1.34, Packet 867
20210419::154130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 2.2dbar, CTD 1.2psu, index 1.34, Packet 921
20210419::154200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154230: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 2.2dbar, CTD 1.0psu, index 1.34, Packet 974
20210419::154230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 25.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.8C, CTD 2.2dbar, CTD 1.0psu, index 1.34, Packet 1027
20210419::154300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.0C, CTD 2.2dbar, CTD 1.2psu, index 1.34, Packet 1081
20210419::154330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154400: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.1C, CTD 2.2dbar, CTD 1.2psu, index 1.34, Packet 1134
20210419::154400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154430: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.2C, CTD 2.2dbar, CTD 1.0psu, index 1.34, Packet 1187
20210419::154430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 26.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154500: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.4C, CTD 2.3dbar, CTD 1.2psu, index 1.34, Packet 1241
20210419::154500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154530: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 2.3dbar, CTD 1.0psu, index 1.34, Packet 1294
20210419::154530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154600: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.4C, CTD 2.3dbar, CTD 1.2psu, index 1.34, Packet 1347
20210419::154600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 21C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154630: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.2C, CTD 2.3dbar, CTD 1.0psu, index 1.34, Packet 1401
20210419::154630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 27.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154700: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.7C, CTD 2.3dbar, CTD 0.0psu, index 1.34, Packet 1454
20210419::154700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154730: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.7C, CTD 2.3dbar, CTD 0.0psu, index 1.34, Packet 1507
20210419::154730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154800: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.7C, CTD 2.3dbar, CTD 0.0psu, index 1.34, Packet 1561
20210419::154800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154810: Head 1: Comm CTD Error, disconnecting
20210419::154810: Head 2: Comm CTD Error, disconnecting
20210419::154811: Head 1: Warning, CTD not recieved within 2 minutes.
20210419::154811: Head 2: Warning, CTD not recieved within 2 minutes.
20210419::154811: Head 1: Restarting CTD Ethernet connection ...
20210419::154811: Head 2: Restarting CTD Ethernet connection ...
20210419::154830: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.7C, CTD 2.3dbar, CTD 0.0psu, index 1.34, Packet 1614
20210419::154830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 20%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 21%, OPB 22C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154900: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 17.7C, CTD 2.3dbar, CTD 0.0psu, index 1.34, Packet 1668
20210419::154900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 23C, Laser 28.0C, Dig 21.0C, Scan Az fault 0, gain 0, laser state 0
20210419::154929: GUI: OnBnClickedOk
20210419::154929: GUI: Exiting the WiSSL GUI..
20210419::154929: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210419::154929: GUI: Wrote configuration data.
