20210911::233600: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210911::233600: GUI: Live mode ON.
20210911::233600: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210911::233600: GUI: WiSSL GUI started at 2021_09_11_23:36:00
20210911::233600: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_09_11.txt
20210911::233600: GUI: Attempting Communications with Head 1...
20210911::233600: GUI: Attempting Communications with Head 2...
20210911::233643: GUI: Established Communications with Head 2.
20210911::233643: GUI: Established Communications with Head 1.
20210911::233644: Head 1: Initializing Communications with GUI ...
20210911::233644: Head 2: Initializing Communications with GUI ...
20210911::233645: Head 2: Communications Established.
20210911::233645: Head 1: Communications Established.
20210911::233645: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210911::233646: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210911::233646: Head 2: Connection Established with the GUI.
20210911::233646: Head 1: Connection Established with the GUI.
20210911::233646: Head 2: Initializing Subsystems, standby ...
20210911::233646: Head 1: Initializing Subsystems, standby ...
20210911::233646: Head 2: Initializing Hardware, Stand by ...
20210911::233646: Head 1: Initializing Hardware, Stand by ...
20210911::233657: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210911::233657: Head 1: NtQuery - testing 1 ...
20210911::233657: Head 1: clock resolution: 10
20210911::233658: Head 1: NtQuery - testing 2, after setting max res ...
20210911::233658: Head 1: clock resolution: 10
20210911::233658: Head 1: Initializing Optics Electronics ...
20210911::233659: Head 1: Power Laser Controller
20210911::233700: System NOT Initialized, Gain 0, Elec PB 22.6C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 48
20210911::233700: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233700: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233702: Head 1: Power Scanner Controller
20210911::233703: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210911::233703: Head 2: NtQuery - testing 1 ...
20210911::233704: Head 2: clock resolution: 10
20210911::233704: Head 2: NtQuery - testing 2, after setting max res ...
20210911::233704: Head 2: clock resolution: 10
20210911::233704: Head 1: Power OPTO Sensor
20210911::233705: Head 2: Initializing Optics Electronics ...
20210911::233705: Head 2: Power Laser Controller
20210911::233709: Head 2: Power Scanner Controller
20210911::233711: Head 2: Power OPTO Sensor
20210911::233724: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20210911::233725: Head 1: Eye Safe Optical Filter check Passed
20210911::233725: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210911::233725: Head 1: Initializing Time Sync Subsystem.
20210911::233726: Head 1: Initializing CTD Subsystem.
20210911::233726: Head 1: CTD Initialization Successful
20210911::233726: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210911::233727: Head 1: Time Sync UDP started, waiting for sync...
20210911::233727: Head 1: Attempting CTD Ethernet connection with ROV...
20210911::233727: Head 1: Time Synchronization Achieved: 2021.09.11   23:37:28::0014
20210911::233730: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 101
20210911::233730: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 31%, OPB 23C, Laser 0.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233731: Head 2: Eye Safe Optical Filter State there 4, not there 26, transition 1
20210911::233731: Head 2: Eye Safe Optical Filter check Passed
20210911::233731: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210911::233732: Head 2: Initializing Time Sync Subsystem.
20210911::233732: Head 2: Initializing CTD Subsystem.
20210911::233732: Head 2: CTD Initialization Successful
20210911::233733: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210911::233733: Head 2: Time Sync UDP started, waiting for sync...
20210911::233733: Head 2: Attempting CTD Ethernet connection with ROV...
20210911::233734: Head 2: Time Synchronization Achieved: 2021.09.11   23:37:35::0013
20210911::233800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 28%, OPB 22C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233800: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 155
20210911::233800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 29%, OPB 23C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 26%, OPB 22C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233830: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 208
20210911::233830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 27%, OPB 23C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 25%, OPB 23C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233900: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 261
20210911::233900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 25%, OPB 24C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233928: Head 2: CTD Ethernet connection established.
20210911::233928: Head 1: CTD Ethernet connection established.
20210911::233930: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 315
20210911::233930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 25%, OPB 24C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::233930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234000: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 368
20210911::234000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 24C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 24%, OPB 23C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 23C, Laser 24.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234030: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 422
20210911::234030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 30C, OCB 23%, OPB 24C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234100: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 475
20210911::234100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 24C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 23C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234130: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 528
20210911::234130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 24C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 23%, OPB 23C, Laser 25.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234200: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 582
20210911::234200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 25C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 31C, OCB 22%, OPB 24C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234230: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 635
20210911::234230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 27.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 26.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234300: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 688
20210911::234300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 27.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234330: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 742
20210911::234330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 27.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234400: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 795
20210911::234400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 28.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 27.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234430: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 849
20210911::234430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234500: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 902
20210911::234500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234530: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 955
20210911::234530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 25C, Laser 29.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 24C, Laser 28.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234600: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1009
20210911::234600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 26C, Laser 30.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234630: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1062
20210911::234630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 32C, OCB 22%, OPB 26C, Laser 30.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234700: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1115
20210911::234700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 30.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234730: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1169
20210911::234730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 30.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234735: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210911::234736: GUI: ERROR: Received Invalid Packet ID: 0
20210911::234736: GUI: Lost Communications with Sensor 1.
20210911::234737: GUI: Attempting Communications with Head 1...
20210911::234737: GUI: Requesing STOP operation, Head 2
20210911::234737: Head 2: Received request: STOP
20210911::234741: GUI: Established Communications with Head 1.
20210911::234741: Head 1: Initializing Communications with GUI ...
20210911::234742: Head 1: Communications Established.
20210911::234743: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210911::234743: Head 1: Connection Established with the GUI.
20210911::234744: Head 1: Initializing Subsystems, standby ...
20210911::234744: Head 1: Initializing Hardware, Stand by ...
20210911::234745: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210911::234745: Head 1: NtQuery - testing 1 ...
20210911::234745: Head 1: clock resolution: 1
20210911::234746: Head 1: NtQuery - testing 2, after setting max res ...
20210911::234746: Head 1: clock resolution: 1
20210911::234746: Head 1: Initializing Optics Electronics ...
20210911::234746: Head 1: Power Laser Controller
20210911::234750: Head 1: Power Scanner Controller
20210911::234752: Head 1: Power OPTO Sensor
20210911::234800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 29.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234800: System NOT Initialized, Gain 0, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 35
20210911::234800: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234811: Head 1: Eye Safe Optical Filter State there 14, not there 16, transition 1
20210911::234811: Head 1: Eye Safe Optical Filter check Passed
20210911::234812: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210911::234812: Head 1: Initializing Time Sync Subsystem.
20210911::234812: Head 1: Initializing CTD Subsystem.
20210911::234812: Head 1: CTD Initialization Successful
20210911::234813: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210911::234813: Head 1: Time Sync UDP started, waiting for sync...
20210911::234813: Head 1: Attempting CTD Ethernet connection with ROV...
20210911::234814: Head 1: Time Synchronization Achieved: 2021.09.11   23:48:15::0013
20210911::234814: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210911::234815: GUI: ERROR: Received Invalid Packet ID: 0
20210911::234816: GUI: Lost Communications with Head 2.
20210911::234816: GUI: Attempting Communications with Head 2...
20210911::234816: GUI: Requesing STOP operation, Head 1
20210911::234816: Head 1: Received request: STOP
20210911::234819: GUI: Established Communications with Head 2.
20210911::234819: Head 2: Initializing Communications with GUI ...
20210911::234820: Head 2: Communications Established.
20210911::234821: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210911::234821: Head 2: Connection Established with the GUI.
20210911::234822: Head 2: Initializing Subsystems, standby ...
20210911::234822: Head 2: Initializing Hardware, Stand by ...
20210911::234823: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20210911::234823: Head 2: NtQuery - testing 1 ...
20210911::234823: Head 2: clock resolution: 1
20210911::234824: Head 2: NtQuery - testing 2, after setting max res ...
20210911::234824: Head 2: clock resolution: 1
20210911::234824: Head 2: Initializing Optics Electronics ...
20210911::234825: Head 2: Power Laser Controller
20210911::234828: Head 2: Power Scanner Controller
20210911::234830: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 88
20210911::234830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234830: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234830: Head 2: Power OPTO Sensor
20210911::234849: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210911::234849: Head 2: Eye Safe Optical Filter check Passed
20210911::234850: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210911::234850: Head 2: Initializing Time Sync Subsystem.
20210911::234850: Head 2: Initializing CTD Subsystem.
20210911::234850: Head 2: CTD Initialization Successful
20210911::234851: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210911::234851: Head 2: Time Sync UDP started, waiting for sync...
20210911::234851: Head 2: Attempting CTD Ethernet connection with ROV...
20210911::234852: Head 2: Time Synchronization Achieved: 2021.09.11   23:48:53::0012
20210911::234900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 29.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234900: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 142
20210911::234900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::234930: System  Initialized, Gain 1, Elec PB 33.4C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 195
20210911::234930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235000: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 248
20210911::235000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 25C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235018: Head 2: CTD Ethernet connection established.
20210911::235018: Head 1: CTD Ethernet connection established.
20210911::235019: Head 2: Comm CTD: read error - invalid header received
20210911::235019: Head 1: Comm CTD: read error - invalid header received
20210911::235020: Head 2: Comm CTD: read error - invalid header received
20210911::235020: Head 1: Comm CTD: read error - invalid header received
20210911::235020: Head 2: Comm CTD: read error - invalid header received
20210911::235020: Head 1: Comm CTD: read error - invalid header received
20210911::235020: Head 2: Comm CTD: read error - invalid header received
20210911::235020: Head 1: Comm CTD: read error - invalid header received
20210911::235021: Head 2: Comm CTD: read error - invalid header received
20210911::235021: Head 1: Comm CTD: read error - invalid header received
20210911::235021: Head 2: Comm CTD: read error - invalid header received
20210911::235021: Head 1: Comm CTD: read error - invalid header received
20210911::235021: Head 2: Comm CTD: read error - invalid header received
20210911::235021: Head 1: Comm CTD: read error - invalid header received
20210911::235022: Head 2: Comm CTD: read error - invalid header received
20210911::235022: Head 1: Comm CTD: read error - invalid header received
20210911::235022: Head 2: Comm CTD: read error - invalid header received
20210911::235022: Head 1: Comm CTD: read error - invalid header received
20210911::235022: Head 2: Comm CTD: read error - invalid header received
20210911::235022: Head 1: Comm CTD: read error - invalid header received
20210911::235022: Head 2: Comm CTD: read error - invalid header received
20210911::235022: Head 1: Comm CTD: read error - invalid header received
20210911::235023: Head 2: Comm CTD: read error - invalid header received
20210911::235023: Head 1: Comm CTD: read error - invalid header received
20210911::235023: Head 2: Comm CTD: read error - invalid header received
20210911::235023: Head 1: Comm CTD: read error - invalid header received
20210911::235023: Head 2: Comm CTD: read error - invalid header received
20210911::235023: Head 1: Comm CTD: read error - invalid header received
20210911::235024: Head 2: Comm CTD: read error - invalid header received
20210911::235024: Head 1: Comm CTD: read error - invalid header received
20210911::235024: Head 2: Comm CTD: read error - invalid header received
20210911::235024: Head 1: Comm CTD: read error - invalid header received
20210911::235024: Head 2: Comm CTD: read error - invalid header received
20210911::235024: Head 1: Comm CTD: read error - invalid header received
20210911::235025: Head 2: Comm CTD: read error - invalid header received
20210911::235025: Head 1: Comm CTD: read error - invalid header received
20210911::235025: Head 2: Comm CTD: read error - invalid header received
20210911::235025: Head 1: Comm CTD: read error - invalid header received
20210911::235025: Head 2: Comm CTD: read error - invalid header received
20210911::235025: Head 1: Comm CTD: read error - invalid header received
20210911::235025: Head 2: Comm CTD: read error - invalid header received
20210911::235026: Head 1: Comm CTD: read error - invalid header received
20210911::235026: Head 2: Comm CTD: read error - invalid header received
20210911::235026: Head 1: Comm CTD: read error - invalid header received
20210911::235026: Head 2: Comm CTD: read error - invalid header received
20210911::235026: Head 1: Comm CTD: read error - invalid header received
20210911::235026: Head 2: Comm CTD: read error - invalid header received
20210911::235026: Head 1: Comm CTD: read error - invalid header received
20210911::235027: Head 2: Comm CTD: read error - invalid header received
20210911::235027: Head 1: Comm CTD: read error - invalid header received
20210911::235027: Head 2: Comm CTD: read error - invalid header received
20210911::235027: Head 1: Comm CTD: read error - invalid header received
20210911::235027: Head 2: Comm CTD: read error - invalid header received
20210911::235027: Head 1: Comm CTD: read error - invalid header received
20210911::235028: Head 2: Comm CTD: read error - invalid header received
20210911::235028: Head 1: Comm CTD: read error - invalid header received
20210911::235028: Head 2: Comm CTD: read error - invalid header received
20210911::235028: Head 1: Comm CTD: read error - invalid header received
20210911::235028: Head 2: Comm CTD: read error - invalid header received
20210911::235028: Head 1: Comm CTD: read error - invalid header received
20210911::235029: Head 2: Comm CTD: read error - invalid header received
20210911::235029: Head 1: Comm CTD: read error - invalid header received
20210911::235029: Head 2: Comm CTD: read error - invalid header received
20210911::235029: Head 1: Comm CTD: read error - invalid header received
20210911::235029: Head 2: Comm CTD: read error - invalid header received
20210911::235029: Head 1: Comm CTD: read error - invalid header received
20210911::235029: Head 2: Comm CTD: read error - invalid header received
20210911::235029: Head 1: Comm CTD: read error - invalid header received
20210911::235030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235030: Head 2: Comm CTD: read error - invalid header received
20210911::235030: Head 1: Comm CTD: read error - invalid header received
20210911::235030: System  Initialized, Gain 1, Elec PB 32.4C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 302
20210911::235030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 31.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235030: Head 2: Comm CTD: read error - invalid header received
20210911::235030: Head 1: Comm CTD: read error - invalid header received
20210911::235030: Head 2: Comm CTD: read error - invalid header received
20210911::235030: Head 1: Comm CTD: read error - invalid header received
20210911::235031: Head 2: Comm CTD: read error - invalid header received
20210911::235031: Head 1: Comm CTD: read error - invalid header received
20210911::235031: Head 2: Comm CTD: read error - invalid header received
20210911::235031: Head 1: Comm CTD: read error - invalid header received
20210911::235031: Head 2: Comm CTD: read error - invalid header received
20210911::235031: Head 1: Comm CTD: read error - invalid header received
20210911::235032: Head 2: Comm CTD: read error - invalid header received
20210911::235032: Head 1: Comm CTD: read error - invalid header received
20210911::235032: Head 2: Comm CTD: read error - invalid header received
20210911::235032: Head 1: Comm CTD: read error - invalid header received
20210911::235032: Head 2: Comm CTD: read error - invalid header received
20210911::235032: Head 1: Comm CTD: read error - invalid header received
20210911::235032: Head 2: Comm CTD: read error - invalid header received
20210911::235032: Head 1: Comm CTD: read error - invalid header received
20210911::235033: Head 2: Comm CTD: read error - invalid header received
20210911::235033: Head 1: Comm CTD: read error - invalid header received
20210911::235033: Head 2: Comm CTD: read error - invalid header received
20210911::235033: Head 1: Comm CTD: read error - invalid header received
20210911::235033: Head 2: Comm CTD: read error - invalid header received
20210911::235033: Head 1: Comm CTD: read error - invalid header received
20210911::235034: Head 2: Comm CTD: read error - invalid header received
20210911::235034: Head 1: Comm CTD: read error - invalid header received
20210911::235034: Head 2: Comm CTD: read error - invalid header received
20210911::235034: Head 1: Comm CTD: read error - invalid header received
20210911::235034: Head 2: Comm CTD: read error - invalid header received
20210911::235034: Head 1: Comm CTD: read error - invalid header received
20210911::235035: Head 2: Comm CTD: read error - invalid header received
20210911::235035: Head 1: Comm CTD: read error - invalid header received
20210911::235035: Head 2: Comm CTD: read error - invalid header received
20210911::235035: Head 1: Comm CTD: read error - invalid header received
20210911::235035: Head 2: Comm CTD: read error - invalid header received
20210911::235035: Head 1: Comm CTD: read error - invalid header received
20210911::235035: Head 2: Comm CTD: read error - invalid header received
20210911::235035: Head 1: Comm CTD: read error - invalid header received
20210911::235036: Head 2: Comm CTD: read error - invalid header received
20210911::235036: Head 1: Comm CTD: read error - invalid header received
20210911::235036: Head 2: Comm CTD: read error - invalid header received
20210911::235036: Head 1: Comm CTD: read error - invalid header received
20210911::235036: Head 2: Comm CTD: read error - invalid header received
20210911::235036: Head 1: Comm CTD: read error - invalid header received
20210911::235037: Head 2: Comm CTD: read error - invalid header received
20210911::235037: Head 1: Comm CTD: read error - invalid header received
20210911::235037: Head 2: Comm CTD: read error - invalid header received
20210911::235037: Head 1: Comm CTD: read error - invalid header received
20210911::235037: Head 2: Comm CTD: read error - invalid header received
20210911::235037: Head 1: Comm CTD: read error - invalid header received
20210911::235038: Head 2: Comm CTD: read error - invalid header received
20210911::235038: Head 1: Comm CTD: read error - invalid header received
20210911::235038: Head 2: Comm CTD: read error - invalid header received
20210911::235038: Head 1: Comm CTD: read error - invalid header received
20210911::235038: Head 2: Comm CTD: read error - invalid header received
20210911::235038: Head 1: Comm CTD: read error - invalid header received
20210911::235038: Head 2: Comm CTD: read error - invalid header received
20210911::235038: Head 1: Comm CTD: read error - invalid header received
20210911::235039: Head 2: Comm CTD: read error - invalid header received
20210911::235039: Head 1: Comm CTD: read error - invalid header received
20210911::235039: Head 2: Comm CTD: read error - invalid header received
20210911::235039: Head 1: Comm CTD: read error - invalid header received
20210911::235039: Head 2: Comm CTD: read error - invalid header received
20210911::235039: Head 1: Comm CTD: read error - invalid header received
20210911::235040: Head 2: Comm CTD: read error - invalid header received
20210911::235040: Head 1: Comm CTD: read error - invalid header received
20210911::235040: Head 2: Comm CTD: read error - invalid header received
20210911::235040: Head 1: Comm CTD: read error - invalid header received
20210911::235040: Head 2: Comm CTD: read error - invalid header received
20210911::235040: Head 1: Comm CTD: read error - invalid header received
20210911::235041: Head 2: Comm CTD: read error - invalid header received
20210911::235041: Head 1: Comm CTD: read error - invalid header received
20210911::235041: Head 2: Comm CTD: read error - invalid header received
20210911::235041: Head 1: Comm CTD: read error - invalid header received
20210911::235041: Head 2: Comm CTD: read error - invalid header received
20210911::235041: Head 1: Comm CTD: read error - invalid header received
20210911::235042: Head 2: Comm CTD: read error - invalid header received
20210911::235042: Head 1: Comm CTD: read error - invalid header received
20210911::235042: Head 2: Comm CTD: read error - invalid header received
20210911::235042: Head 1: Comm CTD: read error - invalid header received
20210911::235042: Head 2: Comm CTD: read error - invalid header received
20210911::235042: Head 1: Comm CTD: read error - invalid header received
20210911::235042: Head 2: Comm CTD: read error - invalid header received
20210911::235042: Head 1: Comm CTD: read error - invalid header received
20210911::235043: Head 2: Comm CTD: read error - invalid header received
20210911::235043: Head 1: Comm CTD: read error - invalid header received
20210911::235043: Head 2: Comm CTD: read error - invalid header received
20210911::235043: Head 1: Comm CTD: read error - invalid header received
20210911::235043: Head 2: Comm CTD: read error - invalid header received
20210911::235043: Head 1: Comm CTD: read error - invalid header received
20210911::235044: Head 2: Comm CTD: read error - invalid header received
20210911::235044: Head 1: Comm CTD: read error - invalid header received
20210911::235044: Head 2: Comm CTD: read error - invalid header received
20210911::235044: Head 1: Comm CTD: read error - invalid header received
20210911::235044: Head 2: Comm CTD: read error - invalid header received
20210911::235044: Head 1: Comm CTD: read error - invalid header received
20210911::235045: Head 2: Comm CTD: read error - invalid header received
20210911::235045: Head 1: Comm CTD: read error - invalid header received
20210911::235045: Head 2: Comm CTD: read error - invalid header received
20210911::235045: Head 1: Comm CTD: read error - invalid header received
20210911::235045: Head 2: Comm CTD: read error - invalid header received
20210911::235045: Head 1: Comm CTD: read error - invalid header received
20210911::235045: Head 2: Comm CTD: read error - invalid header received
20210911::235045: Head 1: Comm CTD: read error - invalid header received
20210911::235046: Head 2: Comm CTD: read error - invalid header received
20210911::235046: Head 1: Comm CTD: read error - invalid header received
20210911::235046: Head 2: Comm CTD: read error - invalid header received
20210911::235046: Head 1: Comm CTD: read error - invalid header received
20210911::235046: Head 2: Comm CTD: read error - invalid header received
20210911::235046: Head 1: Comm CTD: read error - invalid header received
20210911::235047: Head 2: Comm CTD: read error - invalid header received
20210911::235047: Head 1: Comm CTD: read error - invalid header received
20210911::235047: Head 2: Comm CTD: read error - invalid header received
20210911::235047: Head 1: Comm CTD: read error - invalid header received
20210911::235047: Head 2: Comm CTD: read error - invalid header received
20210911::235047: Head 1: Comm CTD: read error - invalid header received
20210911::235048: Head 2: Comm CTD: read error - invalid header received
20210911::235048: Head 1: Comm CTD: read error - invalid header received
20210911::235048: Head 2: Comm CTD: read error - invalid header received
20210911::235048: Head 1: Comm CTD: read error - invalid header received
20210911::235048: Head 2: Comm CTD: read error - invalid header received
20210911::235048: Head 1: Comm CTD: read error - invalid header received
20210911::235048: Head 2: Comm CTD: read error - invalid header received
20210911::235048: Head 1: Comm CTD: read error - invalid header received
20210911::235049: Head 2: Comm CTD: read error - invalid header received
20210911::235049: Head 1: Comm CTD: read error - invalid header received
20210911::235049: Head 2: Comm CTD: read error - invalid header received
20210911::235049: Head 1: Comm CTD: read error - invalid header received
20210911::235049: Head 2: Comm CTD: read error - invalid header received
20210911::235049: Head 1: Comm CTD: read error - invalid header received
20210911::235050: Head 2: Comm CTD: read error - invalid header received
20210911::235050: Head 1: Comm CTD: read error - invalid header received
20210911::235050: Head 2: Comm CTD: read error - invalid header received
20210911::235050: Head 1: Comm CTD: read error - invalid header received
20210911::235050: Head 2: Comm CTD: read error - invalid header received
20210911::235050: Head 1: Comm CTD: read error - invalid header received
20210911::235051: Head 2: Comm CTD: read error - invalid header received
20210911::235051: Head 1: Comm CTD: read error - invalid header received
20210911::235051: Head 2: Comm CTD: read error - invalid header received
20210911::235051: Head 1: Comm CTD: read error - invalid header received
20210911::235051: Head 2: Comm CTD: read error - invalid header received
20210911::235051: Head 1: Comm CTD: read error - invalid header received
20210911::235051: Head 2: Comm CTD: read error - invalid header received
20210911::235052: Head 1: Comm CTD: read error - invalid header received
20210911::235052: Head 2: Comm CTD: read error - invalid header received
20210911::235052: Head 1: Comm CTD: read error - invalid header received
20210911::235052: Head 2: Comm CTD: read error - invalid header received
20210911::235052: Head 1: Comm CTD: read error - invalid header received
20210911::235052: Head 2: Comm CTD: read error - invalid header received
20210911::235052: Head 1: Comm CTD: read error - invalid header received
20210911::235053: Head 2: Comm CTD: read error - invalid header received
20210911::235053: Head 1: Comm CTD: read error - invalid header received
20210911::235053: Head 2: Comm CTD: read error - invalid header received
20210911::235053: Head 1: Comm CTD: read error - invalid header received
20210911::235053: Head 2: Comm CTD: read error - invalid header received
20210911::235053: Head 1: Comm CTD: read error - invalid header received
20210911::235054: Head 2: Comm CTD: read error - invalid header received
20210911::235054: Head 1: Comm CTD: read error - invalid header received
20210911::235054: Head 2: Comm CTD: read error - invalid header received
20210911::235054: Head 1: Comm CTD: read error - invalid header received
20210911::235054: Head 2: Comm CTD: read error - invalid header received
20210911::235054: Head 1: Comm CTD: read error - invalid header received
20210911::235054: Head 2: Comm CTD: read error - invalid header received
20210911::235055: Head 1: Comm CTD: read error - invalid header received
20210911::235055: Head 2: Comm CTD: read error - invalid header received
20210911::235055: Head 1: Comm CTD: read error - invalid header received
20210911::235055: Head 2: Comm CTD: read error - invalid header received
20210911::235055: Head 1: Comm CTD: read error - invalid header received
20210911::235055: Head 2: Comm CTD: read error - invalid header received
20210911::235055: Head 1: Comm CTD: read error - invalid header received
20210911::235056: Head 2: Comm CTD: read error - invalid header received
20210911::235056: Head 1: Comm CTD: read error - invalid header received
20210911::235056: Head 2: Comm CTD: read error - invalid header received
20210911::235056: Head 1: Comm CTD: read error - invalid header received
20210911::235056: Head 2: Comm CTD: read error - invalid header received
20210911::235056: Head 1: Comm CTD: read error - invalid header received
20210911::235057: Head 2: Comm CTD: read error - invalid header received
20210911::235057: Head 1: Comm CTD: read error - invalid header received
20210911::235057: Head 2: Comm CTD: read error - invalid header received
20210911::235057: Head 1: Comm CTD: read error - invalid header received
20210911::235057: Head 2: Comm CTD: read error - invalid header received
20210911::235057: Head 1: Comm CTD: read error - invalid header received
20210911::235058: Head 2: Comm CTD: read error - invalid header received
20210911::235058: Head 1: Comm CTD: read error - invalid header received
20210911::235058: Head 2: Comm CTD: read error - invalid header received
20210911::235058: Head 1: Comm CTD: read error - invalid header received
20210911::235058: Head 2: Comm CTD: read error - invalid header received
20210911::235058: Head 1: Comm CTD: read error - invalid header received
20210911::235058: Head 2: Comm CTD: read error - invalid header received
20210911::235058: Head 1: Comm CTD: read error - invalid header received
20210911::235059: Head 2: Comm CTD: read error - invalid header received
20210911::235059: Head 1: Comm CTD: read error - invalid header received
20210911::235059: Head 2: Comm CTD: read error - invalid header received
20210911::235059: Head 1: Comm CTD: read error - invalid header received
20210911::235059: Head 2: Comm CTD: read error - invalid header received
20210911::235059: Head 1: Comm CTD: read error - invalid header received
20210911::235100: Head 2: Comm CTD: read error - invalid header received
20210911::235100: Head 1: Comm CTD: read error - invalid header received
20210911::235100: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 355
20210911::235100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235100: Head 2: Comm CTD: read error - invalid header received
20210911::235100: Head 1: Comm CTD: read error - invalid header received
20210911::235100: Head 2: Comm CTD: read error - invalid header received
20210911::235100: Head 1: Comm CTD: read error - invalid header received
20210911::235101: Head 2: Comm CTD: read error - invalid header received
20210911::235101: Head 1: Comm CTD: read error - invalid header received
20210911::235101: Head 2: Comm CTD: read error - invalid header received
20210911::235101: Head 1: Comm CTD: read error - invalid header received
20210911::235101: Head 2: Comm CTD: read error - invalid header received
20210911::235101: Head 1: Comm CTD: read error - invalid header received
20210911::235101: Head 2: Comm CTD: read error - invalid header received
20210911::235101: Head 1: Comm CTD: read error - invalid header received
20210911::235102: Head 2: Comm CTD: read error - invalid header received
20210911::235102: Head 1: Comm CTD: read error - invalid header received
20210911::235102: Head 2: Comm CTD: read error - invalid header received
20210911::235102: Head 1: Comm CTD: read error - invalid header received
20210911::235102: Head 2: Comm CTD: read error - invalid header received
20210911::235102: Head 1: Comm CTD: read error - invalid header received
20210911::235103: Head 2: Comm CTD: read error - invalid header received
20210911::235103: Head 1: Comm CTD: read error - invalid header received
20210911::235103: Head 2: Comm CTD: read error - invalid header received
20210911::235103: Head 1: Comm CTD: read error - invalid header received
20210911::235103: Head 2: Comm CTD: read error - invalid header received
20210911::235103: Head 1: Comm CTD: read error - invalid header received
20210911::235104: Head 2: Comm CTD: read error - invalid header received
20210911::235104: Head 1: Comm CTD: read error - invalid header received
20210911::235104: Head 2: Comm CTD: read error - invalid header received
20210911::235104: Head 1: Comm CTD: read error - invalid header received
20210911::235104: Head 2: Comm CTD: read error - invalid header received
20210911::235104: Head 1: Comm CTD: read error - invalid header received
20210911::235104: Head 2: Comm CTD: read error - invalid header received
20210911::235104: Head 1: Comm CTD: read error - invalid header received
20210911::235105: Head 2: Comm CTD: read error - invalid header received
20210911::235105: Head 1: Comm CTD: read error - invalid header received
20210911::235105: Head 2: Comm CTD: read error - invalid header received
20210911::235105: Head 1: Comm CTD: read error - invalid header received
20210911::235105: Head 2: Comm CTD: read error - invalid header received
20210911::235105: Head 1: Comm CTD: read error - invalid header received
20210911::235106: Head 2: Comm CTD: read error - invalid header received
20210911::235106: Head 1: Comm CTD: read error - invalid header received
20210911::235106: Head 2: Comm CTD: read error - invalid header received
20210911::235106: Head 1: Comm CTD: read error - invalid header received
20210911::235106: Head 2: Comm CTD: read error - invalid header received
20210911::235106: Head 1: Comm CTD: read error - invalid header received
20210911::235107: Head 2: Comm CTD: read error - invalid header received
20210911::235107: Head 1: Comm CTD: read error - invalid header received
20210911::235107: Head 2: Comm CTD: read error - invalid header received
20210911::235107: Head 1: Comm CTD: read error - invalid header received
20210911::235107: Head 2: Comm CTD: read error - invalid header received
20210911::235107: Head 1: Comm CTD: read error - invalid header received
20210911::235107: Head 2: Comm CTD: read error - invalid header received
20210911::235108: Head 1: Comm CTD: read error - invalid header received
20210911::235108: Head 2: Comm CTD: read error - invalid header received
20210911::235108: Head 1: Comm CTD: read error - invalid header received
20210911::235108: Head 2: Comm CTD: read error - invalid header received
20210911::235108: Head 1: Comm CTD: read error - invalid header received
20210911::235108: Head 2: Comm CTD: read error - invalid header received
20210911::235108: Head 1: Comm CTD: read error - invalid header received
20210911::235109: Head 2: Comm CTD: read error - invalid header received
20210911::235109: Head 1: Comm CTD: read error - invalid header received
20210911::235109: Head 2: Comm CTD: read error - invalid header received
20210911::235109: Head 1: Comm CTD: read error - invalid header received
20210911::235109: Head 2: Comm CTD: read error - invalid header received
20210911::235109: Head 1: Comm CTD: read error - invalid header received
20210911::235110: Head 2: Comm CTD: read error - invalid header received
20210911::235110: Head 1: Comm CTD: read error - invalid header received
20210911::235110: Head 2: Comm CTD: read error - invalid header received
20210911::235110: Head 1: Comm CTD: read error - invalid header received
20210911::235110: Head 2: Comm CTD: read error - invalid header received
20210911::235110: Head 1: Comm CTD: read error - invalid header received
20210911::235111: Head 2: Comm CTD: read error - invalid header received
20210911::235111: Head 1: Comm CTD: read error - invalid header received
20210911::235111: Head 2: Comm CTD: read error - invalid header received
20210911::235111: Head 1: Comm CTD: read error - invalid header received
20210911::235111: Head 2: Comm CTD: read error - invalid header received
20210911::235111: Head 1: Comm CTD: read error - invalid header received
20210911::235111: Head 2: Comm CTD: read error - invalid header received
20210911::235111: Head 1: Comm CTD: read error - invalid header received
20210911::235112: Head 2: Comm CTD: read error - invalid header received
20210911::235112: Head 1: Comm CTD: read error - invalid header received
20210911::235112: Head 2: Comm CTD: read error - invalid header received
20210911::235112: Head 1: Comm CTD: read error - invalid header received
20210911::235112: Head 2: Comm CTD: read error - invalid header received
20210911::235112: Head 1: Comm CTD: read error - invalid header received
20210911::235113: Head 2: Comm CTD: read error - invalid header received
20210911::235113: Head 1: Comm CTD: read error - invalid header received
20210911::235113: Head 2: Comm CTD: read error - invalid header received
20210911::235113: Head 1: Comm CTD: read error - invalid header received
20210911::235113: Head 2: Comm CTD: read error - invalid header received
20210911::235113: Head 1: Comm CTD: read error - invalid header received
20210911::235114: Head 2: Comm CTD: read error - invalid header received
20210911::235114: Head 1: Comm CTD: read error - invalid header received
20210911::235114: Head 2: Comm CTD: read error - invalid header received
20210911::235114: Head 1: Comm CTD: read error - invalid header received
20210911::235114: Head 2: Comm CTD: read error - invalid header received
20210911::235114: Head 1: Comm CTD: read error - invalid header received
20210911::235114: Head 2: Comm CTD: read error - invalid header received
20210911::235114: Head 1: Comm CTD: read error - invalid header received
20210911::235115: Head 2: Comm CTD: read error - invalid header received
20210911::235115: Head 1: Comm CTD: read error - invalid header received
20210911::235115: Head 2: Comm CTD: read error - invalid header received
20210911::235115: Head 1: Comm CTD: read error - invalid header received
20210911::235115: Head 2: Comm CTD: read error - invalid header received
20210911::235115: Head 1: Comm CTD: read error - invalid header received
20210911::235116: Head 2: Comm CTD: read error - invalid header received
20210911::235116: Head 1: Comm CTD: read error - invalid header received
20210911::235116: Head 2: Comm CTD: read error - invalid header received
20210911::235116: Head 1: Comm CTD: read error - invalid header received
20210911::235116: Head 2: Comm CTD: read error - invalid header received
20210911::235116: Head 1: Comm CTD: read error - invalid header received
20210911::235117: Head 2: Comm CTD: read error - invalid header received
20210911::235117: Head 1: Comm CTD: read error - invalid header received
20210911::235117: Head 2: Comm CTD: read error - invalid header received
20210911::235117: Head 1: Comm CTD: read error - invalid header received
20210911::235117: Head 2: Comm CTD: read error - invalid header received
20210911::235117: Head 1: Comm CTD: read error - invalid header received
20210911::235117: Head 2: Comm CTD: read error - invalid header received
20210911::235117: Head 1: Comm CTD: read error - invalid header received
20210911::235118: Head 2: Comm CTD: read error - invalid header received
20210911::235118: Head 1: Comm CTD: read error - invalid header received
20210911::235118: Head 2: Comm CTD: read error - invalid header received
20210911::235118: Head 1: Comm CTD: read error - invalid header received
20210911::235118: Head 2: Comm CTD: read error - invalid header received
20210911::235118: Head 1: Comm CTD: read error - invalid header received
20210911::235119: Head 2: Comm CTD: read error - invalid header received
20210911::235119: Head 1: Comm CTD: read error - invalid header received
20210911::235119: Head 2: Comm CTD: read error - invalid header received
20210911::235119: Head 1: Comm CTD: read error - invalid header received
20210911::235119: Head 2: Comm CTD: read error - invalid header received
20210911::235119: Head 1: Comm CTD: read error - invalid header received
20210911::235120: Head 2: Comm CTD: read error - invalid header received
20210911::235120: Head 1: Comm CTD: read error - invalid header received
20210911::235120: Head 2: Comm CTD: read error - invalid header received
20210911::235120: Head 1: Comm CTD: read error - invalid header received
20210911::235120: Head 2: Comm CTD: read error - invalid header received
20210911::235120: Head 1: Comm CTD: read error - invalid header received
20210911::235120: Head 2: Comm CTD: read error - invalid header received
20210911::235121: Head 1: Comm CTD: read error - invalid header received
20210911::235121: Head 2: Comm CTD: read error - invalid header received
20210911::235121: Head 1: Comm CTD: read error - invalid header received
20210911::235121: Head 2: Comm CTD: read error - invalid header received
20210911::235121: Head 1: Comm CTD: read error - invalid header received
20210911::235121: Head 2: Comm CTD: read error - invalid header received
20210911::235121: Head 1: Comm CTD: read error - invalid header received
20210911::235122: Head 2: Comm CTD: read error - invalid header received
20210911::235122: Head 1: Comm CTD: read error - invalid header received
20210911::235122: Head 2: Comm CTD: read error - invalid header received
20210911::235122: Head 1: Comm CTD: read error - invalid header received
20210911::235122: Head 2: Comm CTD: read error - invalid header received
20210911::235122: Head 1: Comm CTD: read error - invalid header received
20210911::235123: Head 2: Comm CTD: read error - invalid header received
20210911::235123: Head 1: Comm CTD: read error - invalid header received
20210911::235123: Head 2: Comm CTD: read error - invalid header received
20210911::235123: Head 1: Comm CTD: read error - invalid header received
20210911::235123: Head 2: Comm CTD: read error - invalid header received
20210911::235123: Head 1: Comm CTD: read error - invalid header received
20210911::235123: Head 2: Comm CTD: read error - invalid header received
20210911::235124: Head 1: Comm CTD: read error - invalid header received
20210911::235124: Head 2: Comm CTD: read error - invalid header received
20210911::235124: Head 1: Comm CTD: read error - invalid header received
20210911::235124: Head 2: Comm CTD: read error - invalid header received
20210911::235124: Head 1: Comm CTD: read error - invalid header received
20210911::235124: Head 2: Comm CTD: read error - invalid header received
20210911::235124: Head 1: Comm CTD: read error - invalid header received
20210911::235125: Head 2: Comm CTD: read error - invalid header received
20210911::235125: Head 1: Comm CTD: read error - invalid header received
20210911::235125: Head 2: Comm CTD: read error - invalid header received
20210911::235125: Head 1: Comm CTD: read error - invalid header received
20210911::235125: Head 2: Comm CTD: read error - invalid header received
20210911::235125: Head 1: Comm CTD: read error - invalid header received
20210911::235126: Head 2: Comm CTD: read error - invalid header received
20210911::235126: Head 1: Comm CTD: read error - invalid header received
20210911::235126: Head 2: Comm CTD: read error - invalid header received
20210911::235126: Head 1: Comm CTD: read error - invalid header received
20210911::235126: Head 2: Comm CTD: read error - invalid header received
20210911::235126: Head 1: Comm CTD: read error - invalid header received
20210911::235127: Head 2: Comm CTD: read error - invalid header received
20210911::235127: Head 1: Comm CTD: read error - invalid header received
20210911::235127: Head 2: Comm CTD: read error - invalid header received
20210911::235127: Head 1: Comm CTD: read error - invalid header received
20210911::235127: Head 2: Comm CTD: read error - invalid header received
20210911::235127: Head 1: Comm CTD: read error - invalid header received
20210911::235127: Head 2: Comm CTD: read error - invalid header received
20210911::235127: Head 1: Comm CTD: read error - invalid header received
20210911::235128: Head 2: Comm CTD: read error - invalid header received
20210911::235128: Head 1: Comm CTD: read error - invalid header received
20210911::235130: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 408
20210911::235130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 30.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235200: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 462
20210911::235200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235230: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 515
20210911::235230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235300: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 568
20210911::235300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235330: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 622
20210911::235330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235400: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 675
20210911::235400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 22%, OPB 27C, Laser 32.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235430: System  Initialized, Gain 1, Elec PB 34.6C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 728
20210911::235430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235500: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 782
20210911::235500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 26C, Laser 31.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235530: System  Initialized, Gain 1, Elec PB 36.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 835
20210911::235530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235600: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 889
20210911::235600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235630: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 942
20210911::235630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235700: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 995
20210911::235700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235730: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1049
20210911::235730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235800: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1102
20210911::235800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 33.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235830: System  Initialized, Gain 1, Elec PB 37.8C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1155
20210911::235830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235900: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1209
20210911::235900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 34C, OCB 23%, OPB 27C, Laser 32.0C, Dig 42.0C, Scan Az fault 0, gain 0, laser state 0
20210911::235930: System  Initialized, Gain 1, Elec PB 38.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 1262
20210911::235930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 33C, OCB 23%, OPB 28C, Laser 34.0C, Dig 37.0C, Scan Az fault 0, gain 0, laser state 0
