20201015::131320: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20201015::131320: GUI: Live mode ON.
20201015::131320: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20201015::131320: GUI: WiSSL GUI started at 2020_10_15_13:13:20
20201015::131320: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2020_10_15.txt
20201015::131320: GUI: Attempting Communications with Head 1...
20201015::131320: GUI: Attempting Communications with Head 2...
20201015::133148: GUI: Established Communications with Head 1.
20201015::133148: Head 1: Initializing Communications with GUI ...
20201015::133149: Head 1: Communications Established.
20201015::133150: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::133150: GUI: Established Communications with Head 2.
20201015::133150: Head 1: Connection Established with the GUI.
20201015::133151: Head 1: Initializing Subsystems, standby ...
20201015::133151: Head 1: Initializing Hardware, Stand by ...
20201015::133151: Head 2: Initializing Communications with GUI ...
20201015::133152: Head 2: Communications Established.
20201015::133153: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::133154: Head 2: Connection Established with the GUI.
20201015::133154: Head 2: Initializing Subsystems, standby ...
20201015::133154: Head 2: Initializing Hardware, Stand by ...
20201015::133200: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133200: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 23
20201015::133200: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133205: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201015::133206: Head 1: NtQuery - testing 1 ...
20201015::133206: Head 1: clock resolution: 10
20201015::133206: Head 1: NtQuery - testing 2, after setting max res ...
20201015::133207: Head 1: clock resolution: 10
20201015::133207: Head 1: Initializing Optics Electronics ...
20201015::133207: Head 1: Power Laser Controller
20201015::133211: Head 1: Power Scanner Controller
20201015::133212: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201015::133212: Head 2: NtQuery - testing 1 ...
20201015::133212: Head 2: clock resolution: 10
20201015::133213: Head 2: NtQuery - testing 2, after setting max res ...
20201015::133213: Head 2: clock resolution: 10
20201015::133213: Head 1: Power OPTO Sensor
20201015::133213: Head 2: Initializing Optics Electronics ...
20201015::133214: Head 2: Power Laser Controller
20201015::133217: Head 2: Power Scanner Controller
20201015::133220: Head 2: Power OPTO Sensor
20201015::133230: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133230: System NOT Initialized, Gain 0, Elec PB 18.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 77
20201015::133230: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133233: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::133233: Head 1: Eye Safe Optical Filter check Passed
20201015::133234: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201015::133234: Head 1: Initializing Time Sync Subsystem.
20201015::133234: Head 1: Initializing CTD Subsystem.
20201015::133235: Head 1: CTD Initialization Successful
20201015::133235: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201015::133235: Head 1: Time Sync UDP started, waiting for sync...
20201015::133236: Head 1: Attempting CTD Ethernet connection with ROV...
20201015::133236: Head 1: Time Synchronization Achieved: 2020.10.15   13:32:37::0015
20201015::133240: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::133240: Head 2: Eye Safe Optical Filter check Passed
20201015::133240: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201015::133241: Head 2: Initializing Time Sync Subsystem.
20201015::133241: Head 2: Initializing CTD Subsystem.
20201015::133241: Head 2: CTD Initialization Successful
20201015::133241: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201015::133242: Head 2: Time Sync UDP started, waiting for sync...
20201015::133242: Head 2: Attempting CTD Ethernet connection with ROV...
20201015::133243: Head 2: Time Synchronization Achieved: 2020.10.15   13:32:44::0015
20201015::133300: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 132
20201015::133300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 29%, OPB 17C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 28%, OPB 18C, Laser 17.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133316: Head 1: CTD Ethernet connection established.
20201015::133316: Head 2: CTD Ethernet connection established.
20201015::133330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 187
20201015::133330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 26%, OPB 18C, Laser 18.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 26%, OPB 17C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133341: Head 1: Setting Gain 1
20201015::133341: Head 2: Setting Gain 1
20201015::133345: GUI: Live mode ON.
20201015::133345: GUI: Requesing START operation, Head 1
20201015::133345: GUI: Requesing START operation, Head 2
20201015::133346: Head 1: Received request: START
20201015::133346: Head 2: Received request: START
20201015::133346: Head 1: Starting Scan Operation
20201015::133346: Head 2: Starting Scan Operation
20201015::133347: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::133347: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20201015::133347: Head 1: Eye Safe Optical Filter check Passed
20201015::133348: Head 2: Eye Safe Optical Filter check Passed
20201015::133352: Head 1: Configured for WATER Processing
20201015::133352: Head 2: Configured for WATER Processing
20201015::133352: Head 1: Configured for WATER Processing
20201015::133352: Head 2: Configured for WATER Processing
20201015::133352: Head 1: Configured for WATER Processing
20201015::133353: Head 2: Configured for WATER Processing
20201015::133353: Head 1: Configured for WATER Processing
20201015::133353: Head 2: Configured for WATER Processing
20201015::133353: Head 1: Configured for WATER Processing
20201015::133353: Head 2: Configured for WATER Processing
20201015::133353: Head 1: Configured for WATER Processing
20201015::133353: Head 2: Configured for WATER Processing
20201015::133354: Head 1: Configured for WATER Processing
20201015::133354: Head 2: Configured for WATER Processing
20201015::133354: Head 1: Configured for WATER Processing
20201015::133354: Head 2: Configured for WATER Processing
20201015::133354: Head 1: Configured for WATER Processing
20201015::133354: Head 2: Configured for WATER Processing
20201015::133355: Head 1: Configured for WATER Processing
20201015::133355: Head 2: Configured for WATER Processing
20201015::133355: Head 1: Configured for WATER Processing
20201015::133355: Head 2: Configured for WATER Processing
20201015::133355: Head 1: Configured for WATER Processing
20201015::133355: Head 2: Configured for WATER Processing
20201015::133355: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_133354_wf.raa
20201015::133356: Head 1: Configured for WATER Processing
20201015::133356: Head 2: Configured for WATER Processing
20201015::133356: Head 1: Configured for WATER Processing
20201015::133356: Head 2: Configured for WATER Processing
20201015::133356: Head 1: Configured for WATER Processing
20201015::133356: Head 2: Configured for WATER Processing
20201015::133356: Head 1: Configured for WATER Processing
20201015::133356: Head 2: Configured for WATER Processing
20201015::133357: Head 1: Configured for WATER Processing
20201015::133357: Head 2: Configured for WATER Processing
20201015::133357: Head 1: Configured for WATER Processing
20201015::133357: Head 2: Configured for WATER Processing
20201015::133357: Head 1: Configured for WATER Processing
20201015::133357: Head 2: Configured for WATER Processing
20201015::133358: Head 1: Configured for WATER Processing
20201015::133358: Head 2: Configured for WATER Processing
20201015::133400: GUI: Live mode ON.
20201015::133400: GUI: Requesing STOP operation, Head 1
20201015::133400: GUI: Requesing STOP operation, Head 2
20201015::133400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 18C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 1
20201015::133400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 242
20201015::133400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 19C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 1
20201015::133400: Head 1: Received request: STOP
20201015::133400: Head 2: Received request: STOP
20201015::133400: Head 1: Stopping Scan Operation
20201015::133400: Head 2: Stopping Scan Operation
20201015::133402: Head 1: ProcessingMgr stopped all worker threads.
20201015::133402: Head 2: ProcessingMgr stopped all worker threads.
20201015::133403: Head 1:       Stop finished, may now recover.
20201015::133403: Head 2:       Stop finished, may now recover.
20201015::133408: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20201015::133408: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::133408: Head 1: Eye Safe Optical Filter check Passed
20201015::133408: Head 2: Eye Safe Optical Filter check Passed
20201015::133430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 297
20201015::133430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 18C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 352
20201015::133500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 407
20201015::133530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 462
20201015::133600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 517
20201015::133630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 572
20201015::133700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 626
20201015::133730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 682
20201015::133800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 737
20201015::133830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 792
20201015::133900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::133930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.8C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 847
20201015::133930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.9C, CTD 4.6dbar, CTD 0.8psu, index 1.34, Packet 901
20201015::134000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.9C, CTD 4.5dbar, CTD 0.5psu, index 1.34, Packet 956
20201015::134030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.9C, CTD 3.9dbar, CTD 0.8psu, index 1.34, Packet 1012
20201015::134100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.9C, CTD 4.9dbar, CTD 0.7psu, index 1.34, Packet 1067
20201015::134130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 19C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.8C, CTD 12.8dbar, CTD 34.9psu, index 1.34, Packet 1122
20201015::134200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.7C, CTD 16.1dbar, CTD 34.6psu, index 1.34, Packet 1176
20201015::134230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.6C, CTD 16.4dbar, CTD 34.7psu, index 1.34, Packet 1232
20201015::134300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.6C, CTD 19.5dbar, CTD 34.4psu, index 1.34, Packet 1286
20201015::134330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.5C, CTD 20.7dbar, CTD 34.4psu, index 1.34, Packet 1342
20201015::134400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.4C, CTD 23.8dbar, CTD 34.3psu, index 1.34, Packet 1397
20201015::134430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 12.7C, CTD 29.6dbar, CTD 33.4psu, index 1.34, Packet 1451
20201015::134500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 13.0C, CTD 28.7dbar, CTD 33.5psu, index 1.34, Packet 1507
20201015::134530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 35.8dbar, CTD 33.4psu, index 1.34, Packet 1561
20201015::134600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 34.8dbar, CTD 33.4psu, index 1.34, Packet 1617
20201015::134630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.5C, CTD 37.5dbar, CTD 33.4psu, index 1.34, Packet 1672
20201015::134700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.5C, CTD 37.9dbar, CTD 33.4psu, index 1.34, Packet 1726
20201015::134730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.5C, CTD 37.9dbar, CTD 33.4psu, index 1.34, Packet 1781
20201015::134800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 37.7dbar, CTD 33.4psu, index 1.34, Packet 1836
20201015::134830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 18C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.7C, CTD 37.9dbar, CTD 33.4psu, index 1.34, Packet 1891
20201015::134900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::134930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 38.0dbar, CTD 33.4psu, index 1.34, Packet 1946
20201015::134930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 37.5dbar, CTD 33.4psu, index 1.34, Packet 2001
20201015::135000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 19C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.6C, CTD 37.7dbar, CTD 33.4psu, index 1.34, Packet 2056
20201015::135030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 11.5C, CTD 41.1dbar, CTD 33.4psu, index 1.34, Packet 2110
20201015::135100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.6C, CTD 47.9dbar, CTD 33.3psu, index 1.34, Packet 2165
20201015::135130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135159: Head 1: Time Synchronization: 2020.10.15   13:52:00::0014
20201015::135200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 55.4dbar, CTD 33.4psu, index 1.34, Packet 2220
20201015::135200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 67.2dbar, CTD 33.5psu, index 1.34, Packet 2275
20201015::135230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.2C, CTD 78.8dbar, CTD 33.7psu, index 1.34, Packet 2330
20201015::135300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.2C, CTD 89.9dbar, CTD 33.8psu, index 1.34, Packet 2385
20201015::135330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 99.4dbar, CTD 33.8psu, index 1.34, Packet 2440
20201015::135400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 97.2dbar, CTD 33.8psu, index 1.34, Packet 2495
20201015::135430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 18C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 113.4dbar, CTD 33.9psu, index 1.34, Packet 2550
20201015::135500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.9C, CTD 125.6dbar, CTD 33.9psu, index 1.34, Packet 2605
20201015::135530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 137.7dbar, CTD 33.9psu, index 1.34, Packet 2660
20201015::135600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 137.3dbar, CTD 33.9psu, index 1.34, Packet 2715
20201015::135630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 130.9dbar, CTD 33.9psu, index 1.34, Packet 2770
20201015::135700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 135.2dbar, CTD 33.9psu, index 1.34, Packet 2825
20201015::135730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 16C, Laser 25.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.5C, CTD 142.1dbar, CTD 33.9psu, index 1.34, Packet 2880
20201015::135800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.5C, CTD 136.3dbar, CTD 33.9psu, index 1.34, Packet 2935
20201015::135830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 127.5dbar, CTD 33.9psu, index 1.34, Packet 2990
20201015::135900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 16C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::135930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.5C, CTD 146.7dbar, CTD 33.9psu, index 1.34, Packet 3045
20201015::135930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 158.6dbar, CTD 34.0psu, index 1.34, Packet 3100
20201015::140000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 163.6dbar, CTD 34.0psu, index 1.34, Packet 3155
20201015::140030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 17C, Laser 26.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 176.7dbar, CTD 34.0psu, index 1.34, Packet 3210
20201015::140100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.0C, CTD 192.1dbar, CTD 34.0psu, index 1.34, Packet 3265
20201015::140130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 207.1dbar, CTD 34.1psu, index 1.34, Packet 3320
20201015::140200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 24.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 215.8dbar, CTD 34.1psu, index 1.34, Packet 3375
20201015::140230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.7C, CTD 226.8dbar, CTD 34.1psu, index 1.34, Packet 3430
20201015::140300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.5C, CTD 240.1dbar, CTD 34.1psu, index 1.34, Packet 3485
20201015::140330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.3C, CTD 252.0dbar, CTD 34.2psu, index 1.34, Packet 3540
20201015::140400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 263.2dbar, CTD 34.1psu, index 1.34, Packet 3595
20201015::140430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.1C, CTD 274.9dbar, CTD 34.2psu, index 1.34, Packet 3650
20201015::140500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 288.9dbar, CTD 34.2psu, index 1.34, Packet 3705
20201015::140530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 15C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.9C, CTD 304.2dbar, CTD 34.2psu, index 1.34, Packet 3760
20201015::140600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.7C, CTD 319.7dbar, CTD 34.2psu, index 1.34, Packet 3815
20201015::140630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 16C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.5C, CTD 336.0dbar, CTD 34.2psu, index 1.34, Packet 3870
20201015::140700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.4C, CTD 353.1dbar, CTD 34.2psu, index 1.34, Packet 3925
20201015::140730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 15C, Laser 25.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.2C, CTD 370.1dbar, CTD 34.2psu, index 1.34, Packet 3980
20201015::140800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 386.1dbar, CTD 34.2psu, index 1.34, Packet 4035
20201015::140830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 23.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.0C, CTD 401.5dbar, CTD 34.2psu, index 1.34, Packet 4090
20201015::140900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 14C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::140930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.9C, CTD 417.3dbar, CTD 34.2psu, index 1.34, Packet 4144
20201015::140930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 23%, OPB 14C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.6C, CTD 434.0dbar, CTD 34.2psu, index 1.34, Packet 4200
20201015::141000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.4C, CTD 449.1dbar, CTD 34.2psu, index 1.34, Packet 4255
20201015::141030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 15C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.3C, CTD 462.4dbar, CTD 34.2psu, index 1.34, Packet 4310
20201015::141100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 14C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.2C, CTD 475.5dbar, CTD 34.2psu, index 1.34, Packet 4364
20201015::141130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.0C, CTD 488.7dbar, CTD 34.2psu, index 1.34, Packet 4419
20201015::141200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.8C, CTD 510.0dbar, CTD 34.2psu, index 1.34, Packet 4474
20201015::141230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 14C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.7C, CTD 533.3dbar, CTD 34.2psu, index 1.34, Packet 4529
20201015::141300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 24.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.7C, CTD 544.2dbar, CTD 34.2psu, index 1.34, Packet 4584
20201015::141330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 13C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.6C, CTD 562.1dbar, CTD 34.2psu, index 1.34, Packet 4639
20201015::141400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 12C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 576.9dbar, CTD 34.2psu, index 1.34, Packet 4694
20201015::141430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 591.8dbar, CTD 34.3psu, index 1.34, Packet 4748
20201015::141500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 14C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 606.6dbar, CTD 34.3psu, index 1.34, Packet 4803
20201015::141530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 22.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 620.9dbar, CTD 34.3psu, index 1.34, Packet 4858
20201015::141600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 635.4dbar, CTD 34.3psu, index 1.34, Packet 4913
20201015::141630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 649.7dbar, CTD 34.3psu, index 1.34, Packet 4968
20201015::141700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.2C, CTD 664.1dbar, CTD 34.3psu, index 1.34, Packet 5023
20201015::141730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 678.6dbar, CTD 34.3psu, index 1.34, Packet 5078
20201015::141800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 693.3dbar, CTD 34.3psu, index 1.34, Packet 5133
20201015::141830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 708.6dbar, CTD 34.3psu, index 1.34, Packet 5188
20201015::141900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::141930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 723.8dbar, CTD 34.3psu, index 1.34, Packet 5243
20201015::141930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 23.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 739.8dbar, CTD 34.3psu, index 1.34, Packet 5298
20201015::142000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 755.8dbar, CTD 34.4psu, index 1.34, Packet 5353
20201015::142030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 770.2dbar, CTD 34.4psu, index 1.34, Packet 5408
20201015::142100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 785.2dbar, CTD 34.4psu, index 1.34, Packet 5463
20201015::142130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 800.7dbar, CTD 34.4psu, index 1.34, Packet 5518
20201015::142200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 816.7dbar, CTD 34.4psu, index 1.34, Packet 5573
20201015::142230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 12C, Laser 22.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 836.9dbar, CTD 34.4psu, index 1.34, Packet 5628
20201015::142300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 855.2dbar, CTD 34.4psu, index 1.34, Packet 5683
20201015::142330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 872.1dbar, CTD 34.4psu, index 1.34, Packet 5738
20201015::142400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 890.2dbar, CTD 34.4psu, index 1.34, Packet 5793
20201015::142430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 907.1dbar, CTD 34.4psu, index 1.34, Packet 5848
20201015::142500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 923.9dbar, CTD 34.4psu, index 1.34, Packet 5903
20201015::142530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 940.3dbar, CTD 34.4psu, index 1.34, Packet 5958
20201015::142600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 12C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 957.1dbar, CTD 34.4psu, index 1.34, Packet 6013
20201015::142630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 973.5dbar, CTD 34.4psu, index 1.34, Packet 6068
20201015::142700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.9C, CTD 989.5dbar, CTD 34.5psu, index 1.34, Packet 6123
20201015::142730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1006.7dbar, CTD 34.5psu, index 1.34, Packet 6178
20201015::142800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1023.2dbar, CTD 34.5psu, index 1.34, Packet 6233
20201015::142830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 24%, OPB 11C, Laser 21.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1040.6dbar, CTD 34.5psu, index 1.34, Packet 6288
20201015::142900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::142930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1056.8dbar, CTD 34.5psu, index 1.34, Packet 6343
20201015::142930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1073.9dbar, CTD 34.5psu, index 1.34, Packet 6398
20201015::143000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1090.8dbar, CTD 34.5psu, index 1.34, Packet 6453
20201015::143030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1106.1dbar, CTD 34.5psu, index 1.34, Packet 6508
20201015::143100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1121.7dbar, CTD 34.5psu, index 1.34, Packet 6563
20201015::143130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1137.0dbar, CTD 34.5psu, index 1.34, Packet 6618
20201015::143200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1152.2dbar, CTD 34.5psu, index 1.34, Packet 6673
20201015::143230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1166.9dbar, CTD 34.5psu, index 1.34, Packet 6728
20201015::143300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1181.9dbar, CTD 34.5psu, index 1.34, Packet 6783
20201015::143330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1198.4dbar, CTD 34.5psu, index 1.34, Packet 6838
20201015::143400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.2dbar, CTD 34.5psu, index 1.34, Packet 6893
20201015::143430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.6dbar, CTD 34.5psu, index 1.34, Packet 6948
20201015::143500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1250.8dbar, CTD 34.5psu, index 1.34, Packet 7003
20201015::143530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1267.4dbar, CTD 34.5psu, index 1.34, Packet 7058
20201015::143600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1284.7dbar, CTD 34.5psu, index 1.34, Packet 7113
20201015::143630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1301.1dbar, CTD 34.5psu, index 1.34, Packet 7168
20201015::143700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1317.8dbar, CTD 34.5psu, index 1.34, Packet 7223
20201015::143730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1334.5dbar, CTD 34.5psu, index 1.34, Packet 7278
20201015::143800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.9C, CTD 1350.4dbar, CTD 34.5psu, index 1.34, Packet 7333
20201015::143830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.9C, CTD 1367.2dbar, CTD 34.5psu, index 1.34, Packet 7388
20201015::143900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.9C, CTD 1384.0dbar, CTD 34.5psu, index 1.34, Packet 7443
20201015::143930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::143930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.8C, CTD 1400.6dbar, CTD 34.5psu, index 1.34, Packet 7497
20201015::144000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.8C, CTD 1417.1dbar, CTD 34.5psu, index 1.34, Packet 7553
20201015::144030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.8C, CTD 1433.5dbar, CTD 34.5psu, index 1.34, Packet 7607
20201015::144100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.8C, CTD 1450.0dbar, CTD 34.5psu, index 1.34, Packet 7662
20201015::144130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.7C, CTD 1467.0dbar, CTD 34.6psu, index 1.35, Packet 7718
20201015::144200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.7C, CTD 1483.4dbar, CTD 34.6psu, index 1.35, Packet 7773
20201015::144230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.7C, CTD 1500.2dbar, CTD 34.6psu, index 1.35, Packet 7828
20201015::144300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.6C, CTD 1516.6dbar, CTD 34.6psu, index 1.35, Packet 7882
20201015::144330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.6C, CTD 1533.6dbar, CTD 34.6psu, index 1.35, Packet 7938
20201015::144400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.6C, CTD 1550.5dbar, CTD 34.6psu, index 1.35, Packet 7992
20201015::144430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.6C, CTD 1567.6dbar, CTD 34.6psu, index 1.35, Packet 8048
20201015::144500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.5C, CTD 1582.2dbar, CTD 34.6psu, index 1.35, Packet 8103
20201015::144530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.5C, CTD 1597.2dbar, CTD 34.6psu, index 1.35, Packet 8158
20201015::144600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.5C, CTD 1617.2dbar, CTD 34.6psu, index 1.35, Packet 8213
20201015::144630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.4C, CTD 1635.6dbar, CTD 34.6psu, index 1.35, Packet 8267
20201015::144700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.4C, CTD 1653.0dbar, CTD 34.6psu, index 1.35, Packet 8323
20201015::144730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.4C, CTD 1670.1dbar, CTD 34.6psu, index 1.35, Packet 8378
20201015::144800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.3C, CTD 1687.5dbar, CTD 34.6psu, index 1.35, Packet 8433
20201015::144830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.3C, CTD 1704.5dbar, CTD 34.6psu, index 1.35, Packet 8487
20201015::144900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::144930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.3C, CTD 1722.0dbar, CTD 34.6psu, index 1.35, Packet 8543
20201015::144930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.3C, CTD 1739.5dbar, CTD 34.6psu, index 1.35, Packet 8598
20201015::145000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.3C, CTD 1756.8dbar, CTD 34.6psu, index 1.35, Packet 8652
20201015::145030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.2C, CTD 1774.4dbar, CTD 34.6psu, index 1.35, Packet 8708
20201015::145100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.2C, CTD 1792.2dbar, CTD 34.6psu, index 1.35, Packet 8763
20201015::145130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.2C, CTD 1811.5dbar, CTD 34.6psu, index 1.35, Packet 8818
20201015::145200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.2C, CTD 1830.9dbar, CTD 34.6psu, index 1.35, Packet 8873
20201015::145230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1850.0dbar, CTD 34.6psu, index 1.35, Packet 8928
20201015::145300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1869.0dbar, CTD 34.6psu, index 1.35, Packet 8983
20201015::145330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1887.8dbar, CTD 34.6psu, index 1.35, Packet 9038
20201015::145400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1905.8dbar, CTD 34.6psu, index 1.35, Packet 9093
20201015::145430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1922.5dbar, CTD 34.6psu, index 1.35, Packet 9148
20201015::145500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.1C, CTD 1934.8dbar, CTD 34.6psu, index 1.35, Packet 9203
20201015::145530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 1946.7dbar, CTD 34.6psu, index 1.35, Packet 9258
20201015::145600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 1964.7dbar, CTD 34.6psu, index 1.35, Packet 9313
20201015::145630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 1987.3dbar, CTD 34.6psu, index 1.35, Packet 9368
20201015::145700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 2004.2dbar, CTD 34.6psu, index 1.35, Packet 9423
20201015::145730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 8C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 2020.8dbar, CTD 34.6psu, index 1.35, Packet 9478
20201015::145800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 18.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 2039.0dbar, CTD 34.6psu, index 1.35, Packet 9533
20201015::145830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 2057.7dbar, CTD 34.6psu, index 1.35, Packet 9588
20201015::145900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.0C, CTD 2076.3dbar, CTD 34.6psu, index 1.35, Packet 9643
20201015::145930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::145930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2094.8dbar, CTD 34.6psu, index 1.35, Packet 9698
20201015::150000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2113.4dbar, CTD 34.6psu, index 1.35, Packet 9753
20201015::150030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2132.0dbar, CTD 34.6psu, index 1.35, Packet 9808
20201015::150100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2150.5dbar, CTD 34.6psu, index 1.35, Packet 9863
20201015::150130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2168.8dbar, CTD 34.6psu, index 1.35, Packet 9918
20201015::150200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2186.8dbar, CTD 34.6psu, index 1.35, Packet 9973
20201015::150230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2205.0dbar, CTD 34.6psu, index 1.35, Packet 10028
20201015::150300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2223.4dbar, CTD 34.6psu, index 1.35, Packet 10083
20201015::150330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2241.6dbar, CTD 34.6psu, index 1.35, Packet 10138
20201015::150400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2260.1dbar, CTD 34.6psu, index 1.35, Packet 10193
20201015::150430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2278.2dbar, CTD 34.6psu, index 1.35, Packet 10248
20201015::150500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.9C, CTD 2294.9dbar, CTD 34.6psu, index 1.35, Packet 10303
20201015::150530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2310.1dbar, CTD 34.6psu, index 1.35, Packet 10358
20201015::150600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2328.0dbar, CTD 34.6psu, index 1.35, Packet 10413
20201015::150630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2346.5dbar, CTD 34.6psu, index 1.35, Packet 10467
20201015::150700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2365.8dbar, CTD 34.6psu, index 1.35, Packet 10523
20201015::150730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 9C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2384.6dbar, CTD 34.6psu, index 1.35, Packet 10578
20201015::150800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2403.0dbar, CTD 34.6psu, index 1.35, Packet 10632
20201015::150830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2421.8dbar, CTD 34.6psu, index 1.35, Packet 10687
20201015::150900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2439.7dbar, CTD 34.6psu, index 1.35, Packet 10742
20201015::150930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::150930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151000: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2457.1dbar, CTD 34.6psu, index 1.35, Packet 10798
20201015::151000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151030: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2476.0dbar, CTD 34.6psu, index 1.35, Packet 10853
20201015::151030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2495.6dbar, CTD 34.6psu, index 1.35, Packet 10908
20201015::151100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2515.0dbar, CTD 34.6psu, index 1.35, Packet 10963
20201015::151130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2531.8dbar, CTD 34.6psu, index 1.35, Packet 11017
20201015::151200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2548.4dbar, CTD 34.6psu, index 1.35, Packet 11072
20201015::151230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.8C, CTD 2565.5dbar, CTD 34.6psu, index 1.35, Packet 11128
20201015::151300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151330: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2578.1dbar, CTD 34.6psu, index 1.35, Packet 11183
20201015::151330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151400: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2595.0dbar, CTD 34.6psu, index 1.35, Packet 11238
20201015::151400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151430: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2611.2dbar, CTD 34.7psu, index 1.35, Packet 11292
20201015::151430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151500: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2624.7dbar, CTD 34.7psu, index 1.35, Packet 11347
20201015::151500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151530: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2636.0dbar, CTD 34.7psu, index 1.35, Packet 11402
20201015::151530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151600: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2648.8dbar, CTD 34.7psu, index 1.35, Packet 11457
20201015::151600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151630: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2668.2dbar, CTD 34.7psu, index 1.35, Packet 11512
20201015::151630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151700: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2685.9dbar, CTD 34.7psu, index 1.35, Packet 11567
20201015::151700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2706.1dbar, CTD 34.7psu, index 1.35, Packet 11622
20201015::151730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2718.9dbar, CTD 34.7psu, index 1.35, Packet 11677
20201015::151800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151830: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2733.9dbar, CTD 34.7psu, index 1.35, Packet 11732
20201015::151830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2742.9dbar, CTD 34.7psu, index 1.35, Packet 11787
20201015::151900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2758.9dbar, CTD 34.7psu, index 1.35, Packet 11842
20201015::151930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 0, laser state 0
20201015::151958: Head 1: Setting Gain 8
20201015::151958: Head 2: Setting Gain 8
20201015::152000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152000: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2775.5dbar, CTD 34.7psu, index 1.35, Packet 11897
20201015::152000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152030: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2790.4dbar, CTD 34.7psu, index 1.35, Packet 11952
20201015::152030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152100: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2809.8dbar, CTD 34.7psu, index 1.35, Packet 12007
20201015::152100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152130: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2822.7dbar, CTD 34.7psu, index 1.35, Packet 12062
20201015::152130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152200: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2838.6dbar, CTD 34.7psu, index 1.35, Packet 12117
20201015::152200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152230: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2853.2dbar, CTD 34.7psu, index 1.35, Packet 12172
20201015::152230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152300: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2865.4dbar, CTD 34.7psu, index 1.35, Packet 12227
20201015::152300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152330: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 12282
20201015::152330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152400: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 12337
20201015::152400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152430: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 12391
20201015::152430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152500: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 12446
20201015::152500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152530: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 12502
20201015::152530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152600: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 12557
20201015::152600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152630: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 12612
20201015::152630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152700: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 12667
20201015::152700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152730: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 12722
20201015::152730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152800: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 12777
20201015::152800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152830: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 12832
20201015::152830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152900: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 12887
20201015::152900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::152930: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 12942
20201015::152930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153000: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 12997
20201015::153000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153030: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 13052
20201015::153030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153100: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 13107
20201015::153100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153130: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 13162
20201015::153130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153200: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 13217
20201015::153200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153230: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 13272
20201015::153230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153300: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 13327
20201015::153300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153330: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 13381
20201015::153330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153400: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 13436
20201015::153400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153430: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13491
20201015::153430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153500: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13546
20201015::153500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153530: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13601
20201015::153530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153600: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13656
20201015::153600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153630: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13710
20201015::153630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153700: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 13766
20201015::153700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153730: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 13821
20201015::153730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153800: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 13876
20201015::153800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153830: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 13931
20201015::153830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153900: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 13985
20201015::153900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::153930: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 14041
20201015::153930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154000: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 14096
20201015::154000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154030: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 14151
20201015::154030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154100: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 14205
20201015::154100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154130: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 14260
20201015::154130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154200: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14315
20201015::154200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154230: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14369
20201015::154230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154300: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14424
20201015::154300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154330: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14479
20201015::154330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 0
20201015::154344: GUI: Live mode ON.
20201015::154344: GUI: Requesing START operation, Head 1
20201015::154344: GUI: Requesing START operation, Head 2
20201015::154345: Head 1: Received request: START
20201015::154345: Head 2: Received request: START
20201015::154345: Head 1: Starting Scan Operation
20201015::154345: Head 2: Starting Scan Operation
20201015::154346: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::154346: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::154346: Head 2: Eye Safe Optical Filter check Passed
20201015::154347: Head 1: Eye Safe Optical Filter check Passed
20201015::154352: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::154353: Head 2: Eye Safe Optical Filter check Passed
20201015::154356: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::154356: Head 1: Eye Safe Optical Filter check Passed
20201015::154400: Head 1: Configured for WATER Processing
20201015::154400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 15.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 1
20201015::154400: Head 1: Configured for WATER Processing
20201015::154400: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14534
20201015::154400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 20.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154400: Head 1: Configured for WATER Processing
20201015::154401: Head 1: Configured for WATER Processing
20201015::154401: Head 1: Configured for WATER Processing
20201015::154401: Head 1: Configured for WATER Processing
20201015::154401: Head 1: Configured for WATER Processing
20201015::154402: Head 1: Configured for WATER Processing
20201015::154402: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154400_wf.raa
20201015::154402: Head 1: Configured for WATER Processing
20201015::154402: Head 1: Configured for WATER Processing
20201015::154403: Head 1: Configured for WATER Processing
20201015::154403: Head 1: Configured for WATER Processing
20201015::154403: Head 1: Configured for WATER Processing
20201015::154404: Head 1: Configured for WATER Processing
20201015::154404: Head 1: Configured for WATER Processing
20201015::154405: Head 1: Configured for WATER Processing
20201015::154405: Head 1: Configured for WATER Processing
20201015::154405: Head 1: Configured for WATER Processing
20201015::154406: Head 1: Configured for WATER Processing
20201015::154406: Head 1: Configured for WATER Processing
20201015::154410: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154410_wf.raa
20201015::154418: Head 2: Configured for WATER Processing
20201015::154418: Head 2: Configured for WATER Processing
20201015::154418: Head 2: Configured for WATER Processing
20201015::154418: Head 2: Configured for WATER Processing
20201015::154419: Head 2: Configured for WATER Processing
20201015::154419: Head 2: Configured for WATER Processing
20201015::154419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154420_wf.raa
20201015::154419: Head 2: Configured for WATER Processing
20201015::154420: Head 2: Configured for WATER Processing
20201015::154420: Head 2: Configured for WATER Processing
20201015::154420: Head 2: Configured for WATER Processing
20201015::154421: Head 2: Configured for WATER Processing
20201015::154421: Head 2: Configured for WATER Processing
20201015::154421: Head 2: Configured for WATER Processing
20201015::154421: Head 2: Configured for WATER Processing
20201015::154422: Head 2: Configured for WATER Processing
20201015::154422: Head 2: Configured for WATER Processing
20201015::154422: Head 2: Configured for WATER Processing
20201015::154423: Head 2: Configured for WATER Processing
20201015::154423: Head 2: Configured for WATER Processing
20201015::154423: Head 2: Configured for WATER Processing
20201015::154429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154430_wf.raa
20201015::154430: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14588
20201015::154430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 20.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 16.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154440_wf.raa
20201015::154449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154450_wf.raa
20201015::154459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154500_wf.raa
20201015::154500: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14642
20201015::154500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 24%, OPB 7C, Laser 17.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154510_wf.raa
20201015::154519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154520_wf.raa
20201015::154529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154530_wf.raa
20201015::154530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154530: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 14697
20201015::154530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154540_wf.raa
20201015::154549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154550_wf.raa
20201015::154559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154600_wf.raa
20201015::154600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154600: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14752
20201015::154600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154610_wf.raa
20201015::154619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154620_wf.raa
20201015::154629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154630_wf.raa
20201015::154630: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14806
20201015::154630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154640_wf.raa
20201015::154649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154650_wf.raa
20201015::154659: Head 2: Time Synchronization: 2020.10.15   15:47:00::0014
20201015::154659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154700_wf.raa
20201015::154700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154700: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14862
20201015::154700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154710_wf.raa
20201015::154719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154720_wf.raa
20201015::154729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154730_wf.raa
20201015::154730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154730: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14917
20201015::154730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154740_wf.raa
20201015::154749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154750_wf.raa
20201015::154759: Head 1: Time Synchronization: 2020.10.15   15:48:00::0016
20201015::154759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154800_wf.raa
20201015::154800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154800: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 14972
20201015::154800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154810_wf.raa
20201015::154819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154820_wf.raa
20201015::154829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154830_wf.raa
20201015::154830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154830: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15027
20201015::154830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154840_wf.raa
20201015::154849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154850_wf.raa
20201015::154859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154900_wf.raa
20201015::154900: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15082
20201015::154900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154910_wf.raa
20201015::154919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154920_wf.raa
20201015::154929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154930_wf.raa
20201015::154930: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15137
20201015::154930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201015::154939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154940_wf.raa
20201015::154949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_154950_wf.raa
20201015::154951: Head 1: Setting Gain 7
20201015::154951: Head 2: Setting Gain 7
20201015::154959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155000_wf.raa
20201015::155000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15193
20201015::155000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155010_wf.raa
20201015::155019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155020_wf.raa
20201015::155024: Head 2: Setting Gain 8
20201015::155024: Head 1: Setting Gain 8
20201015::155029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155030_wf.raa
20201015::155030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201015::155030: System  Initialized, Gain 8, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15248
20201015::155030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20201015::155039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155040_wf.raa
20201015::155046: Head 1: Setting Gain 7
20201015::155046: Head 2: Setting Gain 7
20201015::155049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155050_wf.raa
20201015::155059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155100_wf.raa
20201015::155100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15303
20201015::155100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155110_wf.raa
20201015::155119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155120_wf.raa
20201015::155129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155130_wf.raa
20201015::155130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15358
20201015::155130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155140_wf.raa
20201015::155149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155150_wf.raa
20201015::155159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155200_wf.raa
20201015::155200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15413
20201015::155200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155210_wf.raa
20201015::155219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155220_wf.raa
20201015::155229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155230_wf.raa
20201015::155230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15468
20201015::155230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155240_wf.raa
20201015::155249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155250_wf.raa
20201015::155259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155300_wf.raa
20201015::155300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15523
20201015::155300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155310_wf.raa
20201015::155319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155320_wf.raa
20201015::155329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155330_wf.raa
20201015::155330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15578
20201015::155330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155340_wf.raa
20201015::155349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155350_wf.raa
20201015::155359: Head 1: Time Synchronization: 2020.10.15   15:54:00::0016
20201015::155359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155400_wf.raa
20201015::155400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15634
20201015::155400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155410_wf.raa
20201015::155419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155420_wf.raa
20201015::155429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155430_wf.raa
20201015::155430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15689
20201015::155430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155440_wf.raa
20201015::155449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155450_wf.raa
20201015::155459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155500_wf.raa
20201015::155500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15744
20201015::155500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155510_wf.raa
20201015::155519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155520_wf.raa
20201015::155529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155530_wf.raa
20201015::155530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15799
20201015::155530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155540_wf.raa
20201015::155549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155550_wf.raa
20201015::155559: Head 1: Time Synchronization: 2020.10.15   15:56:00::0016
20201015::155559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155600_wf.raa
20201015::155600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 15855
20201015::155600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155610_wf.raa
20201015::155619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155620_wf.raa
20201015::155629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155630_wf.raa
20201015::155630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 15909
20201015::155630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155640_wf.raa
20201015::155649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155650_wf.raa
20201015::155659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155700_wf.raa
20201015::155700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 15965
20201015::155700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155710_wf.raa
20201015::155719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155720_wf.raa
20201015::155729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155730_wf.raa
20201015::155730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 16019
20201015::155730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155740_wf.raa
20201015::155749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155750_wf.raa
20201015::155759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155800_wf.raa
20201015::155800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 16074
20201015::155800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155810_wf.raa
20201015::155819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155820_wf.raa
20201015::155829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155830_wf.raa
20201015::155830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 16130
20201015::155830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155840_wf.raa
20201015::155849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155850_wf.raa
20201015::155859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155900_wf.raa
20201015::155900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 16185
20201015::155900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155910_wf.raa
20201015::155919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155920_wf.raa
20201015::155929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155930_wf.raa
20201015::155930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 16240
20201015::155930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::155939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155940_wf.raa
20201015::155949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_155950_wf.raa
20201015::155959: Head 1: Time Synchronization: 2020.10.15   16:00:00::0015
20201015::155959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160000_wf.raa
20201015::160000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 16295
20201015::160000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160010_wf.raa
20201015::160019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160020_wf.raa
20201015::160029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160030_wf.raa
20201015::160030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 16350
20201015::160030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160040_wf.raa
20201015::160049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160050_wf.raa
20201015::160059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160100_wf.raa
20201015::160100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 16405
20201015::160100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160110_wf.raa
20201015::160119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160120_wf.raa
20201015::160129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160130_wf.raa
20201015::160130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 16460
20201015::160130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160140_wf.raa
20201015::160149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160150_wf.raa
20201015::160159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160200_wf.raa
20201015::160200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 16515
20201015::160200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160210_wf.raa
20201015::160219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160220_wf.raa
20201015::160229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160230_wf.raa
20201015::160230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 16569
20201015::160230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160240_wf.raa
20201015::160249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160250_wf.raa
20201015::160259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160300_wf.raa
20201015::160300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 16624
20201015::160300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160310_wf.raa
20201015::160319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160320_wf.raa
20201015::160329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160330_wf.raa
20201015::160330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 16679
20201015::160330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160340_wf.raa
20201015::160349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160350_wf.raa
20201015::160359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160400_wf.raa
20201015::160400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 16735
20201015::160400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160410_wf.raa
20201015::160419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160420_wf.raa
20201015::160429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160430_wf.raa
20201015::160430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.3dbar, CTD 34.7psu, index 1.35, Packet 16790
20201015::160430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160440_wf.raa
20201015::160449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160450_wf.raa
20201015::160459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160500_wf.raa
20201015::160500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.3dbar, CTD 34.7psu, index 1.35, Packet 16845
20201015::160500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160510_wf.raa
20201015::160519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160520_wf.raa
20201015::160529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160530_wf.raa
20201015::160530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.3dbar, CTD 34.7psu, index 1.35, Packet 16901
20201015::160530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160540_wf.raa
20201015::160549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160550_wf.raa
20201015::160559: Head 1: Time Synchronization: 2020.10.15   16:06:00::0015
20201015::160559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160600_wf.raa
20201015::160600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 16956
20201015::160600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160610_wf.raa
20201015::160619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160620_wf.raa
20201015::160629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160630_wf.raa
20201015::160630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 17012
20201015::160630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160640_wf.raa
20201015::160649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160650_wf.raa
20201015::160659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160700_wf.raa
20201015::160700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 17067
20201015::160700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160710_wf.raa
20201015::160719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160720_wf.raa
20201015::160729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160730_wf.raa
20201015::160730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 17122
20201015::160730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160740_wf.raa
20201015::160749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160750_wf.raa
20201015::160759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160800_wf.raa
20201015::160800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 17177
20201015::160800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160810_wf.raa
20201015::160819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160820_wf.raa
20201015::160829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160830_wf.raa
20201015::160830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 17232
20201015::160830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160840_wf.raa
20201015::160849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160850_wf.raa
20201015::160859: Head 1: Time Synchronization: 2020.10.15   16:09:00::0015
20201015::160859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160900_wf.raa
20201015::160900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 17288
20201015::160900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160910_wf.raa
20201015::160919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160920_wf.raa
20201015::160929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160930_wf.raa
20201015::160930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 17343
20201015::160930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::160939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160940_wf.raa
20201015::160949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_160950_wf.raa
20201015::160959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161000_wf.raa
20201015::161000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 17398
20201015::161000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161010_wf.raa
20201015::161019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161020_wf.raa
20201015::161029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161030_wf.raa
20201015::161030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 17453
20201015::161030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161040_wf.raa
20201015::161049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161050_wf.raa
20201015::161059: Head 1: Time Synchronization: 2020.10.15   16:11:00::0018
20201015::161059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161100_wf.raa
20201015::161100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 17508
20201015::161100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161110_wf.raa
20201015::161119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161120_wf.raa
20201015::161129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161130_wf.raa
20201015::161130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 17563
20201015::161130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161140_wf.raa
20201015::161149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161150_wf.raa
20201015::161159: Head 1: Time Synchronization: 2020.10.15   16:12:00::0015
20201015::161159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161200_wf.raa
20201015::161200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 17617
20201015::161200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161210_wf.raa
20201015::161219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161220_wf.raa
20201015::161229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161230_wf.raa
20201015::161230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 17673
20201015::161230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161240_wf.raa
20201015::161249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161250_wf.raa
20201015::161259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161300_wf.raa
20201015::161300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 17727
20201015::161300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161310_wf.raa
20201015::161319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161320_wf.raa
20201015::161329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161330_wf.raa
20201015::161330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 17782
20201015::161330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161340_wf.raa
20201015::161349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161350_wf.raa
20201015::161359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161400_wf.raa
20201015::161400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 17837
20201015::161400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161410_wf.raa
20201015::161419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161420_wf.raa
20201015::161429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161430_wf.raa
20201015::161430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 17891
20201015::161430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161440_wf.raa
20201015::161449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161450_wf.raa
20201015::161459: Head 1: Time Synchronization: 2020.10.15   16:15:00::0014
20201015::161459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161500_wf.raa
20201015::161500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 17946
20201015::161500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161510_wf.raa
20201015::161519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161520_wf.raa
20201015::161529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161530_wf.raa
20201015::161530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 18001
20201015::161530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161540_wf.raa
20201015::161549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161550_wf.raa
20201015::161559: Head 1: Time Synchronization: 2020.10.15   16:16:00::0015
20201015::161559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161600_wf.raa
20201015::161600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 18056
20201015::161600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161610_wf.raa
20201015::161619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161620_wf.raa
20201015::161629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161630_wf.raa
20201015::161630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 18111
20201015::161630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161640_wf.raa
20201015::161649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161650_wf.raa
20201015::161659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161700_wf.raa
20201015::161700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 18166
20201015::161700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161710_wf.raa
20201015::161719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161720_wf.raa
20201015::161729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161730_wf.raa
20201015::161730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 18220
20201015::161730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161740_wf.raa
20201015::161749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161750_wf.raa
20201015::161759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161800_wf.raa
20201015::161800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 18275
20201015::161800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161810_wf.raa
20201015::161819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161820_wf.raa
20201015::161829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161830_wf.raa
20201015::161830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 18330
20201015::161830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161840_wf.raa
20201015::161849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161850_wf.raa
20201015::161859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161900_wf.raa
20201015::161900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 18385
20201015::161900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161910_wf.raa
20201015::161919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161920_wf.raa
20201015::161929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161930_wf.raa
20201015::161930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 18440
20201015::161930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::161939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161940_wf.raa
20201015::161949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_161950_wf.raa
20201015::161959: Head 2: Time Synchronization: 2020.10.15   16:20:00::0015
20201015::161959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162000_wf.raa
20201015::162000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 18495
20201015::162000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162010_wf.raa
20201015::162019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162020_wf.raa
20201015::162029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162030_wf.raa
20201015::162030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 18549
20201015::162030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162040_wf.raa
20201015::162049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162050_wf.raa
20201015::162059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162100_wf.raa
20201015::162100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 18604
20201015::162100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162110_wf.raa
20201015::162119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162120_wf.raa
20201015::162129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162130_wf.raa
20201015::162130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 18658
20201015::162130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162140_wf.raa
20201015::162149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162150_wf.raa
20201015::162159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162200_wf.raa
20201015::162200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 18714
20201015::162200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162210_wf.raa
20201015::162219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162220_wf.raa
20201015::162229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162230_wf.raa
20201015::162230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 18768
20201015::162230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162240_wf.raa
20201015::162249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162250_wf.raa
20201015::162259: Head 1: Time Synchronization: 2020.10.15   16:23:00::0014
20201015::162259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162300_wf.raa
20201015::162300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 18823
20201015::162300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162310_wf.raa
20201015::162319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162320_wf.raa
20201015::162329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162330_wf.raa
20201015::162330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 18878
20201015::162330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162340_wf.raa
20201015::162349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162350_wf.raa
20201015::162359: Head 1: Time Synchronization: 2020.10.15   16:24:00::0015
20201015::162359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162400_wf.raa
20201015::162400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 18933
20201015::162400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162410_wf.raa
20201015::162419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162420_wf.raa
20201015::162429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162430_wf.raa
20201015::162430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 18987
20201015::162430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162440_wf.raa
20201015::162449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162450_wf.raa
20201015::162459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162500_wf.raa
20201015::162500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 19042
20201015::162500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162510_wf.raa
20201015::162519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162520_wf.raa
20201015::162529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162530_wf.raa
20201015::162530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 19097
20201015::162530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162540_wf.raa
20201015::162549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162550_wf.raa
20201015::162559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162600_wf.raa
20201015::162600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 19151
20201015::162600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162610_wf.raa
20201015::162619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162620_wf.raa
20201015::162629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162630_wf.raa
20201015::162630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 19206
20201015::162630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162640_wf.raa
20201015::162649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162650_wf.raa
20201015::162659: Head 2: Time Synchronization: 2020.10.15   16:27:00::0015
20201015::162659: Head 1: Time Synchronization: 2020.10.15   16:27:00::0015
20201015::162659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162700_wf.raa
20201015::162700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 19261
20201015::162700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162710_wf.raa
20201015::162719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162720_wf.raa
20201015::162729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162730_wf.raa
20201015::162730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 19316
20201015::162730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162740_wf.raa
20201015::162749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162750_wf.raa
20201015::162759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162800_wf.raa
20201015::162800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 19370
20201015::162800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162810_wf.raa
20201015::162819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162820_wf.raa
20201015::162829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162830_wf.raa
20201015::162830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 19425
20201015::162830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162840_wf.raa
20201015::162849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162850_wf.raa
20201015::162859: Head 2: Time Synchronization: 2020.10.15   16:29:00::0015
20201015::162859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162900_wf.raa
20201015::162900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 19479
20201015::162900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162910_wf.raa
20201015::162919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162920_wf.raa
20201015::162929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162930_wf.raa
20201015::162930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 19534
20201015::162930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::162939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162940_wf.raa
20201015::162949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_162950_wf.raa
20201015::162959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163000_wf.raa
20201015::163000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 19588
20201015::163000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163010_wf.raa
20201015::163019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163020_wf.raa
20201015::163029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163030_wf.raa
20201015::163030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 19643
20201015::163030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163040_wf.raa
20201015::163049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163050_wf.raa
20201015::163059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163100_wf.raa
20201015::163100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 19698
20201015::163100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163110_wf.raa
20201015::163119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163120_wf.raa
20201015::163129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163130_wf.raa
20201015::163130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 19752
20201015::163130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163140_wf.raa
20201015::163149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163150_wf.raa
20201015::163159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163200_wf.raa
20201015::163200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 19807
20201015::163200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163210_wf.raa
20201015::163219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163220_wf.raa
20201015::163229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163230_wf.raa
20201015::163230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 19861
20201015::163230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163240_wf.raa
20201015::163249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163250_wf.raa
20201015::163259: Head 1: Time Synchronization: 2020.10.15   16:33:00::0017
20201015::163259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163300_wf.raa
20201015::163300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 19917
20201015::163300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163310_wf.raa
20201015::163319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163320_wf.raa
20201015::163329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163330_wf.raa
20201015::163330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 19971
20201015::163330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163340_wf.raa
20201015::163349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163350_wf.raa
20201015::163359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163400_wf.raa
20201015::163400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 20026
20201015::163400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163410_wf.raa
20201015::163419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163420_wf.raa
20201015::163429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163430_wf.raa
20201015::163430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 20081
20201015::163430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163440_wf.raa
20201015::163449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163450_wf.raa
20201015::163459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163500_wf.raa
20201015::163500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 20135
20201015::163500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163510_wf.raa
20201015::163519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163520_wf.raa
20201015::163529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163530_wf.raa
20201015::163530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 20191
20201015::163530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163540_wf.raa
20201015::163549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163550_wf.raa
20201015::163559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163600_wf.raa
20201015::163600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 20246
20201015::163600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163610_wf.raa
20201015::163619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163620_wf.raa
20201015::163629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163630_wf.raa
20201015::163630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 20301
20201015::163630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163640_wf.raa
20201015::163649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163650_wf.raa
20201015::163659: Head 1: Time Synchronization: 2020.10.15   16:37:00::0015
20201015::163659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163700_wf.raa
20201015::163700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 20356
20201015::163700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163710_wf.raa
20201015::163719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163720_wf.raa
20201015::163729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163730_wf.raa
20201015::163730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 20412
20201015::163730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163740_wf.raa
20201015::163749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163750_wf.raa
20201015::163759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163800_wf.raa
20201015::163800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 20467
20201015::163800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163810_wf.raa
20201015::163819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163820_wf.raa
20201015::163829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163830_wf.raa
20201015::163830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 20521
20201015::163830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163840_wf.raa
20201015::163849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163850_wf.raa
20201015::163859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163900_wf.raa
20201015::163900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 20576
20201015::163900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163910_wf.raa
20201015::163919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163920_wf.raa
20201015::163929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163930_wf.raa
20201015::163930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 20631
20201015::163930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::163939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163940_wf.raa
20201015::163949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_163950_wf.raa
20201015::163959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164000_wf.raa
20201015::164000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 20686
20201015::164000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164010_wf.raa
20201015::164019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164020_wf.raa
20201015::164029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164030_wf.raa
20201015::164030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 20742
20201015::164030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164040_wf.raa
20201015::164049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164050_wf.raa
20201015::164059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164100_wf.raa
20201015::164100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 20796
20201015::164100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164110_wf.raa
20201015::164119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164120_wf.raa
20201015::164129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164130_wf.raa
20201015::164130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 20852
20201015::164130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164140_wf.raa
20201015::164149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164150_wf.raa
20201015::164159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164200_wf.raa
20201015::164200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 20907
20201015::164200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164210_wf.raa
20201015::164219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164220_wf.raa
20201015::164229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164230_wf.raa
20201015::164230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 20962
20201015::164230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164240_wf.raa
20201015::164249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164250_wf.raa
20201015::164259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164300_wf.raa
20201015::164300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 21016
20201015::164300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164310_wf.raa
20201015::164319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164320_wf.raa
20201015::164329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164330_wf.raa
20201015::164330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 21072
20201015::164330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164340_wf.raa
20201015::164349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164350_wf.raa
20201015::164359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164400_wf.raa
20201015::164400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 21127
20201015::164400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164410_wf.raa
20201015::164419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164420_wf.raa
20201015::164429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164430_wf.raa
20201015::164430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 21182
20201015::164430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164440_wf.raa
20201015::164449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164450_wf.raa
20201015::164459: Head 2: Time Synchronization: 2020.10.15   16:45:00::0015
20201015::164459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164500_wf.raa
20201015::164500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 21237
20201015::164500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164510_wf.raa
20201015::164519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164520_wf.raa
20201015::164529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164530_wf.raa
20201015::164530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 21293
20201015::164530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164540_wf.raa
20201015::164549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164550_wf.raa
20201015::164559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164600_wf.raa
20201015::164600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 21348
20201015::164600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164610_wf.raa
20201015::164619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164620_wf.raa
20201015::164629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164630_wf.raa
20201015::164630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 21403
20201015::164630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164640_wf.raa
20201015::164649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164650_wf.raa
20201015::164659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164700_wf.raa
20201015::164700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 21459
20201015::164700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164710_wf.raa
20201015::164719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164720_wf.raa
20201015::164729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164730_wf.raa
20201015::164730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 21514
20201015::164730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164740_wf.raa
20201015::164749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164750_wf.raa
20201015::164759: Head 2: Time Synchronization: 2020.10.15   16:48:00::0015
20201015::164759: Head 1: Time Synchronization: 2020.10.15   16:48:00::0015
20201015::164759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164800_wf.raa
20201015::164800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 21569
20201015::164800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164810_wf.raa
20201015::164819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164820_wf.raa
20201015::164829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164830_wf.raa
20201015::164830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 21625
20201015::164830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164840_wf.raa
20201015::164849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164850_wf.raa
20201015::164859: Head 1: Time Synchronization: 2020.10.15   16:49:00::0015
20201015::164859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164900_wf.raa
20201015::164900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 21680
20201015::164900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164910_wf.raa
20201015::164919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164920_wf.raa
20201015::164929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164930_wf.raa
20201015::164930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 21735
20201015::164930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::164939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164940_wf.raa
20201015::164949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_164950_wf.raa
20201015::164959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165000_wf.raa
20201015::165000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 21790
20201015::165000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165010_wf.raa
20201015::165019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165020_wf.raa
20201015::165029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165030_wf.raa
20201015::165030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 21845
20201015::165030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165040_wf.raa
20201015::165049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165050_wf.raa
20201015::165059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165100_wf.raa
20201015::165100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 21900
20201015::165100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165110_wf.raa
20201015::165119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165120_wf.raa
20201015::165129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165130_wf.raa
20201015::165130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 21956
20201015::165130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165140_wf.raa
20201015::165149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165150_wf.raa
20201015::165159: Head 1: Time Synchronization: 2020.10.15   16:52:00::0015
20201015::165159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165200_wf.raa
20201015::165200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 22010
20201015::165200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165210_wf.raa
20201015::165219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165220_wf.raa
20201015::165229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165230_wf.raa
20201015::165230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 22065
20201015::165230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165240_wf.raa
20201015::165249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165250_wf.raa
20201015::165259: Head 2: Time Synchronization: 2020.10.15   16:53:00::0014
20201015::165259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165300_wf.raa
20201015::165300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 22120
20201015::165300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165310_wf.raa
20201015::165319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165320_wf.raa
20201015::165329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165330_wf.raa
20201015::165330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 22175
20201015::165330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165340_wf.raa
20201015::165349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165350_wf.raa
20201015::165359: Head 1: Time Synchronization: 2020.10.15   16:54:00::0014
20201015::165359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165400_wf.raa
20201015::165400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 22230
20201015::165400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165410_wf.raa
20201015::165419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165420_wf.raa
20201015::165429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165430_wf.raa
20201015::165430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 22286
20201015::165430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165440_wf.raa
20201015::165449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165450_wf.raa
20201015::165459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165500_wf.raa
20201015::165500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 22341
20201015::165500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165510_wf.raa
20201015::165519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165520_wf.raa
20201015::165529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165530_wf.raa
20201015::165530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 22396
20201015::165530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165540_wf.raa
20201015::165549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165550_wf.raa
20201015::165559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165600_wf.raa
20201015::165600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 22451
20201015::165600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165610_wf.raa
20201015::165619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165620_wf.raa
20201015::165629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165630_wf.raa
20201015::165630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 22506
20201015::165630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165640_wf.raa
20201015::165649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165650_wf.raa
20201015::165659: Head 2: Time Synchronization: 2020.10.15   16:57:00::0014
20201015::165659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165700_wf.raa
20201015::165700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 22561
20201015::165700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165710_wf.raa
20201015::165719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165720_wf.raa
20201015::165729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165730_wf.raa
20201015::165730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 22617
20201015::165730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165740_wf.raa
20201015::165749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165750_wf.raa
20201015::165759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165800_wf.raa
20201015::165800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 22673
20201015::165800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165810_wf.raa
20201015::165819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165820_wf.raa
20201015::165829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165830_wf.raa
20201015::165830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 22727
20201015::165830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165840_wf.raa
20201015::165849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165850_wf.raa
20201015::165859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165900_wf.raa
20201015::165900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 22782
20201015::165900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165910_wf.raa
20201015::165919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165920_wf.raa
20201015::165929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165930_wf.raa
20201015::165930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 22838
20201015::165930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::165939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165940_wf.raa
20201015::165949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_165950_wf.raa
20201015::165959: Head 1: Time Synchronization: 2020.10.15   17:00:00::0014
20201015::165959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170000_wf.raa
20201015::170000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 22894
20201015::170000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170010_wf.raa
20201015::170019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170020_wf.raa
20201015::170029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170030_wf.raa
20201015::170030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 22948
20201015::170030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170040_wf.raa
20201015::170049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170050_wf.raa
20201015::170059: Head 1: Time Synchronization: 2020.10.15   17:01:00::0015
20201015::170059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170100_wf.raa
20201015::170100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 23003
20201015::170100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170110_wf.raa
20201015::170119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170120_wf.raa
20201015::170129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170130_wf.raa
20201015::170130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 23058
20201015::170130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170140_wf.raa
20201015::170149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170150_wf.raa
20201015::170159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170200_wf.raa
20201015::170200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 23113
20201015::170200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170210_wf.raa
20201015::170219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170220_wf.raa
20201015::170229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170230_wf.raa
20201015::170230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 23168
20201015::170230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170240_wf.raa
20201015::170249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170250_wf.raa
20201015::170259: Head 1: Time Synchronization: 2020.10.15   17:03:00::0015
20201015::170259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170300_wf.raa
20201015::170300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 23223
20201015::170300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170310_wf.raa
20201015::170319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170320_wf.raa
20201015::170329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170330_wf.raa
20201015::170330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 23279
20201015::170330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170340_wf.raa
20201015::170349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170350_wf.raa
20201015::170359: Head 2: Time Synchronization: 2020.10.15   17:04:00::0015
20201015::170359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170400_wf.raa
20201015::170400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 23333
20201015::170400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170410_wf.raa
20201015::170419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170420_wf.raa
20201015::170429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170430_wf.raa
20201015::170430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 23389
20201015::170430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170440_wf.raa
20201015::170449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170450_wf.raa
20201015::170459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170500_wf.raa
20201015::170500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 23443
20201015::170500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170510_wf.raa
20201015::170519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170520_wf.raa
20201015::170529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170530_wf.raa
20201015::170530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 23499
20201015::170530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170540_wf.raa
20201015::170549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170550_wf.raa
20201015::170559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170600_wf.raa
20201015::170600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 23553
20201015::170600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170610_wf.raa
20201015::170619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170620_wf.raa
20201015::170629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170630_wf.raa
20201015::170630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 23609
20201015::170630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170640_wf.raa
20201015::170649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170650_wf.raa
20201015::170659: Head 1: Time Synchronization: 2020.10.15   17:07:00::0014
20201015::170659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170700_wf.raa
20201015::170700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 23663
20201015::170700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170710_wf.raa
20201015::170719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170720_wf.raa
20201015::170729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170730_wf.raa
20201015::170730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 23718
20201015::170730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170740_wf.raa
20201015::170749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170750_wf.raa
20201015::170759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170800_wf.raa
20201015::170800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 23773
20201015::170800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170810_wf.raa
20201015::170819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170820_wf.raa
20201015::170829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170830_wf.raa
20201015::170830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 23829
20201015::170830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170840_wf.raa
20201015::170849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170850_wf.raa
20201015::170859: Head 1: Time Synchronization: 2020.10.15   17:09:00::0015
20201015::170859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170900_wf.raa
20201015::170900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 23885
20201015::170900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170910_wf.raa
20201015::170919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170920_wf.raa
20201015::170929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170930_wf.raa
20201015::170930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 23940
20201015::170930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::170939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170940_wf.raa
20201015::170949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_170950_wf.raa
20201015::170959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171000_wf.raa
20201015::171000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 23995
20201015::171000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171010_wf.raa
20201015::171019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171020_wf.raa
20201015::171029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171030_wf.raa
20201015::171030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 24050
20201015::171030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171040_wf.raa
20201015::171049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171050_wf.raa
20201015::171059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171100_wf.raa
20201015::171100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 24106
20201015::171100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171110_wf.raa
20201015::171119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171120_wf.raa
20201015::171129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171130_wf.raa
20201015::171130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 24161
20201015::171130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171140_wf.raa
20201015::171149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171150_wf.raa
20201015::171159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171200_wf.raa
20201015::171200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 24217
20201015::171200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171210_wf.raa
20201015::171219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171220_wf.raa
20201015::171229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171230_wf.raa
20201015::171230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 24272
20201015::171230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171240_wf.raa
20201015::171249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171250_wf.raa
20201015::171259: Head 1: Time Synchronization: 2020.10.15   17:13:00::0016
20201015::171259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171300_wf.raa
20201015::171300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 24328
20201015::171300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171310_wf.raa
20201015::171319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171320_wf.raa
20201015::171329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171330_wf.raa
20201015::171330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 24383
20201015::171330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171340_wf.raa
20201015::171350: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171350_wf.raa
20201015::171359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171400_wf.raa
20201015::171400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 24438
20201015::171400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171410_wf.raa
20201015::171419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171420_wf.raa
20201015::171429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171430_wf.raa
20201015::171430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 24493
20201015::171430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171440_wf.raa
20201015::171449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171450_wf.raa
20201015::171459: Head 1: Time Synchronization: 2020.10.15   17:15:00::0016
20201015::171459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171500_wf.raa
20201015::171500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 24548
20201015::171500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171510_wf.raa
20201015::171519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171520_wf.raa
20201015::171529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171530_wf.raa
20201015::171530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 24603
20201015::171530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171540_wf.raa
20201015::171549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171550_wf.raa
20201015::171559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171600_wf.raa
20201015::171600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 24659
20201015::171600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171610_wf.raa
20201015::171619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171620_wf.raa
20201015::171629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171630_wf.raa
20201015::171630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 24714
20201015::171630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171640_wf.raa
20201015::171649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171650_wf.raa
20201015::171659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171700_wf.raa
20201015::171700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 24769
20201015::171700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171710_wf.raa
20201015::171719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171720_wf.raa
20201015::171729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171730_wf.raa
20201015::171730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 24825
20201015::171730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171740_wf.raa
20201015::171749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171750_wf.raa
20201015::171759: Head 2: Time Synchronization: 2020.10.15   17:18:00::0015
20201015::171759: Head 1: Time Synchronization: 2020.10.15   17:18:00::0015
20201015::171759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171800_wf.raa
20201015::171800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 24880
20201015::171800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171810_wf.raa
20201015::171819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171820_wf.raa
20201015::171829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171830_wf.raa
20201015::171830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 24936
20201015::171830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171840_wf.raa
20201015::171849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171850_wf.raa
20201015::171859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171900_wf.raa
20201015::171900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 24991
20201015::171900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171910_wf.raa
20201015::171919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171920_wf.raa
20201015::171929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171930_wf.raa
20201015::171930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 25046
20201015::171930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::171939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171940_wf.raa
20201015::171949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_171950_wf.raa
20201015::171959: Head 1: Time Synchronization: 2020.10.15   17:20:00::0016
20201015::171959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172000_wf.raa
20201015::172000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 25102
20201015::172000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172010_wf.raa
20201015::172019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172020_wf.raa
20201015::172029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172030_wf.raa
20201015::172030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 25156
20201015::172030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172040_wf.raa
20201015::172049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172050_wf.raa
20201015::172059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172100_wf.raa
20201015::172100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 25211
20201015::172100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172110_wf.raa
20201015::172119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172120_wf.raa
20201015::172129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172130_wf.raa
20201015::172130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 25266
20201015::172130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172140_wf.raa
20201015::172149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172150_wf.raa
20201015::172159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172200_wf.raa
20201015::172200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 25321
20201015::172200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172210_wf.raa
20201015::172219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172220_wf.raa
20201015::172229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172230_wf.raa
20201015::172230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 25377
20201015::172230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172240_wf.raa
20201015::172249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172250_wf.raa
20201015::172259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172300_wf.raa
20201015::172300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 25432
20201015::172300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172310_wf.raa
20201015::172319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172320_wf.raa
20201015::172329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172330_wf.raa
20201015::172330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 25487
20201015::172330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172340_wf.raa
20201015::172349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172350_wf.raa
20201015::172359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172400_wf.raa
20201015::172400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 25542
20201015::172400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172410_wf.raa
20201015::172419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172420_wf.raa
20201015::172429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172430_wf.raa
20201015::172430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 25598
20201015::172430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172440_wf.raa
20201015::172449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172450_wf.raa
20201015::172459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172500_wf.raa
20201015::172500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 25653
20201015::172500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172510_wf.raa
20201015::172519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172520_wf.raa
20201015::172529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172530_wf.raa
20201015::172530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 25708
20201015::172530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172540_wf.raa
20201015::172549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172550_wf.raa
20201015::172559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172600_wf.raa
20201015::172600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 25764
20201015::172600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172610_wf.raa
20201015::172619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172620_wf.raa
20201015::172629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172630_wf.raa
20201015::172630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 25819
20201015::172630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172640_wf.raa
20201015::172649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172650_wf.raa
20201015::172659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172700_wf.raa
20201015::172700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 25874
20201015::172700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172710_wf.raa
20201015::172719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172720_wf.raa
20201015::172729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172730_wf.raa
20201015::172730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 25929
20201015::172730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172740_wf.raa
20201015::172749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172750_wf.raa
20201015::172759: Head 1: Time Synchronization: 2020.10.15   17:28:00::0015
20201015::172759: Head 2: Time Synchronization: 2020.10.15   17:28:00::0016
20201015::172759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172800_wf.raa
20201015::172800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 25984
20201015::172800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172810_wf.raa
20201015::172819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172820_wf.raa
20201015::172829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172830_wf.raa
20201015::172830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 26040
20201015::172830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172840_wf.raa
20201015::172849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172850_wf.raa
20201015::172859: Head 1: Time Synchronization: 2020.10.15   17:29:00::0016
20201015::172859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172900_wf.raa
20201015::172900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 26095
20201015::172900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172910_wf.raa
20201015::172919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172920_wf.raa
20201015::172929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172930_wf.raa
20201015::172930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 26151
20201015::172930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::172939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172940_wf.raa
20201015::172949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_172950_wf.raa
20201015::172959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173000_wf.raa
20201015::173000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 26207
20201015::173000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173010_wf.raa
20201015::173019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173020_wf.raa
20201015::173029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173030_wf.raa
20201015::173030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 26261
20201015::173030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173040_wf.raa
20201015::173049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173050_wf.raa
20201015::173059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173100_wf.raa
20201015::173100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 26316
20201015::173100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173110_wf.raa
20201015::173119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173120_wf.raa
20201015::173129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173130_wf.raa
20201015::173130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 26371
20201015::173130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173140_wf.raa
20201015::173149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173150_wf.raa
20201015::173159: Head 2: Time Synchronization: 2020.10.15   17:32:00::0017
20201015::173159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173200_wf.raa
20201015::173200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 26426
20201015::173200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173210_wf.raa
20201015::173219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173220_wf.raa
20201015::173229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173230_wf.raa
20201015::173230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 26481
20201015::173230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173240_wf.raa
20201015::173249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173250_wf.raa
20201015::173259: Head 1: Time Synchronization: 2020.10.15   17:33:00::0016
20201015::173259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173300_wf.raa
20201015::173300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 26536
20201015::173300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173310_wf.raa
20201015::173319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173320_wf.raa
20201015::173329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173330_wf.raa
20201015::173330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 26591
20201015::173330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173340_wf.raa
20201015::173349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173350_wf.raa
20201015::173359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173400_wf.raa
20201015::173400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 26646
20201015::173400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173410_wf.raa
20201015::173419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173420_wf.raa
20201015::173429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173430_wf.raa
20201015::173430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 26700
20201015::173430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173440_wf.raa
20201015::173449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173450_wf.raa
20201015::173459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173500_wf.raa
20201015::173500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 26755
20201015::173500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173510_wf.raa
20201015::173519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173520_wf.raa
20201015::173529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173530_wf.raa
20201015::173530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 26809
20201015::173530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173540_wf.raa
20201015::173549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173550_wf.raa
20201015::173559: Head 1: Time Synchronization: 2020.10.15   17:36:00::0015
20201015::173559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173600_wf.raa
20201015::173600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 26864
20201015::173600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173610_wf.raa
20201015::173619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173620_wf.raa
20201015::173629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173630_wf.raa
20201015::173630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 26919
20201015::173630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173640_wf.raa
20201015::173649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173650_wf.raa
20201015::173659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173700_wf.raa
20201015::173700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 26974
20201015::173700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173710_wf.raa
20201015::173719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173720_wf.raa
20201015::173729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173730_wf.raa
20201015::173730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 27029
20201015::173730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173740_wf.raa
20201015::173749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173750_wf.raa
20201015::173759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173800_wf.raa
20201015::173800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 27083
20201015::173800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173810_wf.raa
20201015::173819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173820_wf.raa
20201015::173829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173830_wf.raa
20201015::173830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 27138
20201015::173830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173840_wf.raa
20201015::173849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173850_wf.raa
20201015::173859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173900_wf.raa
20201015::173900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 27193
20201015::173900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173910_wf.raa
20201015::173919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173920_wf.raa
20201015::173929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173930_wf.raa
20201015::173930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 27248
20201015::173930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::173939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173940_wf.raa
20201015::173949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_173950_wf.raa
20201015::173959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174000_wf.raa
20201015::174000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 27303
20201015::174000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174010_wf.raa
20201015::174019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174020_wf.raa
20201015::174029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174030_wf.raa
20201015::174030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 27357
20201015::174030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174040_wf.raa
20201015::174049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174050_wf.raa
20201015::174059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174100_wf.raa
20201015::174100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 27413
20201015::174100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174110_wf.raa
20201015::174119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174120_wf.raa
20201015::174129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174130_wf.raa
20201015::174130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 27467
20201015::174130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174140_wf.raa
20201015::174149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174150_wf.raa
20201015::174159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174200_wf.raa
20201015::174200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 27522
20201015::174200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174210_wf.raa
20201015::174219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174220_wf.raa
20201015::174229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174230_wf.raa
20201015::174230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 27576
20201015::174230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174240_wf.raa
20201015::174249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174250_wf.raa
20201015::174259: Head 1: Time Synchronization: 2020.10.15   17:43:00::0015
20201015::174259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174300_wf.raa
20201015::174300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 27631
20201015::174300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174310_wf.raa
20201015::174319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174320_wf.raa
20201015::174329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174330_wf.raa
20201015::174330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 27685
20201015::174330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174340_wf.raa
20201015::174349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174350_wf.raa
20201015::174359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174400_wf.raa
20201015::174400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 27740
20201015::174400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174410_wf.raa
20201015::174419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174420_wf.raa
20201015::174429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174430_wf.raa
20201015::174430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 27795
20201015::174430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174440_wf.raa
20201015::174449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174450_wf.raa
20201015::174459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174500_wf.raa
20201015::174500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 27849
20201015::174500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174510_wf.raa
20201015::174519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174520_wf.raa
20201015::174529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174530_wf.raa
20201015::174530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 27904
20201015::174530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174540_wf.raa
20201015::174549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174550_wf.raa
20201015::174559: Head 1: Time Synchronization: 2020.10.15   17:46:00::0016
20201015::174559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174600_wf.raa
20201015::174600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 27959
20201015::174600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174610_wf.raa
20201015::174619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174620_wf.raa
20201015::174629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174630_wf.raa
20201015::174630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 28014
20201015::174630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174640_wf.raa
20201015::174649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174650_wf.raa
20201015::174659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174700_wf.raa
20201015::174700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 28068
20201015::174700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174710_wf.raa
20201015::174719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174720_wf.raa
20201015::174729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174730_wf.raa
20201015::174730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 28123
20201015::174730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174740_wf.raa
20201015::174749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174750_wf.raa
20201015::174759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174800_wf.raa
20201015::174800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 28177
20201015::174800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174810_wf.raa
20201015::174819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174820_wf.raa
20201015::174829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174830_wf.raa
20201015::174830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 28232
20201015::174830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174840_wf.raa
20201015::174849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174850_wf.raa
20201015::174859: Head 1: Time Synchronization: 2020.10.15   17:49:00::0014
20201015::174859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174900_wf.raa
20201015::174900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 28286
20201015::174900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174910_wf.raa
20201015::174919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174920_wf.raa
20201015::174929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174930_wf.raa
20201015::174930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 28341
20201015::174930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::174939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174940_wf.raa
20201015::174949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_174950_wf.raa
20201015::174959: Head 1: Time Synchronization: 2020.10.15   17:50:00::0014
20201015::174959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175000_wf.raa
20201015::175000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 28396
20201015::175000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175010_wf.raa
20201015::175019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175020_wf.raa
20201015::175029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175030_wf.raa
20201015::175030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 28450
20201015::175030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175040_wf.raa
20201015::175049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175050_wf.raa
20201015::175059: Head 1: Time Synchronization: 2020.10.15   17:51:00::0014
20201015::175059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175100_wf.raa
20201015::175100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28505
20201015::175100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175110_wf.raa
20201015::175119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175120_wf.raa
20201015::175129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175130_wf.raa
20201015::175130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28560
20201015::175130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175140_wf.raa
20201015::175149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175150_wf.raa
20201015::175159: Head 2: Time Synchronization: 2020.10.15   17:52:00::0014
20201015::175159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175200_wf.raa
20201015::175200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28614
20201015::175200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175210_wf.raa
20201015::175219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175220_wf.raa
20201015::175229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175230_wf.raa
20201015::175230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28669
20201015::175230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175240_wf.raa
20201015::175249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175250_wf.raa
20201015::175259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175300_wf.raa
20201015::175300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28724
20201015::175300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175310_wf.raa
20201015::175319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175320_wf.raa
20201015::175329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175330_wf.raa
20201015::175330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 28778
20201015::175330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175340_wf.raa
20201015::175349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175350_wf.raa
20201015::175359: Head 1: Time Synchronization: 2020.10.15   17:54:00::0015
20201015::175359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175400_wf.raa
20201015::175400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 28833
20201015::175400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175410_wf.raa
20201015::175419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175420_wf.raa
20201015::175429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175430_wf.raa
20201015::175430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 28887
20201015::175430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175440_wf.raa
20201015::175449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175450_wf.raa
20201015::175459: Head 2: Time Synchronization: 2020.10.15   17:55:00::0014
20201015::175459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175500_wf.raa
20201015::175500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 28942
20201015::175500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175510_wf.raa
20201015::175519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175520_wf.raa
20201015::175529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175530_wf.raa
20201015::175530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 29000
20201015::175530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175540_wf.raa
20201015::175549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175550_wf.raa
20201015::175559: Head 1: Time Synchronization: 2020.10.15   17:56:00::0014
20201015::175559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175600_wf.raa
20201015::175600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 29058
20201015::175600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175610_wf.raa
20201015::175619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175620_wf.raa
20201015::175629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175630_wf.raa
20201015::175630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 29115
20201015::175630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175640_wf.raa
20201015::175649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175650_wf.raa
20201015::175659: Head 2: Time Synchronization: 2020.10.15   17:57:00::0020
20201015::175659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175700_wf.raa
20201015::175700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 29173
20201015::175700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175710_wf.raa
20201015::175719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175720_wf.raa
20201015::175729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175730_wf.raa
20201015::175730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 29227
20201015::175730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175740_wf.raa
20201015::175749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175750_wf.raa
20201015::175759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175800_wf.raa
20201015::175800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 29281
20201015::175800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175810_wf.raa
20201015::175819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175820_wf.raa
20201015::175829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175830_wf.raa
20201015::175830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 29334
20201015::175830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175840_wf.raa
20201015::175849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175850_wf.raa
20201015::175859: Head 1: Time Synchronization: 2020.10.15   17:59:00::0013
20201015::175859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175900_wf.raa
20201015::175900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 29388
20201015::175900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175910_wf.raa
20201015::175919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175920_wf.raa
20201015::175929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175930_wf.raa
20201015::175930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 29442
20201015::175930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::175939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175940_wf.raa
20201015::175949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_175950_wf.raa
20201015::175959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180000_wf.raa
20201015::180000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 29500
20201015::180000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180010_wf.raa
20201015::180019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180020_wf.raa
20201015::180029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180030_wf.raa
20201015::180030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 29555
20201015::180030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180040_wf.raa
20201015::180049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180050_wf.raa
20201015::180059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180100_wf.raa
20201015::180100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 29609
20201015::180100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180110_wf.raa
20201015::180119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180120_wf.raa
20201015::180129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180130_wf.raa
20201015::180130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 29663
20201015::180130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180140_wf.raa
20201015::180149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180150_wf.raa
20201015::180159: Head 2: Time Synchronization: 2020.10.15   18:02:00::0015
20201015::180159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180200_wf.raa
20201015::180200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 29717
20201015::180200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180210_wf.raa
20201015::180219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180220_wf.raa
20201015::180229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180230_wf.raa
20201015::180230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 29772
20201015::180230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180240_wf.raa
20201015::180249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180250_wf.raa
20201015::180259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180300_wf.raa
20201015::180300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 29828
20201015::180300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180310_wf.raa
20201015::180319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180320_wf.raa
20201015::180329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180330_wf.raa
20201015::180330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 29881
20201015::180330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180340_wf.raa
20201015::180349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180350_wf.raa
20201015::180359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180400_wf.raa
20201015::180400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 29936
20201015::180400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180410_wf.raa
20201015::180419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180420_wf.raa
20201015::180429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180430_wf.raa
20201015::180430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 29991
20201015::180430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180440_wf.raa
20201015::180449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180450_wf.raa
20201015::180459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180500_wf.raa
20201015::180500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 30045
20201015::180500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180510_wf.raa
20201015::180519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180520_wf.raa
20201015::180529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180530_wf.raa
20201015::180530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 30099
20201015::180530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180540_wf.raa
20201015::180549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180550_wf.raa
20201015::180559: Head 1: Time Synchronization: 2020.10.15   18:06:00::0015
20201015::180559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180600_wf.raa
20201015::180600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 30153
20201015::180600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180610_wf.raa
20201015::180619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180620_wf.raa
20201015::180629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180630_wf.raa
20201015::180630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 30207
20201015::180630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180640_wf.raa
20201015::180649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180650_wf.raa
20201015::180659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180700_wf.raa
20201015::180700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 30261
20201015::180700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180710_wf.raa
20201015::180719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180720_wf.raa
20201015::180729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180730_wf.raa
20201015::180730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 30316
20201015::180730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180740_wf.raa
20201015::180749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180750_wf.raa
20201015::180759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180800_wf.raa
20201015::180800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 30370
20201015::180800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180810_wf.raa
20201015::180819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180820_wf.raa
20201015::180829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180830_wf.raa
20201015::180830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 30424
20201015::180830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180840_wf.raa
20201015::180849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180850_wf.raa
20201015::180859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180900_wf.raa
20201015::180900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 30477
20201015::180900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180910_wf.raa
20201015::180919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180920_wf.raa
20201015::180929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180930_wf.raa
20201015::180930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 30530
20201015::180930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::180939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180940_wf.raa
20201015::180949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_180950_wf.raa
20201015::180959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181000_wf.raa
20201015::181000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 30584
20201015::181000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181010_wf.raa
20201015::181019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181020_wf.raa
20201015::181029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181030_wf.raa
20201015::181030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 30637
20201015::181030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181040_wf.raa
20201015::181049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181050_wf.raa
20201015::181059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181100_wf.raa
20201015::181100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 30691
20201015::181100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181110_wf.raa
20201015::181119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181120_wf.raa
20201015::181129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181130_wf.raa
20201015::181130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 30744
20201015::181130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181140_wf.raa
20201015::181149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181150_wf.raa
20201015::181159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181200_wf.raa
20201015::181200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 30798
20201015::181200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181210_wf.raa
20201015::181219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181220_wf.raa
20201015::181229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181230_wf.raa
20201015::181230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 30851
20201015::181230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181240_wf.raa
20201015::181249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181250_wf.raa
20201015::181259: Head 1: Time Synchronization: 2020.10.15   18:13:00::0014
20201015::181259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181300_wf.raa
20201015::181300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 30905
20201015::181300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181310_wf.raa
20201015::181319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181320_wf.raa
20201015::181329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181330_wf.raa
20201015::181330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 30960
20201015::181330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181340_wf.raa
20201015::181349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181350_wf.raa
20201015::181359: Head 1: Time Synchronization: 2020.10.15   18:14:00::0017
20201015::181359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181400_wf.raa
20201015::181400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 31015
20201015::181400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181410_wf.raa
20201015::181419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181420_wf.raa
20201015::181429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181430_wf.raa
20201015::181430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 31070
20201015::181430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181440_wf.raa
20201015::181449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181450_wf.raa
20201015::181459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181500_wf.raa
20201015::181500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 31125
20201015::181500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181510_wf.raa
20201015::181519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181520_wf.raa
20201015::181529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181530_wf.raa
20201015::181530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 31181
20201015::181530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181540_wf.raa
20201015::181549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181550_wf.raa
20201015::181559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181600_wf.raa
20201015::181600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 31237
20201015::181600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181610_wf.raa
20201015::181619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181620_wf.raa
20201015::181629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181630_wf.raa
20201015::181630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 31294
20201015::181630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181640_wf.raa
20201015::181649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181650_wf.raa
20201015::181659: Head 1: Time Synchronization: 2020.10.15   18:17:00::0014
20201015::181659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181700_wf.raa
20201015::181700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 31352
20201015::181700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181710_wf.raa
20201015::181719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181720_wf.raa
20201015::181729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181730_wf.raa
20201015::181730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 31406
20201015::181730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181740_wf.raa
20201015::181749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181750_wf.raa
20201015::181759: Head 1: Time Synchronization: 2020.10.15   18:18:00::0014
20201015::181759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181800_wf.raa
20201015::181800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 31462
20201015::181800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181810_wf.raa
20201015::181819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181820_wf.raa
20201015::181829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181830_wf.raa
20201015::181830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 31516
20201015::181830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181840_wf.raa
20201015::181849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181850_wf.raa
20201015::181859: Head 1: Time Synchronization: 2020.10.15   18:19:00::0015
20201015::181859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181900_wf.raa
20201015::181900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 31572
20201015::181900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181910_wf.raa
20201015::181919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181920_wf.raa
20201015::181929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181930_wf.raa
20201015::181930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 31625
20201015::181930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::181939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181940_wf.raa
20201015::181949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_181950_wf.raa
20201015::181959: Head 1: Time Synchronization: 2020.10.15   18:20:00::0016
20201015::181959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182000_wf.raa
20201015::182000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 31678
20201015::182000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182010_wf.raa
20201015::182019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182020_wf.raa
20201015::182029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182030_wf.raa
20201015::182030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 31732
20201015::182030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182040_wf.raa
20201015::182049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182050_wf.raa
20201015::182059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182100_wf.raa
20201015::182100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 31785
20201015::182100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182110_wf.raa
20201015::182119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182120_wf.raa
20201015::182129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182130_wf.raa
20201015::182130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 31838
20201015::182130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182140_wf.raa
20201015::182149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182150_wf.raa
20201015::182159: Head 1: Time Synchronization: 2020.10.15   18:22:00::0015
20201015::182159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182200_wf.raa
20201015::182200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 31892
20201015::182200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182210_wf.raa
20201015::182219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182220_wf.raa
20201015::182229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182230_wf.raa
20201015::182230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 31945
20201015::182230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182240_wf.raa
20201015::182249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182250_wf.raa
20201015::182259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182300_wf.raa
20201015::182300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 31998
20201015::182300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182310_wf.raa
20201015::182319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182320_wf.raa
20201015::182329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182330_wf.raa
20201015::182330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 32052
20201015::182330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182340_wf.raa
20201015::182349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182350_wf.raa
20201015::182359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182400_wf.raa
20201015::182400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 32106
20201015::182400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182410_wf.raa
20201015::182419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182420_wf.raa
20201015::182429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182430_wf.raa
20201015::182430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 32161
20201015::182430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182440_wf.raa
20201015::182449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182450_wf.raa
20201015::182459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182500_wf.raa
20201015::182459: Head 1: Time Synchronization: 2020.10.15   18:25:00::0014
20201015::182500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 32214
20201015::182500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182510_wf.raa
20201015::182519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182520_wf.raa
20201015::182529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182530_wf.raa
20201015::182530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 32267
20201015::182530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182540_wf.raa
20201015::182549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182550_wf.raa
20201015::182559: Head 1: Time Synchronization: 2020.10.15   18:26:00::0016
20201015::182559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182600_wf.raa
20201015::182600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 32321
20201015::182600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182610_wf.raa
20201015::182619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182620_wf.raa
20201015::182629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182630_wf.raa
20201015::182630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.4dbar, CTD 34.7psu, index 1.35, Packet 32376
20201015::182630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182640_wf.raa
20201015::182649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182650_wf.raa
20201015::182659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182700_wf.raa
20201015::182700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 32430
20201015::182700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182710_wf.raa
20201015::182719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182720_wf.raa
20201015::182729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182730_wf.raa
20201015::182730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 32485
20201015::182730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182740_wf.raa
20201015::182749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182750_wf.raa
20201015::182759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182800_wf.raa
20201015::182759: Head 2: Time Synchronization: 2020.10.15   18:28:00::0015
20201015::182800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 32539
20201015::182800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182810_wf.raa
20201015::182819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182820_wf.raa
20201015::182829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182830_wf.raa
20201015::182830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 32593
20201015::182830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182840_wf.raa
20201015::182849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182850_wf.raa
20201015::182859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182900_wf.raa
20201015::182900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 32648
20201015::182900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182910_wf.raa
20201015::182919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182920_wf.raa
20201015::182929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182930_wf.raa
20201015::182930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 32702
20201015::182930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::182939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182940_wf.raa
20201015::182949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_182950_wf.raa
20201015::182959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183000_wf.raa
20201015::183000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 32758
20201015::183000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183010_wf.raa
20201015::183019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183020_wf.raa
20201015::183029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183030_wf.raa
20201015::183030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 32812
20201015::183030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183040_wf.raa
20201015::183049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183050_wf.raa
20201015::183059: Head 1: Time Synchronization: 2020.10.15   18:31:00::0015
20201015::183059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183100_wf.raa
20201015::183100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 32868
20201015::183100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183110_wf.raa
20201015::183119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183120_wf.raa
20201015::183129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183130_wf.raa
20201015::183130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 32923
20201015::183130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183140_wf.raa
20201015::183149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183150_wf.raa
20201015::183159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183200_wf.raa
20201015::183200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 32978
20201015::183200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183210_wf.raa
20201015::183219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183220_wf.raa
20201015::183229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183230_wf.raa
20201015::183230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 33034
20201015::183230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183240_wf.raa
20201015::183249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183250_wf.raa
20201015::183259: Head 1: Time Synchronization: 2020.10.15   18:33:00::0017
20201015::183259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183300_wf.raa
20201015::183300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 33088
20201015::183300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183310_wf.raa
20201015::183319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183320_wf.raa
20201015::183329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183330_wf.raa
20201015::183330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 33142
20201015::183330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183340_wf.raa
20201015::183349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183350_wf.raa
20201015::183359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183400_wf.raa
20201015::183400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 33196
20201015::183400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183410_wf.raa
20201015::183419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183420_wf.raa
20201015::183429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183430_wf.raa
20201015::183430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 33250
20201015::183430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183440_wf.raa
20201015::183449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183450_wf.raa
20201015::183459: Head 1: Time Synchronization: 2020.10.15   18:35:00::0016
20201015::183459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183500_wf.raa
20201015::183500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 33304
20201015::183500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183510_wf.raa
20201015::183519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183520_wf.raa
20201015::183529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183530_wf.raa
20201015::183530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 33358
20201015::183530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183540_wf.raa
20201015::183549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183550_wf.raa
20201015::183559: Head 1: Time Synchronization: 2020.10.15   18:36:00::0016
20201015::183559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183600_wf.raa
20201015::183600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 33411
20201015::183600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183610_wf.raa
20201015::183619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183620_wf.raa
20201015::183629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183630_wf.raa
20201015::183630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 33466
20201015::183630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183640_wf.raa
20201015::183649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183650_wf.raa
20201015::183659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183700_wf.raa
20201015::183700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 33522
20201015::183700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183710_wf.raa
20201015::183719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183720_wf.raa
20201015::183729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183730_wf.raa
20201015::183730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 33577
20201015::183730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183740_wf.raa
20201015::183749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183750_wf.raa
20201015::183759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183800_wf.raa
20201015::183800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 33631
20201015::183800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183810_wf.raa
20201015::183819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183820_wf.raa
20201015::183829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183830_wf.raa
20201015::183830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 33686
20201015::183830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183840_wf.raa
20201015::183849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183850_wf.raa
20201015::183859: Head 1: Time Synchronization: 2020.10.15   18:39:00::0014
20201015::183859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183900_wf.raa
20201015::183900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 33740
20201015::183900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183910_wf.raa
20201015::183919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183920_wf.raa
20201015::183929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183930_wf.raa
20201015::183930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 33795
20201015::183930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::183939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183940_wf.raa
20201015::183949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_183950_wf.raa
20201015::183959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184000_wf.raa
20201015::184000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 33849
20201015::184000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184010_wf.raa
20201015::184019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184020_wf.raa
20201015::184029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184030_wf.raa
20201015::184030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 33905
20201015::184030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184040_wf.raa
20201015::184049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184050_wf.raa
20201015::184059: Head 1: Time Synchronization: 2020.10.15   18:41:00::0015
20201015::184059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184100_wf.raa
20201015::184100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 33961
20201015::184100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184110_wf.raa
20201015::184119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184120_wf.raa
20201015::184129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184130_wf.raa
20201015::184130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 34016
20201015::184130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184140_wf.raa
20201015::184149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184150_wf.raa
20201015::184159: Head 1: Time Synchronization: 2020.10.15   18:42:00::0014
20201015::184159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184200_wf.raa
20201015::184200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.1dbar, CTD 34.7psu, index 1.35, Packet 34069
20201015::184200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184210_wf.raa
20201015::184219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184220_wf.raa
20201015::184229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184230_wf.raa
20201015::184230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.1dbar, CTD 34.7psu, index 1.35, Packet 34122
20201015::184230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184240_wf.raa
20201015::184249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184250_wf.raa
20201015::184259: Head 1: Time Synchronization: 2020.10.15   18:43:00::0016
20201015::184259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184300_wf.raa
20201015::184300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 34176
20201015::184300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184310_wf.raa
20201015::184319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184320_wf.raa
20201015::184329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184330_wf.raa
20201015::184330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 34230
20201015::184330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184340_wf.raa
20201015::184349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184350_wf.raa
20201015::184359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184400_wf.raa
20201015::184400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 34284
20201015::184400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184410_wf.raa
20201015::184419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184420_wf.raa
20201015::184429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184430_wf.raa
20201015::184430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 34339
20201015::184430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184440_wf.raa
20201015::184449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184450_wf.raa
20201015::184459: Head 1: Time Synchronization: 2020.10.15   18:45:00::0017
20201015::184459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184500_wf.raa
20201015::184500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 34397
20201015::184500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184510_wf.raa
20201015::184519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184520_wf.raa
20201015::184529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184530_wf.raa
20201015::184530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 34454
20201015::184530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184540_wf.raa
20201015::184549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184550_wf.raa
20201015::184559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184600_wf.raa
20201015::184600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 34511
20201015::184600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184610_wf.raa
20201015::184619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184620_wf.raa
20201015::184629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184630_wf.raa
20201015::184630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.4dbar, CTD 34.7psu, index 1.35, Packet 34567
20201015::184630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184640_wf.raa
20201015::184649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184650_wf.raa
20201015::184659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184700_wf.raa
20201015::184700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 34623
20201015::184700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184710_wf.raa
20201015::184719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184720_wf.raa
20201015::184729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184730_wf.raa
20201015::184730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 34680
20201015::184730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184740_wf.raa
20201015::184749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184750_wf.raa
20201015::184759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184800_wf.raa
20201015::184759: Head 1: Time Synchronization: 2020.10.15   18:48:00::0015
20201015::184800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 34736
20201015::184800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184810_wf.raa
20201015::184819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184820_wf.raa
20201015::184829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184830_wf.raa
20201015::184830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 34792
20201015::184830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184840_wf.raa
20201015::184849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184850_wf.raa
20201015::184859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184900_wf.raa
20201015::184900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 34847
20201015::184900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184910_wf.raa
20201015::184919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184920_wf.raa
20201015::184929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184930_wf.raa
20201015::184930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 34901
20201015::184930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::184939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184940_wf.raa
20201015::184949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_184950_wf.raa
20201015::184959: Head 2: Time Synchronization: 2020.10.15   18:50:00::0014
20201015::184959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185000_wf.raa
20201015::185000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 34956
20201015::185000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185010_wf.raa
20201015::185019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185020_wf.raa
20201015::185029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185030_wf.raa
20201015::185030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 35010
20201015::185030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185040_wf.raa
20201015::185049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185050_wf.raa
20201015::185059: Head 1: Time Synchronization: 2020.10.15   18:51:00::0014
20201015::185059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185100_wf.raa
20201015::185100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 35066
20201015::185100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185110_wf.raa
20201015::185119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185120_wf.raa
20201015::185129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185130_wf.raa
20201015::185130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 35121
20201015::185130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185140_wf.raa
20201015::185149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185150_wf.raa
20201015::185159: Head 1: Time Synchronization: 2020.10.15   18:52:00::0015
20201015::185159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185200_wf.raa
20201015::185200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 35176
20201015::185200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185210_wf.raa
20201015::185219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185220_wf.raa
20201015::185229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185230_wf.raa
20201015::185230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 35231
20201015::185230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185240_wf.raa
20201015::185249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185250_wf.raa
20201015::185259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185300_wf.raa
20201015::185300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 35286
20201015::185300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185310_wf.raa
20201015::185319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185320_wf.raa
20201015::185329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185330_wf.raa
20201015::185330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 35342
20201015::185330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185340_wf.raa
20201015::185349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185350_wf.raa
20201015::185359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185400_wf.raa
20201015::185400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 35397
20201015::185400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185410_wf.raa
20201015::185419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185420_wf.raa
20201015::185429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185430_wf.raa
20201015::185430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 35452
20201015::185430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185440_wf.raa
20201015::185449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185450_wf.raa
20201015::185459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185500_wf.raa
20201015::185500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 35507
20201015::185500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185510_wf.raa
20201015::185519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185520_wf.raa
20201015::185529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185530_wf.raa
20201015::185530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 35561
20201015::185530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185540_wf.raa
20201015::185549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185550_wf.raa
20201015::185559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185600_wf.raa
20201015::185600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 35616
20201015::185600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185610_wf.raa
20201015::185619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185620_wf.raa
20201015::185629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185630_wf.raa
20201015::185630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 35671
20201015::185630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185640_wf.raa
20201015::185649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185650_wf.raa
20201015::185659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185700_wf.raa
20201015::185700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 35727
20201015::185700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185710_wf.raa
20201015::185719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185720_wf.raa
20201015::185729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185730_wf.raa
20201015::185730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 35782
20201015::185730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185740_wf.raa
20201015::185749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185750_wf.raa
20201015::185759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185800_wf.raa
20201015::185800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 35837
20201015::185800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185810_wf.raa
20201015::185819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185820_wf.raa
20201015::185829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185830_wf.raa
20201015::185830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 35892
20201015::185830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185840_wf.raa
20201015::185849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185850_wf.raa
20201015::185859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185900_wf.raa
20201015::185900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 35948
20201015::185900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185910_wf.raa
20201015::185919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185920_wf.raa
20201015::185929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185930_wf.raa
20201015::185930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 36004
20201015::185930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::185939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185940_wf.raa
20201015::185949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_185950_wf.raa
20201015::185959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190000_wf.raa
20201015::190000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 36061
20201015::190000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190010_wf.raa
20201015::190019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190020_wf.raa
20201015::190029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190030_wf.raa
20201015::190030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 36115
20201015::190030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190040_wf.raa
20201015::190049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190050_wf.raa
20201015::190059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190100_wf.raa
20201015::190100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 36170
20201015::190100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190110_wf.raa
20201015::190119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190120_wf.raa
20201015::190129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190130_wf.raa
20201015::190130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 36228
20201015::190130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190140_wf.raa
20201015::190149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190150_wf.raa
20201015::190159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190200_wf.raa
20201015::190200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.1dbar, CTD 34.7psu, index 1.35, Packet 36285
20201015::190200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190210_wf.raa
20201015::190219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190220_wf.raa
20201015::190229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190230_wf.raa
20201015::190230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.1dbar, CTD 34.7psu, index 1.35, Packet 36343
20201015::190230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190240_wf.raa
20201015::190249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190250_wf.raa
20201015::190259: Head 1: Time Synchronization: 2020.10.15   19:03:00::0014
20201015::190259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190300_wf.raa
20201015::190300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 36401
20201015::190300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190310_wf.raa
20201015::190319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190320_wf.raa
20201015::190329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190330_wf.raa
20201015::190330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 36459
20201015::190330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190340_wf.raa
20201015::190349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190350_wf.raa
20201015::190359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190400_wf.raa
20201015::190400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 36516
20201015::190400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190410_wf.raa
20201015::190419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190420_wf.raa
20201015::190429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190430_wf.raa
20201015::190430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 36573
20201015::190430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190440_wf.raa
20201015::190449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190450_wf.raa
20201015::190459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190500_wf.raa
20201015::190500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 36632
20201015::190500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190510_wf.raa
20201015::190519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190520_wf.raa
20201015::190529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190530_wf.raa
20201015::190530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 36686
20201015::190530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190540_wf.raa
20201015::190549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190550_wf.raa
20201015::190559: Head 1: Time Synchronization: 2020.10.15   19:06:00::0015
20201015::190559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190600_wf.raa
20201015::190600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 36739
20201015::190600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190610_wf.raa
20201015::190619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190620_wf.raa
20201015::190629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190630_wf.raa
20201015::190630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.4dbar, CTD 34.7psu, index 1.35, Packet 36793
20201015::190630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190640_wf.raa
20201015::190649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190650_wf.raa
20201015::190659: Head 1: Time Synchronization: 2020.10.15   19:07:00::0014
20201015::190659: Head 2: Time Synchronization: 2020.10.15   19:07:00::0014
20201015::190659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190700_wf.raa
20201015::190700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 36847
20201015::190700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190710_wf.raa
20201015::190719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190720_wf.raa
20201015::190729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190730_wf.raa
20201015::190730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 36901
20201015::190730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190740_wf.raa
20201015::190749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190750_wf.raa
20201015::190759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190800_wf.raa
20201015::190800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 36956
20201015::190800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190810_wf.raa
20201015::190819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190820_wf.raa
20201015::190829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190830_wf.raa
20201015::190830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 37010
20201015::190830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190840_wf.raa
20201015::190849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190850_wf.raa
20201015::190859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190900_wf.raa
20201015::190900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 37064
20201015::190900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190910_wf.raa
20201015::190919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190920_wf.raa
20201015::190929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190930_wf.raa
20201015::190930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 37119
20201015::190930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::190939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190940_wf.raa
20201015::190949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_190950_wf.raa
20201015::190959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191000_wf.raa
20201015::191000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 37178
20201015::191000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191010_wf.raa
20201015::191019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191020_wf.raa
20201015::191029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191030_wf.raa
20201015::191030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 37235
20201015::191030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191040_wf.raa
20201015::191049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191050_wf.raa
20201015::191059: Head 2: Time Synchronization: 2020.10.15   19:11:00::0015
20201015::191059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191100_wf.raa
20201015::191100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 37288
20201015::191100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191110_wf.raa
20201015::191119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191120_wf.raa
20201015::191129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191130_wf.raa
20201015::191130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 37344
20201015::191130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191140_wf.raa
20201015::191149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191150_wf.raa
20201015::191159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191200_wf.raa
20201015::191200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 37400
20201015::191200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191210_wf.raa
20201015::191219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191220_wf.raa
20201015::191229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191230_wf.raa
20201015::191230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 37457
20201015::191230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191240_wf.raa
20201015::191249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191250_wf.raa
20201015::191259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191300_wf.raa
20201015::191300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 37514
20201015::191300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191310_wf.raa
20201015::191319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191320_wf.raa
20201015::191329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191330_wf.raa
20201015::191330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 37567
20201015::191330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191340_wf.raa
20201015::191349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191350_wf.raa
20201015::191359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191400_wf.raa
20201015::191400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 37621
20201015::191400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191410_wf.raa
20201015::191419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191420_wf.raa
20201015::191429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191430_wf.raa
20201015::191430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 37675
20201015::191430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191440_wf.raa
20201015::191449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191450_wf.raa
20201015::191459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191500_wf.raa
20201015::191500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 37730
20201015::191500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191510_wf.raa
20201015::191519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191520_wf.raa
20201015::191529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191530_wf.raa
20201015::191530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 37786
20201015::191530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191540_wf.raa
20201015::191549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191550_wf.raa
20201015::191559: Head 1: Time Synchronization: 2020.10.15   19:16:00::0015
20201015::191559: Head 2: Time Synchronization: 2020.10.15   19:16:00::0014
20201015::191559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191600_wf.raa
20201015::191600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 37842
20201015::191600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191610_wf.raa
20201015::191619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191620_wf.raa
20201015::191629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191630_wf.raa
20201015::191630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 37897
20201015::191630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191640_wf.raa
20201015::191649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191650_wf.raa
20201015::191659: Head 1: Time Synchronization: 2020.10.15   19:17:00::0014
20201015::191659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191700_wf.raa
20201015::191700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 37952
20201015::191700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191710_wf.raa
20201015::191719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191720_wf.raa
20201015::191729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191730_wf.raa
20201015::191730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 38007
20201015::191730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191740_wf.raa
20201015::191749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191750_wf.raa
20201015::191759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191800_wf.raa
20201015::191800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 38062
20201015::191800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191810_wf.raa
20201015::191819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191820_wf.raa
20201015::191829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191830_wf.raa
20201015::191830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 38118
20201015::191830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191840_wf.raa
20201015::191849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191850_wf.raa
20201015::191859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191900_wf.raa
20201015::191900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 38173
20201015::191900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191910_wf.raa
20201015::191919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191920_wf.raa
20201015::191929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191930_wf.raa
20201015::191930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 38228
20201015::191930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::191939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191940_wf.raa
20201015::191949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_191950_wf.raa
20201015::191959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192000_wf.raa
20201015::192000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 38283
20201015::192000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192010_wf.raa
20201015::192019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192020_wf.raa
20201015::192029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192030_wf.raa
20201015::192030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 38338
20201015::192030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192040_wf.raa
20201015::192049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192050_wf.raa
20201015::192059: Head 1: Time Synchronization: 2020.10.15   19:21:00::0014
20201015::192059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192100_wf.raa
20201015::192100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 38394
20201015::192100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192110_wf.raa
20201015::192119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192120_wf.raa
20201015::192129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192130_wf.raa
20201015::192130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 38450
20201015::192130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192140_wf.raa
20201015::192149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192150_wf.raa
20201015::192159: Head 2: Time Synchronization: 2020.10.15   19:22:00::0014
20201015::192159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192200_wf.raa
20201015::192200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 38506
20201015::192200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192210_wf.raa
20201015::192219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192220_wf.raa
20201015::192229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192230_wf.raa
20201015::192230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.1dbar, CTD 34.7psu, index 1.35, Packet 38561
20201015::192230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192240_wf.raa
20201015::192249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192250_wf.raa
20201015::192259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192300_wf.raa
20201015::192300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2879.0dbar, CTD 34.7psu, index 1.35, Packet 38616
20201015::192300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192310_wf.raa
20201015::192319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192320_wf.raa
20201015::192329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192330_wf.raa
20201015::192330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 38672
20201015::192330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192340_wf.raa
20201015::192349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192350_wf.raa
20201015::192359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192400_wf.raa
20201015::192400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 38727
20201015::192400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192410_wf.raa
20201015::192419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192420_wf.raa
20201015::192429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192430_wf.raa
20201015::192430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 38782
20201015::192430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192440_wf.raa
20201015::192449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192450_wf.raa
20201015::192459: Head 1: Time Synchronization: 2020.10.15   19:25:00::0015
20201015::192459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192500_wf.raa
20201015::192500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 38838
20201015::192500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192510_wf.raa
20201015::192519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192520_wf.raa
20201015::192529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192530_wf.raa
20201015::192530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 38893
20201015::192530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192540_wf.raa
20201015::192549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192550_wf.raa
20201015::192559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192600_wf.raa
20201015::192600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 38947
20201015::192600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192610_wf.raa
20201015::192619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192620_wf.raa
20201015::192629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192630_wf.raa
20201015::192630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 39002
20201015::192630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192640_wf.raa
20201015::192649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192650_wf.raa
20201015::192659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192700_wf.raa
20201015::192700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 39057
20201015::192700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192710_wf.raa
20201015::192719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192720_wf.raa
20201015::192729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192730_wf.raa
20201015::192730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 39112
20201015::192730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192740_wf.raa
20201015::192749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192750_wf.raa
20201015::192759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192800_wf.raa
20201015::192800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 39167
20201015::192800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192810_wf.raa
20201015::192819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192820_wf.raa
20201015::192829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192830_wf.raa
20201015::192830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 39223
20201015::192830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192840_wf.raa
20201015::192849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192850_wf.raa
20201015::192859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192900_wf.raa
20201015::192900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 39278
20201015::192900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192910_wf.raa
20201015::192919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192920_wf.raa
20201015::192929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192930_wf.raa
20201015::192930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 39333
20201015::192930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::192939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192940_wf.raa
20201015::192949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_192950_wf.raa
20201015::192959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193000_wf.raa
20201015::193000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 39388
20201015::193000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193010_wf.raa
20201015::193019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193020_wf.raa
20201015::193029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193030_wf.raa
20201015::193030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 39443
20201015::193030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193040_wf.raa
20201015::193049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193050_wf.raa
20201015::193059: Head 1: Time Synchronization: 2020.10.15   19:31:00::0014
20201015::193059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193100_wf.raa
20201015::193100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 39497
20201015::193100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193110_wf.raa
20201015::193119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193120_wf.raa
20201015::193129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193130_wf.raa
20201015::193130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 39552
20201015::193130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193140_wf.raa
20201015::193149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193150_wf.raa
20201015::193159: Head 1: Time Synchronization: 2020.10.15   19:32:00::0014
20201015::193159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193200_wf.raa
20201015::193200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 39608
20201015::193200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193210_wf.raa
20201015::193219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193220_wf.raa
20201015::193229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193230_wf.raa
20201015::193230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 39663
20201015::193230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193240_wf.raa
20201015::193249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193250_wf.raa
20201015::193259: Head 1: Time Synchronization: 2020.10.15   19:33:00::0015
20201015::193259: Head 2: Time Synchronization: 2020.10.15   19:33:00::0015
20201015::193259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193300_wf.raa
20201015::193300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 39719
20201015::193300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193310_wf.raa
20201015::193319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193320_wf.raa
20201015::193329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193330_wf.raa
20201015::193330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 39773
20201015::193330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193340_wf.raa
20201015::193349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193350_wf.raa
20201015::193359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193400_wf.raa
20201015::193400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 39829
20201015::193400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193410_wf.raa
20201015::193419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193420_wf.raa
20201015::193429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193430_wf.raa
20201015::193430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 39884
20201015::193430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193440_wf.raa
20201015::193449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193450_wf.raa
20201015::193459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193500_wf.raa
20201015::193500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 39939
20201015::193500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193510_wf.raa
20201015::193519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193520_wf.raa
20201015::193529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193530_wf.raa
20201015::193530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 39995
20201015::193530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193540_wf.raa
20201015::193549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193550_wf.raa
20201015::193559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193600_wf.raa
20201015::193600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 40051
20201015::193600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193610_wf.raa
20201015::193619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193620_wf.raa
20201015::193629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193630_wf.raa
20201015::193630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 40106
20201015::193630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193640_wf.raa
20201015::193649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193650_wf.raa
20201015::193659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193700_wf.raa
20201015::193700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 40161
20201015::193700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193710_wf.raa
20201015::193719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193720_wf.raa
20201015::193729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193730_wf.raa
20201015::193730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 40216
20201015::193730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193740_wf.raa
20201015::193749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193750_wf.raa
20201015::193759: Head 1: Time Synchronization: 2020.10.15   19:38:00::0014
20201015::193759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193800_wf.raa
20201015::193800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 40272
20201015::193800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193810_wf.raa
20201015::193819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193820_wf.raa
20201015::193829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193830_wf.raa
20201015::193830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 40328
20201015::193830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193840_wf.raa
20201015::193849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193850_wf.raa
20201015::193859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193900_wf.raa
20201015::193900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 40384
20201015::193900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193910_wf.raa
20201015::193919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193920_wf.raa
20201015::193929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193930_wf.raa
20201015::193930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 40439
20201015::193930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::193939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193940_wf.raa
20201015::193949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_193950_wf.raa
20201015::193959: Head 1: Time Synchronization: 2020.10.15   19:40:00::0015
20201015::193959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194000_wf.raa
20201015::194000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 40494
20201015::194000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194010_wf.raa
20201015::194019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194020_wf.raa
20201015::194029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194030_wf.raa
20201015::194030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 40549
20201015::194030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194040_wf.raa
20201015::194049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194050_wf.raa
20201015::194059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194100_wf.raa
20201015::194100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 40604
20201015::194100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194110_wf.raa
20201015::194119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194120_wf.raa
20201015::194129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194130_wf.raa
20201015::194130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 40658
20201015::194130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194140_wf.raa
20201015::194149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194150_wf.raa
20201015::194159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194200_wf.raa
20201015::194200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 40713
20201015::194200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194210_wf.raa
20201015::194219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194220_wf.raa
20201015::194229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194230_wf.raa
20201015::194230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 40768
20201015::194230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194240_wf.raa
20201015::194249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194250_wf.raa
20201015::194259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194300_wf.raa
20201015::194300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 40823
20201015::194300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194310_wf.raa
20201015::194319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194320_wf.raa
20201015::194329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194330_wf.raa
20201015::194330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 40878
20201015::194330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194340_wf.raa
20201015::194349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194350_wf.raa
20201015::194359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194400_wf.raa
20201015::194400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 40933
20201015::194400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194410_wf.raa
20201015::194419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194420_wf.raa
20201015::194429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194430_wf.raa
20201015::194430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 40989
20201015::194430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194440_wf.raa
20201015::194449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194450_wf.raa
20201015::194459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194500_wf.raa
20201015::194500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 41044
20201015::194500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194510_wf.raa
20201015::194519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194520_wf.raa
20201015::194529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194530_wf.raa
20201015::194530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 41099
20201015::194530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194540_wf.raa
20201015::194549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194550_wf.raa
20201015::194559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194600_wf.raa
20201015::194600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 41154
20201015::194600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194610_wf.raa
20201015::194619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194620_wf.raa
20201015::194629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194630_wf.raa
20201015::194630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 41209
20201015::194630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194640_wf.raa
20201015::194649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194650_wf.raa
20201015::194659: Head 1: Time Synchronization: 2020.10.15   19:47:00::0015
20201015::194659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194700_wf.raa
20201015::194700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 41264
20201015::194700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194710_wf.raa
20201015::194719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194720_wf.raa
20201015::194729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194730_wf.raa
20201015::194730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 41320
20201015::194730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194740_wf.raa
20201015::194749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194750_wf.raa
20201015::194759: Head 2: Time Synchronization: 2020.10.15   19:48:00::0016
20201015::194759: Head 1: Time Synchronization: 2020.10.15   19:48:00::0016
20201015::194759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194800_wf.raa
20201015::194800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 41375
20201015::194800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194810_wf.raa
20201015::194819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194820_wf.raa
20201015::194829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194830_wf.raa
20201015::194830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 41430
20201015::194830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194840_wf.raa
20201015::194849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194850_wf.raa
20201015::194859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194900_wf.raa
20201015::194900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 41485
20201015::194900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194910_wf.raa
20201015::194919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194920_wf.raa
20201015::194929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194930_wf.raa
20201015::194930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 41540
20201015::194930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::194939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194940_wf.raa
20201015::194949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_194950_wf.raa
20201015::194959: Head 1: Time Synchronization: 2020.10.15   19:50:00::0018
20201015::194959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195000_wf.raa
20201015::195000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 41595
20201015::195000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195010_wf.raa
20201015::195019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195020_wf.raa
20201015::195029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195030_wf.raa
20201015::195030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 41650
20201015::195030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195040_wf.raa
20201015::195049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195050_wf.raa
20201015::195059: Head 1: Time Synchronization: 2020.10.15   19:51:00::0015
20201015::195059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195100_wf.raa
20201015::195100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 41706
20201015::195100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195110_wf.raa
20201015::195119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195120_wf.raa
20201015::195129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195130_wf.raa
20201015::195130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 41761
20201015::195130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195140_wf.raa
20201015::195149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195150_wf.raa
20201015::195159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195200_wf.raa
20201015::195200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 41817
20201015::195200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195210_wf.raa
20201015::195219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195220_wf.raa
20201015::195229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195230_wf.raa
20201015::195230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 41872
20201015::195230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195240_wf.raa
20201015::195249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195250_wf.raa
20201015::195259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195300_wf.raa
20201015::195300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 41927
20201015::195300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195310_wf.raa
20201015::195319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195320_wf.raa
20201015::195329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195330_wf.raa
20201015::195330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 41983
20201015::195330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195340_wf.raa
20201015::195349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195350_wf.raa
20201015::195359: Head 1: Time Synchronization: 2020.10.15   19:54:00::0016
20201015::195359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195400_wf.raa
20201015::195400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 42038
20201015::195400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195410_wf.raa
20201015::195419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195420_wf.raa
20201015::195429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195430_wf.raa
20201015::195430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 42093
20201015::195430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195440_wf.raa
20201015::195449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195450_wf.raa
20201015::195459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195500_wf.raa
20201015::195500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 42149
20201015::195500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195510_wf.raa
20201015::195519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195520_wf.raa
20201015::195529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195530_wf.raa
20201015::195530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 42204
20201015::195530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195540_wf.raa
20201015::195549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195550_wf.raa
20201015::195559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195600_wf.raa
20201015::195600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 42259
20201015::195600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195610_wf.raa
20201015::195619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195620_wf.raa
20201015::195629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195630_wf.raa
20201015::195630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 42314
20201015::195630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195640_wf.raa
20201015::195649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195650_wf.raa
20201015::195659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195700_wf.raa
20201015::195659: Head 1: Time Synchronization: 2020.10.15   19:57:00::0016
20201015::195700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 42370
20201015::195700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195710_wf.raa
20201015::195719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195720_wf.raa
20201015::195729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195730_wf.raa
20201015::195730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 42424
20201015::195730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195740_wf.raa
20201015::195749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195750_wf.raa
20201015::195759: Head 1: Time Synchronization: 2020.10.15   19:58:00::0016
20201015::195759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195800_wf.raa
20201015::195800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 42480
20201015::195800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195810_wf.raa
20201015::195819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195820_wf.raa
20201015::195829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195830_wf.raa
20201015::195830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 42535
20201015::195830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195840_wf.raa
20201015::195849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195850_wf.raa
20201015::195859: Head 1: Time Synchronization: 2020.10.15   19:59:00::0014
20201015::195859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195900_wf.raa
20201015::195900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 42589
20201015::195900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195910_wf.raa
20201015::195919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195920_wf.raa
20201015::195929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195930_wf.raa
20201015::195930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 42644
20201015::195930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::195939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195940_wf.raa
20201015::195949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_195950_wf.raa
20201015::195959: Head 1: Time Synchronization: 2020.10.15   20:00:00::0014
20201015::195959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200000_wf.raa
20201015::200000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 42700
20201015::200000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200010_wf.raa
20201015::200019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200020_wf.raa
20201015::200029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200030_wf.raa
20201015::200030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 42755
20201015::200030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200040_wf.raa
20201015::200049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200050_wf.raa
20201015::200059: Head 2: Time Synchronization: 2020.10.15   20:01:00::0014
20201015::200059: Head 1: Time Synchronization: 2020.10.15   20:01:00::0015
20201015::200059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200100_wf.raa
20201015::200100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 42810
20201015::200100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200110_wf.raa
20201015::200119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200120_wf.raa
20201015::200129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200130_wf.raa
20201015::200130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 42865
20201015::200130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200140_wf.raa
20201015::200149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200150_wf.raa
20201015::200159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200200_wf.raa
20201015::200200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 42920
20201015::200200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200210_wf.raa
20201015::200219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200220_wf.raa
20201015::200229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200230_wf.raa
20201015::200230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 42976
20201015::200230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200240_wf.raa
20201015::200249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200250_wf.raa
20201015::200259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200300_wf.raa
20201015::200300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 43031
20201015::200300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200310_wf.raa
20201015::200319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200320_wf.raa
20201015::200329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200330_wf.raa
20201015::200330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 43085
20201015::200330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200340_wf.raa
20201015::200349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200350_wf.raa
20201015::200359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200400_wf.raa
20201015::200400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 43141
20201015::200400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200410_wf.raa
20201015::200419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200420_wf.raa
20201015::200429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200430_wf.raa
20201015::200430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 43196
20201015::200430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200440_wf.raa
20201015::200449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200450_wf.raa
20201015::200459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200500_wf.raa
20201015::200500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 43250
20201015::200500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200510_wf.raa
20201015::200519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200520_wf.raa
20201015::200529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200530_wf.raa
20201015::200530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 43305
20201015::200530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200540_wf.raa
20201015::200549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200550_wf.raa
20201015::200559: Head 1: Time Synchronization: 2020.10.15   20:06:00::0014
20201015::200559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200600_wf.raa
20201015::200600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 43360
20201015::200600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200610_wf.raa
20201015::200619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200620_wf.raa
20201015::200629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200630_wf.raa
20201015::200630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 43416
20201015::200630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200640_wf.raa
20201015::200649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200650_wf.raa
20201015::200659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200700_wf.raa
20201015::200700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 43471
20201015::200700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200710_wf.raa
20201015::200719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200720_wf.raa
20201015::200729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200730_wf.raa
20201015::200730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 43525
20201015::200730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200740_wf.raa
20201015::200749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200750_wf.raa
20201015::200759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200800_wf.raa
20201015::200800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 43580
20201015::200800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200810_wf.raa
20201015::200819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200820_wf.raa
20201015::200829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200830_wf.raa
20201015::200830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 43635
20201015::200830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200840_wf.raa
20201015::200849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200850_wf.raa
20201015::200859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200900_wf.raa
20201015::200900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 43691
20201015::200900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200910_wf.raa
20201015::200919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200920_wf.raa
20201015::200929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200930_wf.raa
20201015::200930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 43746
20201015::200930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::200939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200940_wf.raa
20201015::200949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_200950_wf.raa
20201015::200959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201000_wf.raa
20201015::201000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 43801
20201015::201000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201010_wf.raa
20201015::201019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201020_wf.raa
20201015::201029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201030_wf.raa
20201015::201030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 43857
20201015::201030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201040_wf.raa
20201015::201049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201050_wf.raa
20201015::201059: Head 1: Time Synchronization: 2020.10.15   20:11:00::0015
20201015::201059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201100_wf.raa
20201015::201100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 43912
20201015::201100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201110_wf.raa
20201015::201119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201120_wf.raa
20201015::201129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201130_wf.raa
20201015::201130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 43968
20201015::201130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201140_wf.raa
20201015::201149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201150_wf.raa
20201015::201159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201200_wf.raa
20201015::201200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 44023
20201015::201200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201210_wf.raa
20201015::201219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201220_wf.raa
20201015::201229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201230_wf.raa
20201015::201230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 44078
20201015::201230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201240_wf.raa
20201015::201249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201250_wf.raa
20201015::201259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201300_wf.raa
20201015::201300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 44133
20201015::201300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201310_wf.raa
20201015::201319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201320_wf.raa
20201015::201329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201330_wf.raa
20201015::201330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 44188
20201015::201330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201340_wf.raa
20201015::201349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201350_wf.raa
20201015::201359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201400_wf.raa
20201015::201400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 44243
20201015::201400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201410_wf.raa
20201015::201419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201420_wf.raa
20201015::201429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201430_wf.raa
20201015::201430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 44299
20201015::201430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201440_wf.raa
20201015::201449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201450_wf.raa
20201015::201459: Head 2: Time Synchronization: 2020.10.15   20:15:00::0014
20201015::201459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201500_wf.raa
20201015::201500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 44354
20201015::201500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201510_wf.raa
20201015::201519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201520_wf.raa
20201015::201529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201530_wf.raa
20201015::201530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 44408
20201015::201530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201540_wf.raa
20201015::201549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201550_wf.raa
20201015::201559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201600_wf.raa
20201015::201600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 44461
20201015::201600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201610_wf.raa
20201015::201619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201620_wf.raa
20201015::201629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201630_wf.raa
20201015::201630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 44515
20201015::201630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201640_wf.raa
20201015::201649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201650_wf.raa
20201015::201659: Head 1: Time Synchronization: 2020.10.15   20:17:00::0014
20201015::201659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201700_wf.raa
20201015::201700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 44568
20201015::201700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201710_wf.raa
20201015::201719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201720_wf.raa
20201015::201729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201730_wf.raa
20201015::201730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 44621
20201015::201730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201740_wf.raa
20201015::201749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201750_wf.raa
20201015::201759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201800_wf.raa
20201015::201800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 44675
20201015::201800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201810_wf.raa
20201015::201819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201820_wf.raa
20201015::201829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201830_wf.raa
20201015::201830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 44728
20201015::201830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201840_wf.raa
20201015::201849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201850_wf.raa
20201015::201859: Head 1: Time Synchronization: 2020.10.15   20:19:00::0015
20201015::201859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201900_wf.raa
20201015::201900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 44781
20201015::201900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201910_wf.raa
20201015::201919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201920_wf.raa
20201015::201929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201930_wf.raa
20201015::201930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 44835
20201015::201930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::201939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201940_wf.raa
20201015::201949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_201950_wf.raa
20201015::201959: Head 1: Time Synchronization: 2020.10.15   20:20:00::0014
20201015::201959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202000_wf.raa
20201015::202000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 44888
20201015::202000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202010_wf.raa
20201015::202019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202020_wf.raa
20201015::202029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202030_wf.raa
20201015::202030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 44942
20201015::202030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202040_wf.raa
20201015::202049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202050_wf.raa
20201015::202059: Head 1: Time Synchronization: 2020.10.15   20:21:00::0015
20201015::202059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202100_wf.raa
20201015::202100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 44996
20201015::202100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202110_wf.raa
20201015::202119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202120_wf.raa
20201015::202129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202130_wf.raa
20201015::202130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.2dbar, CTD 34.7psu, index 1.35, Packet 45051
20201015::202130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202140_wf.raa
20201015::202149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202150_wf.raa
20201015::202159: Head 1: Time Synchronization: 2020.10.15   20:22:00::0014
20201015::202159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202200_wf.raa
20201015::202200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 45105
20201015::202200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202210_wf.raa
20201015::202219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202220_wf.raa
20201015::202229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202230_wf.raa
20201015::202230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 45160
20201015::202230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202240_wf.raa
20201015::202249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202250_wf.raa
20201015::202259: Head 1: Time Synchronization: 2020.10.15   20:23:00::0015
20201015::202259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202300_wf.raa
20201015::202300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 45214
20201015::202300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202310_wf.raa
20201015::202319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202320_wf.raa
20201015::202329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202330_wf.raa
20201015::202330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 45268
20201015::202330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202340_wf.raa
20201015::202349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202350_wf.raa
20201015::202359: Head 1: Time Synchronization: 2020.10.15   20:24:00::0015
20201015::202359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202400_wf.raa
20201015::202400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 45322
20201015::202400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202410_wf.raa
20201015::202419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202420_wf.raa
20201015::202429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202430_wf.raa
20201015::202430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 45377
20201015::202430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202440: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202440_wf.raa
20201015::202449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202450_wf.raa
20201015::202459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202500_wf.raa
20201015::202500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.6dbar, CTD 34.7psu, index 1.35, Packet 45430
20201015::202500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202510_wf.raa
20201015::202519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202520_wf.raa
20201015::202529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202530_wf.raa
20201015::202530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 45485
20201015::202530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202540_wf.raa
20201015::202549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202550_wf.raa
20201015::202559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202600_wf.raa
20201015::202600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 45540
20201015::202600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202610_wf.raa
20201015::202619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202620_wf.raa
20201015::202629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202630_wf.raa
20201015::202630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 45596
20201015::202630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202640_wf.raa
20201015::202649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202650_wf.raa
20201015::202659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202700_wf.raa
20201015::202700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 45651
20201015::202700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202710_wf.raa
20201015::202719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202720_wf.raa
20201015::202729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202730_wf.raa
20201015::202730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 45706
20201015::202730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202740_wf.raa
20201015::202749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202750_wf.raa
20201015::202759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202800_wf.raa
20201015::202800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 45761
20201015::202800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202810_wf.raa
20201015::202819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202820_wf.raa
20201015::202829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202830_wf.raa
20201015::202830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 45816
20201015::202830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202840_wf.raa
20201015::202849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202850_wf.raa
20201015::202859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202900_wf.raa
20201015::202859: Head 1: Time Synchronization: 2020.10.15   20:29:00::0015
20201015::202859: Head 2: Time Synchronization: 2020.10.15   20:29:00::0014
20201015::202900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 45871
20201015::202900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202910_wf.raa
20201015::202919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202920_wf.raa
20201015::202929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202930_wf.raa
20201015::202930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 45926
20201015::202930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::202939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202940_wf.raa
20201015::202949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_202950_wf.raa
20201015::202959: Head 1: Time Synchronization: 2020.10.15   20:30:00::0014
20201015::202959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203000_wf.raa
20201015::203000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 45981
20201015::203000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203010_wf.raa
20201015::203019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203020_wf.raa
20201015::203029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203030_wf.raa
20201015::203030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 46036
20201015::203030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203040_wf.raa
20201015::203049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203050_wf.raa
20201015::203059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203100_wf.raa
20201015::203100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 46092
20201015::203100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203110_wf.raa
20201015::203119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203120_wf.raa
20201015::203129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203130_wf.raa
20201015::203130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 46147
20201015::203130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203140_wf.raa
20201015::203149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203150_wf.raa
20201015::203159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203200_wf.raa
20201015::203200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 46202
20201015::203200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203210_wf.raa
20201015::203219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203220_wf.raa
20201015::203229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203230_wf.raa
20201015::203230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 46257
20201015::203230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203240_wf.raa
20201015::203249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203250_wf.raa
20201015::203259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203300_wf.raa
20201015::203300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 46312
20201015::203300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203310_wf.raa
20201015::203319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203320_wf.raa
20201015::203329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203330_wf.raa
20201015::203330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 46367
20201015::203330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203340_wf.raa
20201015::203349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203350_wf.raa
20201015::203359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203400_wf.raa
20201015::203400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 46422
20201015::203400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203410_wf.raa
20201015::203419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203420_wf.raa
20201015::203429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203430_wf.raa
20201015::203430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 46477
20201015::203430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203440_wf.raa
20201015::203449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203450_wf.raa
20201015::203459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203500_wf.raa
20201015::203500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 46533
20201015::203500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203510_wf.raa
20201015::203519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203520_wf.raa
20201015::203529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203530_wf.raa
20201015::203530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 46588
20201015::203530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203540_wf.raa
20201015::203549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203550_wf.raa
20201015::203559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203600_wf.raa
20201015::203600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 46643
20201015::203600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203610_wf.raa
20201015::203619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203620_wf.raa
20201015::203629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203630_wf.raa
20201015::203630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 46698
20201015::203630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203640_wf.raa
20201015::203649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203650_wf.raa
20201015::203659: Head 1: Time Synchronization: 2020.10.15   20:37:00::0015
20201015::203659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203700_wf.raa
20201015::203700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 46753
20201015::203700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203710_wf.raa
20201015::203719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203720_wf.raa
20201015::203729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203730_wf.raa
20201015::203730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 46809
20201015::203730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203740_wf.raa
20201015::203749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203750_wf.raa
20201015::203759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203800_wf.raa
20201015::203800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 46864
20201015::203800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203810_wf.raa
20201015::203819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203820_wf.raa
20201015::203829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203830_wf.raa
20201015::203830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 46920
20201015::203830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203840_wf.raa
20201015::203849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203850_wf.raa
20201015::203859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203900_wf.raa
20201015::203900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 46975
20201015::203900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203910_wf.raa
20201015::203919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203920_wf.raa
20201015::203929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203930_wf.raa
20201015::203930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 47030
20201015::203930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::203939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203940_wf.raa
20201015::203949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_203950_wf.raa
20201015::203959: Head 1: Time Synchronization: 2020.10.15   20:40:00::0015
20201015::203959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204000_wf.raa
20201015::204000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 47085
20201015::204000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204010_wf.raa
20201015::204019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204020_wf.raa
20201015::204029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204030_wf.raa
20201015::204030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 47140
20201015::204030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204040_wf.raa
20201015::204049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204050_wf.raa
20201015::204059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204100_wf.raa
20201015::204100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 47196
20201015::204100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204110_wf.raa
20201015::204119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204120_wf.raa
20201015::204129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204130_wf.raa
20201015::204130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 47251
20201015::204130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204140_wf.raa
20201015::204149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204150_wf.raa
20201015::204159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204200_wf.raa
20201015::204200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 47306
20201015::204200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204210_wf.raa
20201015::204219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204220_wf.raa
20201015::204229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204230_wf.raa
20201015::204230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 47360
20201015::204230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204240_wf.raa
20201015::204249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204250_wf.raa
20201015::204259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204300_wf.raa
20201015::204300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 47416
20201015::204300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204310_wf.raa
20201015::204319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204320_wf.raa
20201015::204329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204330_wf.raa
20201015::204330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 47471
20201015::204330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204340_wf.raa
20201015::204349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204350_wf.raa
20201015::204359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204400_wf.raa
20201015::204400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 47526
20201015::204400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204410_wf.raa
20201015::204419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204420_wf.raa
20201015::204429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204430_wf.raa
20201015::204430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 47581
20201015::204430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204440_wf.raa
20201015::204449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204450_wf.raa
20201015::204459: Head 1: Time Synchronization: 2020.10.15   20:45:00::0014
20201015::204459: Head 2: Time Synchronization: 2020.10.15   20:45:00::0014
20201015::204459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204500_wf.raa
20201015::204500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 47637
20201015::204500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204510_wf.raa
20201015::204519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204520_wf.raa
20201015::204529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204530_wf.raa
20201015::204530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 47692
20201015::204530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204540_wf.raa
20201015::204549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204550_wf.raa
20201015::204559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204600_wf.raa
20201015::204600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 47747
20201015::204600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204610_wf.raa
20201015::204619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204620_wf.raa
20201015::204629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204630_wf.raa
20201015::204630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.4dbar, CTD 34.7psu, index 1.35, Packet 47802
20201015::204630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204640_wf.raa
20201015::204649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204650_wf.raa
20201015::204659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204700_wf.raa
20201015::204700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 47857
20201015::204700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204710_wf.raa
20201015::204719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204720_wf.raa
20201015::204729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204730_wf.raa
20201015::204730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 47912
20201015::204730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204740_wf.raa
20201015::204749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204750_wf.raa
20201015::204759: Head 1: Time Synchronization: 2020.10.15   20:48:00::0016
20201015::204759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204800_wf.raa
20201015::204800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 47967
20201015::204800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204810_wf.raa
20201015::204819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204820_wf.raa
20201015::204829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204830_wf.raa
20201015::204830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 48022
20201015::204830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204840_wf.raa
20201015::204849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204850_wf.raa
20201015::204859: Head 1: Time Synchronization: 2020.10.15   20:49:00::0017
20201015::204859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204900_wf.raa
20201015::204900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 48077
20201015::204900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204910_wf.raa
20201015::204919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204920_wf.raa
20201015::204929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204930_wf.raa
20201015::204930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 48133
20201015::204930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::204939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204940_wf.raa
20201015::204949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_204950_wf.raa
20201015::204959: Head 1: Time Synchronization: 2020.10.15   20:50:00::0015
20201015::204959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205000_wf.raa
20201015::205000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 48188
20201015::205000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205010_wf.raa
20201015::205019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205020_wf.raa
20201015::205029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205030_wf.raa
20201015::205030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 48244
20201015::205030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205040_wf.raa
20201015::205049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205050_wf.raa
20201015::205059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205100_wf.raa
20201015::205100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 48299
20201015::205100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205110_wf.raa
20201015::205119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205120_wf.raa
20201015::205129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205130_wf.raa
20201015::205130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 48354
20201015::205130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205140_wf.raa
20201015::205149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205150_wf.raa
20201015::205159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205200_wf.raa
20201015::205200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 48409
20201015::205200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205210_wf.raa
20201015::205219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205220_wf.raa
20201015::205229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205230_wf.raa
20201015::205230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 48464
20201015::205230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205240_wf.raa
20201015::205249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205250_wf.raa
20201015::205259: Head 1: Time Synchronization: 2020.10.15   20:53:00::0015
20201015::205259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205300_wf.raa
20201015::205300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 48520
20201015::205300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205310_wf.raa
20201015::205319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205320_wf.raa
20201015::205329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205330_wf.raa
20201015::205330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 48575
20201015::205330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205340_wf.raa
20201015::205349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205350_wf.raa
20201015::205359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205400_wf.raa
20201015::205400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 48630
20201015::205400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205410_wf.raa
20201015::205419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205420_wf.raa
20201015::205429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205430_wf.raa
20201015::205430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 48685
20201015::205430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205440_wf.raa
20201015::205449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205450_wf.raa
20201015::205459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205500_wf.raa
20201015::205500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 48740
20201015::205500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205510_wf.raa
20201015::205519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205520_wf.raa
20201015::205529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205530_wf.raa
20201015::205530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 48795
20201015::205530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205540_wf.raa
20201015::205549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205550_wf.raa
20201015::205559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205600_wf.raa
20201015::205600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 48851
20201015::205600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205610_wf.raa
20201015::205619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205620_wf.raa
20201015::205629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205630_wf.raa
20201015::205630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 48906
20201015::205630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205640_wf.raa
20201015::205649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205650_wf.raa
20201015::205659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205700_wf.raa
20201015::205700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 48961
20201015::205700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205710_wf.raa
20201015::205719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205720_wf.raa
20201015::205729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205730_wf.raa
20201015::205730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 49015
20201015::205730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205740_wf.raa
20201015::205749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205750_wf.raa
20201015::205759: Head 1: Time Synchronization: 2020.10.15   20:58:00::0016
20201015::205759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205800_wf.raa
20201015::205800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 49070
20201015::205800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205810_wf.raa
20201015::205819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205820_wf.raa
20201015::205829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205830_wf.raa
20201015::205830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 49126
20201015::205830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205840_wf.raa
20201015::205849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205850_wf.raa
20201015::205859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205900_wf.raa
20201015::205900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 49181
20201015::205900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205910_wf.raa
20201015::205919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205920_wf.raa
20201015::205929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205930_wf.raa
20201015::205930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 49236
20201015::205930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::205939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205940_wf.raa
20201015::205949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_205950_wf.raa
20201015::205959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210000_wf.raa
20201015::210000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 49291
20201015::210000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210010_wf.raa
20201015::210019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210020_wf.raa
20201015::210029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210030_wf.raa
20201015::210030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 49346
20201015::210030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210040_wf.raa
20201015::210049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210050_wf.raa
20201015::210059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210100_wf.raa
20201015::210100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 49401
20201015::210100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210110_wf.raa
20201015::210119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210120_wf.raa
20201015::210129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210130_wf.raa
20201015::210130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 49457
20201015::210130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210140_wf.raa
20201015::210149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210150_wf.raa
20201015::210159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210200_wf.raa
20201015::210200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 49511
20201015::210200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210210_wf.raa
20201015::210219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210220_wf.raa
20201015::210229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210230_wf.raa
20201015::210230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 49566
20201015::210230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210240_wf.raa
20201015::210249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210250_wf.raa
20201015::210259: Head 1: Time Synchronization: 2020.10.15   21:03:00::0017
20201015::210259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210300_wf.raa
20201015::210300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 49621
20201015::210300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210310_wf.raa
20201015::210319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210320_wf.raa
20201015::210329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210330_wf.raa
20201015::210330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 49676
20201015::210330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210340_wf.raa
20201015::210349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210350_wf.raa
20201015::210359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210400_wf.raa
20201015::210400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 49731
20201015::210400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210410_wf.raa
20201015::210419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210420_wf.raa
20201015::210429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210430_wf.raa
20201015::210430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 49787
20201015::210430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210440_wf.raa
20201015::210449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210450_wf.raa
20201015::210459: Head 1: Time Synchronization: 2020.10.15   21:05:00::0014
20201015::210459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210500_wf.raa
20201015::210500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 49842
20201015::210500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210510_wf.raa
20201015::210519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210520_wf.raa
20201015::210529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210530_wf.raa
20201015::210530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 49898
20201015::210530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210540_wf.raa
20201015::210549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210550_wf.raa
20201015::210559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210600_wf.raa
20201015::210600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 49955
20201015::210600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210610_wf.raa
20201015::210619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210620_wf.raa
20201015::210629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210630_wf.raa
20201015::210630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 50014
20201015::210630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210640_wf.raa
20201015::210649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210650_wf.raa
20201015::210659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210700_wf.raa
20201015::210700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 50071
20201015::210700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210710_wf.raa
20201015::210719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210720_wf.raa
20201015::210729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210730_wf.raa
20201015::210730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 50124
20201015::210730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210740_wf.raa
20201015::210749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210750_wf.raa
20201015::210759: Head 1: Time Synchronization: 2020.10.15   21:08:00::0016
20201015::210759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210800_wf.raa
20201015::210800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 50180
20201015::210800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210810_wf.raa
20201015::210819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210820_wf.raa
20201015::210829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210830_wf.raa
20201015::210830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 50236
20201015::210830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210840_wf.raa
20201015::210849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210850_wf.raa
20201015::210859: Head 1: Time Synchronization: 2020.10.15   21:09:00::0015
20201015::210859: Head 2: Time Synchronization: 2020.10.15   21:09:00::0015
20201015::210859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210900_wf.raa
20201015::210900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 50292
20201015::210900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210910_wf.raa
20201015::210919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210920_wf.raa
20201015::210929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210930_wf.raa
20201015::210930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 50349
20201015::210930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::210939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210940_wf.raa
20201015::210949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_210950_wf.raa
20201015::210959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211000_wf.raa
20201015::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 50407
20201015::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211010_wf.raa
20201015::211019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211020_wf.raa
20201015::211029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211030_wf.raa
20201015::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 50464
20201015::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211040_wf.raa
20201015::211049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211050_wf.raa
20201015::211059: Head 1: Time Synchronization: 2020.10.15   21:11:00::0015
20201015::211059: Head 2: Time Synchronization: 2020.10.15   21:11:00::0016
20201015::211059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211100_wf.raa
20201015::211100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 50520
20201015::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211110_wf.raa
20201015::211119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211120_wf.raa
20201015::211129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211130_wf.raa
20201015::211130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 50576
20201015::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211140_wf.raa
20201015::211149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211150_wf.raa
20201015::211159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211200_wf.raa
20201015::211200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 50633
20201015::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211210_wf.raa
20201015::211219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211220_wf.raa
20201015::211229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211230_wf.raa
20201015::211230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 50690
20201015::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211240_wf.raa
20201015::211249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211250_wf.raa
20201015::211259: Head 2: Time Synchronization: 2020.10.15   21:13:00::0015
20201015::211259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211300_wf.raa
20201015::211300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 50748
20201015::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211310_wf.raa
20201015::211319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211320_wf.raa
20201015::211329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211330_wf.raa
20201015::211330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 50805
20201015::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211340_wf.raa
20201015::211349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211350_wf.raa
20201015::211359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211400_wf.raa
20201015::211400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 50861
20201015::211400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211410_wf.raa
20201015::211419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211420_wf.raa
20201015::211429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211430_wf.raa
20201015::211430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 50917
20201015::211430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211440_wf.raa
20201015::211449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211450_wf.raa
20201015::211459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211500_wf.raa
20201015::211500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 50975
20201015::211500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211510_wf.raa
20201015::211519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211520_wf.raa
20201015::211529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211530_wf.raa
20201015::211530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 51032
20201015::211530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211540_wf.raa
20201015::211549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211550_wf.raa
20201015::211559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211600_wf.raa
20201015::211600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 51088
20201015::211600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211610_wf.raa
20201015::211619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211620_wf.raa
20201015::211629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211630_wf.raa
20201015::211630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 51144
20201015::211630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211640_wf.raa
20201015::211649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211650_wf.raa
20201015::211659: Head 1: Time Synchronization: 2020.10.15   21:17:00::0014
20201015::211659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211700_wf.raa
20201015::211700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 51200
20201015::211700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211710_wf.raa
20201015::211719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211720_wf.raa
20201015::211729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211730_wf.raa
20201015::211730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 51258
20201015::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211740_wf.raa
20201015::211749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211750_wf.raa
20201015::211759: Head 2: Time Synchronization: 2020.10.15   21:18:00::0016
20201015::211759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211800_wf.raa
20201015::211800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 51315
20201015::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211810_wf.raa
20201015::211819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211820_wf.raa
20201015::211829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211830_wf.raa
20201015::211830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 51372
20201015::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211840_wf.raa
20201015::211849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211850_wf.raa
20201015::211859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211900_wf.raa
20201015::211900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 51429
20201015::211900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211910_wf.raa
20201015::211919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211920_wf.raa
20201015::211929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211930_wf.raa
20201015::211930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 51486
20201015::211930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::211939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211940_wf.raa
20201015::211949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_211950_wf.raa
20201015::211959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212000_wf.raa
20201015::212000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 51542
20201015::212000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212010_wf.raa
20201015::212019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212020_wf.raa
20201015::212029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212030_wf.raa
20201015::212030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 51599
20201015::212030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212040_wf.raa
20201015::212049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212050_wf.raa
20201015::212059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212100_wf.raa
20201015::212100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 51656
20201015::212100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212110_wf.raa
20201015::212119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212120_wf.raa
20201015::212129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212130_wf.raa
20201015::212130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 51712
20201015::212130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212140_wf.raa
20201015::212149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212150_wf.raa
20201015::212159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212200_wf.raa
20201015::212200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 51768
20201015::212200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212210_wf.raa
20201015::212219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212220_wf.raa
20201015::212229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212230_wf.raa
20201015::212230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 51824
20201015::212230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212240_wf.raa
20201015::212249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212250_wf.raa
20201015::212259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212300_wf.raa
20201015::212300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 51880
20201015::212300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212310_wf.raa
20201015::212319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212320_wf.raa
20201015::212329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212330_wf.raa
20201015::212330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 51937
20201015::212330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212340_wf.raa
20201015::212349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212350_wf.raa
20201015::212359: Head 2: Time Synchronization: 2020.10.15   21:24:00::0015
20201015::212359: Head 1: Time Synchronization: 2020.10.15   21:24:00::0016
20201015::212359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212400_wf.raa
20201015::212400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 51993
20201015::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212410: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212410_wf.raa
20201015::212419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212420_wf.raa
20201015::212429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212430_wf.raa
20201015::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 52049
20201015::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212440_wf.raa
20201015::212449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212450_wf.raa
20201015::212459: Head 1: Time Synchronization: 2020.10.15   21:25:00::0017
20201015::212459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212500_wf.raa
20201015::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 52107
20201015::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212510_wf.raa
20201015::212519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212520_wf.raa
20201015::212529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212530_wf.raa
20201015::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.1dbar, CTD 34.7psu, index 1.35, Packet 52166
20201015::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212540_wf.raa
20201015::212549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212550_wf.raa
20201015::212559: Head 2: Time Synchronization: 2020.10.15   21:26:00::0015
20201015::212559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212600_wf.raa
20201015::212600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 52223
20201015::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212610_wf.raa
20201015::212619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212620_wf.raa
20201015::212629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212630_wf.raa
20201015::212630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.9dbar, CTD 34.7psu, index 1.35, Packet 52280
20201015::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212640_wf.raa
20201015::212649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212650_wf.raa
20201015::212659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212700_wf.raa
20201015::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 52338
20201015::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212710_wf.raa
20201015::212719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212720_wf.raa
20201015::212729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212730_wf.raa
20201015::212730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 52396
20201015::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212740_wf.raa
20201015::212749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212750_wf.raa
20201015::212759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212800_wf.raa
20201015::212800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 52455
20201015::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212810_wf.raa
20201015::212819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212820_wf.raa
20201015::212829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212830_wf.raa
20201015::212830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 52513
20201015::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212840_wf.raa
20201015::212849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212850_wf.raa
20201015::212859: Head 1: Time Synchronization: 2020.10.15   21:29:00::0014
20201015::212859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212900_wf.raa
20201015::212900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 52570
20201015::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212910_wf.raa
20201015::212919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212920_wf.raa
20201015::212929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212930_wf.raa
20201015::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 52628
20201015::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::212939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212940_wf.raa
20201015::212949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_212950_wf.raa
20201015::212959: Head 1: Time Synchronization: 2020.10.15   21:30:00::0014
20201015::212959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213000_wf.raa
20201015::213000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 52684
20201015::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213010_wf.raa
20201015::213019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213020_wf.raa
20201015::213029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213030_wf.raa
20201015::213030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 52742
20201015::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213040_wf.raa
20201015::213049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213050_wf.raa
20201015::213059: Head 1: Time Synchronization: 2020.10.15   21:31:00::0014
20201015::213059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213100_wf.raa
20201015::213100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 52801
20201015::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213110_wf.raa
20201015::213119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213120_wf.raa
20201015::213129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213130_wf.raa
20201015::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 52858
20201015::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213140_wf.raa
20201015::213149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213150_wf.raa
20201015::213159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213200_wf.raa
20201015::213200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 52914
20201015::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213210_wf.raa
20201015::213219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213220_wf.raa
20201015::213229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213230_wf.raa
20201015::213230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 52971
20201015::213230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213240_wf.raa
20201015::213249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213250_wf.raa
20201015::213259: Head 1: Time Synchronization: 2020.10.15   21:33:00::0014
20201015::213259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213300_wf.raa
20201015::213300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 53028
20201015::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213310_wf.raa
20201015::213319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213320_wf.raa
20201015::213329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213330_wf.raa
20201015::213330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 53085
20201015::213330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213340_wf.raa
20201015::213349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213350_wf.raa
20201015::213359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213400_wf.raa
20201015::213400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 53141
20201015::213400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213410_wf.raa
20201015::213419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213420_wf.raa
20201015::213429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213430_wf.raa
20201015::213430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 53199
20201015::213430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213440_wf.raa
20201015::213449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213450_wf.raa
20201015::213459: Head 2: Time Synchronization: 2020.10.15   21:35:00::0016
20201015::213459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213500_wf.raa
20201015::213500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 53256
20201015::213500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213510_wf.raa
20201015::213519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213520_wf.raa
20201015::213529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213530_wf.raa
20201015::213530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 53312
20201015::213530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213540_wf.raa
20201015::213549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213550_wf.raa
20201015::213559: Head 1: Time Synchronization: 2020.10.15   21:36:00::0014
20201015::213559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213600_wf.raa
20201015::213600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 53370
20201015::213600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213610_wf.raa
20201015::213619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213620_wf.raa
20201015::213629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213630_wf.raa
20201015::213630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 53427
20201015::213630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213640_wf.raa
20201015::213649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213650_wf.raa
20201015::213659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213700_wf.raa
20201015::213700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 53484
20201015::213700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213710_wf.raa
20201015::213719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213720_wf.raa
20201015::213729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213730_wf.raa
20201015::213730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 53540
20201015::213730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213740_wf.raa
20201015::213749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213750_wf.raa
20201015::213759: Head 1: Time Synchronization: 2020.10.15   21:38:00::0014
20201015::213759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213800_wf.raa
20201015::213800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 53596
20201015::213800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213810_wf.raa
20201015::213819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213820_wf.raa
20201015::213829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213830_wf.raa
20201015::213830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 53652
20201015::213830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213840_wf.raa
20201015::213849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213850_wf.raa
20201015::213859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213900_wf.raa
20201015::213900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 53708
20201015::213900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213910_wf.raa
20201015::213919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213920_wf.raa
20201015::213929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213930_wf.raa
20201015::213930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 53764
20201015::213930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::213939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213940_wf.raa
20201015::213949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_213950_wf.raa
20201015::213959: Head 1: Time Synchronization: 2020.10.15   21:40:00::0013
20201015::213959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214000_wf.raa
20201015::214000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 53820
20201015::214000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214010_wf.raa
20201015::214019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214020_wf.raa
20201015::214029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214030_wf.raa
20201015::214030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 53876
20201015::214030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214040_wf.raa
20201015::214049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214050_wf.raa
20201015::214059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214100_wf.raa
20201015::214100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 53933
20201015::214100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214110_wf.raa
20201015::214119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214120_wf.raa
20201015::214129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214130_wf.raa
20201015::214130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 53989
20201015::214130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214140_wf.raa
20201015::214149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214150_wf.raa
20201015::214159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214200_wf.raa
20201015::214200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 54045
20201015::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214210_wf.raa
20201015::214219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214220_wf.raa
20201015::214229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214230_wf.raa
20201015::214230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 54101
20201015::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214240_wf.raa
20201015::214249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214250_wf.raa
20201015::214259: Head 1: Time Synchronization: 2020.10.15   21:43:00::0014
20201015::214259: Head 2: Time Synchronization: 2020.10.15   21:43:00::0014
20201015::214259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214300_wf.raa
20201015::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 54157
20201015::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214310_wf.raa
20201015::214319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214320_wf.raa
20201015::214329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214330_wf.raa
20201015::214330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 54213
20201015::214330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214340_wf.raa
20201015::214349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214350_wf.raa
20201015::214359: Head 1: Time Synchronization: 2020.10.15   21:44:00::0014
20201015::214359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214400_wf.raa
20201015::214400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 54269
20201015::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214410_wf.raa
20201015::214419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214420_wf.raa
20201015::214429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214430_wf.raa
20201015::214430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 54324
20201015::214430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214440_wf.raa
20201015::214449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214450_wf.raa
20201015::214459: Head 1: Time Synchronization: 2020.10.15   21:45:00::0015
20201015::214459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214500_wf.raa
20201015::214500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 54378
20201015::214500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214510_wf.raa
20201015::214519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214520_wf.raa
20201015::214529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214530_wf.raa
20201015::214530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 54431
20201015::214530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214540_wf.raa
20201015::214549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214550_wf.raa
20201015::214559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214600_wf.raa
20201015::214600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 54484
20201015::214600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214610_wf.raa
20201015::214619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214620_wf.raa
20201015::214629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214630_wf.raa
20201015::214630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 54537
20201015::214630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214640_wf.raa
20201015::214649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214650_wf.raa
20201015::214659: Head 1: Time Synchronization: 2020.10.15   21:47:00::0015
20201015::214659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214700_wf.raa
20201015::214700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 54591
20201015::214700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214710_wf.raa
20201015::214719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214720_wf.raa
20201015::214729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214730_wf.raa
20201015::214730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 54644
20201015::214730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214740_wf.raa
20201015::214749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214750_wf.raa
20201015::214759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214800_wf.raa
20201015::214800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 54698
20201015::214800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214810_wf.raa
20201015::214819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214820_wf.raa
20201015::214829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214830_wf.raa
20201015::214830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 54755
20201015::214830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214840_wf.raa
20201015::214849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214850_wf.raa
20201015::214859: Head 1: Time Synchronization: 2020.10.15   21:49:00::0014
20201015::214859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214900_wf.raa
20201015::214900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 54812
20201015::214900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214910_wf.raa
20201015::214919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214920_wf.raa
20201015::214929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214930_wf.raa
20201015::214930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 54868
20201015::214930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::214939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214940_wf.raa
20201015::214949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_214950_wf.raa
20201015::214959: Head 1: Time Synchronization: 2020.10.15   21:50:00::0016
20201015::214959: Head 2: Time Synchronization: 2020.10.15   21:50:00::0015
20201015::214959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215000_wf.raa
20201015::215000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 54923
20201015::215000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215010_wf.raa
20201015::215019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215020_wf.raa
20201015::215029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215030_wf.raa
20201015::215030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 54977
20201015::215030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215040_wf.raa
20201015::215049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215050_wf.raa
20201015::215059: Head 2: Time Synchronization: 2020.10.15   21:51:00::0014
20201015::215059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215100_wf.raa
20201015::215100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 55031
20201015::215100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215110_wf.raa
20201015::215119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215120_wf.raa
20201015::215129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215130_wf.raa
20201015::215130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 55084
20201015::215130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215140_wf.raa
20201015::215149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215150_wf.raa
20201015::215159: Head 2: Time Synchronization: 2020.10.15   21:52:00::0013
20201015::215159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215200_wf.raa
20201015::215200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 55138
20201015::215200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215210_wf.raa
20201015::215219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215220_wf.raa
20201015::215229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215230_wf.raa
20201015::215230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 55191
20201015::215230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215240_wf.raa
20201015::215249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215250_wf.raa
20201015::215259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215300_wf.raa
20201015::215300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 55245
20201015::215300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215310_wf.raa
20201015::215319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215320_wf.raa
20201015::215329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215330_wf.raa
20201015::215330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 55299
20201015::215330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215340_wf.raa
20201015::215349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215350_wf.raa
20201015::215359: Head 1: Time Synchronization: 2020.10.15   21:54:00::0014
20201015::215359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215400_wf.raa
20201015::215400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 55352
20201015::215400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215410_wf.raa
20201015::215419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215420_wf.raa
20201015::215429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215430_wf.raa
20201015::215430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 55405
20201015::215430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215440_wf.raa
20201015::215449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215450_wf.raa
20201015::215459: Head 1: Time Synchronization: 2020.10.15   21:55:00::0017
20201015::215459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215500_wf.raa
20201015::215500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 55459
20201015::215500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215510_wf.raa
20201015::215519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215520_wf.raa
20201015::215529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215530_wf.raa
20201015::215530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 55512
20201015::215530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215540_wf.raa
20201015::215549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215550_wf.raa
20201015::215559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215600_wf.raa
20201015::215600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 55565
20201015::215600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215610_wf.raa
20201015::215619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215620_wf.raa
20201015::215629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215630_wf.raa
20201015::215630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 55619
20201015::215630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215640_wf.raa
20201015::215649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215650_wf.raa
20201015::215659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215700_wf.raa
20201015::215700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 55672
20201015::215700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215710_wf.raa
20201015::215719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215720_wf.raa
20201015::215729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215730_wf.raa
20201015::215730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 55726
20201015::215730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215740_wf.raa
20201015::215749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215750_wf.raa
20201015::215759: Head 1: Time Synchronization: 2020.10.15   21:58:00::0015
20201015::215759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215800_wf.raa
20201015::215800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 55781
20201015::215800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215810_wf.raa
20201015::215819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215820_wf.raa
20201015::215829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215830_wf.raa
20201015::215830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 55835
20201015::215830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215840_wf.raa
20201015::215849: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215850_wf.raa
20201015::215859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215900_wf.raa
20201015::215900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 55890
20201015::215900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215910_wf.raa
20201015::215919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215920_wf.raa
20201015::215929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215930_wf.raa
20201015::215930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 55944
20201015::215930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::215939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215940_wf.raa
20201015::215949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_215950_wf.raa
20201015::215959: Head 1: Time Synchronization: 2020.10.15   22:00:00::0014
20201015::215959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220000_wf.raa
20201015::220000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 56000
20201015::220000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220010_wf.raa
20201015::220019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220020_wf.raa
20201015::220029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220030_wf.raa
20201015::220030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 56053
20201015::220030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220040_wf.raa
20201015::220049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220050_wf.raa
20201015::220059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220100_wf.raa
20201015::220100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 56106
20201015::220100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220110_wf.raa
20201015::220119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220120_wf.raa
20201015::220129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220130_wf.raa
20201015::220130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 56163
20201015::220130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220140_wf.raa
20201015::220149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220150_wf.raa
20201015::220159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220200_wf.raa
20201015::220200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 56219
20201015::220200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220210_wf.raa
20201015::220219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220220_wf.raa
20201015::220229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220230_wf.raa
20201015::220230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 56274
20201015::220230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220240_wf.raa
20201015::220249: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220250_wf.raa
20201015::220259: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220300_wf.raa
20201015::220300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220300: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 56330
20201015::220300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220309: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220310_wf.raa
20201015::220319: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220320_wf.raa
20201015::220329: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220330_wf.raa
20201015::220330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220330: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 56385
20201015::220330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220339: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220340_wf.raa
20201015::220349: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220350_wf.raa
20201015::220359: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220400_wf.raa
20201015::220400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220400: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 56440
20201015::220400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220409: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220410_wf.raa
20201015::220419: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220420_wf.raa
20201015::220429: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220430_wf.raa
20201015::220430: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.8dbar, CTD 34.7psu, index 1.35, Packet 56495
20201015::220430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220439: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220440_wf.raa
20201015::220449: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220450_wf.raa
20201015::220459: Head 1: Time Synchronization: 2020.10.15   22:05:00::0014
20201015::220459: Head 2: Time Synchronization: 2020.10.15   22:05:00::0014
20201015::220459: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220500_wf.raa
20201015::220500: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 56550
20201015::220500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220509: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220510_wf.raa
20201015::220519: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220520_wf.raa
20201015::220529: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220530_wf.raa
20201015::220530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220530: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 56606
20201015::220530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220539: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220540_wf.raa
20201015::220549: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220550_wf.raa
20201015::220559: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220600_wf.raa
20201015::220600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220600: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 56662
20201015::220600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220609: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220610_wf.raa
20201015::220619: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220620_wf.raa
20201015::220629: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220630_wf.raa
20201015::220630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220630: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 56717
20201015::220630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220639: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220640_wf.raa
20201015::220649: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220650_wf.raa
20201015::220659: Head 1: Time Synchronization: 2020.10.15   22:07:00::0016
20201015::220659: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220700_wf.raa
20201015::220700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220700: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 56772
20201015::220700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220709: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220710_wf.raa
20201015::220719: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220720_wf.raa
20201015::220729: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220730_wf.raa
20201015::220730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220730: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 56827
20201015::220730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220739: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220740_wf.raa
20201015::220749: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220750_wf.raa
20201015::220759: Head 1: Time Synchronization: 2020.10.15   22:08:00::0014
20201015::220759: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220800_wf.raa
20201015::220800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220800: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.4dbar, CTD 34.7psu, index 1.35, Packet 56883
20201015::220800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220809: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220810_wf.raa
20201015::220819: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220820_wf.raa
20201015::220829: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220830_wf.raa
20201015::220830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220830: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 56940
20201015::220830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220839: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220840_wf.raa
20201015::220850: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220850_wf.raa
20201015::220859: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220900_wf.raa
20201015::220900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220900: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 56995
20201015::220900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220909: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220910_wf.raa
20201015::220919: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220920_wf.raa
20201015::220929: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220930_wf.raa
20201015::220930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220930: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 57051
20201015::220930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::220939: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220940_wf.raa
20201015::220949: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_220950_wf.raa
20201015::220959: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221000_wf.raa
20201015::221000: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 57109
20201015::221000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221009: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221010_wf.raa
20201015::221019: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221020_wf.raa
20201015::221029: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221030_wf.raa
20201015::221030: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 57167
20201015::221030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221039: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221040_wf.raa
20201015::221049: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221050_wf.raa
20201015::221059: Head 1: Time Synchronization: 2020.10.15   22:11:00::0014
20201015::221059: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221100_wf.raa
20201015::221100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221100: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 57224
20201015::221100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221109: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221110_wf.raa
20201015::221119: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221120_wf.raa
20201015::221129: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221130_wf.raa
20201015::221130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221130: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 57278
20201015::221130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221139: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221140_wf.raa
20201015::221149: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221150_wf.raa
20201015::221159: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221200_wf.raa
20201015::221200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221200: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 57332
20201015::221200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221209: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221210_wf.raa
20201015::221219: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221220_wf.raa
20201015::221229: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221230_wf.raa
20201015::221230: System  Initialized, Gain 7, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 57385
20201015::221230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::221239: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_221240_wf.raa
20201015::221259: GUI: Lost Communications with Head 2.
20201015::221259: GUI: Lost Communications with Sensor 1.
20201015::221308: GUI: Attempting Communications with Head 2...
20201015::221310: GUI: Attempting Communications with Head 1...
20201015::221851: GUI: Established Communications with Head 1.
20201015::221852: Head 1: Initializing Communications with GUI ...
20201015::221852: GUI: Established Communications with Head 2.
20201015::221853: Head 1: Communications Established.
20201015::221853: Head 2: Initializing Communications with GUI ...
20201015::221853: Head 2: Communications Established.
20201015::221854: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::221854: Head 1: Connection Established with the GUI.
20201015::221854: Head 1: Initializing Subsystems, standby ...
20201015::221854: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::221855: Head 1: Initializing Hardware, Stand by ...
20201015::221855: Head 2: Connection Established with the GUI.
20201015::221855: Head 2: Initializing Subsystems, standby ...
20201015::221855: Head 2: Initializing Hardware, Stand by ...
20201015::221900: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201015::221900: System NOT Initialized, Gain 0, Elec PB 13.9C, Elec PB 33.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 16
20201015::221900: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201015::221901: Head 2: DAQmx Error: -200324: NI-DAQmx is unable to communicate with the device. Make sure the device is present in and accessible to the system, is not currently being reset, and is not reserved by another driver such as Traditional NI-DAQ (Legacy). 
20201015::221901: Head 2: 
20201015::221906: Head 2: DAQmx Error: -200324: NI-DAQmx is unable to communicate with the device. Make sure the device is present in and accessible to the system, is not currently being reset, and is not reserved by another driver such as Traditional NI-DAQ (Legacy). 
20201015::221906: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201015::221906: Head 2: 
20201015::221906: Head 1: NtQuery - testing 1 ...
20201015::221906: Head 2: DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZIN1  Status Code: -200478
20201015::221906: Head 1: clock resolution: 10
20201015::221907: Head 2: 
20201015::221907: Head 1: NtQuery - testing 2, after setting max res ...
20201015::221907: Head 2: DAQmx Error: -200486: Specified channel is not in the task. Channel Name: DAQ1/ai4  Task Name: Sc_AZIN1  Status Code: -200486
20201015::221907: Head 1: clock resolution: 10
20201015::221907: Head 2: 
20201015::221907: Head 1: Initializing Optics Electronics ...
20201015::221908: Head 2:    Error Initializing DAQ Subsystem
20201015::221908: Head 1: Power Laser Controller
20201015::221911: Head 1: Power Scanner Controller
20201015::221914: Head 1: Power OPTO Sensor
20201015::221916: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201015::221916: Head 2: NtQuery - testing 1 ...
20201015::221917: Head 2: clock resolution: 10
20201015::221917: Head 2: NtQuery - testing 2, after setting max res ...
20201015::221917: Head 2: clock resolution: 10
20201015::221917: Head 2: Initializing Optics Electronics ...
20201015::221918: Head 2: Power Laser Controller
20201015::221922: Head 2: Power Scanner Controller
20201015::221924: Head 2: Power OPTO Sensor
20201015::221930: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::221930: System NOT Initialized, Gain 0, Elec PB 13.9C, Elec PB 33.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 70
20201015::221930: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::221934: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::221934: Head 1: Eye Safe Optical Filter check Passed
20201015::221934: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201015::221935: Head 1: Initializing Time Sync Subsystem.
20201015::221935: Head 1: Initializing CTD Subsystem.
20201015::221935: Head 1: CTD Initialization Successful
20201015::221935: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201015::221936: Head 1: Time Sync UDP started, waiting for sync...
20201015::221936: Head 1: Attempting CTD Ethernet connection with ROV...
20201015::221937: Head 1: Time Synchronization Achieved: 2020.10.15   22:19:38::0015
20201015::221944: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201015::221944: Head 2: Eye Safe Optical Filter check Passed
20201015::221944: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201015::221945: Head 2: Initializing Time Sync Subsystem.
20201015::221945: Head 2: Initializing CTD Subsystem.
20201015::221945: Head 2: CTD Initialization Successful
20201015::221945: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201015::221946: Head 2: Time Sync UDP started, waiting for sync...
20201015::221946: Head 2: Attempting CTD Ethernet connection with ROV...
20201015::221947: Head 2: Time Synchronization Achieved: 2020.10.15   22:19:48::0014
20201015::222000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 10C, OCB 37%, OPB 5C, Laser 11.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222000: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 30.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 123
20201015::222000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 10C, OCB 38%, OPB 7C, Laser 12.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 11C, OCB 34%, OPB 5C, Laser 11.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222030: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 30.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 177
20201015::222030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 11C, OCB 35%, OPB 7C, Laser 13.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222031: Head 2: CTD Ethernet connection established.
20201015::222031: Head 1: CTD Ethernet connection established.
20201015::222100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 12C, OCB 32%, OPB 6C, Laser 11.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222100: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 231
20201015::222100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 12C, OCB 33%, OPB 7C, Laser 13.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 13C, OCB 30%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222130: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 284
20201015::222130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 12C, OCB 31%, OPB 7C, Laser 13.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 13C, OCB 29%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222200: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 28.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 338
20201015::222200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 13C, OCB 30%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 28%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222230: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 28.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 392
20201015::222230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 13C, OCB 29%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 27%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222300: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 27.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 445
20201015::222300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 29%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 27%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222330: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 27.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 499
20201015::222330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 28%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 26%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222400: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 27.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 553
20201015::222400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 28%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 26%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222430: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 27.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 606
20201015::222430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 27%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222500: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 659
20201015::222500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 27%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 6C, Laser 12.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222530: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 713
20201015::222530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 27%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222600: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 767
20201015::222600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 26%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222630: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 820
20201015::222630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 14C, OCB 26%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222700: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 874
20201015::222700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 7C, Laser 14.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222730: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 927
20201015::222730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222800: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 982
20201015::222800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222830: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1037
20201015::222830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222900: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1091
20201015::222900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::222930: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1146
20201015::222930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223000: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 1200
20201015::223000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223030: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 1256
20201015::223030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223059: Head 1: Time Synchronization: 2020.10.15   22:31:00::0016
20201015::223100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223100: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1311
20201015::223100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223130: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1366
20201015::223130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223159: Head 1: Time Synchronization: 2020.10.15   22:32:00::0013
20201015::223200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223200: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 1421
20201015::223200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223230: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1476
20201015::223230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223259: Head 1: Time Synchronization: 2020.10.15   22:33:00::0015
20201015::223300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223300: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1531
20201015::223300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223330: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1586
20201015::223330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223359: Head 1: Time Synchronization: 2020.10.15   22:34:00::0015
20201015::223400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223400: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1641
20201015::223400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 6C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223430: System  Initialized, Gain 1, Elec PB 13.9C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1695
20201015::223430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223459: Head 1: Time Synchronization: 2020.10.15   22:35:00::0015
20201015::223500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 13.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223500: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 1750
20201015::223500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223530: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 1805
20201015::223530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223559: Head 1: Time Synchronization: 2020.10.15   22:36:00::0014
20201015::223600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223600: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 1861
20201015::223600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223630: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 1916
20201015::223630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 15.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223700: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 1970
20201015::223700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223730: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 2025
20201015::223730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223800: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 2080
20201015::223800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223830: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 2135
20201015::223830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223859: Head 2: Time Synchronization: 2020.10.15   22:39:00::0014
20201015::223859: Head 1: Time Synchronization: 2020.10.15   22:39:00::0015
20201015::223900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223900: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.2dbar, CTD 34.7psu, index 1.35, Packet 2190
20201015::223900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223930: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 2244
20201015::223930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::223936: GUI: Live mode ON.
20201015::223936: GUI: Requesing START operation, Head 1
20201015::223936: GUI: Requesing START operation, Head 2
20201015::223937: Head 1: Received request: START
20201015::223937: Head 2: Received request: START
20201015::223937: Head 1: Starting Scan Operation
20201015::223937: Head 2: Starting Scan Operation
20201015::223938: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20201015::223938: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::223938: Head 1: Eye Safe Optical Filter check Passed
20201015::223939: Head 2: Eye Safe Optical Filter check Passed
20201015::223939: Head 2: DAQmxDisableStartTrig AZout, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223939: Head 2: 
20201015::223940: Head 2: DAQmxDisableStartTrig AZIn, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZIN1  Status Code: -200477
20201015::223940: Head 2: 
20201015::223940: Head 2: DAQmxCfgSampClkTiming AZIn, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZIN1  Status Code: -200477
20201015::223941: Head 2: 
20201015::223941: Head 2: DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZIN1  Status Code: -200478
20201015::223941: Head 2: 
20201015::223942: Head 2: DAQmxReadAnalogF64 AZIn, DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZIN1  Status Code: -200478
20201015::223942: Head 2: 
20201015::223942: Head 2: DAQmxCfgSampClkTiming AZout, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223942: Head 2: 
20201015::223943: Head 2: DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223943: Head 1: Configured for WATER Processing
20201015::223943: Head 2: 
20201015::223943: Head 1: Configured for WATER Processing
20201015::223943: Head 2: Configured for WATER Processing
20201015::223943: Head 1: Configured for WATER Processing
20201015::223944: Head 2: Configured for WATER Processing
20201015::223944: Head 1: Configured for WATER Processing
20201015::223944: Head 2: Configured for WATER Processing
20201015::223944: Head 1: Configured for WATER Processing
20201015::223944: Head 2: Configured for WATER Processing
20201015::223944: Head 1: Configured for WATER Processing
20201015::223945: Head 2: Configured for WATER Processing
20201015::223945: Head 1: Configured for WATER Processing
20201015::223945: Head 2: Configured for WATER Processing
20201015::223945: Head 1: Configured for WATER Processing
20201015::223945: Head 2: Configured for WATER Processing
20201015::223945: Head 1: Configured for WATER Processing
20201015::223945: Head 2: Configured for WATER Processing
20201015::223946: Head 1: Configured for WATER Processing
20201015::223946: Head 2: Configured for WATER Processing
20201015::223946: Head 1: Configured for WATER Processing
20201015::223946: Head 2: Configured for WATER Processing
20201015::223946: Head 1: Configured for WATER Processing
20201015::223946: Head 2: Configured for WATER Processing
20201015::223946: Head 1: Configured for WATER Processing
20201015::223946: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_223945_wf.raa
20201015::223947: Head 2: Configured for WATER Processing
20201015::223947: Head 1: Configured for WATER Processing
20201015::223947: Head 2: Configured for WATER Processing
20201015::223947: Head 1: Configured for WATER Processing
20201015::223947: Head 2: Configured for WATER Processing
20201015::223947: Head 1: Configured for WATER Processing
20201015::223948: Head 2: Configured for WATER Processing
20201015::223948: Head 1: Configured for WATER Processing
20201015::223948: Head 2: Configured for WATER Processing
20201015::223948: Head 1: Configured for WATER Processing
20201015::223948: Head 2: Configured for WATER Processing
20201015::223948: Head 1: Configured for WATER Processing
20201015::223948: Head 2: Configured for WATER Processing
20201015::223949: Head 1: Configured for WATER Processing
20201015::223949: Head 2: Configured for WATER Processing
20201015::223949: Head 2: Configured for WATER Processing
20201015::223949: Head 2: InitScan, DAQmxCfgSampClkTiming out, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223950: Head 2: 
20201015::223950: Head 2: InitScan, DAQmxCfgDigEdgeStartTrig out, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223950: Head 2: 
20201015::223951: Head 2: DAQmxWriteAnalogF64, DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZOut1  Status Code: -200477
20201015::223951: Head 2: 
20201015::223951: Head 2: ArmScan, DAQmxTaskControl AZOut start, DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZOut1  Status Code: -200478
20201015::223952: Head 2: 
20201015::223952: Head 2: InitScan, DAQmxCfgSampClkTiming In , DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZIN1  Status Code: -200477
20201015::223952: Head 2: 
20201015::223952: Head 2: InitScan, DAQmxCfgDigEdgeStartTrig In , DAQmx Error: -200477: Specified operation cannot be performed when there are no devices in the task. Task Name: Sc_AZIN1  Status Code: -200477
20201015::223953: Head 2: 
20201015::223953: Head 2: ArmScan, DAQmxTaskControl AZIn start, DAQmx Error: -200478: Specified operation cannot be performed when there are no channels in the task. Task Name: Sc_AZIN1  Status Code: -200478
20201015::223953: Head 2: 
20201015::223954: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_223955_wf.raa
20201015::223957: GUI: Live mode ON.
20201015::223957: GUI: Requesing STOP operation, Head 2
20201015::223957: GUI: Requesing STOP operation, Head 1
20201015::223957: Head 2: Received request: STOP
20201015::223957: Head 1: Received request: STOP
20201015::223957: Head 2: Stopping Scan Operation
20201015::223957: Head 1: Stopping Scan Operation
20201015::223959: Head 2: ProcessingMgr stopped all worker threads.
20201015::224000: Head 2:       Stop finished, may now recover.
20201015::224000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 0
20201015::224000: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 2300
20201015::224000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 2, laser state 0
20201015::224001: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::224002: Head 2: Eye Safe Optical Filter check Passed
20201015::224005: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::224005: Head 1: Eye Safe Optical Filter check Passed
20201015::224030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224030: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 2355
20201015::224030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224035: Head 1: ProcessingMgr stopped all worker threads.
20201015::224035: Head 1:       Stop finished, may now recover.
20201015::224036: Head 2: Wide Swath Embedded Image is Shutting Down ...
20201015::224037: GUI: ERROR: Received Invalid Packet ID: 0
20201015::224037: GUI: Lost Communications with Head 2.
20201015::224037: GUI: Attempting Communications with Head 2...
20201015::224038: GUI: Established Communications with Head 2.
20201015::224038: GUI: Requesing STOP operation, Head 1
20201015::224038: Head 1: Received request: STOP
20201015::224038: GUI: Requesing STOP operation, Head 2
20201015::224039: Head 2: Initializing Communications with GUI ...
20201015::224039: Head 2: Communications Established.
20201015::224040: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::224040: Head 2: Connection Established with the GUI.
20201015::224041: Head 2: Initializing Subsystems, standby ...
20201015::224041: Head 2: Initializing Hardware, Stand by ...
20201015::224042: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20201015::224042: Head 2: NtQuery - testing 1 ...
20201015::224042: Head 2: clock resolution: 1
20201015::224043: Head 2: NtQuery - testing 2, after setting max res ...
20201015::224043: Head 2: clock resolution: 1
20201015::224043: Head 2: Initializing Optics Electronics ...
20201015::224044: Head 2: Power Laser Controller
20201015::224047: Head 2: Power Scanner Controller
20201015::224049: Head 2: Power OPTO Sensor
20201015::224100: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224100: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 2410
20201015::224100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224108: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::224108: Head 2: Eye Safe Optical Filter check Passed
20201015::224109: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201015::224109: Head 2: Initializing Time Sync Subsystem.
20201015::224109: Head 2: Initializing CTD Subsystem.
20201015::224110: Head 2: CTD Initialization Successful
20201015::224110: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201015::224110: Head 2: Time Sync UDP started, waiting for sync...
20201015::224110: Head 2: Attempting CTD Ethernet connection with ROV...
20201015::224111: Head 1: Wide Swath Embedded Image is Shutting Down ...
20201015::224111: Head 2: Time Synchronization Achieved: 2020.10.15   22:41:12::0021
20201015::224112: GUI: ERROR: Received Invalid Packet ID: 0
20201015::224113: GUI: Lost Communications with Sensor 1.
20201015::224113: GUI: Requesing STOP operation, Head 2
20201015::224113: Head 2: Received request: STOP
20201015::224113: GUI: Attempting Communications with Head 1...
20201015::224114: GUI: Established Communications with Head 1.
20201015::224114: Head 1: Initializing Communications with GUI ...
20201015::224115: Head 1: Communications Established.
20201015::224116: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201015::224117: Head 1: Connection Established with the GUI.
20201015::224117: Head 1: Initializing Subsystems, standby ...
20201015::224117: Head 1: Initializing Hardware, Stand by ...
20201015::224118: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 10000
20201015::224118: Head 1: NtQuery - testing 1 ...
20201015::224119: Head 1: clock resolution: 1
20201015::224119: Head 1: NtQuery - testing 2, after setting max res ...
20201015::224119: Head 1: clock resolution: 1
20201015::224120: Head 1: Initializing Optics Electronics ...
20201015::224120: Head 1: Power Laser Controller
20201015::224124: Head 1: Power Scanner Controller
20201015::224126: Head 1: Power OPTO Sensor
20201015::224130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224130: System NOT Initialized, Gain 0, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 30
20201015::224130: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224145: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20201015::224145: Head 1: Eye Safe Optical Filter check Passed
20201015::224145: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201015::224145: Head 1: Initializing Time Sync Subsystem.
20201015::224146: Head 1: Initializing CTD Subsystem.
20201015::224146: Head 1: CTD Initialization Successful
20201015::224146: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201015::224147: Head 1: Time Sync UDP started, waiting for sync...
20201015::224147: Head 1: Attempting CTD Ethernet connection with ROV...
20201015::224148: Head 1: Time Synchronization Achieved: 2020.10.15   22:41:49::0014
20201015::224200: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 84
20201015::224200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 0
20201015::224204: Head 2: CTD Ethernet connection established.
20201015::224204: Head 1: CTD Ethernet connection established.
20201015::224208: GUI: Live mode ON.
20201015::224208: GUI: Requesing START operation, Head 2
20201015::224208: GUI: Requesing START operation, Head 1
20201015::224208: Head 2: Received request: START
20201015::224208: Head 1: Received request: START
20201015::224209: Head 2: Starting Scan Operation
20201015::224209: Head 1: Starting Scan Operation
20201015::224210: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20201015::224210: Head 1: Eye Safe Optical Filter check Passed
20201015::224211: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201015::224211: Head 2: Eye Safe Optical Filter check Passed
20201015::224216: Head 2: Configured for WATER Processing
20201015::224216: Head 2: Configured for WATER Processing
20201015::224216: Head 2: Configured for WATER Processing
20201015::224216: Head 2: Configured for WATER Processing
20201015::224217: Head 2: Configured for WATER Processing
20201015::224217: Head 2: Configured for WATER Processing
20201015::224217: Head 2: Configured for WATER Processing
20201015::224218: Head 2: Configured for WATER Processing
20201015::224218: Head 2: Configured for WATER Processing
20201015::224218: Head 2: Configured for WATER Processing
20201015::224219: Head 2: Configured for WATER Processing
20201015::224219: Head 2: Configured for WATER Processing
20201015::224219: Head 2: Configured for WATER Processing
20201015::224219: Head 2: Configured for WATER Processing
20201015::224220: Head 2: Configured for WATER Processing
20201015::224220: Head 2: Configured for WATER Processing
20201015::224220: Head 2: Configured for WATER Processing
20201015::224221: Head 2: Configured for WATER Processing
20201015::224221: Head 2: Configured for WATER Processing
20201015::224221: Head 2: Configured for WATER Processing
20201015::224230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 14.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224230: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 139
20201015::224230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 16.0C, Dig 20.0C, Scan Az fault 0, gain 0, laser state 1
20201015::224242: Head 1: Configured for WATER Processing
20201015::224242: Head 1: Configured for WATER Processing
20201015::224242: Head 1: Configured for WATER Processing
20201015::224243: Head 1: Configured for WATER Processing
20201015::224243: Head 1: Configured for WATER Processing
20201015::224243: Head 1: Configured for WATER Processing
20201015::224244: Head 1: Configured for WATER Processing
20201015::224244: Head 1: Configured for WATER Processing
20201015::224244: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224242_wf.raa
20201015::224244: Head 1: Configured for WATER Processing
20201015::224244: Head 1: Configured for WATER Processing
20201015::224245: Head 1: Configured for WATER Processing
20201015::224245: Head 1: Configured for WATER Processing
20201015::224246: Head 1: Configured for WATER Processing
20201015::224246: Head 1: Configured for WATER Processing
20201015::224246: Head 1: Configured for WATER Processing
20201015::224247: Head 1: Configured for WATER Processing
20201015::224247: Head 1: Configured for WATER Processing
20201015::224248: Head 1: Configured for WATER Processing
20201015::224248: Head 1: Configured for WATER Processing
20201015::224249: Head 1: Configured for WATER Processing
20201015::224251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224252_wf.raa
20201015::224300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 194
20201015::224300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 20.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224302_wf.raa
20201015::224311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224312_wf.raa
20201015::224321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224322_wf.raa
20201015::224330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 248
20201015::224330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 17.0C, Dig 21.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 15.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224332_wf.raa
20201015::224341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224342_wf.raa
20201015::224351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224352_wf.raa
20201015::224400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 303
20201015::224400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 16.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224402_wf.raa
20201015::224411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224412_wf.raa
20201015::224421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224422_wf.raa
20201015::224430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 358
20201015::224430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 16.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224432: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224432_wf.raa
20201015::224441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224442_wf.raa
20201015::224451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224452_wf.raa
20201015::224500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 412
20201015::224500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 16.0C, Dig 27.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224502_wf.raa
20201015::224511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224512_wf.raa
20201015::224521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224522_wf.raa
20201015::224530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 467
20201015::224530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224532_wf.raa
20201015::224541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224542_wf.raa
20201015::224551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224552_wf.raa
20201015::224600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 521
20201015::224600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224602_wf.raa
20201015::224611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224612_wf.raa
20201015::224621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224622_wf.raa
20201015::224630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 576
20201015::224630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224632_wf.raa
20201015::224641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224642_wf.raa
20201015::224651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224652_wf.raa
20201015::224659: Head 1: Time Synchronization: 2020.10.15   22:47:00::0016
20201015::224700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 631
20201015::224700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224702_wf.raa
20201015::224711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224712_wf.raa
20201015::224721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224722_wf.raa
20201015::224730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 686
20201015::224730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224732_wf.raa
20201015::224741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224742_wf.raa
20201015::224751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224752_wf.raa
20201015::224759: Head 1: Time Synchronization: 2020.10.15   22:48:00::0014
20201015::224800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 741
20201015::224800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224802_wf.raa
20201015::224811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224812_wf.raa
20201015::224821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224822_wf.raa
20201015::224830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 796
20201015::224830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224832_wf.raa
20201015::224841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224842_wf.raa
20201015::224851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224852_wf.raa
20201015::224859: Head 1: Time Synchronization: 2020.10.15   22:49:00::0014
20201015::224900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 24%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 851
20201015::224900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 23.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224902_wf.raa
20201015::224911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224912_wf.raa
20201015::224921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224922_wf.raa
20201015::224930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 906
20201015::224930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::224931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224932_wf.raa
20201015::224941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224942_wf.raa
20201015::224951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_224952_wf.raa
20201015::224959: Head 1: Time Synchronization: 2020.10.15   22:50:00::0014
20201015::225000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 17.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 960
20201015::225000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225002_wf.raa
20201015::225011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225012_wf.raa
20201015::225021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225022_wf.raa
20201015::225030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 1014
20201015::225030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225032_wf.raa
20201015::225041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225042_wf.raa
20201015::225051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225052_wf.raa
20201015::225059: Head 1: Time Synchronization: 2020.10.15   22:51:00::0013
20201015::225100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 1069
20201015::225100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 8C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225102_wf.raa
20201015::225111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225112_wf.raa
20201015::225121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225122_wf.raa
20201015::225130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 17.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 1123
20201015::225130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 19.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225132_wf.raa
20201015::225141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225142_wf.raa
20201015::225151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225152_wf.raa
20201015::225200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 1178
20201015::225200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225202_wf.raa
20201015::225211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225212_wf.raa
20201015::225221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225222_wf.raa
20201015::225230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 1232
20201015::225230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225232_wf.raa
20201015::225241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225242_wf.raa
20201015::225251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225252_wf.raa
20201015::225300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 1286
20201015::225300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225302_wf.raa
20201015::225311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225312_wf.raa
20201015::225321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225322_wf.raa
20201015::225330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 1341
20201015::225330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225332_wf.raa
20201015::225341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225342_wf.raa
20201015::225351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225352_wf.raa
20201015::225400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 1396
20201015::225400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225402_wf.raa
20201015::225411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225412_wf.raa
20201015::225421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225422_wf.raa
20201015::225430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.4dbar, CTD 34.7psu, index 1.35, Packet 1451
20201015::225430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225432_wf.raa
20201015::225441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225442_wf.raa
20201015::225451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225452_wf.raa
20201015::225459: Head 1: Time Synchronization: 2020.10.15   22:55:00::0014
20201015::225500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 1506
20201015::225500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225502_wf.raa
20201015::225511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225512_wf.raa
20201015::225521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225522_wf.raa
20201015::225530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.3dbar, CTD 34.7psu, index 1.35, Packet 1560
20201015::225530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225532_wf.raa
20201015::225541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225542_wf.raa
20201015::225551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225552_wf.raa
20201015::225559: Head 2: Time Synchronization: 2020.10.15   22:56:00::0021
20201015::225600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 1614
20201015::225600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225602_wf.raa
20201015::225611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225612_wf.raa
20201015::225621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225622_wf.raa
20201015::225630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.4dbar, CTD 34.7psu, index 1.35, Packet 1669
20201015::225630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225632_wf.raa
20201015::225641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225642_wf.raa
20201015::225651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225652_wf.raa
20201015::225659: Head 1: Time Synchronization: 2020.10.15   22:57:00::0014
20201015::225700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.8dbar, CTD 34.7psu, index 1.35, Packet 1724
20201015::225700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225702_wf.raa
20201015::225711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225712_wf.raa
20201015::225721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225722_wf.raa
20201015::225730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 7C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 1779
20201015::225730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225732_wf.raa
20201015::225741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225742_wf.raa
20201015::225751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225752_wf.raa
20201015::225800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.7dbar, CTD 34.7psu, index 1.35, Packet 1833
20201015::225800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225802_wf.raa
20201015::225811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225812_wf.raa
20201015::225821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225822_wf.raa
20201015::225830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 1888
20201015::225830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225832_wf.raa
20201015::225841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225842_wf.raa
20201015::225851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225852_wf.raa
20201015::225900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 1942
20201015::225900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225902_wf.raa
20201015::225911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225912_wf.raa
20201015::225921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225922_wf.raa
20201015::225930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 1997
20201015::225930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::225931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225932_wf.raa
20201015::225941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225942_wf.raa
20201015::225951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_225952_wf.raa
20201015::230000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 2052
20201015::230000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230002_wf.raa
20201015::230011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230012_wf.raa
20201015::230021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230022_wf.raa
20201015::230030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 2107
20201015::230030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230032_wf.raa
20201015::230041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230042_wf.raa
20201015::230051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230052_wf.raa
20201015::230100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 2161
20201015::230100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 20.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230102_wf.raa
20201015::230111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230112_wf.raa
20201015::230121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230122_wf.raa
20201015::230130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 2216
20201015::230130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230132_wf.raa
20201015::230141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230142_wf.raa
20201015::230151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230152_wf.raa
20201015::230200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 2271
20201015::230200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230202_wf.raa
20201015::230211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230212_wf.raa
20201015::230221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230222_wf.raa
20201015::230230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 2326
20201015::230230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230232_wf.raa
20201015::230241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230242_wf.raa
20201015::230251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230252_wf.raa
20201015::230259: Head 1: Time Synchronization: 2020.10.15   23:03:00::0014
20201015::230300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 2381
20201015::230300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230302_wf.raa
20201015::230311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230312_wf.raa
20201015::230321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230322_wf.raa
20201015::230330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 2435
20201015::230330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230332_wf.raa
20201015::230341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230342_wf.raa
20201015::230351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230352_wf.raa
20201015::230400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 2490
20201015::230400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 18.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230402_wf.raa
20201015::230411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230412_wf.raa
20201015::230421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230422_wf.raa
20201015::230430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 2545
20201015::230430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230432_wf.raa
20201015::230441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230442_wf.raa
20201015::230451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230452_wf.raa
20201015::230500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 2599
20201015::230500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230502_wf.raa
20201015::230511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230512_wf.raa
20201015::230521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230522_wf.raa
20201015::230530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.5dbar, CTD 34.7psu, index 1.35, Packet 2654
20201015::230530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230532_wf.raa
20201015::230541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230542_wf.raa
20201015::230551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230552_wf.raa
20201015::230600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 2709
20201015::230600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 15C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230602_wf.raa
20201015::230611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230612_wf.raa
20201015::230621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230622_wf.raa
20201015::230630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 2764
20201015::230630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230632_wf.raa
20201015::230641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230642_wf.raa
20201015::230651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230652_wf.raa
20201015::230700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 2818
20201015::230700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230702_wf.raa
20201015::230711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230712_wf.raa
20201015::230721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230722_wf.raa
20201015::230730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 2873
20201015::230730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230732_wf.raa
20201015::230741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230742_wf.raa
20201015::230751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230752_wf.raa
20201015::230759: Head 1: Time Synchronization: 2020.10.15   23:08:00::0014
20201015::230800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 2928
20201015::230800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230802_wf.raa
20201015::230811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230812_wf.raa
20201015::230821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230822_wf.raa
20201015::230830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 2983
20201015::230830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230832_wf.raa
20201015::230841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230842_wf.raa
20201015::230851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230852_wf.raa
20201015::230859: Head 1: Time Synchronization: 2020.10.15   23:09:00::0015
20201015::230900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 3037
20201015::230900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230902_wf.raa
20201015::230911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230912_wf.raa
20201015::230921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230922_wf.raa
20201015::230930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 3091
20201015::230930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::230931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230932_wf.raa
20201015::230941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230942_wf.raa
20201015::230951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_230952_wf.raa
20201015::231000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 3146
20201015::231000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231002_wf.raa
20201015::231011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231012_wf.raa
20201015::231021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231022_wf.raa
20201015::231030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 3201
20201015::231030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231032_wf.raa
20201015::231041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231042_wf.raa
20201015::231051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231052_wf.raa
20201015::231100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 3256
20201015::231100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231102_wf.raa
20201015::231111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231112_wf.raa
20201015::231121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231122_wf.raa
20201015::231130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 3311
20201015::231130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231132_wf.raa
20201015::231141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231142_wf.raa
20201015::231151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231152_wf.raa
20201015::231200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 3365
20201015::231200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231202_wf.raa
20201015::231211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231212_wf.raa
20201015::231221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231222_wf.raa
20201015::231230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 3420
20201015::231230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231232_wf.raa
20201015::231241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231242_wf.raa
20201015::231251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231252_wf.raa
20201015::231300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 3475
20201015::231300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231302_wf.raa
20201015::231311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231312_wf.raa
20201015::231321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231322_wf.raa
20201015::231330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 3529
20201015::231330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231332_wf.raa
20201015::231341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231342_wf.raa
20201015::231351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231352_wf.raa
20201015::231400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 3584
20201015::231400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231402_wf.raa
20201015::231411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231412_wf.raa
20201015::231421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231422_wf.raa
20201015::231430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 3639
20201015::231430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231432_wf.raa
20201015::231441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231442_wf.raa
20201015::231451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231452_wf.raa
20201015::231459: Head 1: Time Synchronization: 2020.10.15   23:15:00::0016
20201015::231500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 3694
20201015::231500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231502_wf.raa
20201015::231511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231512_wf.raa
20201015::231521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231522_wf.raa
20201015::231530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 3748
20201015::231530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231532_wf.raa
20201015::231541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231542_wf.raa
20201015::231551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231552_wf.raa
20201015::231600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 3803
20201015::231600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231602_wf.raa
20201015::231611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231612_wf.raa
20201015::231621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231622_wf.raa
20201015::231630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.6dbar, CTD 34.7psu, index 1.35, Packet 3857
20201015::231630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231632_wf.raa
20201015::231641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231642_wf.raa
20201015::231651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231652_wf.raa
20201015::231659: Head 1: Time Synchronization: 2020.10.15   23:17:00::0015
20201015::231700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.5dbar, CTD 34.7psu, index 1.35, Packet 3912
20201015::231700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231702_wf.raa
20201015::231711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231712_wf.raa
20201015::231721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231722_wf.raa
20201015::231730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.9dbar, CTD 34.7psu, index 1.35, Packet 3967
20201015::231730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231732_wf.raa
20201015::231741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231742_wf.raa
20201015::231751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231752_wf.raa
20201015::231800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.3dbar, CTD 34.7psu, index 1.35, Packet 4021
20201015::231800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231802_wf.raa
20201015::231811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231812_wf.raa
20201015::231821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231822_wf.raa
20201015::231830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.8dbar, CTD 34.7psu, index 1.35, Packet 4076
20201015::231830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231832_wf.raa
20201015::231841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231842_wf.raa
20201015::231851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231852_wf.raa
20201015::231859: Head 1: Time Synchronization: 2020.10.15   23:19:00::0016
20201015::231900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 4131
20201015::231900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231902_wf.raa
20201015::231911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231912_wf.raa
20201015::231921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231922_wf.raa
20201015::231930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 4185
20201015::231930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::231931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231932_wf.raa
20201015::231941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231942_wf.raa
20201015::231951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_231952_wf.raa
20201015::232000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 4240
20201015::232000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232002_wf.raa
20201015::232011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232012_wf.raa
20201015::232021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232022_wf.raa
20201015::232030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 4295
20201015::232030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232032_wf.raa
20201015::232041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232042_wf.raa
20201015::232051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232052_wf.raa
20201015::232059: Head 1: Time Synchronization: 2020.10.15   23:21:00::0017
20201015::232100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 4350
20201015::232100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232102_wf.raa
20201015::232111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232112_wf.raa
20201015::232121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232122_wf.raa
20201015::232130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 4405
20201015::232130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232132_wf.raa
20201015::232141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232142_wf.raa
20201015::232151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232152_wf.raa
20201015::232159: Head 1: Time Synchronization: 2020.10.15   23:22:00::0015
20201015::232159: Head 2: Time Synchronization: 2020.10.15   23:22:00::0015
20201015::232200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 4459
20201015::232200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232202_wf.raa
20201015::232211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232212_wf.raa
20201015::232221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232222_wf.raa
20201015::232230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.6dbar, CTD 34.7psu, index 1.35, Packet 4514
20201015::232230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232232_wf.raa
20201015::232241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232242_wf.raa
20201015::232251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232252_wf.raa
20201015::232259: Head 1: Time Synchronization: 2020.10.15   23:23:00::0015
20201015::232300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 4569
20201015::232300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232302_wf.raa
20201015::232311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232312_wf.raa
20201015::232321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232322_wf.raa
20201015::232330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 4624
20201015::232330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232332_wf.raa
20201015::232341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232342_wf.raa
20201015::232351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232352_wf.raa
20201015::232359: Head 1: Time Synchronization: 2020.10.15   23:24:00::0015
20201015::232400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 4679
20201015::232400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232402_wf.raa
20201015::232411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232412_wf.raa
20201015::232421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232422_wf.raa
20201015::232430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 4734
20201015::232430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232432_wf.raa
20201015::232441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232442_wf.raa
20201015::232451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232452_wf.raa
20201015::232500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 4789
20201015::232500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232502_wf.raa
20201015::232511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232512_wf.raa
20201015::232521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232522_wf.raa
20201015::232530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 4844
20201015::232530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232532_wf.raa
20201015::232541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232542_wf.raa
20201015::232551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232552_wf.raa
20201015::232559: Head 1: Time Synchronization: 2020.10.15   23:26:00::0015
20201015::232600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 4899
20201015::232600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232602_wf.raa
20201015::232611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232612_wf.raa
20201015::232621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232622_wf.raa
20201015::232630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 4954
20201015::232630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232632_wf.raa
20201015::232641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232642_wf.raa
20201015::232651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232652_wf.raa
20201015::232659: Head 1: Time Synchronization: 2020.10.15   23:27:00::0013
20201015::232700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 5009
20201015::232700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232702_wf.raa
20201015::232711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232712_wf.raa
20201015::232721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232722_wf.raa
20201015::232730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 5064
20201015::232730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232732_wf.raa
20201015::232741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232742_wf.raa
20201015::232751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232752_wf.raa
20201015::232800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 5119
20201015::232800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232802_wf.raa
20201015::232811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232812_wf.raa
20201015::232821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232822_wf.raa
20201015::232830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 5173
20201015::232830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232832_wf.raa
20201015::232841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232842_wf.raa
20201015::232851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232852_wf.raa
20201015::232900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.1dbar, CTD 34.7psu, index 1.35, Packet 5228
20201015::232900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232902_wf.raa
20201015::232911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232912_wf.raa
20201015::232921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232922_wf.raa
20201015::232930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.3dbar, CTD 34.7psu, index 1.35, Packet 5282
20201015::232930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::232931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232932_wf.raa
20201015::232941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232942_wf.raa
20201015::232951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_232952_wf.raa
20201015::232959: Head 2: Time Synchronization: 2020.10.15   23:30:00::0016
20201015::232959: Head 1: Time Synchronization: 2020.10.15   23:30:00::0016
20201015::233000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 5337
20201015::233000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233002_wf.raa
20201015::233011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233012_wf.raa
20201015::233021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233022_wf.raa
20201015::233030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 5392
20201015::233030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233032_wf.raa
20201015::233041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233042_wf.raa
20201015::233051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233052_wf.raa
20201015::233100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 5447
20201015::233100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233102_wf.raa
20201015::233111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233112_wf.raa
20201015::233121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233122_wf.raa
20201015::233130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 5501
20201015::233130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233132_wf.raa
20201015::233141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233142_wf.raa
20201015::233151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233152_wf.raa
20201015::233200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 5556
20201015::233200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233202_wf.raa
20201015::233211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233212_wf.raa
20201015::233221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233222_wf.raa
20201015::233230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.0dbar, CTD 34.7psu, index 1.35, Packet 5610
20201015::233230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233232_wf.raa
20201015::233241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233242_wf.raa
20201015::233251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233252_wf.raa
20201015::233259: Head 1: Time Synchronization: 2020.10.15   23:33:00::0015
20201015::233300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.1dbar, CTD 34.7psu, index 1.35, Packet 5664
20201015::233300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233302_wf.raa
20201015::233311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233312_wf.raa
20201015::233321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233322_wf.raa
20201015::233330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.3dbar, CTD 34.7psu, index 1.35, Packet 5719
20201015::233330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233332_wf.raa
20201015::233341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233342_wf.raa
20201015::233351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233352_wf.raa
20201015::233359: Head 1: Time Synchronization: 2020.10.15   23:34:00::0015
20201015::233400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.5dbar, CTD 34.7psu, index 1.35, Packet 5774
20201015::233400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233402_wf.raa
20201015::233411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233412_wf.raa
20201015::233421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233422_wf.raa
20201015::233430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.0dbar, CTD 34.7psu, index 1.35, Packet 5829
20201015::233430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233432_wf.raa
20201015::233441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233442_wf.raa
20201015::233451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233452_wf.raa
20201015::233500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.5dbar, CTD 34.7psu, index 1.35, Packet 5883
20201015::233500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233502_wf.raa
20201015::233511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233512_wf.raa
20201015::233521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233522_wf.raa
20201015::233530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.0dbar, CTD 34.7psu, index 1.35, Packet 5938
20201015::233530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233532_wf.raa
20201015::233541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233542_wf.raa
20201015::233551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233552_wf.raa
20201015::233600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 5992
20201015::233600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233602_wf.raa
20201015::233611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233612_wf.raa
20201015::233621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233622_wf.raa
20201015::233630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.9dbar, CTD 34.7psu, index 1.35, Packet 6047
20201015::233630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233632_wf.raa
20201015::233641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233642_wf.raa
20201015::233651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233652_wf.raa
20201015::233700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 6102
20201015::233700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233702_wf.raa
20201015::233711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233712_wf.raa
20201015::233721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233722_wf.raa
20201015::233730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.7dbar, CTD 34.7psu, index 1.35, Packet 6157
20201015::233730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233732_wf.raa
20201015::233741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233742_wf.raa
20201015::233751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233752_wf.raa
20201015::233800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2878.2dbar, CTD 34.7psu, index 1.35, Packet 6211
20201015::233800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233802_wf.raa
20201015::233811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233812_wf.raa
20201015::233821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233822_wf.raa
20201015::233830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.7dbar, CTD 34.7psu, index 1.35, Packet 6266
20201015::233830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233832_wf.raa
20201015::233841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233842_wf.raa
20201015::233851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233852_wf.raa
20201015::233859: Head 1: Time Synchronization: 2020.10.15   23:39:00::0015
20201015::233900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2877.1dbar, CTD 34.7psu, index 1.35, Packet 6321
20201015::233900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233902_wf.raa
20201015::233911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233912_wf.raa
20201015::233921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233922_wf.raa
20201015::233930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.6dbar, CTD 34.7psu, index 1.35, Packet 6376
20201015::233930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::233931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233932_wf.raa
20201015::233941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233942_wf.raa
20201015::233951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_233952_wf.raa
20201015::233959: Head 1: Time Synchronization: 2020.10.15   23:40:00::0012
20201015::234000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2876.2dbar, CTD 34.7psu, index 1.35, Packet 6429
20201015::234000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234002_wf.raa
20201015::234011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234012_wf.raa
20201015::234021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234022_wf.raa
20201015::234030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.9dbar, CTD 34.7psu, index 1.35, Packet 6484
20201015::234030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 26%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234032_wf.raa
20201015::234041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234042_wf.raa
20201015::234051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234052_wf.raa
20201015::234100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.7dbar, CTD 34.7psu, index 1.35, Packet 6539
20201015::234100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234102_wf.raa
20201015::234111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234112_wf.raa
20201015::234121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234122_wf.raa
20201015::234130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.4dbar, CTD 34.7psu, index 1.35, Packet 6594
20201015::234130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234132_wf.raa
20201015::234141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234142_wf.raa
20201015::234151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234152_wf.raa
20201015::234200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 6648
20201015::234200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234202_wf.raa
20201015::234211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234212_wf.raa
20201015::234221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234222_wf.raa
20201015::234230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.0dbar, CTD 34.7psu, index 1.35, Packet 6703
20201015::234230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234232_wf.raa
20201015::234241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234242_wf.raa
20201015::234251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234252_wf.raa
20201015::234259: Head 1: Time Synchronization: 2020.10.15   23:43:00::0015
20201015::234300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 6757
20201015::234300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234302_wf.raa
20201015::234311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234312_wf.raa
20201015::234321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234322_wf.raa
20201015::234330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.8dbar, CTD 34.7psu, index 1.35, Packet 6812
20201015::234330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234332_wf.raa
20201015::234341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234342_wf.raa
20201015::234351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234352_wf.raa
20201015::234359: Head 1: Time Synchronization: 2020.10.15   23:44:00::0015
20201015::234400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.7dbar, CTD 34.7psu, index 1.35, Packet 6867
20201015::234400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234402_wf.raa
20201015::234411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234412_wf.raa
20201015::234421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234422_wf.raa
20201015::234430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.4dbar, CTD 34.7psu, index 1.35, Packet 6921
20201015::234430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234432_wf.raa
20201015::234441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234442_wf.raa
20201015::234451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234452_wf.raa
20201015::234459: Head 1: Time Synchronization: 2020.10.15   23:45:00::0016
20201015::234500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.3dbar, CTD 34.7psu, index 1.35, Packet 6976
20201015::234500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234502_wf.raa
20201015::234511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234512_wf.raa
20201015::234521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234522_wf.raa
20201015::234530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.1dbar, CTD 34.7psu, index 1.35, Packet 7030
20201015::234530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234532_wf.raa
20201015::234541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234542_wf.raa
20201015::234551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234552_wf.raa
20201015::234559: Head 1: Time Synchronization: 2020.10.15   23:46:00::0016
20201015::234600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.0dbar, CTD 34.7psu, index 1.35, Packet 7085
20201015::234600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234602_wf.raa
20201015::234611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234612_wf.raa
20201015::234621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234622_wf.raa
20201015::234630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.9dbar, CTD 34.7psu, index 1.35, Packet 7140
20201015::234630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234632_wf.raa
20201015::234641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234642_wf.raa
20201015::234651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234652_wf.raa
20201015::234659: Head 1: Time Synchronization: 2020.10.15   23:47:00::0014
20201015::234700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.8dbar, CTD 34.7psu, index 1.35, Packet 7195
20201015::234700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234702_wf.raa
20201015::234711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234712_wf.raa
20201015::234721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234722_wf.raa
20201015::234730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.6dbar, CTD 34.7psu, index 1.35, Packet 7250
20201015::234730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234732_wf.raa
20201015::234741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234742_wf.raa
20201015::234751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234752_wf.raa
20201015::234759: Head 1: Time Synchronization: 2020.10.15   23:48:00::0015
20201015::234800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.5dbar, CTD 34.7psu, index 1.35, Packet 7304
20201015::234800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234802_wf.raa
20201015::234811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234812_wf.raa
20201015::234821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234822_wf.raa
20201015::234830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.4dbar, CTD 34.7psu, index 1.35, Packet 7359
20201015::234830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234832_wf.raa
20201015::234841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234842_wf.raa
20201015::234851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234852_wf.raa
20201015::234859: Head 1: Time Synchronization: 2020.10.15   23:49:00::0014
20201015::234900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.2dbar, CTD 34.7psu, index 1.35, Packet 7414
20201015::234900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234902_wf.raa
20201015::234911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234912_wf.raa
20201015::234921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234922_wf.raa
20201015::234930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.1dbar, CTD 34.7psu, index 1.35, Packet 7469
20201015::234930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::234931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234932_wf.raa
20201015::234941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234942_wf.raa
20201015::234951: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_234952_wf.raa
20201015::234959: Head 1: Time Synchronization: 2020.10.15   23:50:00::0014
20201015::235000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235000: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.0dbar, CTD 34.7psu, index 1.35, Packet 7523
20201015::235000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235001: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235002_wf.raa
20201015::235011: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235012_wf.raa
20201015::235021: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235022_wf.raa
20201015::235030: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2872.9dbar, CTD 34.7psu, index 1.35, Packet 7578
20201015::235030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235031: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235032_wf.raa
20201015::235041: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235042_wf.raa
20201015::235051: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235052_wf.raa
20201015::235100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235100: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2872.8dbar, CTD 34.7psu, index 1.35, Packet 7633
20201015::235100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235101: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235102_wf.raa
20201015::235111: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235112_wf.raa
20201015::235121: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235122_wf.raa
20201015::235130: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2872.8dbar, CTD 34.7psu, index 1.35, Packet 7687
20201015::235130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235131: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235132_wf.raa
20201015::235141: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235142_wf.raa
20201015::235151: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235152_wf.raa
20201015::235159: Head 1: Time Synchronization: 2020.10.15   23:52:00::0014
20201015::235200: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2872.8dbar, CTD 34.7psu, index 1.35, Packet 7742
20201015::235200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235201: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235202_wf.raa
20201015::235211: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235212_wf.raa
20201015::235221: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235222_wf.raa
20201015::235230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235230: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2872.9dbar, CTD 34.7psu, index 1.35, Packet 7797
20201015::235230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235231: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235232_wf.raa
20201015::235241: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235242_wf.raa
20201015::235251: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235252_wf.raa
20201015::235300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235300: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.0dbar, CTD 34.7psu, index 1.35, Packet 7852
20201015::235300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235301: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235302_wf.raa
20201015::235311: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235312_wf.raa
20201015::235321: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235322_wf.raa
20201015::235330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235330: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.1dbar, CTD 34.7psu, index 1.35, Packet 7907
20201015::235330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235331: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235332_wf.raa
20201015::235341: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235342_wf.raa
20201015::235351: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235352_wf.raa
20201015::235359: Head 1: Time Synchronization: 2020.10.15   23:54:00::0017
20201015::235400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235400: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.2dbar, CTD 34.7psu, index 1.35, Packet 7961
20201015::235400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235401: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235402_wf.raa
20201015::235411: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235412_wf.raa
20201015::235421: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235422_wf.raa
20201015::235430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235430: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.3dbar, CTD 34.7psu, index 1.35, Packet 8017
20201015::235430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235431: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235432_wf.raa
20201015::235441: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235442_wf.raa
20201015::235451: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235452_wf.raa
20201015::235500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235500: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.4dbar, CTD 34.7psu, index 1.35, Packet 8071
20201015::235500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235501: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235502_wf.raa
20201015::235511: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235512_wf.raa
20201015::235521: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235522_wf.raa
20201015::235530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235530: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.6dbar, CTD 34.7psu, index 1.35, Packet 8126
20201015::235530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235531: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235532_wf.raa
20201015::235541: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235542_wf.raa
20201015::235551: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235552_wf.raa
20201015::235559: Head 1: Time Synchronization: 2020.10.15   23:56:00::0014
20201015::235600: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.7dbar, CTD 34.7psu, index 1.35, Packet 8181
20201015::235600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235601: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235602_wf.raa
20201015::235611: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235612_wf.raa
20201015::235621: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235622_wf.raa
20201015::235630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235630: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2873.9dbar, CTD 34.7psu, index 1.35, Packet 8236
20201015::235630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235631: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235632_wf.raa
20201015::235641: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235642_wf.raa
20201015::235651: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235652_wf.raa
20201015::235659: Head 2: Time Synchronization: 2020.10.15   23:57:00::0014
20201015::235659: Head 1: Time Synchronization: 2020.10.15   23:57:00::0014
20201015::235700: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.2dbar, CTD 34.7psu, index 1.35, Packet 8290
20201015::235700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235701: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235702_wf.raa
20201015::235711: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235712_wf.raa
20201015::235721: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235722_wf.raa
20201015::235730: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.6dbar, CTD 34.7psu, index 1.35, Packet 8345
20201015::235730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235731: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235732_wf.raa
20201015::235741: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235742_wf.raa
20201015::235751: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235752_wf.raa
20201015::235759: Head 1: Time Synchronization: 2020.10.15   23:58:00::0016
20201015::235800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235800: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2874.9dbar, CTD 34.7psu, index 1.35, Packet 8400
20201015::235800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235801: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235802_wf.raa
20201015::235811: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235812_wf.raa
20201015::235821: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235822_wf.raa
20201015::235830: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.2dbar, CTD 34.7psu, index 1.35, Packet 8454
20201015::235830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235831: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235832_wf.raa
20201015::235841: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235842_wf.raa
20201015::235851: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235852_wf.raa
20201015::235900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235900: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.5dbar, CTD 34.7psu, index 1.35, Packet 8510
20201015::235900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235901: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235902_wf.raa
20201015::235911: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235912_wf.raa
20201015::235921: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235922_wf.raa
20201015::235930: System  Initialized, Gain 7, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 1.7C, CTD 2875.8dbar, CTD 34.7psu, index 1.35, Packet 8564
20201015::235930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 15C, OCB 27%, OPB 9C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 16C, OCB 25%, OPB 8C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 2, laser state 1
20201015::235931: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235932_wf.raa
20201015::235941: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235942_wf.raa
20201015::235953: GUI: Archiving data to file --> C:\Data\20201014d2\20201015_235952_wf.raa
20201015::235959: Head 1: Time Synchronization: 2020.10.16   00:00:00::0014
