20210901::211635: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210901::211635: GUI: Live mode ON.
20210901::211635: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210901::211635: GUI: WiSSL GUI started at 2021_09_01_21:16:35
20210901::211635: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_09_01.txt
20210901::211635: GUI: Attempting Communications with Head 1...
20210901::211635: GUI: Attempting Communications with Head 2...
20210901::211639: GUI: Established Communications with Head 1.
20210901::211640: Head 1: Initializing Communications with GUI ...
20210901::211640: Head 1: Communications Established.
20210901::211641: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210901::211642: Head 1: Connection Established with the GUI.
20210901::211642: Head 1: Initializing Subsystems, standby ...
20210901::211642: Head 1: Initializing Hardware, Stand by ...
20210901::211645: GUI: Established Communications with Head 2.
20210901::211646: Head 2: Initializing Communications with GUI ...
20210901::211647: Head 2: Communications Established.
20210901::211648: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210901::211648: Head 2: Connection Established with the GUI.
20210901::211648: Head 2: Initializing Subsystems, standby ...
20210901::211649: Head 2: Initializing Hardware, Stand by ...
20210901::211659: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210901::211659: Head 1: NtQuery - testing 1 ...
20210901::211659: Head 1: clock resolution: 10
20210901::211700: Head 1: NtQuery - testing 2, after setting max res ...
20210901::211700: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211700: Head 1: clock resolution: 10
20210901::211700: System NOT Initialized, Gain 0, Elec PB 15.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 43
20210901::211700: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211700: Head 1: Initializing Optics Electronics ...
20210901::211700: Head 1: Power Laser Controller
20210901::211704: Head 1: Power Scanner Controller
20210901::211705: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210901::211705: Head 2: NtQuery - testing 1 ...
20210901::211706: Head 2: clock resolution: 10
20210901::211706: Head 2: NtQuery - testing 2, after setting max res ...
20210901::211706: Head 1: Power OPTO Sensor
20210901::211706: Head 2: clock resolution: 10
20210901::211707: Head 2: Initializing Optics Electronics ...
20210901::211707: Head 2: Power Laser Controller
20210901::211711: Head 2: Power Scanner Controller
20210901::211713: Head 2: Power OPTO Sensor
20210901::211726: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210901::211727: Head 1: Eye Safe Optical Filter check Passed
20210901::211727: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210901::211727: Head 1: Initializing Time Sync Subsystem.
20210901::211728: Head 1: Initializing CTD Subsystem.
20210901::211728: Head 1: CTD Initialization Successful
20210901::211728: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210901::211729: Head 1: Time Sync UDP started, waiting for sync...
20210901::211729: Head 1: Attempting CTD Ethernet connection with ROV...
20210901::211730: Head 1: Time Synchronization Achieved: 2021.09.01   21:17:40::0014
20210901::211730: System  Initialized, Gain 1, Elec PB 15.3C, Elec PB 23.3%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 96
20210901::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 31%, OPB 16C, Laser 0.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211730: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211733: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20210901::211733: Head 2: Eye Safe Optical Filter check Passed
20210901::211734: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210901::211734: Head 2: Initializing Time Sync Subsystem.
20210901::211734: Head 2: Initializing CTD Subsystem.
20210901::211734: Head 2: CTD Initialization Successful
20210901::211735: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210901::211735: Head 2: Time Sync UDP started, waiting for sync...
20210901::211735: Head 2: Attempting CTD Ethernet connection with ROV...
20210901::211736: Head 2: Time Synchronization Achieved: 2021.09.01   21:17:46::0016
20210901::211750: Head 1: Time Synchronization: 2021.09.01   21:18:00::0017
20210901::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 29%, OPB 15C, Laser 14.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211800: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 150
20210901::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 29%, OPB 16C, Laser 15.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211805: Head 1: CTD Ethernet connection established.
20210901::211805: Head 2: CTD Ethernet connection established.
20210901::211830: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.8dbar, CTD -1.$psu, index -1.#J, Packet 203
20210901::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 27%, OPB 16C, Laser 16.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 26%, OPB 15C, Laser 15.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211850: Head 1: Time Synchronization: 2021.09.01   21:19:00::0015
20210901::211900: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.8dbar, CTD -1.$psu, index -1.#J, Packet 256
20210901::211900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 17C, Laser 17.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 25%, OPB 16C, Laser 16.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 24%, OPB 16C, Laser 17.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211930: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.8dbar, CTD -1.$psu, index -1.#J, Packet 310
20210901::211930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 24%, OPB 17C, Laser 17.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::211940: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 219 msec
20210901::211940: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 219 msec
20210901::211943: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 942 msec
20210901::211943: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 942 msec
20210901::211945: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 669 msec
20210901::211945: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 669 msec
20210901::211947: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 398 msec
20210901::211947: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 399 msec
20210901::211949: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 124 msec
20210901::211949: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 124 msec
20210901::211952: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 857 msec
20210901::211952: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 857 msec
20210901::211954: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 579 msec
20210901::211954: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 579 msec
20210901::211956: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 307 msec
20210901::211956: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 307 msec
20210901::212000: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 363
20210901::212000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 17C, Laser 18.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 23%, OPB 16C, Laser 17.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212001: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 760 msec
20210901::212001: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 760 msec
20210901::212003: Head 1: Error: Time Sync, Invalid time from PPS to serial ZDA: 486 msec
20210901::212003: Head 2: Error: Time Sync, Invalid time from PPS to serial ZDA: 486 msec
20210901::212030: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 416
20210901::212030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 17C, Laser 19.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 16C, Laser 18.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 16C, Laser 18.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 470
20210901::212100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 17C, Laser 19.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 523
20210901::212130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 22%, OPB 17C, Laser 19.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 16C, Laser 19.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 1.9dbar, CTD -1.$psu, index -1.#J, Packet 576
20210901::212200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 18C, Laser 20.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 17C, Laser 19.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 630
20210901::212230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 18C, Laser 20.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 19.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212242: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::212242: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::212300: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 683
20210901::212300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 21%, OPB 18C, Laser 20.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 20.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 17C, Laser 20.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212330: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 737
20210901::212330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 21.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212400: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 790
20210901::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 21.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 20.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212430: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 843
20210901::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 21.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212447: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::212447: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 17C, Laser 21.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212500: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 897
20210901::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212530: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 950
20210901::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 18C, Laser 22.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 20%, OPB 18C, Laser 21.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212600: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1003
20210901::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 23.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212630: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1057
20210901::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 23.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212648: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::212648: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::212700: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1110
20210901::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 23.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212730: System  Initialized, Gain 1, Elec PB 23.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1164
20210901::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 23.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212750: Head 1: Time Synchronization: 2021.09.01   21:28:00::0015
20210901::212800: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1217
20210901::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212830: System  Initialized, Gain 1, Elec PB 24.7C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1271
20210901::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 21%, OPB 19C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212849: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::212849: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::212900: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1324
20210901::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 20%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212930: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1377
20210901::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 22.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213000: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1431
20210901::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213030: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1484
20210901::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 24.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213050: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::213050: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 23.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213100: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1538
20210901::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 25.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213130: System  Initialized, Gain 1, Elec PB 26.0C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1591
20210901::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 25.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213200: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1644
20210901::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 25.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213223: GUI: OnBnClickedOk
20210901::213223: GUI: Exiting the WiSSL GUI..
20210901::213223: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20210901::213223: GUI: Wrote configuration data.
20210901::213226: GUI: Reading configuration data from file --> C:\3D\CFG\WiSSL_Gui.cfg
20210901::213226: GUI: Live mode ON.
20210901::213226: GUI: 3D at Depth WiSSL GUI, version 2.02.10
20210901::213226: GUI: WiSSL GUI started at 2021_09_01_21:32:26
20210901::213226: GUI: Logging status to C:\3D\LOG\WiSSL_LOG_2021_09_01.txt
20210901::213226: GUI: Attempting Communications with Head 1...
20210901::213226: GUI: Attempting Communications with Head 2...
20210901::213227: GUI: Established Communications with Head 1.
20210901::213227: GUI: Established Communications with Head 2.
20210901::213228: Head 2: Lost Communications with GUI
20210901::213228: Head 1: Lost Communications with GUI
20210901::213228: Head 1: Initializing Communications with GUI ...
20210901::213228: Head 2: Initializing Communications with GUI ...
20210901::213229: Head 1: Communications Established.
20210901::213229: Head 2: Communications Established.
20210901::213251: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::213251: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::213300: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1744
20210901::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 25.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213330: System  Initialized, Gain 1, Elec PB 26.9C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1797
20210901::213330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 24.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213400: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1851
20210901::213400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 20C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 24.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213430: System  Initialized, Gain 1, Elec PB 28.2C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1904
20210901::213430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213450: Head 2: Time Synchronization: 2021.09.01   21:35:00::0014
20210901::213452: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::213452: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::213500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213500: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 1958
20210901::213500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213530: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2011
20210901::213530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213600: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2064
20210901::213600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 26.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213630: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2118
20210901::213630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213653: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::213653: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::213700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 25.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213700: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2171
20210901::213700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213730: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2224
20210901::213730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213800: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2278
20210901::213800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213830: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2331
20210901::213830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 22%, OPB 21C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213854: Head 1: Warning, CTD not recieved within 2 minutes.
20210901::213854: Head 2: Warning, CTD not recieved within 2 minutes.
20210901::213900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213900: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2385
20210901::213900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 22C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213930: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.3C, CTD 2.0dbar, CTD -1.$psu, index -1.#J, Packet 2439
20210901::213930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 22C, Laser 27.0C, Dig 16.0C, Scan Az fault 0, gain 0, laser state 0
20210901::213930: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210901::213932: GUI: ERROR: Received Invalid Packet ID: 0
20210901::213932: GUI: Lost Communications with Sensor 1.
20210901::213932: GUI: Requesing STOP operation, Head 2
20210901::213932: Head 2: Received request: STOP
20210901::213932: GUI: Attempting Communications with Head 1...
20210901::213936: GUI: Established Communications with Head 1.
20210901::213937: Head 1: Initializing Communications with GUI ...
20210901::213938: Head 1: Communications Established.
20210901::213939: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210901::213939: Head 1: Connection Established with the GUI.
20210901::213940: Head 1: Initializing Subsystems, standby ...
20210901::213940: Head 1: Initializing Hardware, Stand by ...
20210901::213941: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210901::213941: Head 1: NtQuery - testing 1 ...
20210901::213941: Head 1: clock resolution: 10
20210901::213942: Head 1: NtQuery - testing 2, after setting max res ...
20210901::213942: Head 1: clock resolution: 10
20210901::213942: Head 1: Initializing Optics Electronics ...
20210901::213943: Head 1: Power Laser Controller
20210901::213946: Head 1: Power Scanner Controller
20210901::213948: Head 1: Power OPTO Sensor
20210901::214000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214000: System NOT Initialized, Gain 0, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 43
20210901::214000: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214006: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210901::214007: Head 1: Eye Safe Optical Filter State there 10, not there 20, transition 1
20210901::214007: Head 1: Eye Safe Optical Filter check Passed
20210901::214008: GUI: ERROR: Received Invalid Packet ID: 0
20210901::214008: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20210901::214008: Head 1: Initializing Time Sync Subsystem.
20210901::214008: GUI: Lost Communications with Head 2.
20210901::214008: Head 1: Initializing CTD Subsystem.
20210901::214008: GUI: Attempting Communications with Head 2...
20210901::214008: Head 1: CTD Initialization Successful
20210901::214009: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20210901::214009: Head 1: Time Sync UDP started, waiting for sync...
20210901::214009: Head 1: Attempting CTD Ethernet connection with ROV...
20210901::214010: Head 1: Time Synchronization Achieved: 2021.09.01   21:40:20::0015
20210901::214011: GUI: Established Communications with Head 2.
20210901::214012: Head 2: Initializing Communications with GUI ...
20210901::214012: Head 2: Communications Established.
20210901::214013: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20210901::214014: Head 2: Connection Established with the GUI.
20210901::214014: Head 2: Initializing Subsystems, standby ...
20210901::214014: Head 2: Initializing Hardware, Stand by ...
20210901::214015: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20210901::214015: Head 2: NtQuery - testing 1 ...
20210901::214016: Head 2: clock resolution: 10
20210901::214016: Head 2: NtQuery - testing 2, after setting max res ...
20210901::214016: Head 2: clock resolution: 10
20210901::214017: Head 2: Initializing Optics Electronics ...
20210901::214017: Head 2: Power Laser Controller
20210901::214021: Head 2: Power Scanner Controller
20210901::214023: Head 2: Power OPTO Sensor
20210901::214030: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 97
20210901::214030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214030: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214041: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20210901::214042: Head 2: Eye Safe Optical Filter check Passed
20210901::214042: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20210901::214042: Head 2: Initializing Time Sync Subsystem.
20210901::214042: Head 2: Initializing CTD Subsystem.
20210901::214043: Head 2: CTD Initialization Successful
20210901::214043: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20210901::214043: Head 2: Time Sync UDP started, waiting for sync...
20210901::214044: Head 2: Attempting CTD Ethernet connection with ROV...
20210901::214045: Head 2: Time Synchronization Achieved: 2021.09.01   21:40:55::0014
20210901::214100: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 150
20210901::214100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 26.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214130: System  Initialized, Gain 1, Elec PB 29.1C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 204
20210901::214130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214200: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 259
20210901::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214230: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 313
20210901::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214256: Head 2: CTD Ethernet connection established.
20210901::214256: Head 1: CTD Ethernet connection established.
20210901::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214300: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.7C, CTD 2.1dbar, CTD -1.$psu, index -1.#J, Packet 367
20210901::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214320: Head 2: Comm CTD Error, disconnecting
20210901::214320: Head 1: Comm CTD Error, disconnecting
20210901::214321: Head 2: Restarting CTD Ethernet connection ...
20210901::214321: Head 1: Restarting CTD Ethernet connection ...
20210901::214330: System  Initialized, Gain 1, Elec PB 30.3C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.7C, CTD 2.1dbar, CTD -1.$psu, index -1.#J, Packet 420
20210901::214330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 21C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214400: System  Initialized, Gain 1, Elec PB 31.2C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.7C, CTD 2.1dbar, CTD -1.$psu, index -1.#J, Packet 474
20210901::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 23%, OPB 22C, Laser 28.0C, Dig 35.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214409: Head 1: Wide Swath Embedded Image is Shutting Down ...
20210901::214410: GUI: ERROR: Received Invalid Packet ID: 0
20210901::214411: GUI: Lost Communications with Sensor 1.
20210901::214411: GUI: Requesing STOP operation, Head 2
20210901::214411: GUI: Attempting Communications with Head 1...
20210901::214411: Head 2: Received request: STOP
20210901::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 22%, OPB 22C, Laser 27.0C, Dig 41.0C, Scan Az fault 0, gain 0, laser state 0
20210901::214431: Head 2: Wide Swath Embedded Image is Shutting Down ...
20210901::214432: GUI: ERROR: Received Invalid Packet ID: 0
20210901::214432: GUI: Lost Communications with Head 2.
20210901::214433: GUI: Attempting Communications with Head 2...
