20201014::000000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1186.4dbar, CTD 34.5psu, index 1.34, Packet 65540
20201014::000000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000004: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000005_wf.raa
20201014::000014: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000015_wf.raa
20201014::000024: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000025_wf.raa
20201014::000030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.6dbar, CTD 34.5psu, index 1.34, Packet 65594
20201014::000030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000034: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000035_wf.raa
20201014::000044: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000045_wf.raa
20201014::000054: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000055_wf.raa
20201014::000059: Head 1: Time Synchronization: 2020.10.14   00:01:00::0014
20201014::000100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.6dbar, CTD 34.5psu, index 1.34, Packet 65648
20201014::000100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000104: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000105_wf.raa
20201014::000114: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000115_wf.raa
20201014::000124: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000125_wf.raa
20201014::000130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1187.0dbar, CTD 34.5psu, index 1.34, Packet 65703
20201014::000130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000134: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000135_wf.raa
20201014::000144: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000145_wf.raa
20201014::000154: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000155_wf.raa
20201014::000200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1186.4dbar, CTD 34.5psu, index 1.34, Packet 65756
20201014::000200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000204: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000205_wf.raa
20201014::000214: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000215_wf.raa
20201014::000224: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000225_wf.raa
20201014::000230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1185.7dbar, CTD 34.5psu, index 1.34, Packet 65811
20201014::000230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000234: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000235_wf.raa
20201014::000244: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000245_wf.raa
20201014::000254: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000255_wf.raa
20201014::000259: Head 1: Time Synchronization: 2020.10.14   00:03:00::0015
20201014::000259: Head 2: Time Synchronization: 2020.10.14   00:03:00::0015
20201014::000300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.6dbar, CTD 34.5psu, index 1.34, Packet 65865
20201014::000300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000304: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000305_wf.raa
20201014::000314: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000315_wf.raa
20201014::000324: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000325_wf.raa
20201014::000330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1183.5dbar, CTD 34.5psu, index 1.34, Packet 65919
20201014::000330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000334: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000335_wf.raa
20201014::000344: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000345_wf.raa
20201014::000354: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000355_wf.raa
20201014::000359: Head 2: Time Synchronization: 2020.10.14   00:04:00::0014
20201014::000400: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1183.2dbar, CTD 34.5psu, index 1.34, Packet 65974
20201014::000400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000404: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000405_wf.raa
20201014::000414: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000415_wf.raa
20201014::000424: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000425_wf.raa
20201014::000430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000430: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1183.5dbar, CTD 34.5psu, index 1.34, Packet 66029
20201014::000430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000434: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000435_wf.raa
20201014::000444: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000445_wf.raa
20201014::000454: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000455_wf.raa
20201014::000459: Head 2: Time Synchronization: 2020.10.14   00:05:00::0015
20201014::000500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000500: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.7dbar, CTD 34.5psu, index 1.34, Packet 66083
20201014::000500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000504: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000505_wf.raa
20201014::000514: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000515_wf.raa
20201014::000524: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000525_wf.raa
20201014::000530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000530: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1185.9dbar, CTD 34.5psu, index 1.34, Packet 66138
20201014::000530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000534: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000535_wf.raa
20201014::000544: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000545_wf.raa
20201014::000554: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000555_wf.raa
20201014::000600: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.5dbar, CTD 34.5psu, index 1.34, Packet 66192
20201014::000600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000604: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000605_wf.raa
20201014::000614: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000615_wf.raa
20201014::000624: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000625_wf.raa
20201014::000630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000630: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1187.2dbar, CTD 34.5psu, index 1.34, Packet 66247
20201014::000630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000634: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000635_wf.raa
20201014::000644: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000645_wf.raa
20201014::000654: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000655_wf.raa
20201014::000659: Head 1: Time Synchronization: 2020.10.14   00:07:00::0014
20201014::000700: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.4dbar, CTD 34.5psu, index 1.34, Packet 66301
20201014::000700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000704: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000705_wf.raa
20201014::000714: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000715_wf.raa
20201014::000724: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000725_wf.raa
20201014::000730: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1188.4dbar, CTD 34.5psu, index 1.34, Packet 66355
20201014::000730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000734: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000735_wf.raa
20201014::000744: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000745_wf.raa
20201014::000754: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000755_wf.raa
20201014::000759: Head 2: Time Synchronization: 2020.10.14   00:08:00::0014
20201014::000759: Head 1: Time Synchronization: 2020.10.14   00:08:00::0015
20201014::000800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000800: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.6dbar, CTD 34.5psu, index 1.34, Packet 66411
20201014::000800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000804: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000805_wf.raa
20201014::000815: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000815_wf.raa
20201014::000826: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000826_wf.raa
20201014::000830: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.1dbar, CTD 34.5psu, index 1.34, Packet 66465
20201014::000830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000836: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000836_wf.raa
20201014::000845: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000846_wf.raa
20201014::000855: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000856_wf.raa
20201014::000859: Head 1: Time Synchronization: 2020.10.14   00:09:00::0014
20201014::000900: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.4dbar, CTD 34.5psu, index 1.34, Packet 66519
20201014::000900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000905: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000906_wf.raa
20201014::000915: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000916_wf.raa
20201014::000925: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000926_wf.raa
20201014::000930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000930: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.8dbar, CTD 34.5psu, index 1.34, Packet 66574
20201014::000930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::000935: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000936_wf.raa
20201014::000945: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000946_wf.raa
20201014::000955: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_000956_wf.raa
20201014::000959: Head 1: Time Synchronization: 2020.10.14   00:10:00::0015
20201014::001000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.0dbar, CTD 34.5psu, index 1.34, Packet 66628
20201014::001000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001005: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001006_wf.raa
20201014::001015: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001016_wf.raa
20201014::001025: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001026_wf.raa
20201014::001030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.7dbar, CTD 34.5psu, index 1.34, Packet 66682
20201014::001030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001035: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001036_wf.raa
20201014::001045: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001046_wf.raa
20201014::001055: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001056_wf.raa
20201014::001059: Head 1: Time Synchronization: 2020.10.14   00:11:00::0014
20201014::001100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.1dbar, CTD 34.5psu, index 1.34, Packet 66737
20201014::001100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001105: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001106_wf.raa
20201014::001115: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001116_wf.raa
20201014::001125: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001126_wf.raa
20201014::001130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.4dbar, CTD 34.5psu, index 1.34, Packet 66791
20201014::001130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001135: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001136_wf.raa
20201014::001147: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001147_wf.raa
20201014::001156: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001157_wf.raa
20201014::001159: Head 2: Time Synchronization: 2020.10.14   00:12:00::0015
20201014::001159: Head 1: Time Synchronization: 2020.10.14   00:12:00::0015
20201014::001200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1185.7dbar, CTD 34.5psu, index 1.34, Packet 66845
20201014::001200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001207: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001207_wf.raa
20201014::001217: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001217_wf.raa
20201014::001226: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001227_wf.raa
20201014::001230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.7dbar, CTD 34.5psu, index 1.34, Packet 66899
20201014::001230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001236: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001237_wf.raa
20201014::001246: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001247_wf.raa
20201014::001256: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001257_wf.raa
20201014::001259: Head 1: Time Synchronization: 2020.10.14   00:13:00::0014
20201014::001300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.4dbar, CTD 34.5psu, index 1.34, Packet 66954
20201014::001300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001306: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001307_wf.raa
20201014::001316: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001317_wf.raa
20201014::001326: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001327_wf.raa
20201014::001330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.0dbar, CTD 34.5psu, index 1.34, Packet 67008
20201014::001330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001336: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001337_wf.raa
20201014::001346: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001347_wf.raa
20201014::001356: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001357_wf.raa
20201014::001359: Head 1: Time Synchronization: 2020.10.14   00:14:00::0015
20201014::001400: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.2dbar, CTD 34.5psu, index 1.34, Packet 67062
20201014::001400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001406: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001407_wf.raa
20201014::001416: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001417_wf.raa
20201014::001426: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001427_wf.raa
20201014::001430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001430: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1188.8dbar, CTD 34.5psu, index 1.34, Packet 67117
20201014::001430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001436: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001437_wf.raa
20201014::001446: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001447_wf.raa
20201014::001456: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001457_wf.raa
20201014::001459: Head 1: Time Synchronization: 2020.10.14   00:15:00::0014
20201014::001500: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.3dbar, CTD 34.5psu, index 1.34, Packet 67171
20201014::001500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001506: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001507_wf.raa
20201014::001516: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001517_wf.raa
20201014::001526: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001527_wf.raa
20201014::001530: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.8dbar, CTD 34.5psu, index 1.34, Packet 67225
20201014::001530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001536: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001537_wf.raa
20201014::001547: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001547_wf.raa
20201014::001556: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001557_wf.raa
20201014::001559: Head 1: Time Synchronization: 2020.10.14   00:16:00::0014
20201014::001600: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1187.1dbar, CTD 34.5psu, index 1.34, Packet 67280
20201014::001600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001606: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001607_wf.raa
20201014::001616: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001617_wf.raa
20201014::001627: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001627_wf.raa
20201014::001630: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1185.8dbar, CTD 34.5psu, index 1.34, Packet 67334
20201014::001630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001637: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001637_wf.raa
20201014::001647: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001647_wf.raa
20201014::001657: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001657_wf.raa
20201014::001659: Head 1: Time Synchronization: 2020.10.14   00:17:00::0015
20201014::001700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001700: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.3dbar, CTD 34.5psu, index 1.34, Packet 67389
20201014::001700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001707: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001707_wf.raa
20201014::001717: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001717_wf.raa
20201014::001726: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001727_wf.raa
20201014::001730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001730: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67443
20201014::001730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001736: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001737_wf.raa
20201014::001746: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001747_wf.raa
20201014::001756: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001757_wf.raa
20201014::001759: Head 1: Time Synchronization: 2020.10.14   00:18:00::0015
20201014::001800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001800: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.2dbar, CTD 34.5psu, index 1.34, Packet 67498
20201014::001800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001806: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001807_wf.raa
20201014::001816: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001817_wf.raa
20201014::001826: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001827_wf.raa
20201014::001830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001830: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67553
20201014::001830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001836: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001837_wf.raa
20201014::001846: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001847_wf.raa
20201014::001856: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001857_wf.raa
20201014::001859: Head 1: Time Synchronization: 2020.10.14   00:19:00::0015
20201014::001900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001900: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67607
20201014::001900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::001902: GUI: Live mode ON.
20201014::001902: GUI: Requesing STOP operation, Head 1
20201014::001902: GUI: Requesing STOP operation, Head 2
20201014::001902: Head 2: Received request: STOP
20201014::001902: Head 1: Received request: STOP
20201014::001903: Head 2: Stopping Scan Operation
20201014::001903: Head 1: Stopping Scan Operation
20201014::001905: Head 1: ProcessingMgr stopped all worker threads.
20201014::001905: Head 2: ProcessingMgr stopped all worker threads.
20201014::001905: Head 1:       Stop finished, may now recover.
20201014::001905: Head 2:       Stop finished, may now recover.
20201014::001907: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::001907: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::001907: Head 1: Eye Safe Optical Filter check Passed
20201014::001907: Head 2: Eye Safe Optical Filter check Passed
20201014::001930: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67660
20201014::001930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::001930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::001934: GUI: Live mode ON.
20201014::001934: GUI: Requesing START operation, Head 2
20201014::001934: GUI: Requesing START operation, Head 1
20201014::001934: Head 2: Received request: START
20201014::001934: Head 1: Received request: START
20201014::001935: Head 2: Starting Scan Operation
20201014::001935: Head 1: Starting Scan Operation
20201014::001936: Head 1: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::001936: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::001936: Head 1: Eye Safe Optical Filter check Passed
20201014::001936: Head 2: Eye Safe Optical Filter check Passed
20201014::001941: Head 1: Configured for WATER Processing
20201014::001941: Head 2: Configured for WATER Processing
20201014::001941: Head 1: Configured for WATER Processing
20201014::001941: Head 2: Configured for WATER Processing
20201014::001941: Head 1: Configured for WATER Processing
20201014::001941: Head 2: Configured for WATER Processing
20201014::001941: Head 1: Configured for WATER Processing
20201014::001942: Head 2: Configured for WATER Processing
20201014::001942: Head 1: Configured for WATER Processing
20201014::001942: Head 2: Configured for WATER Processing
20201014::001942: Head 1: Configured for WATER Processing
20201014::001942: Head 2: Configured for WATER Processing
20201014::001942: Head 1: Configured for WATER Processing
20201014::001943: Head 2: Configured for WATER Processing
20201014::001943: Head 1: Configured for WATER Processing
20201014::001943: Head 2: Configured for WATER Processing
20201014::001943: Head 1: Configured for WATER Processing
20201014::001943: Head 2: Configured for WATER Processing
20201014::001943: Head 1: Configured for WATER Processing
20201014::001943: Head 2: Configured for WATER Processing
20201014::001944: Head 1: Configured for WATER Processing
20201014::001944: Head 2: Configured for WATER Processing
20201014::001944: Head 1: Configured for WATER Processing
20201014::001944: Head 2: Configured for WATER Processing
20201014::001944: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001943_wf.raa
20201014::001944: Head 1: Configured for WATER Processing
20201014::001944: Head 2: Configured for WATER Processing
20201014::001945: Head 1: Configured for WATER Processing
20201014::001945: Head 2: Configured for WATER Processing
20201014::001945: Head 1: Configured for WATER Processing
20201014::001945: Head 2: Configured for WATER Processing
20201014::001945: Head 1: Configured for WATER Processing
20201014::001945: Head 2: Configured for WATER Processing
20201014::001945: Head 1: Configured for WATER Processing
20201014::001946: Head 2: Configured for WATER Processing
20201014::001946: Head 1: Configured for WATER Processing
20201014::001946: Head 2: Configured for WATER Processing
20201014::001946: Head 1: Configured for WATER Processing
20201014::001946: Head 2: Configured for WATER Processing
20201014::001946: Head 1: Configured for WATER Processing
20201014::001946: Head 2: Configured for WATER Processing
20201014::001952: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_001953_wf.raa
20201014::001959: Head 2: Time Synchronization: 2020.10.14   00:20:00::0015
20201014::002000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.1dbar, CTD 34.5psu, index 1.34, Packet 67715
20201014::002000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002002: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002003_wf.raa
20201014::002012: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002013_wf.raa
20201014::002022: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002023_wf.raa
20201014::002030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.6dbar, CTD 34.5psu, index 1.34, Packet 67769
20201014::002030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002032: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002033_wf.raa
20201014::002042: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002043_wf.raa
20201014::002052: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002053_wf.raa
20201014::002100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67823
20201014::002100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002102: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002103_wf.raa
20201014::002112: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002113_wf.raa
20201014::002122: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002123_wf.raa
20201014::002130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67877
20201014::002130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002132: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002133_wf.raa
20201014::002142: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002143_wf.raa
20201014::002152: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002153_wf.raa
20201014::002200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67931
20201014::002200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002202: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002203_wf.raa
20201014::002212: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002213_wf.raa
20201014::002222: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002223_wf.raa
20201014::002230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.7dbar, CTD 34.5psu, index 1.34, Packet 67985
20201014::002230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002232: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002233_wf.raa
20201014::002242: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002243_wf.raa
20201014::002252: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002253_wf.raa
20201014::002259: Head 1: Time Synchronization: 2020.10.14   00:23:00::0014
20201014::002300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1183.9dbar, CTD 34.5psu, index 1.34, Packet 68039
20201014::002300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002302: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002303_wf.raa
20201014::002312: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002313_wf.raa
20201014::002322: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002323_wf.raa
20201014::002330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1185.2dbar, CTD 34.5psu, index 1.34, Packet 68092
20201014::002330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002332: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002333_wf.raa
20201014::002342: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002343_wf.raa
20201014::002352: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002353_wf.raa
20201014::002359: Head 1: Time Synchronization: 2020.10.14   00:24:00::0016
20201014::002400: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.9dbar, CTD 34.5psu, index 1.34, Packet 68147
20201014::002400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002402: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002403_wf.raa
20201014::002412: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002413_wf.raa
20201014::002422: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002423_wf.raa
20201014::002430: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.5dbar, CTD 34.5psu, index 1.34, Packet 68200
20201014::002430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002432: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002433_wf.raa
20201014::002442: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002443_wf.raa
20201014::002452: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002453_wf.raa
20201014::002500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002500: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1190.4dbar, CTD 34.5psu, index 1.34, Packet 68254
20201014::002500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002502: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002503_wf.raa
20201014::002512: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002513_wf.raa
20201014::002522: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002523_wf.raa
20201014::002530: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1191.1dbar, CTD 34.5psu, index 1.34, Packet 68308
20201014::002530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002532: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002533_wf.raa
20201014::002542: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002543_wf.raa
20201014::002552: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002553_wf.raa
20201014::002559: Head 1: Time Synchronization: 2020.10.14   00:26:00::0014
20201014::002600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002600: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1190.5dbar, CTD 34.5psu, index 1.34, Packet 68362
20201014::002600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002602: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002603_wf.raa
20201014::002612: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002613_wf.raa
20201014::002622: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002623_wf.raa
20201014::002630: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.7dbar, CTD 34.5psu, index 1.34, Packet 68416
20201014::002630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002632: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002633_wf.raa
20201014::002642: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002643_wf.raa
20201014::002652: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002653_wf.raa
20201014::002659: Head 1: Time Synchronization: 2020.10.14   00:27:00::0014
20201014::002700: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.0dbar, CTD 34.5psu, index 1.34, Packet 68470
20201014::002700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002702: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002703_wf.raa
20201014::002712: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002713_wf.raa
20201014::002722: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002723_wf.raa
20201014::002730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002730: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.5dbar, CTD 34.5psu, index 1.34, Packet 68524
20201014::002730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002733: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002733_wf.raa
20201014::002742: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002743_wf.raa
20201014::002753: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002753_wf.raa
20201014::002759: Head 2: Time Synchronization: 2020.10.14   00:28:00::0014
20201014::002759: Head 1: Time Synchronization: 2020.10.14   00:28:00::0015
20201014::002800: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.1dbar, CTD 34.5psu, index 1.34, Packet 68577
20201014::002800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002803: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002803_wf.raa
20201014::002812: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002813_wf.raa
20201014::002823: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002823_wf.raa
20201014::002830: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.6dbar, CTD 34.5psu, index 1.34, Packet 68631
20201014::002830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 16.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002832: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002833_wf.raa
20201014::002842: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002843_wf.raa
20201014::002853: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002853_wf.raa
20201014::002900: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.1dbar, CTD 34.5psu, index 1.34, Packet 68686
20201014::002900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002903: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002903_wf.raa
20201014::002913: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002913_wf.raa
20201014::002923: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002923_wf.raa
20201014::002930: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.4dbar, CTD 34.5psu, index 1.34, Packet 68740
20201014::002930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::002933: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002933_wf.raa
20201014::002943: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002943_wf.raa
20201014::002952: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_002953_wf.raa
20201014::002959: Head 1: Time Synchronization: 2020.10.14   00:30:00::0014
20201014::003000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1183.3dbar, CTD 34.5psu, index 1.34, Packet 68794
20201014::003000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003003: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003003_wf.raa
20201014::003013: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003013_wf.raa
20201014::003022: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003023_wf.raa
20201014::003030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.7dbar, CTD 34.5psu, index 1.34, Packet 68848
20201014::003030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003033: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003033_wf.raa
20201014::003043: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003043_wf.raa
20201014::003053: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003053_wf.raa
20201014::003059: Head 1: Time Synchronization: 2020.10.14   00:31:00::0016
20201014::003100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.3dbar, CTD 34.5psu, index 1.34, Packet 68902
20201014::003100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003103: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003103_wf.raa
20201014::003112: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003113_wf.raa
20201014::003122: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003123_wf.raa
20201014::003130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.0dbar, CTD 34.5psu, index 1.34, Packet 68956
20201014::003130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003132: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003133_wf.raa
20201014::003142: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003143_wf.raa
20201014::003152: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003153_wf.raa
20201014::003159: Head 1: Time Synchronization: 2020.10.14   00:32:00::0015
20201014::003200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1189.7dbar, CTD 34.5psu, index 1.34, Packet 69009
20201014::003200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003202: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003203_wf.raa
20201014::003212: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003213_wf.raa
20201014::003222: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003223_wf.raa
20201014::003230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1190.9dbar, CTD 34.5psu, index 1.34, Packet 69063
20201014::003230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003232: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003233_wf.raa
20201014::003242: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003243_wf.raa
20201014::003252: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003253_wf.raa
20201014::003300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1190.4dbar, CTD 34.5psu, index 1.34, Packet 69117
20201014::003300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003302: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003303_wf.raa
20201014::003312: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003313_wf.raa
20201014::003322: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003323_wf.raa
20201014::003330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.7dbar, CTD 34.5psu, index 1.34, Packet 69170
20201014::003330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003332: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003333_wf.raa
20201014::003342: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003343_wf.raa
20201014::003352: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003353_wf.raa
20201014::003359: Head 1: Time Synchronization: 2020.10.14   00:34:00::0015
20201014::003400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003400: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.9dbar, CTD 34.5psu, index 1.34, Packet 69224
20201014::003400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003402: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003403_wf.raa
20201014::003412: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003413_wf.raa
20201014::003422: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003423_wf.raa
20201014::003430: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.3dbar, CTD 34.5psu, index 1.34, Packet 69277
20201014::003430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003432: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003433_wf.raa
20201014::003442: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003443_wf.raa
20201014::003452: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003453_wf.raa
20201014::003500: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1183.9dbar, CTD 34.5psu, index 1.34, Packet 69331
20201014::003500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003502: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003503_wf.raa
20201014::003512: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003513_wf.raa
20201014::003522: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003523_wf.raa
20201014::003530: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.3dbar, CTD 34.5psu, index 1.34, Packet 69384
20201014::003530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003532: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003533_wf.raa
20201014::003543: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003543_wf.raa
20201014::003554: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003553_wf.raa
20201014::003559: Head 2: Time Synchronization: 2020.10.14   00:36:00::0014
20201014::003559: Head 1: Time Synchronization: 2020.10.14   00:36:00::0014
20201014::003600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003600: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1181.6dbar, CTD 34.5psu, index 1.34, Packet 69438
20201014::003600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003602: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003603_wf.raa
20201014::003613: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003613_wf.raa
20201014::003623: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003623_wf.raa
20201014::003630: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1182.4dbar, CTD 34.5psu, index 1.34, Packet 69491
20201014::003630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003633: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003633_wf.raa
20201014::003643: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003643_wf.raa
20201014::003652: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003653_wf.raa
20201014::003659: Head 1: Time Synchronization: 2020.10.14   00:37:00::0016
20201014::003700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003700: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1183.0dbar, CTD 34.5psu, index 1.34, Packet 69545
20201014::003700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003703: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003703_wf.raa
20201014::003713: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003713_wf.raa
20201014::003722: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003723_wf.raa
20201014::003730: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1184.4dbar, CTD 34.5psu, index 1.34, Packet 69598
20201014::003730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003733: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003733_wf.raa
20201014::003743: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003743_wf.raa
20201014::003753: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003753_wf.raa
20201014::003759: Head 1: Time Synchronization: 2020.10.14   00:38:00::0015
20201014::003800: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.9dbar, CTD 34.5psu, index 1.34, Packet 69652
20201014::003800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003803: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003803_wf.raa
20201014::003813: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003813_wf.raa
20201014::003822: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003823_wf.raa
20201014::003830: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.2dbar, CTD 34.5psu, index 1.34, Packet 69705
20201014::003830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003832: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003833_wf.raa
20201014::003842: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003843_wf.raa
20201014::003852: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003853_wf.raa
20201014::003859: Head 1: Time Synchronization: 2020.10.14   00:39:00::0014
20201014::003900: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.1dbar, CTD 34.5psu, index 1.34, Packet 69759
20201014::003900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003902: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003903_wf.raa
20201014::003912: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003913_wf.raa
20201014::003922: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003923_wf.raa
20201014::003930: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1188.0dbar, CTD 34.5psu, index 1.34, Packet 69813
20201014::003930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::003932: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003933_wf.raa
20201014::003942: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003943_wf.raa
20201014::003952: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_003953_wf.raa
20201014::003959: Head 1: Time Synchronization: 2020.10.14   00:40:00::0015
20201014::004000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.3dbar, CTD 34.5psu, index 1.34, Packet 69866
20201014::004000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004002: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004003_wf.raa
20201014::004012: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004013_wf.raa
20201014::004022: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004023_wf.raa
20201014::004030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1186.6dbar, CTD 34.5psu, index 1.34, Packet 69920
20201014::004030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004032: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004033_wf.raa
20201014::004042: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004043_wf.raa
20201014::004052: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004053_wf.raa
20201014::004059: Head 1: Time Synchronization: 2020.10.14   00:41:00::0014
20201014::004100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.9dbar, CTD 34.5psu, index 1.34, Packet 69974
20201014::004100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004102: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004103_wf.raa
20201014::004112: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004113_wf.raa
20201014::004122: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004123_wf.raa
20201014::004130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.8dbar, CTD 34.5psu, index 1.34, Packet 70028
20201014::004130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004132: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004133_wf.raa
20201014::004142: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004143_wf.raa
20201014::004152: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004153_wf.raa
20201014::004200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1183.7dbar, CTD 34.5psu, index 1.34, Packet 70081
20201014::004200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004202: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004203_wf.raa
20201014::004212: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004213_wf.raa
20201014::004222: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004223_wf.raa
20201014::004230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.0dbar, CTD 34.5psu, index 1.34, Packet 70135
20201014::004230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004233: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004233_wf.raa
20201014::004242: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004243_wf.raa
20201014::004252: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004253_wf.raa
20201014::004259: Head 1: Time Synchronization: 2020.10.14   00:43:00::0016
20201014::004300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.5dbar, CTD 34.5psu, index 1.34, Packet 70189
20201014::004300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004302: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004303_wf.raa
20201014::004312: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004313_wf.raa
20201014::004322: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004323_wf.raa
20201014::004330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.7dbar, CTD 34.5psu, index 1.34, Packet 70242
20201014::004330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004332: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004333_wf.raa
20201014::004342: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004343_wf.raa
20201014::004352: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004353_wf.raa
20201014::004359: Head 1: Time Synchronization: 2020.10.14   00:44:00::0014
20201014::004400: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.5dbar, CTD 34.5psu, index 1.34, Packet 70296
20201014::004400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004402: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004403_wf.raa
20201014::004412: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004413_wf.raa
20201014::004422: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004423_wf.raa
20201014::004430: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.1dbar, CTD 34.5psu, index 1.34, Packet 70350
20201014::004430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004432: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004433_wf.raa
20201014::004442: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004443_wf.raa
20201014::004452: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004453_wf.raa
20201014::004500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004500: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.7dbar, CTD 34.5psu, index 1.34, Packet 70404
20201014::004500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004502: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004503_wf.raa
20201014::004512: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004513_wf.raa
20201014::004522: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004523_wf.raa
20201014::004530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004530: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.1dbar, CTD 34.5psu, index 1.34, Packet 70457
20201014::004530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004532: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004533_wf.raa
20201014::004542: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004543_wf.raa
20201014::004552: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004553_wf.raa
20201014::004559: Head 2: Time Synchronization: 2020.10.14   00:46:00::0014
20201014::004600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004600: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.9dbar, CTD 34.5psu, index 1.34, Packet 70511
20201014::004600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004602: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004603_wf.raa
20201014::004612: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004613_wf.raa
20201014::004622: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004623_wf.raa
20201014::004630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004630: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1189.0dbar, CTD 34.5psu, index 1.34, Packet 70564
20201014::004630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004632: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004633_wf.raa
20201014::004642: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004643_wf.raa
20201014::004652: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004653_wf.raa
20201014::004659: Head 1: Time Synchronization: 2020.10.14   00:47:00::0014
20201014::004700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004700: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.3dbar, CTD 34.5psu, index 1.34, Packet 70618
20201014::004700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004702: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004703_wf.raa
20201014::004712: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004713_wf.raa
20201014::004722: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004723_wf.raa
20201014::004730: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.7dbar, CTD 34.5psu, index 1.34, Packet 70671
20201014::004730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004732: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004733_wf.raa
20201014::004742: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004743_wf.raa
20201014::004752: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004753_wf.raa
20201014::004800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004800: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.9dbar, CTD 34.5psu, index 1.34, Packet 70725
20201014::004800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004802: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004803_wf.raa
20201014::004812: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004813_wf.raa
20201014::004822: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004823_wf.raa
20201014::004830: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.1dbar, CTD 34.5psu, index 1.34, Packet 70778
20201014::004830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004832: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004833_wf.raa
20201014::004842: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004843_wf.raa
20201014::004852: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004853_wf.raa
20201014::004859: Head 1: Time Synchronization: 2020.10.14   00:49:00::0014
20201014::004900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004900: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.7dbar, CTD 34.5psu, index 1.34, Packet 70832
20201014::004900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004902: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004903_wf.raa
20201014::004912: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004913_wf.raa
20201014::004922: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004923_wf.raa
20201014::004930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004930: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1184.8dbar, CTD 34.5psu, index 1.34, Packet 70886
20201014::004930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::004932: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004933_wf.raa
20201014::004942: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004943_wf.raa
20201014::004952: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_004953_wf.raa
20201014::005000: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1185.2dbar, CTD 34.5psu, index 1.34, Packet 70939
20201014::005000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005002: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005003_wf.raa
20201014::005012: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005013_wf.raa
20201014::005022: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005023_wf.raa
20201014::005030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005030: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1186.5dbar, CTD 34.5psu, index 1.34, Packet 70993
20201014::005030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005032: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005033_wf.raa
20201014::005042: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005043_wf.raa
20201014::005052: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005053_wf.raa
20201014::005059: Head 2: Time Synchronization: 2020.10.14   00:51:00::0014
20201014::005100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005100: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.3dbar, CTD 34.5psu, index 1.34, Packet 71047
20201014::005100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005102: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005103_wf.raa
20201014::005112: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005113_wf.raa
20201014::005122: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005123_wf.raa
20201014::005130: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.0dbar, CTD 34.5psu, index 1.34, Packet 71100
20201014::005130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005132: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005133_wf.raa
20201014::005142: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005143_wf.raa
20201014::005152: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005153_wf.raa
20201014::005159: Head 1: Time Synchronization: 2020.10.14   00:52:00::0015
20201014::005200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005200: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.5dbar, CTD 34.5psu, index 1.34, Packet 71154
20201014::005200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005202: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005203_wf.raa
20201014::005212: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005213_wf.raa
20201014::005222: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005223_wf.raa
20201014::005230: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.9dbar, CTD 34.5psu, index 1.34, Packet 71207
20201014::005230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005232: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005233_wf.raa
20201014::005242: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005243_wf.raa
20201014::005252: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005253_wf.raa
20201014::005259: Head 1: Time Synchronization: 2020.10.14   00:53:00::0014
20201014::005300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005300: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1189.2dbar, CTD 34.5psu, index 1.34, Packet 71261
20201014::005300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005302: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005303_wf.raa
20201014::005312: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005313_wf.raa
20201014::005322: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005323_wf.raa
20201014::005330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005330: System  Initialized, Gain 8, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.9dbar, CTD 34.5psu, index 1.34, Packet 71315
20201014::005330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::005332: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_005333_wf.raa
20201014::005334: GUI: Live mode ON.
20201014::005334: GUI: Requesing STOP operation, Head 2
20201014::005334: GUI: Requesing STOP operation, Head 1
20201014::005334: Head 2: Received request: STOP
20201014::005334: Head 1: Received request: STOP
20201014::005334: Head 2: Stopping Scan Operation
20201014::005334: Head 1: Stopping Scan Operation
20201014::005338: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::005339: Head 2: Eye Safe Optical Filter check Passed
20201014::005339: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::005340: Head 1: Eye Safe Optical Filter check Passed
20201014::005351: Head 2: ProcessingMgr stopped all worker threads.
20201014::005351: Head 2:       Stop finished, may now recover.
20201014::005400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005400: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1188.2dbar, CTD 34.5psu, index 1.34, Packet 71369
20201014::005400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005412: Head 1: ProcessingMgr stopped all worker threads.
20201014::005412: Head 1:       Stop finished, may now recover.
20201014::005430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005430: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1189.6dbar, CTD 34.5psu, index 1.34, Packet 71422
20201014::005430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005500: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1187.5dbar, CTD 34.5psu, index 1.34, Packet 71476
20201014::005500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005530: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1182.6dbar, CTD 34.5psu, index 1.34, Packet 71529
20201014::005530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005600: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1168.5dbar, CTD 34.5psu, index 1.34, Packet 71582
20201014::005600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005630: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1150.9dbar, CTD 34.5psu, index 1.34, Packet 71636
20201014::005630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 21.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005700: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1131.5dbar, CTD 34.5psu, index 1.34, Packet 71689
20201014::005700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005730: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1114.7dbar, CTD 34.5psu, index 1.34, Packet 71743
20201014::005730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005800: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1097.3dbar, CTD 34.5psu, index 1.34, Packet 71796
20201014::005800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005830: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1078.2dbar, CTD 34.5psu, index 1.34, Packet 71849
20201014::005830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005900: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1068.8dbar, CTD 34.5psu, index 1.34, Packet 71903
20201014::005900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::005930: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1057.3dbar, CTD 34.5psu, index 1.34, Packet 71956
20201014::005930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010000: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1041.5dbar, CTD 34.5psu, index 1.34, Packet 72009
20201014::010000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010030: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1022.7dbar, CTD 34.5psu, index 1.34, Packet 72063
20201014::010030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010100: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.9C, CTD 1009.9dbar, CTD 34.5psu, index 1.34, Packet 72116
20201014::010100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010130: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 993.8dbar, CTD 34.4psu, index 1.34, Packet 72170
20201014::010130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010200: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 976.9dbar, CTD 34.4psu, index 1.34, Packet 72223
20201014::010200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010230: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 960.6dbar, CTD 34.4psu, index 1.34, Packet 72276
20201014::010230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010300: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 945.2dbar, CTD 34.4psu, index 1.34, Packet 72330
20201014::010300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010330: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 927.7dbar, CTD 34.4psu, index 1.34, Packet 72383
20201014::010330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010400: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 909.8dbar, CTD 34.4psu, index 1.34, Packet 72436
20201014::010400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010430: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 892.2dbar, CTD 34.4psu, index 1.34, Packet 72490
20201014::010430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010500: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 876.7dbar, CTD 34.4psu, index 1.34, Packet 72543
20201014::010500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010530: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 862.9dbar, CTD 34.4psu, index 1.34, Packet 72596
20201014::010530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010600: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 847.5dbar, CTD 34.4psu, index 1.34, Packet 72650
20201014::010600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010630: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 831.9dbar, CTD 34.4psu, index 1.34, Packet 72703
20201014::010630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010700: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 814.6dbar, CTD 34.4psu, index 1.34, Packet 72757
20201014::010700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010730: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 798.5dbar, CTD 34.4psu, index 1.34, Packet 72810
20201014::010730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010800: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 781.9dbar, CTD 34.4psu, index 1.34, Packet 72863
20201014::010800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010830: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 765.2dbar, CTD 34.4psu, index 1.34, Packet 72917
20201014::010830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010900: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 746.4dbar, CTD 34.4psu, index 1.34, Packet 72970
20201014::010900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010930: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 727.1dbar, CTD 34.4psu, index 1.34, Packet 73023
20201014::010930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::010930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011000: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 711.5dbar, CTD 34.4psu, index 1.34, Packet 73077
20201014::011000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011030: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 695.9dbar, CTD 34.4psu, index 1.34, Packet 73130
20201014::011030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011100: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 680.0dbar, CTD 34.4psu, index 1.34, Packet 73183
20201014::011100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011130: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 663.7dbar, CTD 34.3psu, index 1.34, Packet 73237
20201014::011130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011200: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.2C, CTD 647.3dbar, CTD 34.3psu, index 1.34, Packet 73290
20201014::011200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011230: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.2C, CTD 631.0dbar, CTD 34.3psu, index 1.34, Packet 73343
20201014::011230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011300: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 613.3dbar, CTD 34.3psu, index 1.34, Packet 73397
20201014::011300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011330: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 595.0dbar, CTD 34.3psu, index 1.34, Packet 73450
20201014::011330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011400: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.5C, CTD 576.7dbar, CTD 34.3psu, index 1.34, Packet 73504
20201014::011400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011430: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.6C, CTD 558.9dbar, CTD 34.3psu, index 1.34, Packet 73557
20201014::011430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011500: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.7C, CTD 540.4dbar, CTD 34.3psu, index 1.34, Packet 73610
20201014::011500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011530: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.9C, CTD 522.3dbar, CTD 34.3psu, index 1.34, Packet 73664
20201014::011530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011600: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.0C, CTD 507.7dbar, CTD 34.3psu, index 1.34, Packet 73717
20201014::011600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011630: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.3C, CTD 491.9dbar, CTD 34.2psu, index 1.34, Packet 73770
20201014::011630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011700: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.6C, CTD 475.9dbar, CTD 34.2psu, index 1.34, Packet 73824
20201014::011700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011730: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.8C, CTD 459.1dbar, CTD 34.2psu, index 1.34, Packet 73877
20201014::011730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011759: Head 1: Time Synchronization: 2020.10.14   01:18:00::0014
20201014::011800: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.0C, CTD 441.7dbar, CTD 34.2psu, index 1.34, Packet 73930
20201014::011800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011830: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.1C, CTD 422.7dbar, CTD 34.2psu, index 1.34, Packet 73984
20201014::011830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011900: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.2C, CTD 404.5dbar, CTD 34.2psu, index 1.34, Packet 74037
20201014::011900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 11C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 10C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::011930: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.3C, CTD 386.3dbar, CTD 34.2psu, index 1.34, Packet 74091
20201014::011930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012000: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.5C, CTD 368.0dbar, CTD 34.2psu, index 1.34, Packet 74144
20201014::012000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 26%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012030: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.6C, CTD 350.2dbar, CTD 34.2psu, index 1.34, Packet 74197
20201014::012030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012100: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.7C, CTD 331.3dbar, CTD 34.2psu, index 1.34, Packet 74251
20201014::012100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012130: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.8C, CTD 312.9dbar, CTD 34.2psu, index 1.34, Packet 74304
20201014::012130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012200: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 294.2dbar, CTD 34.2psu, index 1.34, Packet 74358
20201014::012200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012230: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 277.6dbar, CTD 34.2psu, index 1.34, Packet 74411
20201014::012230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012300: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.2C, CTD 270.0dbar, CTD 34.1psu, index 1.34, Packet 74464
20201014::012300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 12C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012330: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.5C, CTD 260.3dbar, CTD 34.1psu, index 1.34, Packet 74518
20201014::012330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 25%, OPB 13C, Laser 19.0C, Dig 27.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 25%, OPB 11C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::012348: GUI: Lost Communications with Sensor 1.
20201014::012348: GUI: Lost Communications with Head 2.
20201014::012356: GUI: Attempting Communications with Head 1...
20201014::012356: GUI: Attempting Communications with Head 2...
20201014::132036: GUI: Established Communications with Head 1.
20201014::132036: GUI: Established Communications with Head 2.
20201014::132036: Head 1: Initializing Communications with GUI ...
20201014::132037: Head 2: Initializing Communications with GUI ...
20201014::132037: Head 1: Communications Established.
20201014::132038: Head 2: Communications Established.
20201014::132038: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201014::132038: Head 1: Connection Established with the GUI.
20201014::132039: Head 1: Initializing Subsystems, standby ...
20201014::132039: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201014::132039: Head 1: Initializing Hardware, Stand by ...
20201014::132039: Head 2: Connection Established with the GUI.
20201014::132039: Head 2: Initializing Subsystems, standby ...
20201014::132040: Head 2: Initializing Hardware, Stand by ...
20201014::132052: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201014::132052: Head 1: NtQuery - testing 1 ...
20201014::132053: Head 1: clock resolution: 10
20201014::132053: Head 1: NtQuery - testing 2, after setting max res ...
20201014::132053: Head 1: clock resolution: 10
20201014::132054: Head 1: Initializing Optics Electronics ...
20201014::132054: Head 1: Power Laser Controller
20201014::132058: Head 1: Power Scanner Controller
20201014::132058: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201014::132058: Head 2: NtQuery - testing 1 ...
20201014::132059: Head 2: clock resolution: 10
20201014::132059: Head 2: NtQuery - testing 2, after setting max res ...
20201014::132059: Head 2: clock resolution: 10
20201014::132100: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132100: Head 2: Initializing Optics Electronics ...
20201014::132100: Head 1: Power OPTO Sensor
20201014::132100: System NOT Initialized, Gain 0, Elec PB 17.4C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 45
20201014::132100: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132100: Head 2: Power Laser Controller
20201014::132104: Head 2: Power Scanner Controller
20201014::132106: Head 2: Power OPTO Sensor
20201014::132120: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::132120: Head 1: Eye Safe Optical Filter check Passed
20201014::132120: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201014::132121: Head 1: Initializing Time Sync Subsystem.
20201014::132121: Head 1: Initializing CTD Subsystem.
20201014::132121: Head 1: CTD Initialization Successful
20201014::132122: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201014::132122: Head 1: Time Sync UDP started, waiting for sync...
20201014::132122: Head 1: Attempting CTD Ethernet connection with ROV...
20201014::132123: Head 1: Time Synchronization Achieved: 2020.10.14   13:21:24::0016
20201014::132126: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::132126: Head 2: Eye Safe Optical Filter check Passed
20201014::132127: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201014::132127: Head 2: Initializing Time Sync Subsystem.
20201014::132127: Head 2: Initializing CTD Subsystem.
20201014::132127: Head 2: CTD Initialization Successful
20201014::132128: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201014::132128: Head 2: Time Sync UDP started, waiting for sync...
20201014::132128: Head 2: Attempting CTD Ethernet connection with ROV...
20201014::132129: Head 2: Time Synchronization Achieved: 2020.10.14   13:21:30::0014
20201014::132130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 29%, OPB 17C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132130: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 23.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 100
20201014::132130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 29%, OPB 18C, Laser 17.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132156: Head 1: CTD Ethernet connection established.
20201014::132156: Head 2: CTD Ethernet connection established.
20201014::132200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 27%, OPB 17C, Laser 16.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132200: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.1C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 154
20201014::132200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 27%, OPB 18C, Laser 18.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 25%, OPB 17C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132230: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.1C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 209
20201014::132230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 25%, OPB 18C, Laser 18.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 17C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132300: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 21.8%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 264
20201014::132300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 24C, OCB 24%, OPB 18C, Laser 19.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 18C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132330: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 1.4dbar, CTD 0.1psu, index 1.34, Packet 319
20201014::132330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 23%, OPB 19C, Laser 20.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132354: GUI: Live mode ON.
20201014::132354: GUI: Requesing START operation, Head 1
20201014::132354: GUI: Requesing START operation, Head 2
20201014::132355: Head 1: Received request: START
20201014::132355: Head 2: Received request: START
20201014::132355: Head 1: Starting Scan Operation
20201014::132355: Head 2: Starting Scan Operation
20201014::132356: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::132356: Head 2: Eye Safe Optical Filter check Passed
20201014::132358: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20201014::132358: Head 1: Eye Safe Optical Filter check Passed
20201014::132359: Head 2: Time Synchronization: 2020.10.14   13:24:00::0016
20201014::132400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 18C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 1
20201014::132400: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 1.9dbar, CTD 0.1psu, index 1.34, Packet 374
20201014::132400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 20.0C, Dig 19.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132403: Head 1: Configured for WATER Processing
20201014::132403: Head 1: Configured for WATER Processing
20201014::132403: Head 1: Configured for WATER Processing
20201014::132404: Head 1: Configured for WATER Processing
20201014::132404: Head 1: Configured for WATER Processing
20201014::132404: Head 1: Configured for WATER Processing
20201014::132405: Head 1: Configured for WATER Processing
20201014::132405: Head 1: Configured for WATER Processing
20201014::132405: Head 1: Configured for WATER Processing
20201014::132406: Head 1: Configured for WATER Processing
20201014::132406: Head 1: Configured for WATER Processing
20201014::132406: Head 1: Configured for WATER Processing
20201014::132406: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_132405_wf.raa
20201014::132406: Head 1: Configured for WATER Processing
20201014::132407: Head 1: Configured for WATER Processing
20201014::132407: Head 1: Configured for WATER Processing
20201014::132407: Head 1: Configured for WATER Processing
20201014::132408: Head 1: Configured for WATER Processing
20201014::132408: Head 1: Configured for WATER Processing
20201014::132408: Head 1: Configured for WATER Processing
20201014::132409: Head 1: Configured for WATER Processing
20201014::132414: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_132415_wf.raa
20201014::132424: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_132425_wf.raa
20201014::132427: Head 2: Configured for WATER Processing
20201014::132427: Head 2: Configured for WATER Processing
20201014::132428: Head 2: Configured for WATER Processing
20201014::132428: Head 2: Configured for WATER Processing
20201014::132428: Head 2: Configured for WATER Processing
20201014::132429: Head 2: Configured for WATER Processing
20201014::132429: Head 2: Configured for WATER Processing
20201014::132429: Head 2: Configured for WATER Processing
20201014::132430: Head 2: Configured for WATER Processing
20201014::132430: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 429
20201014::132430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 25C, OCB 22%, OPB 19C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 1
20201014::132430: Head 2: Configured for WATER Processing
20201014::132430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 4.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 1
20201014::132430: Head 2: Configured for WATER Processing
20201014::132430: Head 2: Configured for WATER Processing
20201014::132431: Head 2: Configured for WATER Processing
20201014::132431: Head 2: Configured for WATER Processing
20201014::132431: Head 2: Configured for WATER Processing
20201014::132432: Head 2: Configured for WATER Processing
20201014::132432: Head 2: Configured for WATER Processing
20201014::132432: Head 2: Configured for WATER Processing
20201014::132433: Head 2: Configured for WATER Processing
20201014::132433: Head 2: Configured for WATER Processing
20201014::132434: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_132435_wf.raa
20201014::132437: GUI: Live mode ON.
20201014::132437: GUI: Requesing STOP operation, Head 1
20201014::132437: GUI: Requesing STOP operation, Head 2
20201014::132437: Head 2: Received request: STOP
20201014::132438: Head 1: Received request: STOP
20201014::132438: Head 2: Stopping Scan Operation
20201014::132438: Head 1: Stopping Scan Operation
20201014::132440: Head 2: ProcessingMgr stopped all worker threads.
20201014::132440: Head 2:       Stop finished, may now recover.
20201014::132442: Head 1: Eye Safe Optical Filter State there 8, not there 22, transition 1
20201014::132442: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::132442: Head 1: Eye Safe Optical Filter check Passed
20201014::132442: Head 2: Eye Safe Optical Filter check Passed
20201014::132500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132500: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 484
20201014::132500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132508: Head 1: ProcessingMgr stopped all worker threads.
20201014::132509: Head 1:       Stop finished, may now recover.
20201014::132530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 18C, Laser 21.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132530: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 539
20201014::132530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 18C, Laser 21.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132600: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 594
20201014::132600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 19C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 21.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132630: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.2psu, index 1.34, Packet 649
20201014::132630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 26C, OCB 21%, OPB 20C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132700: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.2psu, index 1.34, Packet 704
20201014::132700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132730: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.2psu, index 1.34, Packet 759
20201014::132730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 20C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132800: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 814
20201014::132800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132830: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 869
20201014::132830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 22.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 19C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132900: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 924
20201014::132900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 24.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 19C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::132930: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 979
20201014::132930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 20C, Laser 24.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133000: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1034
20201014::133000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 21C, Laser 24.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133030: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1089
20201014::133030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 20%, OPB 21C, Laser 25.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133100: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1144
20201014::133100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 23.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 25.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 24.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133130: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1199
20201014::133130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 27C, OCB 21%, OPB 21C, Laser 25.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 24.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1254
20201014::133200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 25.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1309
20201014::133230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133300: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1364
20201014::133300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133330: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1419
20201014::133330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133400: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1474
20201014::133400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 20C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 21C, Laser 26.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133430: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1529
20201014::133430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133500: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1584
20201014::133500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 25.0C, Dig 30.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133530: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1639
20201014::133530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133538: GUI: Live mode ON.
20201014::133538: GUI: Requesing START operation, Head 1
20201014::133538: GUI: Requesing START operation, Head 2
20201014::133538: Head 2: Received request: START
20201014::133538: Head 1: Received request: START
20201014::133539: Head 2: Starting Scan Operation
20201014::133539: Head 1: Starting Scan Operation
20201014::133540: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20201014::133540: Head 1: Eye Safe Optical Filter check Passed
20201014::133542: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::133543: Head 2: Eye Safe Optical Filter check Passed
20201014::133545: Head 1: Configured for WATER Processing
20201014::133545: Head 1: Configured for WATER Processing
20201014::133545: Head 1: Configured for WATER Processing
20201014::133545: Head 1: Configured for WATER Processing
20201014::133546: Head 1: Configured for WATER Processing
20201014::133546: Head 1: Configured for WATER Processing
20201014::133546: Head 1: Configured for WATER Processing
20201014::133547: Head 1: Configured for WATER Processing
20201014::133547: Head 1: Configured for WATER Processing
20201014::133547: Head 1: Configured for WATER Processing
20201014::133548: Head 1: Configured for WATER Processing
20201014::133548: Head 1: Configured for WATER Processing
20201014::133548: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_133547_wf.raa
20201014::133548: Head 1: Configured for WATER Processing
20201014::133548: Head 1: Configured for WATER Processing
20201014::133549: Head 1: Configured for WATER Processing
20201014::133549: Head 1: Configured for WATER Processing
20201014::133549: Head 1: Configured for WATER Processing
20201014::133550: Head 1: Configured for WATER Processing
20201014::133550: Head 1: Configured for WATER Processing
20201014::133550: Head 1: Configured for WATER Processing
20201014::133556: GUI: Archiving data to file --> C:\Data\202010131d1\20201014_133557_wf.raa
20201014::133558: GUI: Live mode ON.
20201014::133558: GUI: Requesing STOP operation, Head 2
20201014::133558: GUI: Requesing STOP operation, Head 1
20201014::133558: Head 1: Received request: STOP
20201014::133558: Head 2: Received request: STOP
20201014::133558: Head 1: Stopping Scan Operation
20201014::133600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 1
20201014::133600: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1694
20201014::133600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133601: Head 1: ProcessingMgr stopped all worker threads.
20201014::133601: Head 1:       Stop finished, may now recover.
20201014::133606: Head 1: Eye Safe Optical Filter State there 9, not there 21, transition 1
20201014::133606: Head 1: Eye Safe Optical Filter check Passed
20201014::133611: Head 2: Configured for WATER Processing
20201014::133612: Head 2: Configured for WATER Processing
20201014::133612: Head 2: Configured for WATER Processing
20201014::133612: Head 2: Configured for WATER Processing
20201014::133612: Head 2: Configured for WATER Processing
20201014::133613: Head 2: Configured for WATER Processing
20201014::133613: Head 2: Configured for WATER Processing
20201014::133613: Head 2: Configured for WATER Processing
20201014::133614: Head 2: Configured for WATER Processing
20201014::133614: Head 2: Configured for WATER Processing
20201014::133614: Head 2: Configured for WATER Processing
20201014::133615: Head 2: Configured for WATER Processing
20201014::133615: Head 2: Configured for WATER Processing
20201014::133615: Head 2: Configured for WATER Processing
20201014::133615: Head 2: Configured for WATER Processing
20201014::133616: Head 2: Configured for WATER Processing
20201014::133616: Head 2: Configured for WATER Processing
20201014::133616: Head 2: Configured for WATER Processing
20201014::133617: Head 2: Configured for WATER Processing
20201014::133617: Head 2: Configured for WATER Processing
20201014::133617: Head 2: Stopping Scan Operation
20201014::133618: Head 2: ProcessingMgr stopped all worker threads.
20201014::133618: Head 2:       Stop finished, may now recover.
20201014::133618: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::133619: Head 2: Eye Safe Optical Filter check Passed
20201014::133630: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1749
20201014::133630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 27.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133700: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1804
20201014::133700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133730: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 1859
20201014::133730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 26.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133800: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1914
20201014::133800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 20%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133830: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 1969
20201014::133830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 22C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 21C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133900: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 2024
20201014::133900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 23C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133930: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2078
20201014::133930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 23C, Laser 28.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::133930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134000: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.1dbar, CTD 0.1psu, index 1.34, Packet 2133
20201014::134000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 21%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134030: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 15.9C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2188
20201014::134030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134059: Head 1: Time Synchronization: 2020.10.14   13:41:00::0016
20201014::134100: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2243
20201014::134100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134130: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2298
20201014::134130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2353
20201014::134200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 27.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2408
20201014::134230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 29C, OCB 21%, OPB 22C, Laser 28.0C, Dig 39.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134300: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 20.2%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 16.0C, CTD 2.0dbar, CTD 0.1psu, index 1.34, Packet 2445
20201014::134300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 28C, OCB 22%, OPB 23C, Laser 29.0C, Dig 34.0C, Scan Az fault 0, gain 0, laser state 0
20201014::134301: GUI: Lost Communications with Sensor 1.
20201014::134301: GUI: Lost Communications with Head 2.
20201014::134311: GUI: Attempting Communications with Head 2...
20201014::134313: GUI: Attempting Communications with Head 1...
20201014::150612: GUI: Established Communications with Head 2.
20201014::150613: Head 2: Initializing Communications with GUI ...
20201014::150613: Head 2: Communications Established.
20201014::150614: GUI: Established Communications with Head 1.
20201014::150614: Head 2: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201014::150615: Head 2: Connection Established with the GUI.
20201014::150615: Head 1: Initializing Communications with GUI ...
20201014::150615: Head 2: Initializing Subsystems, standby ...
20201014::150615: Head 2: Initializing Hardware, Stand by ...
20201014::150616: Head 1: Communications Established.
20201014::150617: Head 1: 3D at Depth WiSSL Sensor, Firmware Version 01.15.01
20201014::150617: Head 1: Connection Established with the GUI.
20201014::150618: Head 1: Initializing Subsystems, standby ...
20201014::150618: Head 1: Initializing Hardware, Stand by ...
20201014::150628: Head 1: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201014::150628: Head 1: NtQuery - testing 1 ...
20201014::150629: Head 1: clock resolution: 10
20201014::150629: Head 1: NtQuery - testing 2, after setting max res ...
20201014::150629: Head 1: clock resolution: 10
20201014::150630: Head 1: Initializing Optics Electronics ...
20201014::150630: System NOT Initialized, Gain 0, Elec PB 17.4C, Elec PB 33.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 51
20201014::150630: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 0.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150630: Head #1, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150630: Head 1: Power Laser Controller
20201014::150633: Head 2: NtQuery, minRes 156001, maxRes 5000, curRec 100000
20201014::150633: Head 2: NtQuery - testing 1 ...
20201014::150633: Head 2: clock resolution: 10
20201014::150634: Head 2: NtQuery - testing 2, after setting max res ...
20201014::150634: Head 1: Power Scanner Controller
20201014::150634: Head 2: clock resolution: 10
20201014::150634: Head 2: Initializing Optics Electronics ...
20201014::150635: Head 2: Power Laser Controller
20201014::150636: Head 1: Power OPTO Sensor
20201014::150638: Head 2: Power Scanner Controller
20201014::150641: Head 2: Power OPTO Sensor
20201014::150656: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::150656: Head 1: Eye Safe Optical Filter check Passed
20201014::150656: Head 1:    Optics Electronics Initializing Complete, firmware: E.10
20201014::150657: Head 1: Initializing Time Sync Subsystem.
20201014::150657: Head 1: Initializing CTD Subsystem.
20201014::150657: Head 1: CTD Initialization Successful
20201014::150658: Head 1: Wide Swath Sensor Head 1 Initialization Complete
20201014::150658: Head 1: Time Sync UDP started, waiting for sync...
20201014::150658: Head 1: Attempting CTD Ethernet connection with ROV...
20201014::150659: Head 1: Time Synchronization Achieved: 2020.10.14   15:07:00::0014
20201014::150700: Head #2, Init state OFF, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 0, OCB 0C, OCB 0%, OPB 0C, Laser 0.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150700: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 33.6%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 106
20201014::150700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 32%, OPB 13C, Laser 0.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150701: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::150701: Head 2: Eye Safe Optical Filter check Passed
20201014::150701: Head 2:    Optics Electronics Initializing Complete, firmware: E.10
20201014::150702: Head 2: Initializing Time Sync Subsystem.
20201014::150702: Head 2: Initializing CTD Subsystem.
20201014::150702: Head 2: CTD Initialization Successful
20201014::150702: Head 2: Wide Swath Sensor Head 2 Initialization Complete
20201014::150703: Head 2: Time Sync UDP started, waiting for sync...
20201014::150703: Head 2: Attempting CTD Ethernet connection with ROV...
20201014::150704: Head 2: Time Synchronization Achieved: 2020.10.14   15:07:05::0013
20201014::150730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 29%, OPB 12C, Laser 13.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150730: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 0.0C, CTD 0.0dbar, CTD 0.0psu, index 1.33, Packet 161
20201014::150730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 30%, OPB 13C, Laser 14.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150734: Head 1: CTD Ethernet connection established.
20201014::150734: Head 2: CTD Ethernet connection established.
20201014::150800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 27%, OPB 12C, Laser 13.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150800: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 29.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.9C, CTD 103.4dbar, CTD 33.9psu, index 1.34, Packet 216
20201014::150800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 27%, OPB 13C, Laser 15.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150830: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.9C, CTD 98.7dbar, CTD 33.9psu, index 1.34, Packet 271
20201014::150830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 13C, Laser 14.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 26%, OPB 13C, Laser 15.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 13C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150900: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.9C, CTD 93.8dbar, CTD 33.9psu, index 1.34, Packet 326
20201014::150900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 25%, OPB 13C, Laser 16.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150930: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 94.7dbar, CTD 33.9psu, index 1.34, Packet 381
20201014::150930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 24%, OPB 14C, Laser 16.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::150930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 15.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151000: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 98.0dbar, CTD 33.9psu, index 1.34, Packet 436
20201014::151000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 16.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151030: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 97.4dbar, CTD 33.9psu, index 1.34, Packet 490
20201014::151030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151100: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 97.2dbar, CTD 33.9psu, index 1.34, Packet 545
20201014::151100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 17.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151130: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 97.3dbar, CTD 33.9psu, index 1.34, Packet 600
20201014::151130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 97.3dbar, CTD 33.9psu, index 1.34, Packet 655
20201014::151200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 10.0C, CTD 98.5dbar, CTD 33.9psu, index 1.34, Packet 710
20201014::151230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151300: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.9C, CTD 108.1dbar, CTD 33.9psu, index 1.34, Packet 765
20201014::151300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151330: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 113.1dbar, CTD 33.9psu, index 1.34, Packet 820
20201014::151330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151400: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 117.4dbar, CTD 33.9psu, index 1.34, Packet 875
20201014::151400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151430: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.7C, CTD 124.4dbar, CTD 33.9psu, index 1.34, Packet 930
20201014::151430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151500: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.6C, CTD 132.3dbar, CTD 34.0psu, index 1.34, Packet 985
20201014::151500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151530: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.4C, CTD 136.1dbar, CTD 33.9psu, index 1.34, Packet 1040
20201014::151530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151559: Head 2: Time Synchronization: 2020.10.14   15:16:00::0015
20201014::151600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151600: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.4C, CTD 139.5dbar, CTD 34.0psu, index 1.34, Packet 1095
20201014::151600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151630: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 142.2dbar, CTD 34.0psu, index 1.34, Packet 1150
20201014::151630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151700: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 144.2dbar, CTD 34.0psu, index 1.34, Packet 1205
20201014::151700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151730: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 144.3dbar, CTD 34.0psu, index 1.34, Packet 1260
20201014::151730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151800: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.4C, CTD 147.8dbar, CTD 34.0psu, index 1.34, Packet 1315
20201014::151800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151830: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.3C, CTD 155.5dbar, CTD 34.0psu, index 1.34, Packet 1370
20201014::151830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151900: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.2C, CTD 162.5dbar, CTD 34.0psu, index 1.34, Packet 1425
20201014::151900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151930: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 172.0dbar, CTD 34.0psu, index 1.34, Packet 1480
20201014::151930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::151959: Head 2: Time Synchronization: 2020.10.14   15:20:00::0014
20201014::152000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152000: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.1C, CTD 183.6dbar, CTD 34.1psu, index 1.34, Packet 1535
20201014::152000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152030: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 9.0C, CTD 201.6dbar, CTD 34.1psu, index 1.34, Packet 1590
20201014::152030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 15C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152100: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.8C, CTD 219.9dbar, CTD 34.1psu, index 1.34, Packet 1645
20201014::152100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 15C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152130: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.7C, CTD 233.7dbar, CTD 34.1psu, index 1.34, Packet 1700
20201014::152130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 14C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 15C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152200: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.5C, CTD 246.7dbar, CTD 34.1psu, index 1.34, Packet 1755
20201014::152200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152230: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.4C, CTD 259.9dbar, CTD 34.2psu, index 1.34, Packet 1810
20201014::152230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152300: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.3C, CTD 272.2dbar, CTD 34.2psu, index 1.34, Packet 1865
20201014::152300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152330: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 279.4dbar, CTD 34.1psu, index 1.34, Packet 1920
20201014::152330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152400: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 290.0dbar, CTD 34.2psu, index 1.34, Packet 1975
20201014::152400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 21%, OPB 13C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152430: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 8.0C, CTD 301.7dbar, CTD 34.2psu, index 1.34, Packet 2030
20201014::152430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152500: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.9C, CTD 313.7dbar, CTD 34.2psu, index 1.34, Packet 2085
20201014::152500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152530: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.5%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.8C, CTD 325.1dbar, CTD 34.2psu, index 1.34, Packet 2140
20201014::152530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152559: Head 1: Time Synchronization: 2020.10.14   15:26:00::0015
20201014::152600: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.7C, CTD 337.2dbar, CTD 34.2psu, index 1.34, Packet 2195
20201014::152600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152630: System  Initialized, Gain 1, Elec PB 22.6C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.6C, CTD 349.1dbar, CTD 34.2psu, index 1.34, Packet 2250
20201014::152630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152700: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.5C, CTD 365.8dbar, CTD 34.2psu, index 1.34, Packet 2305
20201014::152700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152730: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.3C, CTD 386.9dbar, CTD 34.2psu, index 1.34, Packet 2360
20201014::152730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 23C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152800: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.2C, CTD 407.9dbar, CTD 34.2psu, index 1.34, Packet 2415
20201014::152800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152830: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 7.0C, CTD 425.6dbar, CTD 34.2psu, index 1.34, Packet 2470
20201014::152830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152900: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.8C, CTD 442.7dbar, CTD 34.2psu, index 1.34, Packet 2525
20201014::152900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::152930: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.7C, CTD 459.7dbar, CTD 34.2psu, index 1.34, Packet 2579
20201014::152930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153000: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.6C, CTD 476.9dbar, CTD 34.2psu, index 1.34, Packet 2634
20201014::153000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153030: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.4C, CTD 494.1dbar, CTD 34.3psu, index 1.34, Packet 2689
20201014::153030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 13C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153100: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.2C, CTD 510.4dbar, CTD 34.3psu, index 1.34, Packet 2744
20201014::153100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 14C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153130: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 6.0C, CTD 527.9dbar, CTD 34.3psu, index 1.34, Packet 2799
20201014::153130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153200: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.9C, CTD 545.2dbar, CTD 34.3psu, index 1.34, Packet 2854
20201014::153200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153230: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.8C, CTD 562.7dbar, CTD 34.3psu, index 1.34, Packet 2909
20201014::153230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153300: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.6C, CTD 580.1dbar, CTD 34.3psu, index 1.34, Packet 2964
20201014::153300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153330: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 597.6dbar, CTD 34.3psu, index 1.34, Packet 3019
20201014::153330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153400: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 614.8dbar, CTD 34.3psu, index 1.34, Packet 3074
20201014::153400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 22C, OCB 22%, OPB 12C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153430: System  Initialized, Gain 1, Elec PB 21.7C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.4C, CTD 632.8dbar, CTD 34.3psu, index 1.34, Packet 3129
20201014::153430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153500: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.3C, CTD 650.0dbar, CTD 34.3psu, index 1.34, Packet 3183
20201014::153500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 22.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 12C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153530: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 667.5dbar, CTD 34.3psu, index 1.34, Packet 3238
20201014::153530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153600: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.1C, CTD 684.0dbar, CTD 34.3psu, index 1.34, Packet 3293
20201014::153600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 13C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153630: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 699.9dbar, CTD 34.3psu, index 1.34, Packet 3348
20201014::153630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 21.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153700: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 716.5dbar, CTD 34.3psu, index 1.34, Packet 3403
20201014::153700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153730: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 5.0C, CTD 733.2dbar, CTD 34.4psu, index 1.34, Packet 3458
20201014::153730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 22%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153800: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.9C, CTD 749.9dbar, CTD 34.4psu, index 1.34, Packet 3512
20201014::153800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153830: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 766.6dbar, CTD 34.4psu, index 1.34, Packet 3567
20201014::153830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153900: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 783.2dbar, CTD 34.4psu, index 1.34, Packet 3622
20201014::153900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::153930: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 800.1dbar, CTD 34.4psu, index 1.34, Packet 3677
20201014::153930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154000: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 817.6dbar, CTD 34.4psu, index 1.34, Packet 3732
20201014::154000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 11C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154030: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 835.0dbar, CTD 34.4psu, index 1.34, Packet 3787
20201014::154030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154100: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 852.7dbar, CTD 34.4psu, index 1.34, Packet 3842
20201014::154100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 21C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154130: System  Initialized, Gain 1, Elec PB 19.6C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 871.0dbar, CTD 34.4psu, index 1.34, Packet 3897
20201014::154130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 21.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154200: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 889.1dbar, CTD 34.4psu, index 1.34, Packet 3952
20201014::154200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 12C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 20.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154230: System  Initialized, Gain 1, Elec PB 20.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 906.8dbar, CTD 34.4psu, index 1.34, Packet 4007
20201014::154230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154300: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 924.6dbar, CTD 34.4psu, index 1.34, Packet 4062
20201014::154300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154330: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 941.6dbar, CTD 34.4psu, index 1.34, Packet 4117
20201014::154330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154400: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 959.0dbar, CTD 34.4psu, index 1.34, Packet 4172
20201014::154400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154430: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 976.5dbar, CTD 34.4psu, index 1.34, Packet 4227
20201014::154430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154459: Head 1: Time Synchronization: 2020.10.14   15:45:00::0015
20201014::154500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154500: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 993.8dbar, CTD 34.4psu, index 1.34, Packet 4282
20201014::154500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154530: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1011.3dbar, CTD 34.4psu, index 1.34, Packet 4337
20201014::154530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154600: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1028.0dbar, CTD 34.4psu, index 1.34, Packet 4392
20201014::154600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154630: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 1047.3dbar, CTD 34.4psu, index 1.34, Packet 4447
20201014::154630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 19.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154700: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.9C, CTD 1065.1dbar, CTD 34.5psu, index 1.34, Packet 4502
20201014::154700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154730: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1080.1dbar, CTD 34.5psu, index 1.34, Packet 4557
20201014::154730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154800: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1096.7dbar, CTD 34.5psu, index 1.34, Packet 4612
20201014::154800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 20C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154830: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1117.5dbar, CTD 34.5psu, index 1.34, Packet 4667
20201014::154830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154900: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1138.2dbar, CTD 34.5psu, index 1.34, Packet 4722
20201014::154900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 10C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::154930: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1158.4dbar, CTD 34.5psu, index 1.34, Packet 4777
20201014::154930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155000: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1177.9dbar, CTD 34.5psu, index 1.34, Packet 4832
20201014::155000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155030: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1196.2dbar, CTD 34.5psu, index 1.34, Packet 4887
20201014::155030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 11C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155100: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.3dbar, CTD 34.5psu, index 1.34, Packet 4942
20201014::155100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155130: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1225.2dbar, CTD 34.5psu, index 1.34, Packet 4997
20201014::155130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155200: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 5052
20201014::155200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155230: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1234.6dbar, CTD 34.5psu, index 1.34, Packet 5107
20201014::155230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155300: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1233.7dbar, CTD 34.5psu, index 1.34, Packet 5162
20201014::155300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155330: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1234.9dbar, CTD 34.5psu, index 1.34, Packet 5217
20201014::155330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155400: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1238.0dbar, CTD 34.5psu, index 1.34, Packet 5272
20201014::155400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155430: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1237.6dbar, CTD 34.5psu, index 1.34, Packet 5327
20201014::155430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155500: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1238.5dbar, CTD 34.5psu, index 1.34, Packet 5382
20201014::155500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 19C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155530: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1240.8dbar, CTD 34.5psu, index 1.34, Packet 5437
20201014::155530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155600: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1241.8dbar, CTD 34.5psu, index 1.34, Packet 5492
20201014::155600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155630: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.4dbar, CTD 34.5psu, index 1.34, Packet 5547
20201014::155630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155700: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.3dbar, CTD 34.5psu, index 1.34, Packet 5602
20201014::155700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155730: System  Initialized, Gain 1, Elec PB 18.2C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 5657
20201014::155730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155800: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.8dbar, CTD 34.5psu, index 1.34, Packet 5712
20201014::155800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155830: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 24.9%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1244.3dbar, CTD 34.5psu, index 1.34, Packet 5767
20201014::155830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155900: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1244.8dbar, CTD 34.5psu, index 1.34, Packet 5821
20201014::155900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::155930: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1245.2dbar, CTD 34.5psu, index 1.34, Packet 5876
20201014::155930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160000: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1244.7dbar, CTD 34.5psu, index 1.34, Packet 5931
20201014::160000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 19.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 9C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160030: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1245.7dbar, CTD 34.5psu, index 1.34, Packet 5986
20201014::160030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160100: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1244.1dbar, CTD 34.5psu, index 1.34, Packet 6041
20201014::160100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160130: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.8dbar, CTD 34.5psu, index 1.34, Packet 6096
20201014::160130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160200: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.1dbar, CTD 34.5psu, index 1.34, Packet 6151
20201014::160200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160230: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.8dbar, CTD 34.5psu, index 1.34, Packet 6205
20201014::160230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160300: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.4dbar, CTD 34.5psu, index 1.34, Packet 6260
20201014::160300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160330: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1241.6dbar, CTD 34.5psu, index 1.34, Packet 6315
20201014::160330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160400: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1241.8dbar, CTD 34.5psu, index 1.34, Packet 6370
20201014::160400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160430: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 6425
20201014::160430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160500: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.9dbar, CTD 34.5psu, index 1.34, Packet 6479
20201014::160500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160530: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1242.4dbar, CTD 34.5psu, index 1.34, Packet 6534
20201014::160530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160600: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1243.0dbar, CTD 34.5psu, index 1.34, Packet 6588
20201014::160600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160630: System  Initialized, Gain 1, Elec PB 17.4C, Elec PB 26.0%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.4dbar, CTD 34.5psu, index 1.34, Packet 6643
20201014::160630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160700: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.0dbar, CTD 34.5psu, index 1.34, Packet 6698
20201014::160700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160729: GUI: Live mode ON.
20201014::160729: GUI: Requesing START operation, Head 2
20201014::160729: GUI: Requesing START operation, Head 1
20201014::160729: Head 2: Received request: START
20201014::160729: Head 1: Received request: START
20201014::160729: Head 2: Starting Scan Operation
20201014::160729: Head 1: Starting Scan Operation
20201014::160730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 28.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160730: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.0dbar, CTD 34.5psu, index 1.34, Packet 6753
20201014::160730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 22.0C, Scan Az fault 0, gain 0, laser state 0
20201014::160730: Head 1: Eye Safe Optical Filter State there 7, not there 23, transition 1
20201014::160731: Head 1: Eye Safe Optical Filter check Passed
20201014::160733: Head 2: Eye Safe Optical Filter State there 6, not there 24, transition 1
20201014::160733: Head 2: Eye Safe Optical Filter check Passed
20201014::160735: Head 1: Configured for WATER Processing
20201014::160735: Head 1: Configured for WATER Processing
20201014::160736: Head 1: Configured for WATER Processing
20201014::160736: Head 1: Configured for WATER Processing
20201014::160736: Head 1: Configured for WATER Processing
20201014::160737: Head 1: Configured for WATER Processing
20201014::160737: Head 1: Configured for WATER Processing
20201014::160737: Head 1: Configured for WATER Processing
20201014::160738: Head 1: Configured for WATER Processing
20201014::160738: Head 1: Configured for WATER Processing
20201014::160738: Head 1: Configured for WATER Processing
20201014::160738: Head 1: Configured for WATER Processing
20201014::160739: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160737_wf.raa
20201014::160739: Head 1: Configured for WATER Processing
20201014::160739: Head 1: Configured for WATER Processing
20201014::160739: Head 1: Configured for WATER Processing
20201014::160740: Head 1: Configured for WATER Processing
20201014::160740: Head 1: Configured for WATER Processing
20201014::160740: Head 1: Configured for WATER Processing
20201014::160741: Head 1: Configured for WATER Processing
20201014::160741: Head 1: Configured for WATER Processing
20201014::160746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160747_wf.raa
20201014::160757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160757_wf.raa
20201014::160759: Head 1: Time Synchronization: 2020.10.14   16:08:00::0015
20201014::160800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 1
20201014::160800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.0dbar, CTD 34.5psu, index 1.34, Packet 6808
20201014::160800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 18.0C, Dig 21.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160807_wf.raa
20201014::160812: Head 2: Configured for WATER Processing
20201014::160812: Head 2: Configured for WATER Processing
20201014::160813: Head 2: Configured for WATER Processing
20201014::160813: Head 2: Configured for WATER Processing
20201014::160813: Head 2: Configured for WATER Processing
20201014::160813: Head 2: Configured for WATER Processing
20201014::160814: Head 2: Configured for WATER Processing
20201014::160814: Head 2: Configured for WATER Processing
20201014::160814: Head 2: Configured for WATER Processing
20201014::160815: Head 2: Configured for WATER Processing
20201014::160815: Head 2: Configured for WATER Processing
20201014::160815: Head 2: Configured for WATER Processing
20201014::160816: Head 2: Configured for WATER Processing
20201014::160816: Head 2: Configured for WATER Processing
20201014::160816: Head 2: Configured for WATER Processing
20201014::160816: Head 2: Configured for WATER Processing
20201014::160817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160817_wf.raa
20201014::160817: Head 2: Configured for WATER Processing
20201014::160817: Head 2: Configured for WATER Processing
20201014::160817: Head 2: Configured for WATER Processing
20201014::160818: Head 2: Configured for WATER Processing
20201014::160826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160827_wf.raa
20201014::160830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.1dbar, CTD 34.5psu, index 1.34, Packet 6863
20201014::160830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 17.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 21.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160837_wf.raa
20201014::160846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160847_wf.raa
20201014::160856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160857_wf.raa
20201014::160900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 6917
20201014::160900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160907_wf.raa
20201014::160916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160917_wf.raa
20201014::160926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160927_wf.raa
20201014::160930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 6972
20201014::160930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 22.0C, Scan Az fault 0, gain 3, laser state 1
20201014::160936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160937_wf.raa
20201014::160946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160947_wf.raa
20201014::160956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_160957_wf.raa
20201014::161000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 7027
20201014::161000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161007_wf.raa
20201014::161016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161017_wf.raa
20201014::161026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161027_wf.raa
20201014::161030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1243.2dbar, CTD 34.5psu, index 1.34, Packet 7083
20201014::161030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 23.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161037_wf.raa
20201014::161046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161047_wf.raa
20201014::161056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161057_wf.raa
20201014::161100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.2dbar, CTD 34.5psu, index 1.34, Packet 7138
20201014::161100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161107_wf.raa
20201014::161116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161117_wf.raa
20201014::161126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161127_wf.raa
20201014::161130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1240.9dbar, CTD 34.5psu, index 1.34, Packet 7193
20201014::161130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161137_wf.raa
20201014::161146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161147_wf.raa
20201014::161156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161157_wf.raa
20201014::161200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 18C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1239.2dbar, CTD 34.5psu, index 1.34, Packet 7248
20201014::161200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161207_wf.raa
20201014::161216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161217_wf.raa
20201014::161226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161227_wf.raa
20201014::161230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1237.9dbar, CTD 34.5psu, index 1.34, Packet 7303
20201014::161230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 10C, Laser 20.0C, Dig 24.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 23%, OPB 8C, Laser 18.0C, Dig 29.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161237_wf.raa
20201014::161246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161247_wf.raa
20201014::161256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161257_wf.raa
20201014::161300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 23%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.9dbar, CTD 34.5psu, index 1.34, Packet 7359
20201014::161300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161307_wf.raa
20201014::161316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161317_wf.raa
20201014::161326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161327_wf.raa
20201014::161330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.4dbar, CTD 34.5psu, index 1.34, Packet 7414
20201014::161330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161337_wf.raa
20201014::161346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161347_wf.raa
20201014::161356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161357_wf.raa
20201014::161400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.1dbar, CTD 34.5psu, index 1.34, Packet 7469
20201014::161400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161407_wf.raa
20201014::161416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161417_wf.raa
20201014::161426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161427_wf.raa
20201014::161430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.8dbar, CTD 34.5psu, index 1.34, Packet 7524
20201014::161430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161437_wf.raa
20201014::161446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161447_wf.raa
20201014::161456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161457_wf.raa
20201014::161459: Head 1: Time Synchronization: 2020.10.14   16:15:00::0014
20201014::161500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.3dbar, CTD 34.5psu, index 1.34, Packet 7579
20201014::161500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161507_wf.raa
20201014::161516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161517_wf.raa
20201014::161526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161527_wf.raa
20201014::161530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.1dbar, CTD 34.5psu, index 1.34, Packet 7633
20201014::161530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161537_wf.raa
20201014::161546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161547_wf.raa
20201014::161556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161557_wf.raa
20201014::161559: Head 2: Time Synchronization: 2020.10.14   16:16:00::0014
20201014::161600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.9dbar, CTD 34.5psu, index 1.34, Packet 7688
20201014::161600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161607_wf.raa
20201014::161616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161617_wf.raa
20201014::161626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161627_wf.raa
20201014::161630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.8dbar, CTD 34.5psu, index 1.34, Packet 7743
20201014::161630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161637_wf.raa
20201014::161646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161647_wf.raa
20201014::161656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161657_wf.raa
20201014::161700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.4dbar, CTD 34.5psu, index 1.34, Packet 7798
20201014::161700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161707_wf.raa
20201014::161716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161717_wf.raa
20201014::161726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161727_wf.raa
20201014::161730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1231.4dbar, CTD 34.5psu, index 1.34, Packet 7853
20201014::161730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161737_wf.raa
20201014::161746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161747_wf.raa
20201014::161756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161757_wf.raa
20201014::161759: Head 1: Time Synchronization: 2020.10.14   16:18:00::0014
20201014::161800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1229.5dbar, CTD 34.5psu, index 1.34, Packet 7907
20201014::161800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161807_wf.raa
20201014::161816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161817_wf.raa
20201014::161826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161827_wf.raa
20201014::161830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 30.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 7963
20201014::161830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 25.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161837_wf.raa
20201014::161846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161847_wf.raa
20201014::161856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161857_wf.raa
20201014::161900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1224.8dbar, CTD 34.5psu, index 1.34, Packet 8018
20201014::161900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161907_wf.raa
20201014::161916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161917_wf.raa
20201014::161926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161927_wf.raa
20201014::161930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1222.6dbar, CTD 34.5psu, index 1.34, Packet 8073
20201014::161930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::161936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161937_wf.raa
20201014::161946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161947_wf.raa
20201014::161956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_161957_wf.raa
20201014::161959: Head 1: Time Synchronization: 2020.10.14   16:20:00::0014
20201014::162000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1219.9dbar, CTD 34.5psu, index 1.34, Packet 8128
20201014::162000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162007_wf.raa
20201014::162016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162017_wf.raa
20201014::162026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162027_wf.raa
20201014::162030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 19.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.8dbar, CTD 34.5psu, index 1.34, Packet 8183
20201014::162030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162037_wf.raa
20201014::162046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162047_wf.raa
20201014::162056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162057_wf.raa
20201014::162100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.1dbar, CTD 34.5psu, index 1.34, Packet 8238
20201014::162100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162107_wf.raa
20201014::162116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162117_wf.raa
20201014::162126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162127_wf.raa
20201014::162130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.9dbar, CTD 34.5psu, index 1.34, Packet 8294
20201014::162130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162137_wf.raa
20201014::162146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162147_wf.raa
20201014::162156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162157_wf.raa
20201014::162159: Head 1: Time Synchronization: 2020.10.14   16:22:00::0016
20201014::162200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.5dbar, CTD 34.5psu, index 1.34, Packet 8349
20201014::162200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162207_wf.raa
20201014::162216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162217_wf.raa
20201014::162226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162227_wf.raa
20201014::162230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.4dbar, CTD 34.5psu, index 1.34, Packet 8403
20201014::162230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162237_wf.raa
20201014::162246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162247_wf.raa
20201014::162256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162257_wf.raa
20201014::162300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.1dbar, CTD 34.5psu, index 1.34, Packet 8459
20201014::162300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162307_wf.raa
20201014::162316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162317_wf.raa
20201014::162326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162327_wf.raa
20201014::162330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.2dbar, CTD 34.5psu, index 1.34, Packet 8514
20201014::162330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162337_wf.raa
20201014::162346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162347_wf.raa
20201014::162356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162357_wf.raa
20201014::162359: Head 1: Time Synchronization: 2020.10.14   16:24:00::0014
20201014::162400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.9dbar, CTD 34.5psu, index 1.34, Packet 8569
20201014::162400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162407_wf.raa
20201014::162416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162417_wf.raa
20201014::162426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162427_wf.raa
20201014::162430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.3dbar, CTD 34.5psu, index 1.34, Packet 8624
20201014::162430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162437_wf.raa
20201014::162446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162447_wf.raa
20201014::162456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162457_wf.raa
20201014::162459: Head 1: Time Synchronization: 2020.10.14   16:25:00::0014
20201014::162500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.1dbar, CTD 34.5psu, index 1.34, Packet 8679
20201014::162500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162507_wf.raa
20201014::162516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162517_wf.raa
20201014::162527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162527_wf.raa
20201014::162530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1220.2dbar, CTD 34.5psu, index 1.34, Packet 8734
20201014::162530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162537_wf.raa
20201014::162546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162547_wf.raa
20201014::162556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162557_wf.raa
20201014::162600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1222.9dbar, CTD 34.5psu, index 1.34, Packet 8789
20201014::162600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162607_wf.raa
20201014::162616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162617_wf.raa
20201014::162626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162627_wf.raa
20201014::162630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 8844
20201014::162630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162637_wf.raa
20201014::162646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162647_wf.raa
20201014::162656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162657_wf.raa
20201014::162659: Head 1: Time Synchronization: 2020.10.14   16:27:00::0018
20201014::162700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 8899
20201014::162700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162707_wf.raa
20201014::162716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162717_wf.raa
20201014::162726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162727_wf.raa
20201014::162730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.6dbar, CTD 34.5psu, index 1.34, Packet 8954
20201014::162730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162737_wf.raa
20201014::162746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162747_wf.raa
20201014::162756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162757_wf.raa
20201014::162759: Head 1: Time Synchronization: 2020.10.14   16:28:00::0014
20201014::162800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.4dbar, CTD 34.5psu, index 1.34, Packet 9009
20201014::162800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162807_wf.raa
20201014::162816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162817_wf.raa
20201014::162826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162827_wf.raa
20201014::162830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 9065
20201014::162830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162837_wf.raa
20201014::162846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162847_wf.raa
20201014::162856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162857_wf.raa
20201014::162900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.7dbar, CTD 34.5psu, index 1.34, Packet 9120
20201014::162900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162907_wf.raa
20201014::162916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162917_wf.raa
20201014::162926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162927_wf.raa
20201014::162930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.8dbar, CTD 34.5psu, index 1.34, Packet 9175
20201014::162930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::162936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162937_wf.raa
20201014::162946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162947_wf.raa
20201014::162956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_162957_wf.raa
20201014::162959: Head 2: Time Synchronization: 2020.10.14   16:30:00::0015
20201014::163000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.1dbar, CTD 34.5psu, index 1.34, Packet 9230
20201014::163000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163007_wf.raa
20201014::163016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163017_wf.raa
20201014::163026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163027_wf.raa
20201014::163030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.3dbar, CTD 34.5psu, index 1.34, Packet 9285
20201014::163030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163037_wf.raa
20201014::163046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163047_wf.raa
20201014::163056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163057_wf.raa
20201014::163100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 9341
20201014::163100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163107_wf.raa
20201014::163116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163117_wf.raa
20201014::163126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163127_wf.raa
20201014::163130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.2dbar, CTD 34.5psu, index 1.34, Packet 9396
20201014::163130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163137_wf.raa
20201014::163146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163147_wf.raa
20201014::163156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163157_wf.raa
20201014::163159: Head 1: Time Synchronization: 2020.10.14   16:32:00::0014
20201014::163200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.9dbar, CTD 34.5psu, index 1.34, Packet 9451
20201014::163200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163207_wf.raa
20201014::163216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163217_wf.raa
20201014::163226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163227_wf.raa
20201014::163230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.0dbar, CTD 34.5psu, index 1.34, Packet 9507
20201014::163230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163237_wf.raa
20201014::163246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163247_wf.raa
20201014::163256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163257_wf.raa
20201014::163300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.0dbar, CTD 34.5psu, index 1.34, Packet 9563
20201014::163300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163307_wf.raa
20201014::163316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163317_wf.raa
20201014::163326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163327_wf.raa
20201014::163330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.5dbar, CTD 34.5psu, index 1.34, Packet 9617
20201014::163330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163337_wf.raa
20201014::163346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163347_wf.raa
20201014::163356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163357_wf.raa
20201014::163359: Head 1: Time Synchronization: 2020.10.14   16:34:00::0014
20201014::163400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.1dbar, CTD 34.5psu, index 1.34, Packet 9672
20201014::163400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163407_wf.raa
20201014::163416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163417_wf.raa
20201014::163426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163427_wf.raa
20201014::163430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.4dbar, CTD 34.5psu, index 1.34, Packet 9727
20201014::163430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163437_wf.raa
20201014::163446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163447_wf.raa
20201014::163456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163457_wf.raa
20201014::163459: Head 1: Time Synchronization: 2020.10.14   16:35:00::0014
20201014::163500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1243.0dbar, CTD 34.5psu, index 1.34, Packet 9782
20201014::163500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163507_wf.raa
20201014::163516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163517_wf.raa
20201014::163526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163527_wf.raa
20201014::163530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.7dbar, CTD 34.5psu, index 1.34, Packet 9837
20201014::163530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163537_wf.raa
20201014::163546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163547_wf.raa
20201014::163556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163557_wf.raa
20201014::163559: Head 1: Time Synchronization: 2020.10.14   16:36:00::0014
20201014::163600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 9893
20201014::163600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163607_wf.raa
20201014::163616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163617_wf.raa
20201014::163626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163627_wf.raa
20201014::163630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.9dbar, CTD 34.5psu, index 1.34, Packet 9948
20201014::163630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163637_wf.raa
20201014::163646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163647_wf.raa
20201014::163656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163657_wf.raa
20201014::163700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.3dbar, CTD 34.5psu, index 1.34, Packet 10004
20201014::163700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163707_wf.raa
20201014::163716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163717_wf.raa
20201014::163726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163727_wf.raa
20201014::163730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.3dbar, CTD 34.5psu, index 1.34, Packet 10059
20201014::163730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163737_wf.raa
20201014::163746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163747_wf.raa
20201014::163756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163757_wf.raa
20201014::163759: Head 1: Time Synchronization: 2020.10.14   16:38:00::0014
20201014::163800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1236.3dbar, CTD 34.5psu, index 1.34, Packet 10114
20201014::163800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163807_wf.raa
20201014::163816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163817_wf.raa
20201014::163826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163827_wf.raa
20201014::163830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1234.5dbar, CTD 34.5psu, index 1.34, Packet 10169
20201014::163830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163837_wf.raa
20201014::163846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163847_wf.raa
20201014::163856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163857_wf.raa
20201014::163900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1234.0dbar, CTD 34.5psu, index 1.34, Packet 10224
20201014::163900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163907_wf.raa
20201014::163916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163917_wf.raa
20201014::163926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163927_wf.raa
20201014::163930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1233.3dbar, CTD 34.5psu, index 1.34, Packet 10279
20201014::163930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::163936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163937_wf.raa
20201014::163946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163947_wf.raa
20201014::163956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_163957_wf.raa
20201014::164000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1233.1dbar, CTD 34.5psu, index 1.34, Packet 10335
20201014::164000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164007_wf.raa
20201014::164016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164017_wf.raa
20201014::164026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164027_wf.raa
20201014::164030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1232.8dbar, CTD 34.5psu, index 1.34, Packet 10390
20201014::164030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164037_wf.raa
20201014::164046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164047_wf.raa
20201014::164056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164057_wf.raa
20201014::164059: Head 2: Time Synchronization: 2020.10.14   16:41:00::0015
20201014::164100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1232.4dbar, CTD 34.5psu, index 1.34, Packet 10445
20201014::164100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164107_wf.raa
20201014::164116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164117_wf.raa
20201014::164126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164127_wf.raa
20201014::164130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.1dbar, CTD 34.5psu, index 1.34, Packet 10499
20201014::164130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164137_wf.raa
20201014::164146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164147_wf.raa
20201014::164156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164157_wf.raa
20201014::164200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.4dbar, CTD 34.5psu, index 1.34, Packet 10554
20201014::164200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164207_wf.raa
20201014::164216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164217_wf.raa
20201014::164226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164227_wf.raa
20201014::164230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.8dbar, CTD 34.5psu, index 1.34, Packet 10609
20201014::164230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164237_wf.raa
20201014::164246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164247_wf.raa
20201014::164256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164257_wf.raa
20201014::164259: Head 1: Time Synchronization: 2020.10.14   16:43:00::0014
20201014::164300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 10664
20201014::164300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164307_wf.raa
20201014::164316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164317_wf.raa
20201014::164326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164327_wf.raa
20201014::164330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 10719
20201014::164330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164337_wf.raa
20201014::164346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164347_wf.raa
20201014::164356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164357_wf.raa
20201014::164359: Head 1: Time Synchronization: 2020.10.14   16:44:00::0014
20201014::164400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.6dbar, CTD 34.5psu, index 1.34, Packet 10774
20201014::164400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164407_wf.raa
20201014::164416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164417_wf.raa
20201014::164426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164427_wf.raa
20201014::164430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.6dbar, CTD 34.5psu, index 1.34, Packet 10829
20201014::164430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164437_wf.raa
20201014::164446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164447_wf.raa
20201014::164456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164457_wf.raa
20201014::164500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.3dbar, CTD 34.5psu, index 1.34, Packet 10884
20201014::164500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164507_wf.raa
20201014::164516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164517_wf.raa
20201014::164526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164527_wf.raa
20201014::164530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.5dbar, CTD 34.5psu, index 1.34, Packet 10939
20201014::164530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164537_wf.raa
20201014::164546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164547_wf.raa
20201014::164556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164557_wf.raa
20201014::164600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1211.6dbar, CTD 34.5psu, index 1.34, Packet 10994
20201014::164600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164607_wf.raa
20201014::164616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164617_wf.raa
20201014::164626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164627_wf.raa
20201014::164630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.8dbar, CTD 34.5psu, index 1.34, Packet 11049
20201014::164630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164637_wf.raa
20201014::164646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164647_wf.raa
20201014::164656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164657_wf.raa
20201014::164700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.7dbar, CTD 34.5psu, index 1.34, Packet 11104
20201014::164700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164707_wf.raa
20201014::164716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164717_wf.raa
20201014::164726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164727_wf.raa
20201014::164730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1210.0dbar, CTD 34.5psu, index 1.34, Packet 11160
20201014::164730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164737_wf.raa
20201014::164746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164747_wf.raa
20201014::164756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164757_wf.raa
20201014::164800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1210.1dbar, CTD 34.5psu, index 1.34, Packet 11215
20201014::164800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164807_wf.raa
20201014::164816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164817_wf.raa
20201014::164826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164827_wf.raa
20201014::164830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 24%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.5dbar, CTD 34.5psu, index 1.34, Packet 11270
20201014::164830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164837_wf.raa
20201014::164846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164847_wf.raa
20201014::164856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164857_wf.raa
20201014::164859: Head 1: Time Synchronization: 2020.10.14   16:49:00::0013
20201014::164900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.8dbar, CTD 34.5psu, index 1.34, Packet 11325
20201014::164900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164907_wf.raa
20201014::164916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164917_wf.raa
20201014::164926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164927_wf.raa
20201014::164930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1211.4dbar, CTD 34.5psu, index 1.34, Packet 11380
20201014::164930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::164936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164937_wf.raa
20201014::164946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164947_wf.raa
20201014::164956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_164957_wf.raa
20201014::165000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.0dbar, CTD 34.5psu, index 1.34, Packet 11435
20201014::165000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165007_wf.raa
20201014::165016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165017_wf.raa
20201014::165026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165027_wf.raa
20201014::165030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.1dbar, CTD 34.5psu, index 1.34, Packet 11490
20201014::165030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165037_wf.raa
20201014::165046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165047_wf.raa
20201014::165056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165057_wf.raa
20201014::165100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.5dbar, CTD 34.5psu, index 1.34, Packet 11545
20201014::165100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165107_wf.raa
20201014::165116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165117_wf.raa
20201014::165126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165127_wf.raa
20201014::165130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1223.2dbar, CTD 34.5psu, index 1.34, Packet 11601
20201014::165130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165137_wf.raa
20201014::165146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165147_wf.raa
20201014::165156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165157_wf.raa
20201014::165159: Head 2: Time Synchronization: 2020.10.14   16:52:00::0014
20201014::165200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 11655
20201014::165200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165207_wf.raa
20201014::165216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165217_wf.raa
20201014::165226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165227_wf.raa
20201014::165230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 11711
20201014::165230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165237_wf.raa
20201014::165246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165247_wf.raa
20201014::165256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165257_wf.raa
20201014::165300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.7dbar, CTD 34.5psu, index 1.34, Packet 11766
20201014::165300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165307_wf.raa
20201014::165316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165317_wf.raa
20201014::165326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165327_wf.raa
20201014::165330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1231.0dbar, CTD 34.5psu, index 1.34, Packet 11821
20201014::165330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165337_wf.raa
20201014::165346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165347_wf.raa
20201014::165356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165357_wf.raa
20201014::165400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1231.8dbar, CTD 34.5psu, index 1.34, Packet 11877
20201014::165400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165407_wf.raa
20201014::165416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165417_wf.raa
20201014::165426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165427_wf.raa
20201014::165430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 11932
20201014::165430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165437_wf.raa
20201014::165446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165447_wf.raa
20201014::165456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165457_wf.raa
20201014::165459: Head 1: Time Synchronization: 2020.10.14   16:55:00::0018
20201014::165500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.5dbar, CTD 34.5psu, index 1.34, Packet 11987
20201014::165500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165507_wf.raa
20201014::165516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165517_wf.raa
20201014::165526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165527_wf.raa
20201014::165530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.0dbar, CTD 34.5psu, index 1.34, Packet 12042
20201014::165530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165537_wf.raa
20201014::165546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165547_wf.raa
20201014::165556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165557_wf.raa
20201014::165600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.2dbar, CTD 34.5psu, index 1.34, Packet 12096
20201014::165600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165607_wf.raa
20201014::165616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165617_wf.raa
20201014::165626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165627_wf.raa
20201014::165630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.0dbar, CTD 34.5psu, index 1.34, Packet 12152
20201014::165630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165637_wf.raa
20201014::165646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165647_wf.raa
20201014::165656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165657_wf.raa
20201014::165700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.4dbar, CTD 34.5psu, index 1.34, Packet 12207
20201014::165700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165707_wf.raa
20201014::165716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165717_wf.raa
20201014::165726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165727_wf.raa
20201014::165730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.1dbar, CTD 34.5psu, index 1.34, Packet 12262
20201014::165730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165737_wf.raa
20201014::165747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165747_wf.raa
20201014::165756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165757_wf.raa
20201014::165759: Head 1: Time Synchronization: 2020.10.14   16:58:00::0015
20201014::165800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.2dbar, CTD 34.5psu, index 1.34, Packet 12317
20201014::165800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165807_wf.raa
20201014::165816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165817_wf.raa
20201014::165826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165827_wf.raa
20201014::165830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.9dbar, CTD 34.5psu, index 1.34, Packet 12372
20201014::165830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165837_wf.raa
20201014::165846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165847_wf.raa
20201014::165856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165857_wf.raa
20201014::165859: Head 1: Time Synchronization: 2020.10.14   16:59:00::0015
20201014::165900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1239.4dbar, CTD 34.5psu, index 1.34, Packet 12427
20201014::165900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165907_wf.raa
20201014::165916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165917_wf.raa
20201014::165926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165927_wf.raa
20201014::165930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.0dbar, CTD 34.5psu, index 1.34, Packet 12482
20201014::165930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::165936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165937_wf.raa
20201014::165946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165947_wf.raa
20201014::165956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_165957_wf.raa
20201014::165959: Head 1: Time Synchronization: 2020.10.14   17:00:00::0015
20201014::170000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.4dbar, CTD 34.5psu, index 1.34, Packet 12537
20201014::170000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170007_wf.raa
20201014::170016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170017_wf.raa
20201014::170026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170027_wf.raa
20201014::170030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.7dbar, CTD 34.5psu, index 1.34, Packet 12593
20201014::170030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170037_wf.raa
20201014::170046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170047_wf.raa
20201014::170056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170057_wf.raa
20201014::170059: Head 1: Time Synchronization: 2020.10.14   17:01:00::0014
20201014::170100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.8dbar, CTD 34.5psu, index 1.34, Packet 12648
20201014::170100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170107_wf.raa
20201014::170116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170117_wf.raa
20201014::170126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170127_wf.raa
20201014::170130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.4dbar, CTD 34.5psu, index 1.34, Packet 12703
20201014::170130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170137_wf.raa
20201014::170146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170147_wf.raa
20201014::170156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170157_wf.raa
20201014::170200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.9dbar, CTD 34.5psu, index 1.34, Packet 12757
20201014::170200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170207_wf.raa
20201014::170216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170217_wf.raa
20201014::170226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170227_wf.raa
20201014::170230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.8dbar, CTD 34.5psu, index 1.34, Packet 12813
20201014::170230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170237_wf.raa
20201014::170246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170247_wf.raa
20201014::170256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170257_wf.raa
20201014::170259: Head 1: Time Synchronization: 2020.10.14   17:03:00::0015
20201014::170300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.9dbar, CTD 34.5psu, index 1.34, Packet 12867
20201014::170300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170307_wf.raa
20201014::170316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170317_wf.raa
20201014::170326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170327_wf.raa
20201014::170330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.6dbar, CTD 34.5psu, index 1.34, Packet 12922
20201014::170330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170337_wf.raa
20201014::170346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170347_wf.raa
20201014::170356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170357_wf.raa
20201014::170359: Head 1: Time Synchronization: 2020.10.14   17:04:00::0016
20201014::170400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.4dbar, CTD 34.5psu, index 1.34, Packet 12978
20201014::170400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170407_wf.raa
20201014::170416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170417_wf.raa
20201014::170426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170427_wf.raa
20201014::170430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.7dbar, CTD 34.5psu, index 1.34, Packet 13033
20201014::170430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170437_wf.raa
20201014::170446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170447_wf.raa
20201014::170456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170457_wf.raa
20201014::170459: Head 1: Time Synchronization: 2020.10.14   17:05:00::0015
20201014::170500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.0dbar, CTD 34.5psu, index 1.34, Packet 13089
20201014::170500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170507_wf.raa
20201014::170516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170517_wf.raa
20201014::170526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170527_wf.raa
20201014::170530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.6dbar, CTD 34.5psu, index 1.34, Packet 13143
20201014::170530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170537_wf.raa
20201014::170546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170547_wf.raa
20201014::170556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170557_wf.raa
20201014::170600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 13198
20201014::170600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170607_wf.raa
20201014::170616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170617_wf.raa
20201014::170626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170627_wf.raa
20201014::170630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.9dbar, CTD 34.5psu, index 1.34, Packet 13253
20201014::170630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170637_wf.raa
20201014::170646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170647_wf.raa
20201014::170656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170657_wf.raa
20201014::170700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.2dbar, CTD 34.5psu, index 1.34, Packet 13308
20201014::170700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170707_wf.raa
20201014::170716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170717_wf.raa
20201014::170726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170727_wf.raa
20201014::170730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 13363
20201014::170730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170737_wf.raa
20201014::170746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170747_wf.raa
20201014::170756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170757_wf.raa
20201014::170759: Head 2: Time Synchronization: 2020.10.14   17:08:00::0015
20201014::170759: Head 1: Time Synchronization: 2020.10.14   17:08:00::0015
20201014::170800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 13418
20201014::170800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170807_wf.raa
20201014::170816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170817_wf.raa
20201014::170826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170827_wf.raa
20201014::170830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.8dbar, CTD 34.5psu, index 1.34, Packet 13474
20201014::170830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170837_wf.raa
20201014::170846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170847_wf.raa
20201014::170856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170857_wf.raa
20201014::170900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.5dbar, CTD 34.5psu, index 1.34, Packet 13529
20201014::170900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170907_wf.raa
20201014::170916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170917_wf.raa
20201014::170926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170927_wf.raa
20201014::170930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.1dbar, CTD 34.5psu, index 1.34, Packet 13584
20201014::170930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::170936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170937_wf.raa
20201014::170946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170947_wf.raa
20201014::170956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_170957_wf.raa
20201014::171000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.0dbar, CTD 34.5psu, index 1.34, Packet 13639
20201014::171000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171007_wf.raa
20201014::171016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171017_wf.raa
20201014::171026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171027_wf.raa
20201014::171030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.0dbar, CTD 34.5psu, index 1.34, Packet 13694
20201014::171030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171037_wf.raa
20201014::171046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171047_wf.raa
20201014::171056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171057_wf.raa
20201014::171100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.0dbar, CTD 34.5psu, index 1.34, Packet 13749
20201014::171100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171107_wf.raa
20201014::171116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171117_wf.raa
20201014::171126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171127_wf.raa
20201014::171130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1210.4dbar, CTD 34.5psu, index 1.34, Packet 13804
20201014::171130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171137_wf.raa
20201014::171146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171147_wf.raa
20201014::171156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171157_wf.raa
20201014::171200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.1dbar, CTD 34.5psu, index 1.34, Packet 13860
20201014::171200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171207_wf.raa
20201014::171216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171217_wf.raa
20201014::171227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171227_wf.raa
20201014::171230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.3dbar, CTD 34.5psu, index 1.34, Packet 13916
20201014::171230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171237_wf.raa
20201014::171246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171247_wf.raa
20201014::171256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171257_wf.raa
20201014::171259: Head 1: Time Synchronization: 2020.10.14   17:13:00::0015
20201014::171300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.0dbar, CTD 34.5psu, index 1.34, Packet 13971
20201014::171300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171307_wf.raa
20201014::171316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171317_wf.raa
20201014::171326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171327_wf.raa
20201014::171330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1208.4dbar, CTD 34.5psu, index 1.34, Packet 14026
20201014::171330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171337_wf.raa
20201014::171346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171347_wf.raa
20201014::171356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171357_wf.raa
20201014::171400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1210.3dbar, CTD 34.5psu, index 1.34, Packet 14081
20201014::171400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171407_wf.raa
20201014::171416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171417_wf.raa
20201014::171426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171427_wf.raa
20201014::171430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.2dbar, CTD 34.5psu, index 1.34, Packet 14136
20201014::171430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171437_wf.raa
20201014::171446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171447_wf.raa
20201014::171456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171457_wf.raa
20201014::171500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.3dbar, CTD 34.5psu, index 1.34, Packet 14191
20201014::171500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171507_wf.raa
20201014::171516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171517_wf.raa
20201014::171526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171527_wf.raa
20201014::171530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.0dbar, CTD 34.5psu, index 1.34, Packet 14246
20201014::171530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171537_wf.raa
20201014::171546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171547_wf.raa
20201014::171556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171557_wf.raa
20201014::171600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.2dbar, CTD 34.5psu, index 1.34, Packet 14301
20201014::171600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171607_wf.raa
20201014::171616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171617_wf.raa
20201014::171626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171627_wf.raa
20201014::171630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.7dbar, CTD 34.5psu, index 1.34, Packet 14356
20201014::171630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171637_wf.raa
20201014::171646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171647_wf.raa
20201014::171656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171657_wf.raa
20201014::171700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.0dbar, CTD 34.5psu, index 1.34, Packet 14411
20201014::171700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171707_wf.raa
20201014::171716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171717_wf.raa
20201014::171726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171727_wf.raa
20201014::171730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 14468
20201014::171730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171737_wf.raa
20201014::171746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171747_wf.raa
20201014::171756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171757_wf.raa
20201014::171800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.9dbar, CTD 34.5psu, index 1.34, Packet 14524
20201014::171800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171807_wf.raa
20201014::171816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171817_wf.raa
20201014::171826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171827_wf.raa
20201014::171830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.9dbar, CTD 34.5psu, index 1.34, Packet 14579
20201014::171830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171837_wf.raa
20201014::171846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171847_wf.raa
20201014::171856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171857_wf.raa
20201014::171859: Head 1: Time Synchronization: 2020.10.14   17:19:00::0015
20201014::171900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.5dbar, CTD 34.5psu, index 1.34, Packet 14635
20201014::171900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171907_wf.raa
20201014::171916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171917_wf.raa
20201014::171926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171927_wf.raa
20201014::171930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.0dbar, CTD 34.5psu, index 1.34, Packet 14689
20201014::171930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::171936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171937_wf.raa
20201014::171946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171947_wf.raa
20201014::171956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_171957_wf.raa
20201014::172000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 14743
20201014::172000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172007_wf.raa
20201014::172016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172017_wf.raa
20201014::172026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172027_wf.raa
20201014::172030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.7dbar, CTD 34.5psu, index 1.34, Packet 14799
20201014::172030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172037_wf.raa
20201014::172046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172047_wf.raa
20201014::172056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172057_wf.raa
20201014::172059: Head 1: Time Synchronization: 2020.10.14   17:21:00::0015
20201014::172100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.2dbar, CTD 34.5psu, index 1.34, Packet 14854
20201014::172100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172107_wf.raa
20201014::172116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172117_wf.raa
20201014::172126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172127_wf.raa
20201014::172130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.0dbar, CTD 34.5psu, index 1.34, Packet 14910
20201014::172130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172137_wf.raa
20201014::172146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172147_wf.raa
20201014::172156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172157_wf.raa
20201014::172200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.9dbar, CTD 34.5psu, index 1.34, Packet 14965
20201014::172200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172207_wf.raa
20201014::172216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172217_wf.raa
20201014::172226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172227_wf.raa
20201014::172230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.4dbar, CTD 34.5psu, index 1.34, Packet 15020
20201014::172230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172237_wf.raa
20201014::172246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172247_wf.raa
20201014::172256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172257_wf.raa
20201014::172259: Head 1: Time Synchronization: 2020.10.14   17:23:00::0017
20201014::172300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.5dbar, CTD 34.5psu, index 1.34, Packet 15075
20201014::172300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172307_wf.raa
20201014::172316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172317_wf.raa
20201014::172326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172327_wf.raa
20201014::172330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.3dbar, CTD 34.5psu, index 1.34, Packet 15130
20201014::172330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172337_wf.raa
20201014::172346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172347_wf.raa
20201014::172356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172357_wf.raa
20201014::172400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.6dbar, CTD 34.5psu, index 1.34, Packet 15185
20201014::172400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172407_wf.raa
20201014::172416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172417_wf.raa
20201014::172426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172427_wf.raa
20201014::172430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.9dbar, CTD 34.5psu, index 1.34, Packet 15240
20201014::172430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172437_wf.raa
20201014::172446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172447_wf.raa
20201014::172456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172457_wf.raa
20201014::172500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.0dbar, CTD 34.5psu, index 1.34, Packet 15296
20201014::172500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172507_wf.raa
20201014::172516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172517_wf.raa
20201014::172526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172527_wf.raa
20201014::172530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1242.1dbar, CTD 34.5psu, index 1.34, Packet 15351
20201014::172530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172537_wf.raa
20201014::172546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172547_wf.raa
20201014::172556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172557_wf.raa
20201014::172600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.9dbar, CTD 34.5psu, index 1.34, Packet 15406
20201014::172600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172607_wf.raa
20201014::172616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172617_wf.raa
20201014::172626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172627_wf.raa
20201014::172630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.2dbar, CTD 34.5psu, index 1.34, Packet 15461
20201014::172630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172637_wf.raa
20201014::172646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172647_wf.raa
20201014::172656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172657_wf.raa
20201014::172659: Head 1: Time Synchronization: 2020.10.14   17:27:00::0014
20201014::172700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.4dbar, CTD 34.5psu, index 1.34, Packet 15517
20201014::172700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172707_wf.raa
20201014::172716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172717_wf.raa
20201014::172726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172727_wf.raa
20201014::172730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.5dbar, CTD 34.5psu, index 1.34, Packet 15572
20201014::172730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172737_wf.raa
20201014::172746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172747_wf.raa
20201014::172756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172757_wf.raa
20201014::172800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.3dbar, CTD 34.5psu, index 1.34, Packet 15628
20201014::172800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172807_wf.raa
20201014::172816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172817_wf.raa
20201014::172826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172827_wf.raa
20201014::172830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.0dbar, CTD 34.5psu, index 1.34, Packet 15683
20201014::172830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172837_wf.raa
20201014::172846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172847_wf.raa
20201014::172856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172857_wf.raa
20201014::172900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 15739
20201014::172900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172907_wf.raa
20201014::172916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172917_wf.raa
20201014::172926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172927_wf.raa
20201014::172930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.9dbar, CTD 34.5psu, index 1.34, Packet 15795
20201014::172930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::172936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172937_wf.raa
20201014::172946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172947_wf.raa
20201014::172956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_172957_wf.raa
20201014::173000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.5dbar, CTD 34.5psu, index 1.34, Packet 15850
20201014::173000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173007_wf.raa
20201014::173016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173017_wf.raa
20201014::173026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173027_wf.raa
20201014::173030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.1dbar, CTD 34.5psu, index 1.34, Packet 15905
20201014::173030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173037_wf.raa
20201014::173046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173047_wf.raa
20201014::173056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173057_wf.raa
20201014::173100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.6dbar, CTD 34.5psu, index 1.34, Packet 15960
20201014::173100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173107_wf.raa
20201014::173116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173117_wf.raa
20201014::173126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173127_wf.raa
20201014::173130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 16015
20201014::173130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173137_wf.raa
20201014::173146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173147_wf.raa
20201014::173156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173157_wf.raa
20201014::173159: Head 1: Time Synchronization: 2020.10.14   17:32:00::0014
20201014::173200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.3dbar, CTD 34.5psu, index 1.34, Packet 16071
20201014::173200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173207_wf.raa
20201014::173216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173217_wf.raa
20201014::173226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173227_wf.raa
20201014::173230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.6dbar, CTD 34.5psu, index 1.34, Packet 16126
20201014::173230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173237_wf.raa
20201014::173246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173247_wf.raa
20201014::173256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173257_wf.raa
20201014::173300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 16181
20201014::173300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173307_wf.raa
20201014::173316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173317_wf.raa
20201014::173326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173327_wf.raa
20201014::173330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 16237
20201014::173330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173337_wf.raa
20201014::173346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173347_wf.raa
20201014::173356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173357_wf.raa
20201014::173359: Head 1: Time Synchronization: 2020.10.14   17:34:00::0018
20201014::173400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.3dbar, CTD 34.5psu, index 1.34, Packet 16292
20201014::173400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173407_wf.raa
20201014::173416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173417_wf.raa
20201014::173426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173427_wf.raa
20201014::173430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.7dbar, CTD 34.5psu, index 1.34, Packet 16347
20201014::173430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173437_wf.raa
20201014::173446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173447_wf.raa
20201014::173456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173457_wf.raa
20201014::173500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.4dbar, CTD 34.5psu, index 1.34, Packet 16402
20201014::173500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173507_wf.raa
20201014::173516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173517_wf.raa
20201014::173526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173527_wf.raa
20201014::173530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.6dbar, CTD 34.5psu, index 1.34, Packet 16457
20201014::173530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173537_wf.raa
20201014::173546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173547_wf.raa
20201014::173556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173557_wf.raa
20201014::173600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1211.9dbar, CTD 34.5psu, index 1.34, Packet 16512
20201014::173600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173607_wf.raa
20201014::173616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173617_wf.raa
20201014::173626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173627_wf.raa
20201014::173630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1208.3dbar, CTD 34.5psu, index 1.34, Packet 16567
20201014::173630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173637_wf.raa
20201014::173646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173647_wf.raa
20201014::173656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173657_wf.raa
20201014::173659: Head 2: Time Synchronization: 2020.10.14   17:37:00::0015
20201014::173659: Head 1: Time Synchronization: 2020.10.14   17:37:00::0015
20201014::173700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.4dbar, CTD 34.5psu, index 1.34, Packet 16622
20201014::173700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173707_wf.raa
20201014::173716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173717_wf.raa
20201014::173726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173727_wf.raa
20201014::173730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.9dbar, CTD 34.5psu, index 1.34, Packet 16677
20201014::173730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173737_wf.raa
20201014::173746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173747_wf.raa
20201014::173756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173757_wf.raa
20201014::173759: Head 1: Time Synchronization: 2020.10.14   17:38:00::0014
20201014::173759: Head 2: Time Synchronization: 2020.10.14   17:38:00::0014
20201014::173800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.7dbar, CTD 34.5psu, index 1.34, Packet 16733
20201014::173800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173807_wf.raa
20201014::173816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173817_wf.raa
20201014::173826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173827_wf.raa
20201014::173830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1206.6dbar, CTD 34.5psu, index 1.34, Packet 16788
20201014::173830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173837_wf.raa
20201014::173846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173847_wf.raa
20201014::173856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173857_wf.raa
20201014::173859: Head 1: Time Synchronization: 2020.10.14   17:39:00::0017
20201014::173900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1209.6dbar, CTD 34.5psu, index 1.34, Packet 16843
20201014::173900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173907_wf.raa
20201014::173916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173917_wf.raa
20201014::173926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173927_wf.raa
20201014::173930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.8dbar, CTD 34.5psu, index 1.34, Packet 16897
20201014::173930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::173936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173937_wf.raa
20201014::173946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173947_wf.raa
20201014::173956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_173957_wf.raa
20201014::174000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.9dbar, CTD 34.5psu, index 1.34, Packet 16951
20201014::174000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174007_wf.raa
20201014::174016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174017_wf.raa
20201014::174026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174027_wf.raa
20201014::174030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.3dbar, CTD 34.5psu, index 1.34, Packet 17006
20201014::174030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174037_wf.raa
20201014::174046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174047_wf.raa
20201014::174056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174057_wf.raa
20201014::174100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.8dbar, CTD 34.5psu, index 1.34, Packet 17060
20201014::174100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174107_wf.raa
20201014::174116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174117_wf.raa
20201014::174126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174127_wf.raa
20201014::174130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.2dbar, CTD 34.5psu, index 1.34, Packet 17115
20201014::174130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174137_wf.raa
20201014::174146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174147_wf.raa
20201014::174156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174157_wf.raa
20201014::174200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.0dbar, CTD 34.5psu, index 1.34, Packet 17171
20201014::174200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174207_wf.raa
20201014::174216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174217_wf.raa
20201014::174226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174227_wf.raa
20201014::174230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 17225
20201014::174230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174237_wf.raa
20201014::174246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174247_wf.raa
20201014::174256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174257_wf.raa
20201014::174259: Head 1: Time Synchronization: 2020.10.14   17:43:00::0014
20201014::174300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.3dbar, CTD 34.5psu, index 1.34, Packet 17280
20201014::174300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174307_wf.raa
20201014::174316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174317_wf.raa
20201014::174326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174327_wf.raa
20201014::174330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 17335
20201014::174330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174337_wf.raa
20201014::174346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174347_wf.raa
20201014::174356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174357_wf.raa
20201014::174400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.9dbar, CTD 34.5psu, index 1.34, Packet 17390
20201014::174400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174407_wf.raa
20201014::174416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174417_wf.raa
20201014::174426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174427_wf.raa
20201014::174430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.5dbar, CTD 34.5psu, index 1.34, Packet 17445
20201014::174430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174437_wf.raa
20201014::174446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174447_wf.raa
20201014::174456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174457_wf.raa
20201014::174500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.0dbar, CTD 34.5psu, index 1.34, Packet 17501
20201014::174500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174507_wf.raa
20201014::174516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174517_wf.raa
20201014::174526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174527_wf.raa
20201014::174530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.4dbar, CTD 34.5psu, index 1.34, Packet 17556
20201014::174530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174537_wf.raa
20201014::174546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174547_wf.raa
20201014::174556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174557_wf.raa
20201014::174600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.9dbar, CTD 34.5psu, index 1.34, Packet 17611
20201014::174600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174607_wf.raa
20201014::174616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174617_wf.raa
20201014::174626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174627_wf.raa
20201014::174630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.2dbar, CTD 34.5psu, index 1.34, Packet 17666
20201014::174630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174637_wf.raa
20201014::174646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174647_wf.raa
20201014::174656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174657_wf.raa
20201014::174659: Head 1: Time Synchronization: 2020.10.14   17:47:00::0015
20201014::174700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.4dbar, CTD 34.5psu, index 1.34, Packet 17721
20201014::174700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174707_wf.raa
20201014::174716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174717_wf.raa
20201014::174726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174727_wf.raa
20201014::174730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.8dbar, CTD 34.5psu, index 1.34, Packet 17777
20201014::174730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174737_wf.raa
20201014::174746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174747_wf.raa
20201014::174756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174757_wf.raa
20201014::174800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.8dbar, CTD 34.5psu, index 1.34, Packet 17832
20201014::174800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174807_wf.raa
20201014::174816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174817_wf.raa
20201014::174826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174827_wf.raa
20201014::174830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.6dbar, CTD 34.5psu, index 1.34, Packet 17887
20201014::174830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174837_wf.raa
20201014::174846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174847_wf.raa
20201014::174856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174857_wf.raa
20201014::174900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.5dbar, CTD 34.5psu, index 1.34, Packet 17942
20201014::174900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174907_wf.raa
20201014::174916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174917_wf.raa
20201014::174926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174927_wf.raa
20201014::174930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.1dbar, CTD 34.5psu, index 1.34, Packet 17997
20201014::174930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::174936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174937_wf.raa
20201014::174946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174947_wf.raa
20201014::174956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_174957_wf.raa
20201014::174959: Head 1: Time Synchronization: 2020.10.14   17:50:00::0014
20201014::175000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1241.9dbar, CTD 34.5psu, index 1.34, Packet 18053
20201014::175000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175007_wf.raa
20201014::175016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175017_wf.raa
20201014::175026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175027_wf.raa
20201014::175030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.9dbar, CTD 34.5psu, index 1.34, Packet 18108
20201014::175030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175037_wf.raa
20201014::175046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175047_wf.raa
20201014::175056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175057_wf.raa
20201014::175100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.4dbar, CTD 34.5psu, index 1.34, Packet 18163
20201014::175100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175107_wf.raa
20201014::175116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175117_wf.raa
20201014::175126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175127_wf.raa
20201014::175130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.4dbar, CTD 34.5psu, index 1.34, Packet 18219
20201014::175130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175137_wf.raa
20201014::175146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175147_wf.raa
20201014::175156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175157_wf.raa
20201014::175159: Head 1: Time Synchronization: 2020.10.14   17:52:00::0014
20201014::175200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.4dbar, CTD 34.5psu, index 1.34, Packet 18274
20201014::175200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175207_wf.raa
20201014::175216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175217_wf.raa
20201014::175226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175227_wf.raa
20201014::175230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.2dbar, CTD 34.5psu, index 1.34, Packet 18329
20201014::175230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175237_wf.raa
20201014::175246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175247_wf.raa
20201014::175256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175257_wf.raa
20201014::175300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.9dbar, CTD 34.5psu, index 1.34, Packet 18384
20201014::175300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175307_wf.raa
20201014::175316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175317_wf.raa
20201014::175326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175327_wf.raa
20201014::175330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.7dbar, CTD 34.5psu, index 1.34, Packet 18439
20201014::175330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175337_wf.raa
20201014::175346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175347_wf.raa
20201014::175356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175357_wf.raa
20201014::175400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.5dbar, CTD 34.5psu, index 1.34, Packet 18494
20201014::175400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175407_wf.raa
20201014::175416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175417_wf.raa
20201014::175426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175427_wf.raa
20201014::175430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.0dbar, CTD 34.5psu, index 1.34, Packet 18550
20201014::175430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175437_wf.raa
20201014::175446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175447_wf.raa
20201014::175456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175457_wf.raa
20201014::175459: Head 1: Time Synchronization: 2020.10.14   17:55:00::0013
20201014::175500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.3dbar, CTD 34.5psu, index 1.34, Packet 18605
20201014::175500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175507_wf.raa
20201014::175516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175517_wf.raa
20201014::175526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175527_wf.raa
20201014::175530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.0dbar, CTD 34.5psu, index 1.34, Packet 18660
20201014::175530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175537_wf.raa
20201014::175546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175547_wf.raa
20201014::175556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175557_wf.raa
20201014::175600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.4dbar, CTD 34.5psu, index 1.34, Packet 18715
20201014::175600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175607_wf.raa
20201014::175616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175617_wf.raa
20201014::175626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175627_wf.raa
20201014::175630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.6dbar, CTD 34.5psu, index 1.34, Packet 18770
20201014::175630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175637_wf.raa
20201014::175646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175647_wf.raa
20201014::175656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175657_wf.raa
20201014::175659: Head 1: Time Synchronization: 2020.10.14   17:57:00::0014
20201014::175700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 18826
20201014::175700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175707_wf.raa
20201014::175716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175717_wf.raa
20201014::175726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175727_wf.raa
20201014::175730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.2dbar, CTD 34.5psu, index 1.34, Packet 18881
20201014::175730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175737_wf.raa
20201014::175746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175747_wf.raa
20201014::175756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175757_wf.raa
20201014::175800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.0dbar, CTD 34.5psu, index 1.34, Packet 18935
20201014::175800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175807_wf.raa
20201014::175816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175817_wf.raa
20201014::175826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175827_wf.raa
20201014::175830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.4dbar, CTD 34.5psu, index 1.34, Packet 18990
20201014::175830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175837_wf.raa
20201014::175846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175847_wf.raa
20201014::175856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175857_wf.raa
20201014::175900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1220.9dbar, CTD 34.5psu, index 1.34, Packet 19045
20201014::175900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175907_wf.raa
20201014::175916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175917_wf.raa
20201014::175926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175927_wf.raa
20201014::175930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1218.4dbar, CTD 34.5psu, index 1.34, Packet 19100
20201014::175930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::175936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175937_wf.raa
20201014::175946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175947_wf.raa
20201014::175956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_175957_wf.raa
20201014::180000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.4dbar, CTD 34.5psu, index 1.34, Packet 19155
20201014::180000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180007_wf.raa
20201014::180016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180017_wf.raa
20201014::180026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180027_wf.raa
20201014::180030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.3dbar, CTD 34.5psu, index 1.34, Packet 19210
20201014::180030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180037_wf.raa
20201014::180046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180047_wf.raa
20201014::180056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180057_wf.raa
20201014::180059: Head 1: Time Synchronization: 2020.10.14   18:01:00::0015
20201014::180100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1208.8dbar, CTD 34.5psu, index 1.34, Packet 19266
20201014::180100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180107_wf.raa
20201014::180116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180117_wf.raa
20201014::180126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180127_wf.raa
20201014::180130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1207.5dbar, CTD 34.5psu, index 1.34, Packet 19322
20201014::180130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180137_wf.raa
20201014::180146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180147_wf.raa
20201014::180156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180157_wf.raa
20201014::180159: Head 1: Time Synchronization: 2020.10.14   18:02:00::0016
20201014::180200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.9dbar, CTD 34.5psu, index 1.34, Packet 19376
20201014::180200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180207_wf.raa
20201014::180216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180217_wf.raa
20201014::180226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180227_wf.raa
20201014::180230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.4dbar, CTD 34.5psu, index 1.34, Packet 19431
20201014::180230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180237_wf.raa
20201014::180246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180247_wf.raa
20201014::180256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180257_wf.raa
20201014::180300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1209.7dbar, CTD 34.5psu, index 1.34, Packet 19486
20201014::180300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180307_wf.raa
20201014::180316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180317_wf.raa
20201014::180326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180327_wf.raa
20201014::180330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1209.6dbar, CTD 34.5psu, index 1.34, Packet 19541
20201014::180330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180337_wf.raa
20201014::180346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180347_wf.raa
20201014::180356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180357_wf.raa
20201014::180359: Head 2: Time Synchronization: 2020.10.14   18:04:00::0014
20201014::180400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.7dbar, CTD 34.5psu, index 1.34, Packet 19597
20201014::180400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180407_wf.raa
20201014::180416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180417_wf.raa
20201014::180426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180427_wf.raa
20201014::180430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1215.5dbar, CTD 34.5psu, index 1.34, Packet 19652
20201014::180430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180437_wf.raa
20201014::180446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180447_wf.raa
20201014::180456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180457_wf.raa
20201014::180500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1218.2dbar, CTD 34.5psu, index 1.34, Packet 19707
20201014::180500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180507_wf.raa
20201014::180516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180517_wf.raa
20201014::180526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180527_wf.raa
20201014::180530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1221.0dbar, CTD 34.5psu, index 1.34, Packet 19763
20201014::180530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180537_wf.raa
20201014::180546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180547_wf.raa
20201014::180556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180557_wf.raa
20201014::180600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.4dbar, CTD 34.5psu, index 1.34, Packet 19818
20201014::180600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180607_wf.raa
20201014::180616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180617_wf.raa
20201014::180626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180627_wf.raa
20201014::180630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.7dbar, CTD 34.5psu, index 1.34, Packet 19874
20201014::180630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180637_wf.raa
20201014::180646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180647_wf.raa
20201014::180656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180657_wf.raa
20201014::180700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 19929
20201014::180700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180707_wf.raa
20201014::180716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180717_wf.raa
20201014::180726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180727_wf.raa
20201014::180730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.8dbar, CTD 34.5psu, index 1.34, Packet 19985
20201014::180730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180737_wf.raa
20201014::180746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180747_wf.raa
20201014::180756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180757_wf.raa
20201014::180759: Head 1: Time Synchronization: 2020.10.14   18:08:00::0013
20201014::180800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 20039
20201014::180800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180807_wf.raa
20201014::180816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180817_wf.raa
20201014::180826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180827_wf.raa
20201014::180830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.8dbar, CTD 34.5psu, index 1.34, Packet 20095
20201014::180830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180837_wf.raa
20201014::180846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180847_wf.raa
20201014::180856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180857_wf.raa
20201014::180900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.7dbar, CTD 34.5psu, index 1.34, Packet 20149
20201014::180900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180907_wf.raa
20201014::180916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180917_wf.raa
20201014::180926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180927_wf.raa
20201014::180930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 20205
20201014::180930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::180936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180937_wf.raa
20201014::180946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180947_wf.raa
20201014::180956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_180957_wf.raa
20201014::180959: Head 2: Time Synchronization: 2020.10.14   18:10:00::0014
20201014::181000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.6dbar, CTD 34.5psu, index 1.34, Packet 20260
20201014::181000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181007_wf.raa
20201014::181016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181017_wf.raa
20201014::181026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181027_wf.raa
20201014::181030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1232.2dbar, CTD 34.5psu, index 1.34, Packet 20316
20201014::181030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181037_wf.raa
20201014::181046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181047_wf.raa
20201014::181056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181057_wf.raa
20201014::181059: Head 1: Time Synchronization: 2020.10.14   18:11:00::0015
20201014::181100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.4dbar, CTD 34.5psu, index 1.34, Packet 20371
20201014::181100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181107_wf.raa
20201014::181116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181117_wf.raa
20201014::181126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181127_wf.raa
20201014::181130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1234.6dbar, CTD 34.5psu, index 1.34, Packet 20426
20201014::181130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181137_wf.raa
20201014::181146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181147_wf.raa
20201014::181156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181157_wf.raa
20201014::181159: Head 1: Time Synchronization: 2020.10.14   18:12:00::0012
20201014::181200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1235.9dbar, CTD 34.5psu, index 1.34, Packet 20481
20201014::181200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181207_wf.raa
20201014::181216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181217_wf.raa
20201014::181226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181227_wf.raa
20201014::181230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1237.1dbar, CTD 34.5psu, index 1.34, Packet 20537
20201014::181230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181237_wf.raa
20201014::181246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181247_wf.raa
20201014::181256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181257_wf.raa
20201014::181300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1238.0dbar, CTD 34.5psu, index 1.34, Packet 20592
20201014::181300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181307_wf.raa
20201014::181316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181317_wf.raa
20201014::181326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181327_wf.raa
20201014::181330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1238.8dbar, CTD 34.5psu, index 1.34, Packet 20648
20201014::181330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181337_wf.raa
20201014::181346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181347_wf.raa
20201014::181356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181357_wf.raa
20201014::181359: Head 1: Time Synchronization: 2020.10.14   18:14:00::0015
20201014::181400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1240.4dbar, CTD 34.5psu, index 1.34, Packet 20703
20201014::181400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181407_wf.raa
20201014::181416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181417_wf.raa
20201014::181426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181427_wf.raa
20201014::181430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.6dbar, CTD 34.5psu, index 1.34, Packet 20758
20201014::181430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181437_wf.raa
20201014::181446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181447_wf.raa
20201014::181456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181457_wf.raa
20201014::181500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 20813
20201014::181500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181507_wf.raa
20201014::181516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181517_wf.raa
20201014::181526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181527_wf.raa
20201014::181530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 20868
20201014::181530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181537_wf.raa
20201014::181546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181547_wf.raa
20201014::181556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181557_wf.raa
20201014::181559: Head 1: Time Synchronization: 2020.10.14   18:16:00::0015
20201014::181600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 20924
20201014::181600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181607_wf.raa
20201014::181616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181617_wf.raa
20201014::181626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181627_wf.raa
20201014::181630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.2dbar, CTD 34.5psu, index 1.34, Packet 20979
20201014::181630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181637_wf.raa
20201014::181646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181647_wf.raa
20201014::181656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181657_wf.raa
20201014::181700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21034
20201014::181700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181707_wf.raa
20201014::181716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181717_wf.raa
20201014::181726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181727_wf.raa
20201014::181730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21090
20201014::181730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181737_wf.raa
20201014::181746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181747_wf.raa
20201014::181756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181757_wf.raa
20201014::181800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21145
20201014::181800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181807_wf.raa
20201014::181816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181817_wf.raa
20201014::181826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181827_wf.raa
20201014::181830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21201
20201014::181830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181837_wf.raa
20201014::181846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181847_wf.raa
20201014::181856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181857_wf.raa
20201014::181900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21257
20201014::181900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181907_wf.raa
20201014::181916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181917_wf.raa
20201014::181926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181927_wf.raa
20201014::181930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21312
20201014::181930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::181936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181937_wf.raa
20201014::181946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181947_wf.raa
20201014::181956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_181957_wf.raa
20201014::181959: Head 1: Time Synchronization: 2020.10.14   18:20:00::0015
20201014::182000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 21366
20201014::182000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182007_wf.raa
20201014::182016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182017_wf.raa
20201014::182026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182027_wf.raa
20201014::182030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 21420
20201014::182030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182037_wf.raa
20201014::182046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182047_wf.raa
20201014::182056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182057_wf.raa
20201014::182100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21475
20201014::182100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182107_wf.raa
20201014::182116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182117_wf.raa
20201014::182126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182127_wf.raa
20201014::182130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 21528
20201014::182130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182137_wf.raa
20201014::182146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182147_wf.raa
20201014::182156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182157_wf.raa
20201014::182200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 21582
20201014::182200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182207_wf.raa
20201014::182216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182217_wf.raa
20201014::182226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182227_wf.raa
20201014::182230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.3dbar, CTD 34.5psu, index 1.34, Packet 21637
20201014::182230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182237_wf.raa
20201014::182246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182247_wf.raa
20201014::182256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182257_wf.raa
20201014::182300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.4dbar, CTD 34.5psu, index 1.34, Packet 21691
20201014::182300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182307_wf.raa
20201014::182316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182317_wf.raa
20201014::182326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182327_wf.raa
20201014::182330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1241.2dbar, CTD 34.5psu, index 1.34, Packet 21744
20201014::182330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182337_wf.raa
20201014::182346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182347_wf.raa
20201014::182356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182357_wf.raa
20201014::182400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1240.6dbar, CTD 34.5psu, index 1.34, Packet 21798
20201014::182400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182407_wf.raa
20201014::182416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182417_wf.raa
20201014::182426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182427_wf.raa
20201014::182430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1239.3dbar, CTD 34.5psu, index 1.34, Packet 21853
20201014::182430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182437_wf.raa
20201014::182446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182447_wf.raa
20201014::182456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182457_wf.raa
20201014::182500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1238.1dbar, CTD 34.5psu, index 1.34, Packet 21907
20201014::182500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182507_wf.raa
20201014::182516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182517_wf.raa
20201014::182526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182527_wf.raa
20201014::182530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1237.1dbar, CTD 34.5psu, index 1.34, Packet 21961
20201014::182530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182537_wf.raa
20201014::182546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182547_wf.raa
20201014::182556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182557_wf.raa
20201014::182559: Head 1: Time Synchronization: 2020.10.14   18:26:00::0014
20201014::182600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1235.7dbar, CTD 34.5psu, index 1.34, Packet 22015
20201014::182600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182607_wf.raa
20201014::182616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182617_wf.raa
20201014::182626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182627_wf.raa
20201014::182630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1234.6dbar, CTD 34.5psu, index 1.34, Packet 22069
20201014::182630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182637_wf.raa
20201014::182646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182647_wf.raa
20201014::182656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182657_wf.raa
20201014::182659: Head 1: Time Synchronization: 2020.10.14   18:27:00::0015
20201014::182700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.9dbar, CTD 34.5psu, index 1.34, Packet 22123
20201014::182700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182707_wf.raa
20201014::182716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182717_wf.raa
20201014::182726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182727_wf.raa
20201014::182730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.7dbar, CTD 34.5psu, index 1.34, Packet 22177
20201014::182730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182737_wf.raa
20201014::182746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182747_wf.raa
20201014::182756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182757_wf.raa
20201014::182800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 22233
20201014::182800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182807_wf.raa
20201014::182816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182817_wf.raa
20201014::182826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182827_wf.raa
20201014::182830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.6dbar, CTD 34.5psu, index 1.34, Packet 22288
20201014::182830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182837_wf.raa
20201014::182846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182847_wf.raa
20201014::182856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182857_wf.raa
20201014::182859: Head 1: Time Synchronization: 2020.10.14   18:29:00::0015
20201014::182900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.0dbar, CTD 34.5psu, index 1.34, Packet 22344
20201014::182900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182907_wf.raa
20201014::182916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182917_wf.raa
20201014::182926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182927_wf.raa
20201014::182930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1229.1dbar, CTD 34.5psu, index 1.34, Packet 22398
20201014::182930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::182936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182937_wf.raa
20201014::182946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182947_wf.raa
20201014::182956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_182957_wf.raa
20201014::182959: Head 2: Time Synchronization: 2020.10.14   18:30:00::0015
20201014::183000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 22454
20201014::183000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183007_wf.raa
20201014::183016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183017_wf.raa
20201014::183026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183027_wf.raa
20201014::183030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22508
20201014::183030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183037_wf.raa
20201014::183046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183047_wf.raa
20201014::183056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183057_wf.raa
20201014::183100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22563
20201014::183100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183107_wf.raa
20201014::183116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183117_wf.raa
20201014::183126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183127_wf.raa
20201014::183130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22618
20201014::183130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183137_wf.raa
20201014::183146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183147_wf.raa
20201014::183156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183157_wf.raa
20201014::183159: Head 1: Time Synchronization: 2020.10.14   18:32:00::0015
20201014::183200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 22672
20201014::183200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183207_wf.raa
20201014::183216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183217_wf.raa
20201014::183227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183227_wf.raa
20201014::183230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 22727
20201014::183230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183237_wf.raa
20201014::183246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183247_wf.raa
20201014::183256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183257_wf.raa
20201014::183259: Head 1: Time Synchronization: 2020.10.14   18:33:00::0016
20201014::183300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22782
20201014::183300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183307_wf.raa
20201014::183316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183317_wf.raa
20201014::183326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183327_wf.raa
20201014::183330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22837
20201014::183330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183337_wf.raa
20201014::183346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183347_wf.raa
20201014::183356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183357_wf.raa
20201014::183400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22891
20201014::183400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183407_wf.raa
20201014::183416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183417_wf.raa
20201014::183426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183427_wf.raa
20201014::183430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 22946
20201014::183430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183437_wf.raa
20201014::183446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183447_wf.raa
20201014::183456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183457_wf.raa
20201014::183500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23001
20201014::183500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183507_wf.raa
20201014::183516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183517_wf.raa
20201014::183526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183527_wf.raa
20201014::183530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23055
20201014::183530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183537_wf.raa
20201014::183546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183547_wf.raa
20201014::183556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183557_wf.raa
20201014::183600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23110
20201014::183600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183607_wf.raa
20201014::183616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183617_wf.raa
20201014::183626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183627_wf.raa
20201014::183630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23165
20201014::183630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183637_wf.raa
20201014::183646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183647_wf.raa
20201014::183656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183657_wf.raa
20201014::183659: Head 1: Time Synchronization: 2020.10.14   18:37:00::0014
20201014::183700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23219
20201014::183700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183707_wf.raa
20201014::183716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183717_wf.raa
20201014::183726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183727_wf.raa
20201014::183730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23275
20201014::183730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183737_wf.raa
20201014::183746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183747_wf.raa
20201014::183756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183757_wf.raa
20201014::183759: Head 1: Time Synchronization: 2020.10.14   18:38:00::0014
20201014::183800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23330
20201014::183800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183807_wf.raa
20201014::183816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183817_wf.raa
20201014::183826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183827_wf.raa
20201014::183830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 23384
20201014::183830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183837_wf.raa
20201014::183846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183847_wf.raa
20201014::183856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183857_wf.raa
20201014::183859: Head 2: Time Synchronization: 2020.10.14   18:39:00::0014
20201014::183900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.6dbar, CTD 34.5psu, index 1.34, Packet 23439
20201014::183900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183907_wf.raa
20201014::183916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183917_wf.raa
20201014::183926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183927_wf.raa
20201014::183930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 23494
20201014::183930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::183936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183937_wf.raa
20201014::183946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183947_wf.raa
20201014::183956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_183957_wf.raa
20201014::183959: Head 1: Time Synchronization: 2020.10.14   18:40:00::0015
20201014::184000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 23550
20201014::184000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184007_wf.raa
20201014::184016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184017_wf.raa
20201014::184026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184027_wf.raa
20201014::184030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.6dbar, CTD 34.5psu, index 1.34, Packet 23605
20201014::184030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184037_wf.raa
20201014::184046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184047_wf.raa
20201014::184056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184057_wf.raa
20201014::184100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.2dbar, CTD 34.5psu, index 1.34, Packet 23659
20201014::184100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184107_wf.raa
20201014::184116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184117_wf.raa
20201014::184126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184127_wf.raa
20201014::184130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1231.8dbar, CTD 34.5psu, index 1.34, Packet 23714
20201014::184130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184137_wf.raa
20201014::184146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184147_wf.raa
20201014::184156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184157_wf.raa
20201014::184200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1233.1dbar, CTD 34.5psu, index 1.34, Packet 23769
20201014::184200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184207_wf.raa
20201014::184216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184217_wf.raa
20201014::184226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184227_wf.raa
20201014::184230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1234.7dbar, CTD 34.5psu, index 1.34, Packet 23824
20201014::184230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184237_wf.raa
20201014::184246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184247_wf.raa
20201014::184256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184257_wf.raa
20201014::184259: Head 1: Time Synchronization: 2020.10.14   18:43:00::0015
20201014::184300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1235.7dbar, CTD 34.5psu, index 1.34, Packet 23879
20201014::184300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184307_wf.raa
20201014::184316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184317_wf.raa
20201014::184326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184327_wf.raa
20201014::184330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1237.0dbar, CTD 34.5psu, index 1.34, Packet 23934
20201014::184330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184337_wf.raa
20201014::184346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184347_wf.raa
20201014::184356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184357_wf.raa
20201014::184359: Head 1: Time Synchronization: 2020.10.14   18:44:00::0014
20201014::184359: Head 2: Time Synchronization: 2020.10.14   18:44:00::0015
20201014::184400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1237.8dbar, CTD 34.5psu, index 1.34, Packet 23988
20201014::184400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184407_wf.raa
20201014::184416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184417_wf.raa
20201014::184426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184427_wf.raa
20201014::184430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1237.7dbar, CTD 34.5psu, index 1.34, Packet 24043
20201014::184430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184437_wf.raa
20201014::184446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184447_wf.raa
20201014::184456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184457_wf.raa
20201014::184500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1237.0dbar, CTD 34.5psu, index 1.34, Packet 24097
20201014::184500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184507_wf.raa
20201014::184516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184517_wf.raa
20201014::184526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184527_wf.raa
20201014::184530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1235.8dbar, CTD 34.5psu, index 1.34, Packet 24152
20201014::184530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184537_wf.raa
20201014::184546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184547_wf.raa
20201014::184556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184557_wf.raa
20201014::184559: Head 1: Time Synchronization: 2020.10.14   18:46:00::0012
20201014::184600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1234.5dbar, CTD 34.5psu, index 1.34, Packet 24207
20201014::184600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184607_wf.raa
20201014::184616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184617_wf.raa
20201014::184626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184627_wf.raa
20201014::184630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.2dbar, CTD 34.5psu, index 1.34, Packet 24262
20201014::184630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184637_wf.raa
20201014::184646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184647_wf.raa
20201014::184656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184657_wf.raa
20201014::184659: Head 1: Time Synchronization: 2020.10.14   18:47:00::0015
20201014::184700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.9dbar, CTD 34.5psu, index 1.34, Packet 24317
20201014::184700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184707_wf.raa
20201014::184716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184717_wf.raa
20201014::184726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184727_wf.raa
20201014::184730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.2dbar, CTD 34.5psu, index 1.34, Packet 24372
20201014::184730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184737_wf.raa
20201014::184746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184747_wf.raa
20201014::184756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184757_wf.raa
20201014::184800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.7dbar, CTD 34.5psu, index 1.34, Packet 24427
20201014::184800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 11C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184807_wf.raa
20201014::184816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184817_wf.raa
20201014::184826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184827_wf.raa
20201014::184830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.1dbar, CTD 34.5psu, index 1.34, Packet 24482
20201014::184830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184837_wf.raa
20201014::184846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184847_wf.raa
20201014::184856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184857_wf.raa
20201014::184900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.4dbar, CTD 34.5psu, index 1.34, Packet 24536
20201014::184900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184907_wf.raa
20201014::184916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184917_wf.raa
20201014::184926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184927_wf.raa
20201014::184930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.7dbar, CTD 34.5psu, index 1.34, Packet 24591
20201014::184930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::184936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184937_wf.raa
20201014::184946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184947_wf.raa
20201014::184956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_184957_wf.raa
20201014::184959: Head 1: Time Synchronization: 2020.10.14   18:50:00::0018
20201014::185000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 24645
20201014::185000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185007_wf.raa
20201014::185016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185017_wf.raa
20201014::185026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185027_wf.raa
20201014::185030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 24700
20201014::185030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185037_wf.raa
20201014::185046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185047_wf.raa
20201014::185056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185057_wf.raa
20201014::185059: Head 1: Time Synchronization: 2020.10.14   18:51:00::0015
20201014::185100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.3dbar, CTD 34.5psu, index 1.34, Packet 24755
20201014::185100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185107_wf.raa
20201014::185116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185117_wf.raa
20201014::185126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185127_wf.raa
20201014::185130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.0dbar, CTD 34.5psu, index 1.34, Packet 24810
20201014::185130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185137_wf.raa
20201014::185146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185147_wf.raa
20201014::185156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185157_wf.raa
20201014::185200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1220.4dbar, CTD 34.5psu, index 1.34, Packet 24865
20201014::185200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185207_wf.raa
20201014::185216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185217_wf.raa
20201014::185226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185227_wf.raa
20201014::185230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 33.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.6dbar, CTD 34.5psu, index 1.34, Packet 24921
20201014::185230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185237_wf.raa
20201014::185246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185247_wf.raa
20201014::185256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185257_wf.raa
20201014::185259: Head 1: Time Synchronization: 2020.10.14   18:53:00::0017
20201014::185300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.8dbar, CTD 34.5psu, index 1.34, Packet 24977
20201014::185300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185307_wf.raa
20201014::185316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185317_wf.raa
20201014::185326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185327_wf.raa
20201014::185330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.9dbar, CTD 34.5psu, index 1.34, Packet 25032
20201014::185330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185337_wf.raa
20201014::185346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185347_wf.raa
20201014::185356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185357_wf.raa
20201014::185359: Head 1: Time Synchronization: 2020.10.14   18:54:00::0015
20201014::185400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1209.8dbar, CTD 34.5psu, index 1.34, Packet 25088
20201014::185400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185407_wf.raa
20201014::185416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185417_wf.raa
20201014::185426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185427_wf.raa
20201014::185430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1209.8dbar, CTD 34.5psu, index 1.34, Packet 25143
20201014::185430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185437_wf.raa
20201014::185446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185447_wf.raa
20201014::185456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185457_wf.raa
20201014::185459: Head 1: Time Synchronization: 2020.10.14   18:55:00::0014
20201014::185500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.2dbar, CTD 34.5psu, index 1.34, Packet 25199
20201014::185500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185507_wf.raa
20201014::185516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185517_wf.raa
20201014::185526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185527_wf.raa
20201014::185530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.2dbar, CTD 34.5psu, index 1.34, Packet 25255
20201014::185530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185537_wf.raa
20201014::185546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185547_wf.raa
20201014::185556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185557_wf.raa
20201014::185600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.4dbar, CTD 34.5psu, index 1.34, Packet 25310
20201014::185600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185607_wf.raa
20201014::185616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185617_wf.raa
20201014::185626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185627_wf.raa
20201014::185630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1209.3dbar, CTD 34.5psu, index 1.34, Packet 25366
20201014::185630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185637_wf.raa
20201014::185646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185647_wf.raa
20201014::185656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185657_wf.raa
20201014::185700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.1dbar, CTD 34.5psu, index 1.34, Packet 25421
20201014::185700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185707_wf.raa
20201014::185716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185717_wf.raa
20201014::185726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185727_wf.raa
20201014::185730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.4dbar, CTD 34.5psu, index 1.34, Packet 25476
20201014::185730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185737_wf.raa
20201014::185746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185747_wf.raa
20201014::185756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185757_wf.raa
20201014::185759: Head 1: Time Synchronization: 2020.10.14   18:58:00::0015
20201014::185800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.8dbar, CTD 34.5psu, index 1.34, Packet 25532
20201014::185800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185807_wf.raa
20201014::185816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185817_wf.raa
20201014::185826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185827_wf.raa
20201014::185830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1219.6dbar, CTD 34.5psu, index 1.34, Packet 25587
20201014::185830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185837_wf.raa
20201014::185846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185847_wf.raa
20201014::185856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185857_wf.raa
20201014::185859: Head 1: Time Synchronization: 2020.10.14   18:59:00::0014
20201014::185900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1222.0dbar, CTD 34.5psu, index 1.34, Packet 25642
20201014::185900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185907_wf.raa
20201014::185916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185917_wf.raa
20201014::185926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185927_wf.raa
20201014::185930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1224.2dbar, CTD 34.5psu, index 1.34, Packet 25698
20201014::185930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::185936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185937_wf.raa
20201014::185946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185947_wf.raa
20201014::185956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_185957_wf.raa
20201014::190000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.4dbar, CTD 34.5psu, index 1.34, Packet 25754
20201014::190000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190007_wf.raa
20201014::190016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190017_wf.raa
20201014::190026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190027_wf.raa
20201014::190030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 25809
20201014::190030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190037_wf.raa
20201014::190046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190047_wf.raa
20201014::190056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190057_wf.raa
20201014::190059: Head 1: Time Synchronization: 2020.10.14   19:01:00::0013
20201014::190059: Head 2: Time Synchronization: 2020.10.14   19:01:00::0014
20201014::190100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 25864
20201014::190100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190107_wf.raa
20201014::190116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190117_wf.raa
20201014::190126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190127_wf.raa
20201014::190130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.6dbar, CTD 34.5psu, index 1.34, Packet 25920
20201014::190130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190137_wf.raa
20201014::190146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190147_wf.raa
20201014::190156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190157_wf.raa
20201014::190200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1229.4dbar, CTD 34.5psu, index 1.34, Packet 25976
20201014::190200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190207_wf.raa
20201014::190216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190217_wf.raa
20201014::190226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190227_wf.raa
20201014::190230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 26031
20201014::190230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190237_wf.raa
20201014::190246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190247_wf.raa
20201014::190256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190257_wf.raa
20201014::190300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.6dbar, CTD 34.5psu, index 1.34, Packet 26086
20201014::190300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190307_wf.raa
20201014::190316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190317_wf.raa
20201014::190326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190327_wf.raa
20201014::190330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 26141
20201014::190330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190337_wf.raa
20201014::190346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190347_wf.raa
20201014::190356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190357_wf.raa
20201014::190400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 26197
20201014::190400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190407_wf.raa
20201014::190416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190417_wf.raa
20201014::190426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190427_wf.raa
20201014::190430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1233.8dbar, CTD 34.5psu, index 1.34, Packet 26252
20201014::190430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190437_wf.raa
20201014::190446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190447_wf.raa
20201014::190456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190457_wf.raa
20201014::190459: Head 1: Time Synchronization: 2020.10.14   19:05:00::0014
20201014::190500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1235.1dbar, CTD 34.5psu, index 1.34, Packet 26308
20201014::190500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190507_wf.raa
20201014::190516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190517_wf.raa
20201014::190526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190527_wf.raa
20201014::190530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1236.1dbar, CTD 34.5psu, index 1.34, Packet 26363
20201014::190530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190537_wf.raa
20201014::190546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190547_wf.raa
20201014::190556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190557_wf.raa
20201014::190600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1237.6dbar, CTD 34.5psu, index 1.34, Packet 26418
20201014::190600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190607_wf.raa
20201014::190616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190617_wf.raa
20201014::190626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190627_wf.raa
20201014::190630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1238.6dbar, CTD 34.5psu, index 1.34, Packet 26473
20201014::190630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190637_wf.raa
20201014::190646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190647_wf.raa
20201014::190656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190657_wf.raa
20201014::190659: Head 1: Time Synchronization: 2020.10.14   19:07:00::0014
20201014::190700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1239.6dbar, CTD 34.5psu, index 1.34, Packet 26529
20201014::190700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190707_wf.raa
20201014::190716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190717_wf.raa
20201014::190726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190727_wf.raa
20201014::190730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1240.9dbar, CTD 34.5psu, index 1.34, Packet 26584
20201014::190730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190737_wf.raa
20201014::190746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190747_wf.raa
20201014::190756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190757_wf.raa
20201014::190800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1240.5dbar, CTD 34.5psu, index 1.34, Packet 26640
20201014::190800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190807_wf.raa
20201014::190816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190817_wf.raa
20201014::190826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190827_wf.raa
20201014::190830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1239.1dbar, CTD 34.5psu, index 1.34, Packet 26695
20201014::190830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190837_wf.raa
20201014::190846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190847_wf.raa
20201014::190856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190857_wf.raa
20201014::190859: Head 1: Time Synchronization: 2020.10.14   19:09:00::0015
20201014::190900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1238.1dbar, CTD 34.5psu, index 1.34, Packet 26750
20201014::190900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190907_wf.raa
20201014::190916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190917_wf.raa
20201014::190926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190927_wf.raa
20201014::190930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1236.6dbar, CTD 34.5psu, index 1.34, Packet 26805
20201014::190930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::190936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190937_wf.raa
20201014::190946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190947_wf.raa
20201014::190956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_190957_wf.raa
20201014::191000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1235.4dbar, CTD 34.5psu, index 1.34, Packet 26861
20201014::191000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191007_wf.raa
20201014::191016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191017_wf.raa
20201014::191026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191027_wf.raa
20201014::191030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1234.2dbar, CTD 34.5psu, index 1.34, Packet 26916
20201014::191030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191037_wf.raa
20201014::191046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191047_wf.raa
20201014::191056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191057_wf.raa
20201014::191100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1232.5dbar, CTD 34.5psu, index 1.34, Packet 26971
20201014::191100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191107_wf.raa
20201014::191116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191117_wf.raa
20201014::191126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191127_wf.raa
20201014::191130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 27026
20201014::191130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191137_wf.raa
20201014::191146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191147_wf.raa
20201014::191156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191157_wf.raa
20201014::191159: Head 1: Time Synchronization: 2020.10.14   19:12:00::0014
20201014::191200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.3dbar, CTD 34.5psu, index 1.34, Packet 27081
20201014::191200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191207_wf.raa
20201014::191216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191217_wf.raa
20201014::191226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191227_wf.raa
20201014::191230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1230.0dbar, CTD 34.5psu, index 1.34, Packet 27136
20201014::191230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191237_wf.raa
20201014::191246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191247_wf.raa
20201014::191256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191257_wf.raa
20201014::191300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1229.4dbar, CTD 34.5psu, index 1.34, Packet 27191
20201014::191300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191307_wf.raa
20201014::191316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191317_wf.raa
20201014::191326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191327_wf.raa
20201014::191330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.5dbar, CTD 34.5psu, index 1.34, Packet 27246
20201014::191330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191337_wf.raa
20201014::191346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191347_wf.raa
20201014::191356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191357_wf.raa
20201014::191359: Head 1: Time Synchronization: 2020.10.14   19:14:00::0013
20201014::191400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 27301
20201014::191400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191407_wf.raa
20201014::191416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191417_wf.raa
20201014::191426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191427_wf.raa
20201014::191430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 27357
20201014::191430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191437_wf.raa
20201014::191446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191447_wf.raa
20201014::191456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191457_wf.raa
20201014::191459: Head 1: Time Synchronization: 2020.10.14   19:15:00::0013
20201014::191500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 27412
20201014::191500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191507_wf.raa
20201014::191516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191517_wf.raa
20201014::191526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191527_wf.raa
20201014::191530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1224.6dbar, CTD 34.5psu, index 1.34, Packet 27467
20201014::191530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191537_wf.raa
20201014::191546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191547_wf.raa
20201014::191556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191557_wf.raa
20201014::191559: Head 1: Time Synchronization: 2020.10.14   19:16:00::0015
20201014::191600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1222.5dbar, CTD 34.5psu, index 1.34, Packet 27522
20201014::191600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191607_wf.raa
20201014::191616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191617_wf.raa
20201014::191626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191627_wf.raa
20201014::191630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1220.3dbar, CTD 34.5psu, index 1.34, Packet 27577
20201014::191630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191637_wf.raa
20201014::191646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191647_wf.raa
20201014::191656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191657_wf.raa
20201014::191700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1217.5dbar, CTD 34.5psu, index 1.34, Packet 27632
20201014::191700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191707_wf.raa
20201014::191716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191717_wf.raa
20201014::191726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191727_wf.raa
20201014::191730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.3dbar, CTD 34.5psu, index 1.34, Packet 27688
20201014::191730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191737_wf.raa
20201014::191746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191747_wf.raa
20201014::191756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191757_wf.raa
20201014::191800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1212.3dbar, CTD 34.5psu, index 1.34, Packet 27742
20201014::191800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191807_wf.raa
20201014::191816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191817_wf.raa
20201014::191826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191827_wf.raa
20201014::191830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1209.6dbar, CTD 34.5psu, index 1.34, Packet 27797
20201014::191830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191837_wf.raa
20201014::191846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191847_wf.raa
20201014::191856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191857_wf.raa
20201014::191859: Head 1: Time Synchronization: 2020.10.14   19:19:00::0015
20201014::191900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1210.7dbar, CTD 34.5psu, index 1.34, Packet 27852
20201014::191900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191907_wf.raa
20201014::191916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191917_wf.raa
20201014::191926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191927_wf.raa
20201014::191930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1212.4dbar, CTD 34.5psu, index 1.34, Packet 27907
20201014::191930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::191936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191937_wf.raa
20201014::191946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191947_wf.raa
20201014::191956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_191957_wf.raa
20201014::192000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1213.3dbar, CTD 34.5psu, index 1.34, Packet 27963
20201014::192000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192007_wf.raa
20201014::192016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192017_wf.raa
20201014::192026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192027_wf.raa
20201014::192030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1211.8dbar, CTD 34.5psu, index 1.34, Packet 28017
20201014::192030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192037_wf.raa
20201014::192046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192047_wf.raa
20201014::192056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192057_wf.raa
20201014::192059: Head 1: Time Synchronization: 2020.10.14   19:21:00::0014
20201014::192100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1210.2dbar, CTD 34.5psu, index 1.34, Packet 28072
20201014::192100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192107_wf.raa
20201014::192116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192117_wf.raa
20201014::192126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192127_wf.raa
20201014::192130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.7dbar, CTD 34.5psu, index 1.34, Packet 28128
20201014::192130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192137_wf.raa
20201014::192146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192147_wf.raa
20201014::192156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192157_wf.raa
20201014::192200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.0dbar, CTD 34.5psu, index 1.34, Packet 28183
20201014::192200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192207_wf.raa
20201014::192216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192217_wf.raa
20201014::192226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192227_wf.raa
20201014::192230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.9dbar, CTD 34.5psu, index 1.34, Packet 28239
20201014::192230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192237_wf.raa
20201014::192246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192247_wf.raa
20201014::192256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192257_wf.raa
20201014::192300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1219.5dbar, CTD 34.5psu, index 1.34, Packet 28293
20201014::192300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192307_wf.raa
20201014::192316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192317_wf.raa
20201014::192326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192327_wf.raa
20201014::192330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1220.3dbar, CTD 34.5psu, index 1.34, Packet 28348
20201014::192330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192337_wf.raa
20201014::192346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192347_wf.raa
20201014::192356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192357_wf.raa
20201014::192359: Head 1: Time Synchronization: 2020.10.14   19:24:00::0015
20201014::192400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.8dbar, CTD 34.5psu, index 1.34, Packet 28404
20201014::192400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192407_wf.raa
20201014::192416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192417_wf.raa
20201014::192426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192427_wf.raa
20201014::192430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.1dbar, CTD 34.5psu, index 1.34, Packet 28459
20201014::192430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192437_wf.raa
20201014::192446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192447_wf.raa
20201014::192456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192457_wf.raa
20201014::192500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 28515
20201014::192500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192507_wf.raa
20201014::192516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192517_wf.raa
20201014::192526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192527_wf.raa
20201014::192530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 28571
20201014::192530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192537_wf.raa
20201014::192546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192547_wf.raa
20201014::192556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192557_wf.raa
20201014::192559: Head 1: Time Synchronization: 2020.10.14   19:26:00::0015
20201014::192600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 28626
20201014::192600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192607_wf.raa
20201014::192616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192617_wf.raa
20201014::192626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192627_wf.raa
20201014::192630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 28682
20201014::192630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192637_wf.raa
20201014::192646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192647_wf.raa
20201014::192656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192657_wf.raa
20201014::192659: Head 1: Time Synchronization: 2020.10.14   19:27:00::0014
20201014::192659: Head 2: Time Synchronization: 2020.10.14   19:27:00::0014
20201014::192700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.5dbar, CTD 34.5psu, index 1.34, Packet 28738
20201014::192700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192707_wf.raa
20201014::192716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192717_wf.raa
20201014::192726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192727_wf.raa
20201014::192730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.7dbar, CTD 34.5psu, index 1.34, Packet 28793
20201014::192730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192737_wf.raa
20201014::192746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192747_wf.raa
20201014::192756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192757_wf.raa
20201014::192759: Head 1: Time Synchronization: 2020.10.14   19:28:00::0016
20201014::192800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.5dbar, CTD 34.5psu, index 1.34, Packet 28848
20201014::192800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192807_wf.raa
20201014::192816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192817_wf.raa
20201014::192826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192827_wf.raa
20201014::192830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.4dbar, CTD 34.5psu, index 1.34, Packet 28903
20201014::192830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192837_wf.raa
20201014::192846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192847_wf.raa
20201014::192856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192857_wf.raa
20201014::192900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.4dbar, CTD 34.5psu, index 1.34, Packet 28958
20201014::192900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192907_wf.raa
20201014::192916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192917_wf.raa
20201014::192926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192927_wf.raa
20201014::192930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.9dbar, CTD 34.5psu, index 1.34, Packet 29014
20201014::192930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::192936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192937_wf.raa
20201014::192946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192947_wf.raa
20201014::192956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_192957_wf.raa
20201014::192959: Head 2: Time Synchronization: 2020.10.14   19:30:00::0019
20201014::192959: Head 1: Time Synchronization: 2020.10.14   19:30:00::0020
20201014::193000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.9dbar, CTD 34.5psu, index 1.34, Packet 29069
20201014::193000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193007_wf.raa
20201014::193016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193017_wf.raa
20201014::193026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193027_wf.raa
20201014::193030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.5dbar, CTD 34.5psu, index 1.34, Packet 29124
20201014::193030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193037_wf.raa
20201014::193046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193047_wf.raa
20201014::193056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193057_wf.raa
20201014::193100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.5dbar, CTD 34.5psu, index 1.34, Packet 29179
20201014::193100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193107_wf.raa
20201014::193116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193117_wf.raa
20201014::193126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193127_wf.raa
20201014::193130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.8dbar, CTD 34.5psu, index 1.34, Packet 29234
20201014::193130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193137_wf.raa
20201014::193146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193147_wf.raa
20201014::193156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193157_wf.raa
20201014::193159: Head 1: Time Synchronization: 2020.10.14   19:32:00::0011
20201014::193200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.6dbar, CTD 34.5psu, index 1.34, Packet 29289
20201014::193200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193207_wf.raa
20201014::193216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193217_wf.raa
20201014::193226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193227_wf.raa
20201014::193230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.3dbar, CTD 34.5psu, index 1.34, Packet 29345
20201014::193230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193237_wf.raa
20201014::193246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193247_wf.raa
20201014::193256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193257_wf.raa
20201014::193259: Head 1: Time Synchronization: 2020.10.14   19:33:00::0018
20201014::193300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.4dbar, CTD 34.5psu, index 1.34, Packet 29400
20201014::193300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193307_wf.raa
20201014::193316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193317_wf.raa
20201014::193326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193327_wf.raa
20201014::193330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.8dbar, CTD 34.5psu, index 1.34, Packet 29455
20201014::193330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193337_wf.raa
20201014::193346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193347_wf.raa
20201014::193356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193357_wf.raa
20201014::193400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.3dbar, CTD 34.5psu, index 1.34, Packet 29510
20201014::193400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193407_wf.raa
20201014::193416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193417_wf.raa
20201014::193426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193427_wf.raa
20201014::193430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.1dbar, CTD 34.5psu, index 1.34, Packet 29565
20201014::193430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193437_wf.raa
20201014::193446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193447_wf.raa
20201014::193456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193457_wf.raa
20201014::193500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.6dbar, CTD 34.5psu, index 1.34, Packet 29620
20201014::193500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193507_wf.raa
20201014::193516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193517_wf.raa
20201014::193526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193527_wf.raa
20201014::193530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.3dbar, CTD 34.5psu, index 1.34, Packet 29675
20201014::193530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193537_wf.raa
20201014::193546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193547_wf.raa
20201014::193556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193557_wf.raa
20201014::193559: Head 1: Time Synchronization: 2020.10.14   19:36:00::0015
20201014::193600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.5dbar, CTD 34.5psu, index 1.34, Packet 29730
20201014::193600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193607_wf.raa
20201014::193616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193617_wf.raa
20201014::193626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193627_wf.raa
20201014::193630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.3dbar, CTD 34.5psu, index 1.34, Packet 29785
20201014::193630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193637_wf.raa
20201014::193646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193647_wf.raa
20201014::193656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193657_wf.raa
20201014::193659: Head 1: Time Synchronization: 2020.10.14   19:37:00::0015
20201014::193700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 29840
20201014::193700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193707_wf.raa
20201014::193716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193717_wf.raa
20201014::193726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193727_wf.raa
20201014::193730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 29895
20201014::193730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193737_wf.raa
20201014::193746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193747_wf.raa
20201014::193756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193757_wf.raa
20201014::193800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 29950
20201014::193800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193807_wf.raa
20201014::193816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193817_wf.raa
20201014::193826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193827_wf.raa
20201014::193830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 30005
20201014::193830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193837_wf.raa
20201014::193846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193847_wf.raa
20201014::193856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193857_wf.raa
20201014::193859: Head 1: Time Synchronization: 2020.10.14   19:39:00::0012
20201014::193900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.9dbar, CTD 34.5psu, index 1.34, Packet 30060
20201014::193900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193907_wf.raa
20201014::193916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193917_wf.raa
20201014::193926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193927_wf.raa
20201014::193930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1225.3dbar, CTD 34.5psu, index 1.34, Packet 30115
20201014::193930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::193936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193937_wf.raa
20201014::193946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193947_wf.raa
20201014::193956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_193957_wf.raa
20201014::193959: Head 1: Time Synchronization: 2020.10.14   19:40:00::0014
20201014::194000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.2dbar, CTD 34.5psu, index 1.34, Packet 30170
20201014::194000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194007_wf.raa
20201014::194016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194017_wf.raa
20201014::194026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194027_wf.raa
20201014::194030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.3dbar, CTD 34.5psu, index 1.34, Packet 30225
20201014::194030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194037_wf.raa
20201014::194046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194047_wf.raa
20201014::194056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194057_wf.raa
20201014::194059: Head 2: Time Synchronization: 2020.10.14   19:41:00::0015
20201014::194100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.3dbar, CTD 34.5psu, index 1.34, Packet 30281
20201014::194100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194107_wf.raa
20201014::194116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194117_wf.raa
20201014::194126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194127_wf.raa
20201014::194130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.3dbar, CTD 34.5psu, index 1.34, Packet 30335
20201014::194130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194137_wf.raa
20201014::194146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194147_wf.raa
20201014::194156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194157_wf.raa
20201014::194159: Head 2: Time Synchronization: 2020.10.14   19:42:00::0013
20201014::194200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.5dbar, CTD 34.5psu, index 1.34, Packet 30390
20201014::194200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194207_wf.raa
20201014::194216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194217_wf.raa
20201014::194226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194227_wf.raa
20201014::194230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1210.4dbar, CTD 34.5psu, index 1.34, Packet 30446
20201014::194230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194237_wf.raa
20201014::194246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194247_wf.raa
20201014::194256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194257_wf.raa
20201014::194300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1210.5dbar, CTD 34.5psu, index 1.34, Packet 30501
20201014::194300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194307_wf.raa
20201014::194316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194317_wf.raa
20201014::194326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194327_wf.raa
20201014::194330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.0dbar, CTD 34.5psu, index 1.34, Packet 30556
20201014::194330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194337_wf.raa
20201014::194346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194347_wf.raa
20201014::194356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194357_wf.raa
20201014::194400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.4dbar, CTD 34.5psu, index 1.34, Packet 30612
20201014::194400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194407_wf.raa
20201014::194416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194417_wf.raa
20201014::194426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194427_wf.raa
20201014::194430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.7dbar, CTD 34.5psu, index 1.34, Packet 30667
20201014::194430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194437_wf.raa
20201014::194446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194447_wf.raa
20201014::194456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194457_wf.raa
20201014::194500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.3dbar, CTD 34.5psu, index 1.34, Packet 30722
20201014::194500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194507_wf.raa
20201014::194516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194517_wf.raa
20201014::194526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194527_wf.raa
20201014::194530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1211.0dbar, CTD 34.5psu, index 1.34, Packet 30777
20201014::194530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194537_wf.raa
20201014::194546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194547_wf.raa
20201014::194556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194557_wf.raa
20201014::194600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1210.9dbar, CTD 34.5psu, index 1.34, Packet 30832
20201014::194600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194607_wf.raa
20201014::194616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194617_wf.raa
20201014::194626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194627_wf.raa
20201014::194630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.2dbar, CTD 34.5psu, index 1.34, Packet 30887
20201014::194630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194637_wf.raa
20201014::194646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194647_wf.raa
20201014::194656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194657_wf.raa
20201014::194659: Head 1: Time Synchronization: 2020.10.14   19:47:00::0012
20201014::194700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.1dbar, CTD 34.5psu, index 1.34, Packet 30942
20201014::194700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194707_wf.raa
20201014::194716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194717_wf.raa
20201014::194726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194727_wf.raa
20201014::194730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.9dbar, CTD 34.5psu, index 1.34, Packet 30997
20201014::194730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194737_wf.raa
20201014::194746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194747_wf.raa
20201014::194756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194757_wf.raa
20201014::194759: Head 2: Time Synchronization: 2020.10.14   19:48:00::0015
20201014::194800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.4dbar, CTD 34.5psu, index 1.34, Packet 31053
20201014::194800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194807_wf.raa
20201014::194816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194817_wf.raa
20201014::194826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194827_wf.raa
20201014::194830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1223.0dbar, CTD 34.5psu, index 1.34, Packet 31108
20201014::194830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194837_wf.raa
20201014::194846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194847_wf.raa
20201014::194856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194857_wf.raa
20201014::194859: Head 1: Time Synchronization: 2020.10.14   19:49:00::0015
20201014::194900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1225.8dbar, CTD 34.5psu, index 1.34, Packet 31162
20201014::194900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194907_wf.raa
20201014::194916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194917_wf.raa
20201014::194926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194927_wf.raa
20201014::194930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 31217
20201014::194930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::194936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194937_wf.raa
20201014::194946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194947_wf.raa
20201014::194956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_194957_wf.raa
20201014::195000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1226.8dbar, CTD 34.5psu, index 1.34, Packet 31273
20201014::195000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195007_wf.raa
20201014::195016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195017_wf.raa
20201014::195026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195027_wf.raa
20201014::195030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 31328
20201014::195030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195037_wf.raa
20201014::195046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195047_wf.raa
20201014::195056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195057_wf.raa
20201014::195059: Head 1: Time Synchronization: 2020.10.14   19:51:00::0015
20201014::195100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 31383
20201014::195100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195107_wf.raa
20201014::195116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195117_wf.raa
20201014::195126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195127_wf.raa
20201014::195130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.7dbar, CTD 34.5psu, index 1.34, Packet 31438
20201014::195130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195137_wf.raa
20201014::195146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195147_wf.raa
20201014::195156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195157_wf.raa
20201014::195200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.9dbar, CTD 34.5psu, index 1.34, Packet 31493
20201014::195200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195207_wf.raa
20201014::195216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195217_wf.raa
20201014::195226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195227_wf.raa
20201014::195230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1229.3dbar, CTD 34.5psu, index 1.34, Packet 31548
20201014::195230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195237_wf.raa
20201014::195246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195247_wf.raa
20201014::195256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195257_wf.raa
20201014::195259: Head 1: Time Synchronization: 2020.10.14   19:53:00::0015
20201014::195300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1230.3dbar, CTD 34.5psu, index 1.34, Packet 31604
20201014::195300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195307_wf.raa
20201014::195316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195317_wf.raa
20201014::195326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195327_wf.raa
20201014::195330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1232.3dbar, CTD 34.5psu, index 1.34, Packet 31659
20201014::195330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195337_wf.raa
20201014::195346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195347_wf.raa
20201014::195356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195357_wf.raa
20201014::195359: Head 2: Time Synchronization: 2020.10.14   19:54:00::0015
20201014::195359: Head 1: Time Synchronization: 2020.10.14   19:54:00::0015
20201014::195400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 31714
20201014::195400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195407_wf.raa
20201014::195416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195417_wf.raa
20201014::195426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195427_wf.raa
20201014::195430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1235.6dbar, CTD 34.5psu, index 1.34, Packet 31769
20201014::195430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195437_wf.raa
20201014::195446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195447_wf.raa
20201014::195456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195457_wf.raa
20201014::195459: Head 1: Time Synchronization: 2020.10.14   19:55:00::0015
20201014::195500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1236.8dbar, CTD 34.5psu, index 1.34, Packet 31824
20201014::195500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195507_wf.raa
20201014::195516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195517_wf.raa
20201014::195526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195527_wf.raa
20201014::195530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1238.0dbar, CTD 34.5psu, index 1.34, Packet 31879
20201014::195530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195537_wf.raa
20201014::195546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195547_wf.raa
20201014::195556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195557_wf.raa
20201014::195600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1238.8dbar, CTD 34.5psu, index 1.34, Packet 31934
20201014::195600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195607_wf.raa
20201014::195616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195617_wf.raa
20201014::195626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195627_wf.raa
20201014::195630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.9C, CTD 1240.4dbar, CTD 34.5psu, index 1.34, Packet 31989
20201014::195630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195637_wf.raa
20201014::195646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195647_wf.raa
20201014::195656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195657_wf.raa
20201014::195700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 2.9C, CTD 1239.6dbar, CTD 34.5psu, index 1.34, Packet 32045
20201014::195700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195707_wf.raa
20201014::195716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195717_wf.raa
20201014::195726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195727_wf.raa
20201014::195730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1238.1dbar, CTD 34.5psu, index 1.34, Packet 32100
20201014::195730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195737_wf.raa
20201014::195746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195747_wf.raa
20201014::195756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195757_wf.raa
20201014::195800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1236.6dbar, CTD 34.5psu, index 1.34, Packet 32155
20201014::195800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195807_wf.raa
20201014::195816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195817_wf.raa
20201014::195826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195827_wf.raa
20201014::195830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1235.4dbar, CTD 34.5psu, index 1.34, Packet 32210
20201014::195830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195837_wf.raa
20201014::195846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195847_wf.raa
20201014::195856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195857_wf.raa
20201014::195859: Head 1: Time Synchronization: 2020.10.14   19:59:00::0012
20201014::195900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1233.6dbar, CTD 34.5psu, index 1.34, Packet 32265
20201014::195900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195907_wf.raa
20201014::195916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195917_wf.raa
20201014::195926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195927_wf.raa
20201014::195930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1231.5dbar, CTD 34.5psu, index 1.34, Packet 32320
20201014::195930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::195936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195937_wf.raa
20201014::195946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195947_wf.raa
20201014::195956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_195957_wf.raa
20201014::195959: Head 1: Time Synchronization: 2020.10.14   20:00:00::0015
20201014::200000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1229.3dbar, CTD 34.5psu, index 1.34, Packet 32375
20201014::200000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200007_wf.raa
20201014::200016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200017_wf.raa
20201014::200026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200027_wf.raa
20201014::200030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1229.0dbar, CTD 34.5psu, index 1.34, Packet 32430
20201014::200030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200037_wf.raa
20201014::200046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200047_wf.raa
20201014::200056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200057_wf.raa
20201014::200059: Head 1: Time Synchronization: 2020.10.14   20:01:00::0011
20201014::200100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.7dbar, CTD 34.5psu, index 1.34, Packet 32484
20201014::200100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200107_wf.raa
20201014::200116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200117_wf.raa
20201014::200126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200127_wf.raa
20201014::200130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 32540
20201014::200130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200137_wf.raa
20201014::200146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200147_wf.raa
20201014::200156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200157_wf.raa
20201014::200200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 32594
20201014::200200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200207_wf.raa
20201014::200216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200217_wf.raa
20201014::200226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200227_wf.raa
20201014::200230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 32649
20201014::200230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200237_wf.raa
20201014::200246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200247_wf.raa
20201014::200256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200257_wf.raa
20201014::200300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1226.6dbar, CTD 34.5psu, index 1.34, Packet 32703
20201014::200300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200307_wf.raa
20201014::200316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200317_wf.raa
20201014::200326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200327_wf.raa
20201014::200330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1226.3dbar, CTD 34.5psu, index 1.34, Packet 32758
20201014::200330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200337_wf.raa
20201014::200346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200347_wf.raa
20201014::200356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200357_wf.raa
20201014::200359: Head 1: Time Synchronization: 2020.10.14   20:04:00::0014
20201014::200359: Head 2: Time Synchronization: 2020.10.14   20:04:00::0015
20201014::200400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 32813
20201014::200400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200407_wf.raa
20201014::200416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200417_wf.raa
20201014::200426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200427_wf.raa
20201014::200430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.6dbar, CTD 34.5psu, index 1.34, Packet 32869
20201014::200430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200437_wf.raa
20201014::200446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200447_wf.raa
20201014::200456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200457_wf.raa
20201014::200459: Head 2: Time Synchronization: 2020.10.14   20:05:00::0016
20201014::200500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1220.6dbar, CTD 34.5psu, index 1.34, Packet 32923
20201014::200500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200507_wf.raa
20201014::200516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200517_wf.raa
20201014::200526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200527_wf.raa
20201014::200530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1218.2dbar, CTD 34.5psu, index 1.34, Packet 32978
20201014::200530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200537_wf.raa
20201014::200546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200547_wf.raa
20201014::200556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200557_wf.raa
20201014::200600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1215.2dbar, CTD 34.5psu, index 1.34, Packet 33033
20201014::200600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200607_wf.raa
20201014::200616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200617_wf.raa
20201014::200626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200627_wf.raa
20201014::200630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.6dbar, CTD 34.5psu, index 1.34, Packet 33088
20201014::200630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200637_wf.raa
20201014::200646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200647_wf.raa
20201014::200656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200657_wf.raa
20201014::200659: Head 1: Time Synchronization: 2020.10.14   20:07:00::0014
20201014::200700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.5dbar, CTD 34.5psu, index 1.34, Packet 33143
20201014::200700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200707_wf.raa
20201014::200716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200717_wf.raa
20201014::200726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200727_wf.raa
20201014::200730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.4dbar, CTD 34.5psu, index 1.34, Packet 33197
20201014::200730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200737_wf.raa
20201014::200746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200747_wf.raa
20201014::200756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200757_wf.raa
20201014::200800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1212.5dbar, CTD 34.5psu, index 1.34, Packet 33251
20201014::200800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200807_wf.raa
20201014::200816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200817_wf.raa
20201014::200826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200827_wf.raa
20201014::200830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1213.8dbar, CTD 34.5psu, index 1.34, Packet 33306
20201014::200830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200837_wf.raa
20201014::200846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200847_wf.raa
20201014::200856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200857_wf.raa
20201014::200859: Head 1: Time Synchronization: 2020.10.14   20:09:00::0014
20201014::200900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1214.0dbar, CTD 34.5psu, index 1.34, Packet 33361
20201014::200900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200907_wf.raa
20201014::200916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200917_wf.raa
20201014::200926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200927_wf.raa
20201014::200930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1212.7dbar, CTD 34.5psu, index 1.34, Packet 33416
20201014::200930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::200936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200937_wf.raa
20201014::200946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200947_wf.raa
20201014::200956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_200957_wf.raa
20201014::201000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.8dbar, CTD 34.5psu, index 1.34, Packet 33471
20201014::201000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201007_wf.raa
20201014::201016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201017_wf.raa
20201014::201026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201027_wf.raa
20201014::201030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.0dbar, CTD 34.5psu, index 1.34, Packet 33526
20201014::201030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201037_wf.raa
20201014::201046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201047_wf.raa
20201014::201056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201057_wf.raa
20201014::201059: Head 1: Time Synchronization: 2020.10.14   20:11:00::0016
20201014::201100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.5dbar, CTD 34.5psu, index 1.34, Packet 33582
20201014::201100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201107_wf.raa
20201014::201116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201117_wf.raa
20201014::201126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201127_wf.raa
20201014::201130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.9dbar, CTD 34.5psu, index 1.34, Packet 33636
20201014::201130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201137_wf.raa
20201014::201146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201147_wf.raa
20201014::201156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201157_wf.raa
20201014::201159: Head 1: Time Synchronization: 2020.10.14   20:12:00::0013
20201014::201200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1217.6dbar, CTD 34.5psu, index 1.34, Packet 33691
20201014::201200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201207_wf.raa
20201014::201216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201217_wf.raa
20201014::201226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201227_wf.raa
20201014::201230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1220.9dbar, CTD 34.5psu, index 1.34, Packet 33746
20201014::201230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201237_wf.raa
20201014::201246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201247_wf.raa
20201014::201256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201257_wf.raa
20201014::201259: Head 1: Time Synchronization: 2020.10.14   20:13:00::0014
20201014::201300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1222.3dbar, CTD 34.5psu, index 1.34, Packet 33800
20201014::201300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201307_wf.raa
20201014::201316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201317_wf.raa
20201014::201326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201327_wf.raa
20201014::201330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.5dbar, CTD 34.5psu, index 1.34, Packet 33855
20201014::201330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201337_wf.raa
20201014::201346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201347_wf.raa
20201014::201356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201357_wf.raa
20201014::201400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.2dbar, CTD 34.5psu, index 1.34, Packet 33910
20201014::201400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201407_wf.raa
20201014::201416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201417_wf.raa
20201014::201426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201427_wf.raa
20201014::201430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.6dbar, CTD 34.5psu, index 1.34, Packet 33966
20201014::201430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201437_wf.raa
20201014::201446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201447_wf.raa
20201014::201456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201457_wf.raa
20201014::201500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 34020
20201014::201500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201507_wf.raa
20201014::201516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201517_wf.raa
20201014::201526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201527_wf.raa
20201014::201530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 34075
20201014::201530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201537_wf.raa
20201014::201546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201547_wf.raa
20201014::201556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201557_wf.raa
20201014::201600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.2dbar, CTD 34.5psu, index 1.34, Packet 34130
20201014::201600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201607_wf.raa
20201014::201616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201617_wf.raa
20201014::201626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201627_wf.raa
20201014::201630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.5dbar, CTD 34.5psu, index 1.34, Packet 34184
20201014::201630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201637_wf.raa
20201014::201646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201647_wf.raa
20201014::201656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201657_wf.raa
20201014::201659: Head 1: Time Synchronization: 2020.10.14   20:17:00::0012
20201014::201700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1228.8dbar, CTD 34.5psu, index 1.34, Packet 34238
20201014::201700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201707_wf.raa
20201014::201716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201717_wf.raa
20201014::201726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201727_wf.raa
20201014::201730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 34293
20201014::201730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201737_wf.raa
20201014::201746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201747_wf.raa
20201014::201756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201757_wf.raa
20201014::201800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.5dbar, CTD 34.5psu, index 1.34, Packet 34347
20201014::201800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201807_wf.raa
20201014::201816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201817_wf.raa
20201014::201826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201827_wf.raa
20201014::201830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1232.4dbar, CTD 34.5psu, index 1.34, Packet 34402
20201014::201830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201837_wf.raa
20201014::201846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201847_wf.raa
20201014::201856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201857_wf.raa
20201014::201859: Head 1: Time Synchronization: 2020.10.14   20:19:00::0017
20201014::201900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1234.4dbar, CTD 34.5psu, index 1.34, Packet 34457
20201014::201900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201907_wf.raa
20201014::201916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201917_wf.raa
20201014::201926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201927_wf.raa
20201014::201930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1236.1dbar, CTD 34.5psu, index 1.34, Packet 34511
20201014::201930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::201936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201937_wf.raa
20201014::201946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201947_wf.raa
20201014::201956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_201957_wf.raa
20201014::201959: Head 1: Time Synchronization: 2020.10.14   20:20:00::0014
20201014::202000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1237.7dbar, CTD 34.5psu, index 1.34, Packet 34566
20201014::202000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202007_wf.raa
20201014::202016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202017_wf.raa
20201014::202026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202027_wf.raa
20201014::202030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.0dbar, CTD 34.5psu, index 1.34, Packet 34621
20201014::202030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202037_wf.raa
20201014::202046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202047_wf.raa
20201014::202056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202057_wf.raa
20201014::202059: Head 1: Time Synchronization: 2020.10.14   20:21:00::0016
20201014::202100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1240.4dbar, CTD 34.5psu, index 1.34, Packet 34676
20201014::202100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202107_wf.raa
20201014::202116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202117_wf.raa
20201014::202126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202127_wf.raa
20201014::202130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1238.8dbar, CTD 34.5psu, index 1.34, Packet 34731
20201014::202130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202137_wf.raa
20201014::202146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202147_wf.raa
20201014::202156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202157_wf.raa
20201014::202159: Head 1: Time Synchronization: 2020.10.14   20:22:00::0017
20201014::202200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1237.3dbar, CTD 34.5psu, index 1.34, Packet 34785
20201014::202200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202207_wf.raa
20201014::202216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202217_wf.raa
20201014::202226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202227_wf.raa
20201014::202230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1235.7dbar, CTD 34.5psu, index 1.34, Packet 34840
20201014::202230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202237_wf.raa
20201014::202246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202247_wf.raa
20201014::202256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202257_wf.raa
20201014::202300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.4dbar, CTD 34.5psu, index 1.34, Packet 34895
20201014::202300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202307_wf.raa
20201014::202316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202317_wf.raa
20201014::202326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202327_wf.raa
20201014::202330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.8dbar, CTD 34.5psu, index 1.34, Packet 34950
20201014::202330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202337_wf.raa
20201014::202346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202347_wf.raa
20201014::202356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202357_wf.raa
20201014::202400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.0C, CTD 1230.2dbar, CTD 34.5psu, index 1.34, Packet 35005
20201014::202400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202407_wf.raa
20201014::202416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202417_wf.raa
20201014::202426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202427_wf.raa
20201014::202430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.0dbar, CTD 34.5psu, index 1.34, Packet 35059
20201014::202430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202437_wf.raa
20201014::202446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202447_wf.raa
20201014::202456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202457_wf.raa
20201014::202500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 35113
20201014::202500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202507_wf.raa
20201014::202516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202517_wf.raa
20201014::202526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202527_wf.raa
20201014::202530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 35169
20201014::202530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202537_wf.raa
20201014::202546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202547_wf.raa
20201014::202556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202557_wf.raa
20201014::202600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 35223
20201014::202600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202607_wf.raa
20201014::202616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202617_wf.raa
20201014::202626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202627_wf.raa
20201014::202630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 35278
20201014::202630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202637_wf.raa
20201014::202646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202647_wf.raa
20201014::202656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202657_wf.raa
20201014::202659: Head 1: Time Synchronization: 2020.10.14   20:27:00::0015
20201014::202700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1226.6dbar, CTD 34.5psu, index 1.34, Packet 35332
20201014::202700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202707_wf.raa
20201014::202716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202717_wf.raa
20201014::202726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202727_wf.raa
20201014::202730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1226.3dbar, CTD 34.5psu, index 1.34, Packet 35387
20201014::202730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202737_wf.raa
20201014::202746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202747_wf.raa
20201014::202756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202757_wf.raa
20201014::202800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1225.9dbar, CTD 34.5psu, index 1.34, Packet 35441
20201014::202800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202807_wf.raa
20201014::202816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202817_wf.raa
20201014::202826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202827_wf.raa
20201014::202830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 31.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1224.0dbar, CTD 34.5psu, index 1.34, Packet 35496
20201014::202830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202837_wf.raa
20201014::202846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202847_wf.raa
20201014::202856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202857_wf.raa
20201014::202859: Head 2: Time Synchronization: 2020.10.14   20:29:00::0015
20201014::202900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1221.6dbar, CTD 34.5psu, index 1.34, Packet 35551
20201014::202900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202907_wf.raa
20201014::202916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202917_wf.raa
20201014::202926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202927_wf.raa
20201014::202930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1219.4dbar, CTD 34.5psu, index 1.34, Packet 35605
20201014::202930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::202936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202937_wf.raa
20201014::202946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202947_wf.raa
20201014::202956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_202957_wf.raa
20201014::203000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.8dbar, CTD 34.5psu, index 1.34, Packet 35660
20201014::203000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203007_wf.raa
20201014::203016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203017_wf.raa
20201014::203026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203027_wf.raa
20201014::203030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.5dbar, CTD 34.5psu, index 1.34, Packet 35714
20201014::203030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203037_wf.raa
20201014::203046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203047_wf.raa
20201014::203056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203057_wf.raa
20201014::203100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.6dbar, CTD 34.5psu, index 1.34, Packet 35769
20201014::203100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203107_wf.raa
20201014::203116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203117_wf.raa
20201014::203126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203127_wf.raa
20201014::203130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.8dbar, CTD 34.5psu, index 1.34, Packet 35824
20201014::203130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203137_wf.raa
20201014::203146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203147_wf.raa
20201014::203156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203157_wf.raa
20201014::203159: Head 1: Time Synchronization: 2020.10.14   20:32:00::0015
20201014::203159: Head 2: Time Synchronization: 2020.10.14   20:32:00::0016
20201014::203200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.4dbar, CTD 34.5psu, index 1.34, Packet 35878
20201014::203200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203207_wf.raa
20201014::203216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203217_wf.raa
20201014::203226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203227_wf.raa
20201014::203230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.4dbar, CTD 34.5psu, index 1.34, Packet 35933
20201014::203230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203237_wf.raa
20201014::203246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203247_wf.raa
20201014::203256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203257_wf.raa
20201014::203259: Head 1: Time Synchronization: 2020.10.14   20:33:00::0015
20201014::203300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.1dbar, CTD 34.5psu, index 1.34, Packet 35988
20201014::203300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203307_wf.raa
20201014::203316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203317_wf.raa
20201014::203326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203327_wf.raa
20201014::203330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.2dbar, CTD 34.5psu, index 1.34, Packet 36042
20201014::203330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203337_wf.raa
20201014::203346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203347_wf.raa
20201014::203356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203357_wf.raa
20201014::203359: Head 2: Time Synchronization: 2020.10.14   20:34:00::0015
20201014::203359: Head 1: Time Synchronization: 2020.10.14   20:34:00::0015
20201014::203400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.5dbar, CTD 34.5psu, index 1.34, Packet 36096
20201014::203400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203407_wf.raa
20201014::203416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203417_wf.raa
20201014::203426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203427_wf.raa
20201014::203430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1211.9dbar, CTD 34.5psu, index 1.34, Packet 36152
20201014::203430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203437_wf.raa
20201014::203446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203447_wf.raa
20201014::203456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203457_wf.raa
20201014::203459: Head 1: Time Synchronization: 2020.10.14   20:35:00::0015
20201014::203500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.2dbar, CTD 34.5psu, index 1.34, Packet 36206
20201014::203500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203507_wf.raa
20201014::203516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203517_wf.raa
20201014::203526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203527_wf.raa
20201014::203530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.4dbar, CTD 34.5psu, index 1.34, Packet 36261
20201014::203530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203537_wf.raa
20201014::203546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203547_wf.raa
20201014::203556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203557_wf.raa
20201014::203559: Head 1: Time Synchronization: 2020.10.14   20:36:00::0016
20201014::203600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1216.2dbar, CTD 34.5psu, index 1.34, Packet 36317
20201014::203600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203607_wf.raa
20201014::203616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203617_wf.raa
20201014::203626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203627_wf.raa
20201014::203630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1218.7dbar, CTD 34.5psu, index 1.34, Packet 36371
20201014::203630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203637_wf.raa
20201014::203646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203647_wf.raa
20201014::203656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203657_wf.raa
20201014::203659: Head 1: Time Synchronization: 2020.10.14   20:37:00::0016
20201014::203700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1221.0dbar, CTD 34.5psu, index 1.34, Packet 36425
20201014::203700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203707_wf.raa
20201014::203716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203717_wf.raa
20201014::203726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203727_wf.raa
20201014::203730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1222.9dbar, CTD 34.5psu, index 1.34, Packet 36480
20201014::203730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203737_wf.raa
20201014::203746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203747_wf.raa
20201014::203756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203757_wf.raa
20201014::203759: Head 1: Time Synchronization: 2020.10.14   20:38:00::0017
20201014::203800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1225.3dbar, CTD 34.5psu, index 1.34, Packet 36534
20201014::203800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203807_wf.raa
20201014::203816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203817_wf.raa
20201014::203826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203827_wf.raa
20201014::203830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1226.1dbar, CTD 34.5psu, index 1.34, Packet 36589
20201014::203830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203837_wf.raa
20201014::203846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203847_wf.raa
20201014::203856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203857_wf.raa
20201014::203900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1226.4dbar, CTD 34.5psu, index 1.34, Packet 36644
20201014::203900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203907_wf.raa
20201014::203916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203917_wf.raa
20201014::203926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203927_wf.raa
20201014::203930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.9dbar, CTD 34.5psu, index 1.34, Packet 36699
20201014::203930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::203936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203937_wf.raa
20201014::203946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203947_wf.raa
20201014::203956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_203957_wf.raa
20201014::203959: Head 1: Time Synchronization: 2020.10.14   20:40:00::0015
20201014::204000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 36753
20201014::204000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204007_wf.raa
20201014::204016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204017_wf.raa
20201014::204026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204027_wf.raa
20201014::204030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 36808
20201014::204030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204037_wf.raa
20201014::204046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204047_wf.raa
20201014::204056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204057_wf.raa
20201014::204100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 36863
20201014::204100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204107_wf.raa
20201014::204116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204117_wf.raa
20201014::204126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204127_wf.raa
20201014::204130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 36918
20201014::204130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204137_wf.raa
20201014::204146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204147_wf.raa
20201014::204156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204157_wf.raa
20201014::204159: Head 1: Time Synchronization: 2020.10.14   20:42:00::0015
20201014::204200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 36973
20201014::204200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204207_wf.raa
20201014::204216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204217_wf.raa
20201014::204226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204227_wf.raa
20201014::204230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.7dbar, CTD 34.5psu, index 1.34, Packet 37027
20201014::204230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204237_wf.raa
20201014::204246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204247_wf.raa
20201014::204256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204257_wf.raa
20201014::204300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.9dbar, CTD 34.5psu, index 1.34, Packet 37082
20201014::204300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204307_wf.raa
20201014::204316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204317_wf.raa
20201014::204326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204327_wf.raa
20201014::204330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1233.3dbar, CTD 34.5psu, index 1.34, Packet 37137
20201014::204330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204337_wf.raa
20201014::204346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204347_wf.raa
20201014::204356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204357_wf.raa
20201014::204400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1234.7dbar, CTD 34.5psu, index 1.34, Packet 37192
20201014::204400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204407_wf.raa
20201014::204416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204417_wf.raa
20201014::204426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204427_wf.raa
20201014::204430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1236.7dbar, CTD 34.5psu, index 1.34, Packet 37246
20201014::204430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204437_wf.raa
20201014::204446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204447_wf.raa
20201014::204456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204457_wf.raa
20201014::204500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.5dbar, CTD 34.5psu, index 1.34, Packet 37302
20201014::204500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204507_wf.raa
20201014::204516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204517_wf.raa
20201014::204526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204527_wf.raa
20201014::204530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.1dbar, CTD 34.5psu, index 1.34, Packet 37356
20201014::204530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204537_wf.raa
20201014::204546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204547_wf.raa
20201014::204556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204557_wf.raa
20201014::204559: Head 1: Time Synchronization: 2020.10.14   20:46:00::0017
20201014::204600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.9dbar, CTD 34.5psu, index 1.34, Packet 37411
20201014::204600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204607_wf.raa
20201014::204616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204617_wf.raa
20201014::204626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204627_wf.raa
20201014::204630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1236.8dbar, CTD 34.5psu, index 1.34, Packet 37466
20201014::204630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204637_wf.raa
20201014::204646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204647_wf.raa
20201014::204656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204657_wf.raa
20201014::204659: Head 1: Time Synchronization: 2020.10.14   20:47:00::0017
20201014::204700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1234.9dbar, CTD 34.5psu, index 1.34, Packet 37521
20201014::204700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204707_wf.raa
20201014::204716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204717_wf.raa
20201014::204726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204727_wf.raa
20201014::204730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1232.6dbar, CTD 34.5psu, index 1.34, Packet 37576
20201014::204730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204737_wf.raa
20201014::204746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204747_wf.raa
20201014::204756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204757_wf.raa
20201014::204800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.0dbar, CTD 34.5psu, index 1.34, Packet 37631
20201014::204800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204807_wf.raa
20201014::204816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204817_wf.raa
20201014::204826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204827_wf.raa
20201014::204830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.3dbar, CTD 34.5psu, index 1.34, Packet 37686
20201014::204830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204837_wf.raa
20201014::204846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204847_wf.raa
20201014::204856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204857_wf.raa
20201014::204859: Head 1: Time Synchronization: 2020.10.14   20:49:00::0016
20201014::204900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 37740
20201014::204900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204907_wf.raa
20201014::204916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204917_wf.raa
20201014::204926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204927_wf.raa
20201014::204930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 37795
20201014::204930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::204936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204937_wf.raa
20201014::204946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204947_wf.raa
20201014::204956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_204957_wf.raa
20201014::205000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 37850
20201014::205000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205007_wf.raa
20201014::205016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205017_wf.raa
20201014::205026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205027_wf.raa
20201014::205030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 37905
20201014::205030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205037_wf.raa
20201014::205046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205047_wf.raa
20201014::205056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205057_wf.raa
20201014::205059: Head 1: Time Synchronization: 2020.10.14   20:51:00::0016
20201014::205100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.9dbar, CTD 34.5psu, index 1.34, Packet 37959
20201014::205100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205107_wf.raa
20201014::205116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205117_wf.raa
20201014::205126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205127_wf.raa
20201014::205130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.5dbar, CTD 34.5psu, index 1.34, Packet 38014
20201014::205130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205137_wf.raa
20201014::205146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205147_wf.raa
20201014::205156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205157_wf.raa
20201014::205159: Head 1: Time Synchronization: 2020.10.14   20:52:00::0015
20201014::205159: Head 2: Time Synchronization: 2020.10.14   20:52:00::0014
20201014::205200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.2dbar, CTD 34.5psu, index 1.34, Packet 38069
20201014::205200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205207_wf.raa
20201014::205216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205217_wf.raa
20201014::205226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205227_wf.raa
20201014::205230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 38124
20201014::205230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205237_wf.raa
20201014::205246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205247_wf.raa
20201014::205256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205257_wf.raa
20201014::205259: Head 1: Time Synchronization: 2020.10.14   20:53:00::0015
20201014::205300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.8dbar, CTD 34.5psu, index 1.34, Packet 38179
20201014::205300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205307_wf.raa
20201014::205316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205317_wf.raa
20201014::205326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205327_wf.raa
20201014::205330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1221.7dbar, CTD 34.5psu, index 1.34, Packet 38233
20201014::205330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205337_wf.raa
20201014::205346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205347_wf.raa
20201014::205356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205357_wf.raa
20201014::205359: Head 1: Time Synchronization: 2020.10.14   20:54:00::0014
20201014::205400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1218.6dbar, CTD 34.5psu, index 1.34, Packet 38288
20201014::205400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205407_wf.raa
20201014::205416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205417_wf.raa
20201014::205426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205427_wf.raa
20201014::205430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1216.0dbar, CTD 34.5psu, index 1.34, Packet 38342
20201014::205430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205437_wf.raa
20201014::205446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205447_wf.raa
20201014::205456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205457_wf.raa
20201014::205500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.2dbar, CTD 34.5psu, index 1.34, Packet 38397
20201014::205500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205507_wf.raa
20201014::205516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205517_wf.raa
20201014::205526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205527_wf.raa
20201014::205530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.8dbar, CTD 34.5psu, index 1.34, Packet 38451
20201014::205530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205537_wf.raa
20201014::205546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205547_wf.raa
20201014::205556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205557_wf.raa
20201014::205600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.3dbar, CTD 34.5psu, index 1.34, Packet 38506
20201014::205600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205607_wf.raa
20201014::205616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205617_wf.raa
20201014::205626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205627_wf.raa
20201014::205630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.4dbar, CTD 34.5psu, index 1.34, Packet 38560
20201014::205630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205637_wf.raa
20201014::205646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205647_wf.raa
20201014::205656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205657_wf.raa
20201014::205700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.9dbar, CTD 34.5psu, index 1.34, Packet 38615
20201014::205700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205707_wf.raa
20201014::205716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205717_wf.raa
20201014::205726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205727_wf.raa
20201014::205730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.5dbar, CTD 34.5psu, index 1.34, Packet 38670
20201014::205730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205737_wf.raa
20201014::205746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205747_wf.raa
20201014::205756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205757_wf.raa
20201014::205800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1214.7dbar, CTD 34.5psu, index 1.34, Packet 38724
20201014::205800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205807_wf.raa
20201014::205816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205817_wf.raa
20201014::205826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205827_wf.raa
20201014::205830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.9dbar, CTD 34.5psu, index 1.34, Packet 38779
20201014::205830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205837_wf.raa
20201014::205846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205847_wf.raa
20201014::205856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205857_wf.raa
20201014::205900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1212.2dbar, CTD 34.5psu, index 1.34, Packet 38834
20201014::205900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205907_wf.raa
20201014::205916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205917_wf.raa
20201014::205926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205927_wf.raa
20201014::205930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1213.0dbar, CTD 34.5psu, index 1.34, Packet 38889
20201014::205930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::205937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205937_wf.raa
20201014::205946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205947_wf.raa
20201014::205956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_205957_wf.raa
20201014::205959: Head 1: Time Synchronization: 2020.10.14   21:00:00::0016
20201014::210000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.2dbar, CTD 34.5psu, index 1.34, Packet 38944
20201014::210000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210007_wf.raa
20201014::210016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210017_wf.raa
20201014::210026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210027_wf.raa
20201014::210030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1215.2dbar, CTD 34.5psu, index 1.34, Packet 38999
20201014::210030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210037_wf.raa
20201014::210046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210047_wf.raa
20201014::210056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210057_wf.raa
20201014::210059: Head 1: Time Synchronization: 2020.10.14   21:01:00::0017
20201014::210100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1218.1dbar, CTD 34.5psu, index 1.34, Packet 39054
20201014::210100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210107_wf.raa
20201014::210116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210117_wf.raa
20201014::210126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210127_wf.raa
20201014::210130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1216.8dbar, CTD 34.5psu, index 1.34, Packet 39108
20201014::210130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210137_wf.raa
20201014::210146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210147_wf.raa
20201014::210156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210157_wf.raa
20201014::210159: Head 1: Time Synchronization: 2020.10.14   21:02:00::0015
20201014::210200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1219.6dbar, CTD 34.5psu, index 1.34, Packet 39164
20201014::210200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210207_wf.raa
20201014::210216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210217_wf.raa
20201014::210226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210227_wf.raa
20201014::210230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.4dbar, CTD 34.5psu, index 1.34, Packet 39218
20201014::210230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210237_wf.raa
20201014::210246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210247_wf.raa
20201014::210256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210257_wf.raa
20201014::210300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.4dbar, CTD 34.5psu, index 1.34, Packet 39273
20201014::210300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210307_wf.raa
20201014::210316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210317_wf.raa
20201014::210326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210327_wf.raa
20201014::210330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.1dbar, CTD 34.5psu, index 1.34, Packet 39328
20201014::210330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210337_wf.raa
20201014::210346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210347_wf.raa
20201014::210356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210357_wf.raa
20201014::210359: Head 1: Time Synchronization: 2020.10.14   21:04:00::0014
20201014::210400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.4dbar, CTD 34.5psu, index 1.34, Packet 39383
20201014::210400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210407_wf.raa
20201014::210416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210417_wf.raa
20201014::210426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210427_wf.raa
20201014::210430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.8dbar, CTD 34.5psu, index 1.34, Packet 39438
20201014::210430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210437_wf.raa
20201014::210446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210447_wf.raa
20201014::210456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210457_wf.raa
20201014::210500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.0dbar, CTD 34.5psu, index 1.34, Packet 39493
20201014::210500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210507_wf.raa
20201014::210516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210517_wf.raa
20201014::210526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210527_wf.raa
20201014::210530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 39548
20201014::210530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210537_wf.raa
20201014::210546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210547_wf.raa
20201014::210556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210557_wf.raa
20201014::210600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 39602
20201014::210600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210607_wf.raa
20201014::210616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210617_wf.raa
20201014::210626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210627_wf.raa
20201014::210630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 39657
20201014::210630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210637_wf.raa
20201014::210646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210647_wf.raa
20201014::210656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210657_wf.raa
20201014::210700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 39712
20201014::210700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210707_wf.raa
20201014::210716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210717_wf.raa
20201014::210726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210727_wf.raa
20201014::210730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 39766
20201014::210730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210737_wf.raa
20201014::210746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210747_wf.raa
20201014::210756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210757_wf.raa
20201014::210800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.4dbar, CTD 34.5psu, index 1.34, Packet 39822
20201014::210800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210807_wf.raa
20201014::210816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210817_wf.raa
20201014::210826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210827_wf.raa
20201014::210830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.8dbar, CTD 34.5psu, index 1.34, Packet 39877
20201014::210830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210837_wf.raa
20201014::210846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210847_wf.raa
20201014::210856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210857_wf.raa
20201014::210900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1234.2dbar, CTD 34.5psu, index 1.34, Packet 39931
20201014::210900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210907_wf.raa
20201014::210916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210917_wf.raa
20201014::210926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210927_wf.raa
20201014::210930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1236.0dbar, CTD 34.5psu, index 1.34, Packet 39986
20201014::210930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::210936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210937_wf.raa
20201014::210946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210947_wf.raa
20201014::210956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_210957_wf.raa
20201014::211000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.0dbar, CTD 34.5psu, index 1.34, Packet 40040
20201014::211000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211007_wf.raa
20201014::211016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211017_wf.raa
20201014::211026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211027_wf.raa
20201014::211030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.4dbar, CTD 34.5psu, index 1.34, Packet 40095
20201014::211030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211037_wf.raa
20201014::211046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211047_wf.raa
20201014::211056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211057_wf.raa
20201014::211059: Head 1: Time Synchronization: 2020.10.14   21:11:00::0014
20201014::211059: Head 2: Time Synchronization: 2020.10.14   21:11:00::0015
20201014::211100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1238.5dbar, CTD 34.5psu, index 1.34, Packet 40150
20201014::211100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211107_wf.raa
20201014::211116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211117_wf.raa
20201014::211126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211127_wf.raa
20201014::211130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1239.2dbar, CTD 34.5psu, index 1.34, Packet 40204
20201014::211130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211137_wf.raa
20201014::211146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211147_wf.raa
20201014::211156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211157_wf.raa
20201014::211200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.8dbar, CTD 34.5psu, index 1.34, Packet 40260
20201014::211200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211207_wf.raa
20201014::211216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211217_wf.raa
20201014::211226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211227_wf.raa
20201014::211230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1240.0dbar, CTD 34.5psu, index 1.34, Packet 40314
20201014::211230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211237_wf.raa
20201014::211246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211247_wf.raa
20201014::211256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211257_wf.raa
20201014::211300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.8dbar, CTD 34.5psu, index 1.34, Packet 40369
20201014::211300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211307_wf.raa
20201014::211316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211317_wf.raa
20201014::211326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211327_wf.raa
20201014::211330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.7dbar, CTD 34.5psu, index 1.34, Packet 40424
20201014::211330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211337_wf.raa
20201014::211346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211347_wf.raa
20201014::211356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211357_wf.raa
20201014::211359: Head 1: Time Synchronization: 2020.10.14   21:14:00::0014
20201014::211400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.3dbar, CTD 34.5psu, index 1.34, Packet 40479
20201014::211400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211407_wf.raa
20201014::211416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211417_wf.raa
20201014::211426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211427_wf.raa
20201014::211430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 40534
20201014::211430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211437_wf.raa
20201014::211447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211447_wf.raa
20201014::211456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211457_wf.raa
20201014::211459: Head 2: Time Synchronization: 2020.10.14   21:15:00::0014
20201014::211500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 40589
20201014::211500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211507_wf.raa
20201014::211516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211517_wf.raa
20201014::211526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211527_wf.raa
20201014::211530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1229.4dbar, CTD 34.5psu, index 1.34, Packet 40643
20201014::211530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211537_wf.raa
20201014::211546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211547_wf.raa
20201014::211556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211557_wf.raa
20201014::211559: Head 1: Time Synchronization: 2020.10.14   21:16:00::0015
20201014::211600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 40698
20201014::211600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211607_wf.raa
20201014::211616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211617_wf.raa
20201014::211626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211627_wf.raa
20201014::211630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 40753
20201014::211630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211637_wf.raa
20201014::211646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211647_wf.raa
20201014::211656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211657_wf.raa
20201014::211700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 40808
20201014::211700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211707_wf.raa
20201014::211716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211717_wf.raa
20201014::211726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211727_wf.raa
20201014::211730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 40863
20201014::211730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211737_wf.raa
20201014::211746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211747_wf.raa
20201014::211756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211757_wf.raa
20201014::211759: Head 1: Time Synchronization: 2020.10.14   21:18:00::0015
20201014::211800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 40917
20201014::211800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211807_wf.raa
20201014::211816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211817_wf.raa
20201014::211826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211827_wf.raa
20201014::211830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 40972
20201014::211830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211837_wf.raa
20201014::211846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211847_wf.raa
20201014::211856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211857_wf.raa
20201014::211900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 41027
20201014::211900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211907_wf.raa
20201014::211916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211917_wf.raa
20201014::211926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211927_wf.raa
20201014::211930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.1dbar, CTD 34.5psu, index 1.34, Packet 41082
20201014::211930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::211936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211937_wf.raa
20201014::211946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211947_wf.raa
20201014::211956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_211957_wf.raa
20201014::212000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.2dbar, CTD 34.5psu, index 1.34, Packet 41137
20201014::212000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212007_wf.raa
20201014::212016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212017_wf.raa
20201014::212026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212027_wf.raa
20201014::212030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1223.6dbar, CTD 34.5psu, index 1.34, Packet 41192
20201014::212030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212037_wf.raa
20201014::212046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212047_wf.raa
20201014::212056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212057_wf.raa
20201014::212100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1221.8dbar, CTD 34.5psu, index 1.34, Packet 41247
20201014::212100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212107_wf.raa
20201014::212116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212117_wf.raa
20201014::212126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212127_wf.raa
20201014::212130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.9dbar, CTD 34.5psu, index 1.34, Packet 41302
20201014::212130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212137_wf.raa
20201014::212146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212147_wf.raa
20201014::212156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212157_wf.raa
20201014::212200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.6dbar, CTD 34.5psu, index 1.34, Packet 41358
20201014::212200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212207_wf.raa
20201014::212216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212217_wf.raa
20201014::212226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212227_wf.raa
20201014::212230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1215.8dbar, CTD 34.5psu, index 1.34, Packet 41414
20201014::212230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212237_wf.raa
20201014::212246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212247_wf.raa
20201014::212256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212257_wf.raa
20201014::212259: Head 1: Time Synchronization: 2020.10.14   21:23:00::0014
20201014::212300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.9dbar, CTD 34.5psu, index 1.34, Packet 41469
20201014::212300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212307_wf.raa
20201014::212316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212317_wf.raa
20201014::212326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212327_wf.raa
20201014::212330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.3dbar, CTD 34.5psu, index 1.34, Packet 41524
20201014::212330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212337_wf.raa
20201014::212346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212347_wf.raa
20201014::212356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212357_wf.raa
20201014::212400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.3dbar, CTD 34.5psu, index 1.34, Packet 41579
20201014::212400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212407_wf.raa
20201014::212416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212417_wf.raa
20201014::212426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212427_wf.raa
20201014::212430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.6dbar, CTD 34.5psu, index 1.34, Packet 41633
20201014::212430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212437_wf.raa
20201014::212446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212447_wf.raa
20201014::212456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212457_wf.raa
20201014::212500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.9dbar, CTD 34.5psu, index 1.34, Packet 41688
20201014::212500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212507_wf.raa
20201014::212516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212517_wf.raa
20201014::212526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212527_wf.raa
20201014::212530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.9dbar, CTD 34.5psu, index 1.34, Packet 41742
20201014::212530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212537_wf.raa
20201014::212546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212547_wf.raa
20201014::212556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212557_wf.raa
20201014::212600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.9dbar, CTD 34.5psu, index 1.34, Packet 41797
20201014::212600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212607_wf.raa
20201014::212616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212617_wf.raa
20201014::212626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212627_wf.raa
20201014::212630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.2dbar, CTD 34.5psu, index 1.34, Packet 41851
20201014::212630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212637_wf.raa
20201014::212646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212647_wf.raa
20201014::212656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212657_wf.raa
20201014::212659: Head 1: Time Synchronization: 2020.10.14   21:27:00::0015
20201014::212700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1213.1dbar, CTD 34.5psu, index 1.34, Packet 41906
20201014::212700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212707_wf.raa
20201014::212716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212717_wf.raa
20201014::212726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212727_wf.raa
20201014::212730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.9dbar, CTD 34.5psu, index 1.34, Packet 41960
20201014::212730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212737_wf.raa
20201014::212746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212747_wf.raa
20201014::212756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212757_wf.raa
20201014::212759: Head 2: Time Synchronization: 2020.10.14   21:28:00::0014
20201014::212800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1217.3dbar, CTD 34.5psu, index 1.34, Packet 42016
20201014::212800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212807_wf.raa
20201014::212816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212817_wf.raa
20201014::212826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212827_wf.raa
20201014::212830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1219.2dbar, CTD 34.5psu, index 1.34, Packet 42070
20201014::212830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212837_wf.raa
20201014::212846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212847_wf.raa
20201014::212856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212857_wf.raa
20201014::212859: Head 1: Time Synchronization: 2020.10.14   21:29:00::0011
20201014::212900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1221.3dbar, CTD 34.5psu, index 1.34, Packet 42125
20201014::212900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212907_wf.raa
20201014::212916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212917_wf.raa
20201014::212926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212927_wf.raa
20201014::212930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1222.7dbar, CTD 34.5psu, index 1.34, Packet 42180
20201014::212930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::212936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212937_wf.raa
20201014::212946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212947_wf.raa
20201014::212956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_212957_wf.raa
20201014::213000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1225.0dbar, CTD 34.5psu, index 1.34, Packet 42235
20201014::213000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213007_wf.raa
20201014::213016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213017_wf.raa
20201014::213026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213027_wf.raa
20201014::213030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.1dbar, CTD 34.5psu, index 1.34, Packet 42289
20201014::213030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213037_wf.raa
20201014::213046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213047_wf.raa
20201014::213056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213057_wf.raa
20201014::213100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1226.6dbar, CTD 34.5psu, index 1.34, Packet 42344
20201014::213100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213107_wf.raa
20201014::213116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213117_wf.raa
20201014::213126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213127_wf.raa
20201014::213130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 42399
20201014::213130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213137_wf.raa
20201014::213146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213147_wf.raa
20201014::213156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213157_wf.raa
20201014::213159: Head 1: Time Synchronization: 2020.10.14   21:32:00::0016
20201014::213200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 42453
20201014::213200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213207_wf.raa
20201014::213216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213217_wf.raa
20201014::213226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213227_wf.raa
20201014::213230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 42507
20201014::213230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213237_wf.raa
20201014::213246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213247_wf.raa
20201014::213256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213257_wf.raa
20201014::213259: Head 1: Time Synchronization: 2020.10.14   21:33:00::0014
20201014::213300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 42562
20201014::213300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213307_wf.raa
20201014::213316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213317_wf.raa
20201014::213326: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213327_wf.raa
20201014::213330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 42616
20201014::213330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213336: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213337_wf.raa
20201014::213346: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213347_wf.raa
20201014::213356: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213357_wf.raa
20201014::213400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 42671
20201014::213400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213406: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213407_wf.raa
20201014::213416: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213417_wf.raa
20201014::213426: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213427_wf.raa
20201014::213430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.2dbar, CTD 34.5psu, index 1.34, Packet 42726
20201014::213430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213436: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213437_wf.raa
20201014::213446: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213447_wf.raa
20201014::213456: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213457_wf.raa
20201014::213500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1228.6dbar, CTD 34.5psu, index 1.34, Packet 42781
20201014::213500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213506: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213507_wf.raa
20201014::213516: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213517_wf.raa
20201014::213526: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213527_wf.raa
20201014::213530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1230.4dbar, CTD 34.5psu, index 1.34, Packet 42835
20201014::213530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213536: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213537_wf.raa
20201014::213546: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213547_wf.raa
20201014::213556: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213557_wf.raa
20201014::213559: Head 1: Time Synchronization: 2020.10.14   21:36:00::0014
20201014::213600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.2dbar, CTD 34.5psu, index 1.34, Packet 42890
20201014::213600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213606: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213607_wf.raa
20201014::213616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213617_wf.raa
20201014::213626: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213627_wf.raa
20201014::213630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.7dbar, CTD 34.5psu, index 1.34, Packet 42945
20201014::213630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213636: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213637_wf.raa
20201014::213646: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213647_wf.raa
20201014::213656: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213657_wf.raa
20201014::213659: Head 1: Time Synchronization: 2020.10.14   21:37:00::0014
20201014::213659: Head 2: Time Synchronization: 2020.10.14   21:37:00::0014
20201014::213700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.7dbar, CTD 34.5psu, index 1.34, Packet 43000
20201014::213700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213706: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213707_wf.raa
20201014::213716: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213717_wf.raa
20201014::213726: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213727_wf.raa
20201014::213730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.7dbar, CTD 34.5psu, index 1.34, Packet 43055
20201014::213730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213736: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213737_wf.raa
20201014::213746: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213747_wf.raa
20201014::213756: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213757_wf.raa
20201014::213759: Head 1: Time Synchronization: 2020.10.14   21:38:00::0015
20201014::213800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.3dbar, CTD 34.5psu, index 1.34, Packet 43110
20201014::213800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213806: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213807_wf.raa
20201014::213816: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213817_wf.raa
20201014::213826: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213827_wf.raa
20201014::213830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.6dbar, CTD 34.5psu, index 1.34, Packet 43165
20201014::213830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213836: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213837_wf.raa
20201014::213846: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213847_wf.raa
20201014::213856: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213857_wf.raa
20201014::213859: Head 1: Time Synchronization: 2020.10.14   21:39:00::0014
20201014::213900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.2dbar, CTD 34.5psu, index 1.34, Packet 43220
20201014::213900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213906: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213907_wf.raa
20201014::213916: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213917_wf.raa
20201014::213926: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213927_wf.raa
20201014::213930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.5dbar, CTD 34.5psu, index 1.34, Packet 43274
20201014::213930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::213936: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213937_wf.raa
20201014::213946: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213947_wf.raa
20201014::213956: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_213957_wf.raa
20201014::213959: Head 1: Time Synchronization: 2020.10.14   21:40:00::0013
20201014::214000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 43329
20201014::214000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214006: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214007_wf.raa
20201014::214016: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214017_wf.raa
20201014::214026: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214027_wf.raa
20201014::214030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 43384
20201014::214030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214036: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214037_wf.raa
20201014::214046: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214047_wf.raa
20201014::214056: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214057_wf.raa
20201014::214100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 43439
20201014::214100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214106: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214107_wf.raa
20201014::214116: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214117_wf.raa
20201014::214126: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214127_wf.raa
20201014::214130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 43493
20201014::214130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214136: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214137_wf.raa
20201014::214146: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214147_wf.raa
20201014::214156: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214157_wf.raa
20201014::214159: Head 1: Time Synchronization: 2020.10.14   21:42:00::0013
20201014::214200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 43548
20201014::214200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214206: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214207_wf.raa
20201014::214216: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214217_wf.raa
20201014::214226: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214227_wf.raa
20201014::214230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 43603
20201014::214230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214236: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214237_wf.raa
20201014::214246: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214247_wf.raa
20201014::214256: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214257_wf.raa
20201014::214259: Head 1: Time Synchronization: 2020.10.14   21:43:00::0014
20201014::214300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 43658
20201014::214300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214306: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214307_wf.raa
20201014::214316: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214317_wf.raa
20201014::214328: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214328_wf.raa
20201014::214330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.8dbar, CTD 34.5psu, index 1.34, Packet 43712
20201014::214330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214338: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214338_wf.raa
20201014::214348: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214348_wf.raa
20201014::214358: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214358_wf.raa
20201014::214359: Head 1: Time Synchronization: 2020.10.14   21:44:00::0017
20201014::214400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.3dbar, CTD 34.5psu, index 1.34, Packet 43767
20201014::214400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214408: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214408_wf.raa
20201014::214418: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214418_wf.raa
20201014::214428: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214428_wf.raa
20201014::214430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.5dbar, CTD 34.5psu, index 1.34, Packet 43822
20201014::214430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214438: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214438_wf.raa
20201014::214447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214448_wf.raa
20201014::214457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214458_wf.raa
20201014::214459: Head 1: Time Synchronization: 2020.10.14   21:45:00::0019
20201014::214459: Head 2: Time Synchronization: 2020.10.14   21:45:00::0016
20201014::214500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.7dbar, CTD 34.5psu, index 1.34, Packet 43877
20201014::214500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214508_wf.raa
20201014::214517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214518_wf.raa
20201014::214527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214528_wf.raa
20201014::214530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.6dbar, CTD 34.5psu, index 1.34, Packet 43931
20201014::214530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214538_wf.raa
20201014::214547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214548_wf.raa
20201014::214557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214558_wf.raa
20201014::214559: Head 1: Time Synchronization: 2020.10.14   21:46:00::0015
20201014::214600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.1dbar, CTD 34.5psu, index 1.34, Packet 43986
20201014::214600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214608_wf.raa
20201014::214617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214618_wf.raa
20201014::214627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214628_wf.raa
20201014::214630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.4dbar, CTD 34.5psu, index 1.34, Packet 44040
20201014::214630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214638_wf.raa
20201014::214647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214648_wf.raa
20201014::214657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214658_wf.raa
20201014::214659: Head 1: Time Synchronization: 2020.10.14   21:47:00::0015
20201014::214700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.4dbar, CTD 34.5psu, index 1.34, Packet 44095
20201014::214700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214708_wf.raa
20201014::214717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214718_wf.raa
20201014::214727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214728_wf.raa
20201014::214730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.7dbar, CTD 34.5psu, index 1.34, Packet 44149
20201014::214730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214738_wf.raa
20201014::214747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214748_wf.raa
20201014::214757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214758_wf.raa
20201014::214759: Head 2: Time Synchronization: 2020.10.14   21:48:00::0015
20201014::214759: Head 1: Time Synchronization: 2020.10.14   21:48:00::0014
20201014::214800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.6dbar, CTD 34.5psu, index 1.34, Packet 44204
20201014::214800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214808_wf.raa
20201014::214817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214818_wf.raa
20201014::214827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214828_wf.raa
20201014::214830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.5dbar, CTD 34.5psu, index 1.34, Packet 44259
20201014::214830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214838_wf.raa
20201014::214847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214848_wf.raa
20201014::214857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214858_wf.raa
20201014::214900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.7dbar, CTD 34.5psu, index 1.34, Packet 44313
20201014::214900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214908_wf.raa
20201014::214917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214918_wf.raa
20201014::214927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214928_wf.raa
20201014::214930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.3dbar, CTD 34.5psu, index 1.34, Packet 44367
20201014::214930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::214937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214938_wf.raa
20201014::214947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214948_wf.raa
20201014::214957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_214958_wf.raa
20201014::214959: Head 1: Time Synchronization: 2020.10.14   21:50:00::0014
20201014::215000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.3dbar, CTD 34.5psu, index 1.34, Packet 44422
20201014::215000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215008_wf.raa
20201014::215017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215018_wf.raa
20201014::215027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215028_wf.raa
20201014::215030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.4dbar, CTD 34.5psu, index 1.34, Packet 44477
20201014::215030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215038_wf.raa
20201014::215047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215048_wf.raa
20201014::215057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215058_wf.raa
20201014::215059: Head 1: Time Synchronization: 2020.10.14   21:51:00::0014
20201014::215100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1212.6dbar, CTD 34.5psu, index 1.34, Packet 44531
20201014::215100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215108_wf.raa
20201014::215117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215118_wf.raa
20201014::215127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215128_wf.raa
20201014::215130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.8dbar, CTD 34.5psu, index 1.34, Packet 44586
20201014::215130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215138_wf.raa
20201014::215147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215148_wf.raa
20201014::215157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215158_wf.raa
20201014::215159: Head 1: Time Synchronization: 2020.10.14   21:52:00::0015
20201014::215200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.3dbar, CTD 34.5psu, index 1.34, Packet 44641
20201014::215200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215208_wf.raa
20201014::215217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215218_wf.raa
20201014::215227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215228_wf.raa
20201014::215230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.3dbar, CTD 34.5psu, index 1.34, Packet 44695
20201014::215230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215238_wf.raa
20201014::215247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215248_wf.raa
20201014::215257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215258_wf.raa
20201014::215259: Head 1: Time Synchronization: 2020.10.14   21:53:00::0015
20201014::215300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.1dbar, CTD 34.5psu, index 1.34, Packet 44750
20201014::215300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215308_wf.raa
20201014::215317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215318_wf.raa
20201014::215327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215328_wf.raa
20201014::215330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.4dbar, CTD 34.5psu, index 1.34, Packet 44805
20201014::215330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215338_wf.raa
20201014::215347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215348_wf.raa
20201014::215357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215358_wf.raa
20201014::215400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.9dbar, CTD 34.5psu, index 1.34, Packet 44860
20201014::215400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215408_wf.raa
20201014::215417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215418_wf.raa
20201014::215427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215428_wf.raa
20201014::215430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.2dbar, CTD 34.5psu, index 1.34, Packet 44914
20201014::215430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215438_wf.raa
20201014::215447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215448_wf.raa
20201014::215457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215458_wf.raa
20201014::215500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.2dbar, CTD 34.5psu, index 1.34, Packet 44969
20201014::215500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215508_wf.raa
20201014::215517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215518_wf.raa
20201014::215527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215528_wf.raa
20201014::215530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.6dbar, CTD 34.5psu, index 1.34, Packet 45024
20201014::215530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215538_wf.raa
20201014::215547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215548_wf.raa
20201014::215557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215558_wf.raa
20201014::215600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 45079
20201014::215600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215608_wf.raa
20201014::215617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215618_wf.raa
20201014::215627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215628_wf.raa
20201014::215630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 45133
20201014::215630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215638_wf.raa
20201014::215647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215648_wf.raa
20201014::215657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215658_wf.raa
20201014::215659: Head 1: Time Synchronization: 2020.10.14   21:57:00::0015
20201014::215700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 45188
20201014::215700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215708_wf.raa
20201014::215717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215718_wf.raa
20201014::215727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215728_wf.raa
20201014::215730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 45242
20201014::215730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215738_wf.raa
20201014::215747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215748_wf.raa
20201014::215757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215758_wf.raa
20201014::215759: Head 1: Time Synchronization: 2020.10.14   21:58:00::0016
20201014::215800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 45297
20201014::215800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215808_wf.raa
20201014::215817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215818_wf.raa
20201014::215827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215828_wf.raa
20201014::215830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 45352
20201014::215830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215838_wf.raa
20201014::215847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215848_wf.raa
20201014::215857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215858_wf.raa
20201014::215859: Head 1: Time Synchronization: 2020.10.14   21:59:00::0015
20201014::215900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 45406
20201014::215900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215908_wf.raa
20201014::215917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215918_wf.raa
20201014::215927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215928_wf.raa
20201014::215930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.6dbar, CTD 34.5psu, index 1.34, Packet 45461
20201014::215930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::215937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215938_wf.raa
20201014::215947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215948_wf.raa
20201014::215957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_215958_wf.raa
20201014::215959: Head 1: Time Synchronization: 2020.10.14   22:00:00::0015
20201014::220000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.9dbar, CTD 34.5psu, index 1.34, Packet 45516
20201014::220000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220008_wf.raa
20201014::220017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220018_wf.raa
20201014::220027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220028_wf.raa
20201014::220030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.2dbar, CTD 34.5psu, index 1.34, Packet 45570
20201014::220030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220038_wf.raa
20201014::220047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220048_wf.raa
20201014::220057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220058_wf.raa
20201014::220059: Head 1: Time Synchronization: 2020.10.14   22:01:00::0015
20201014::220100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.3dbar, CTD 34.5psu, index 1.34, Packet 45625
20201014::220100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220108_wf.raa
20201014::220117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220118_wf.raa
20201014::220127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220128_wf.raa
20201014::220130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.3dbar, CTD 34.5psu, index 1.34, Packet 45679
20201014::220130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220138_wf.raa
20201014::220147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220148_wf.raa
20201014::220157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220158_wf.raa
20201014::220159: Head 1: Time Synchronization: 2020.10.14   22:02:00::0015
20201014::220200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1239.0dbar, CTD 34.5psu, index 1.34, Packet 45734
20201014::220200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220208_wf.raa
20201014::220217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220218_wf.raa
20201014::220227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220228_wf.raa
20201014::220230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.3dbar, CTD 34.5psu, index 1.34, Packet 45789
20201014::220230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220238_wf.raa
20201014::220247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220248_wf.raa
20201014::220257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220258_wf.raa
20201014::220300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.6dbar, CTD 34.5psu, index 1.34, Packet 45844
20201014::220300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220308_wf.raa
20201014::220317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220318_wf.raa
20201014::220327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220328_wf.raa
20201014::220330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.5dbar, CTD 34.5psu, index 1.34, Packet 45898
20201014::220330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220338_wf.raa
20201014::220347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220348_wf.raa
20201014::220357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220358_wf.raa
20201014::220359: Head 1: Time Synchronization: 2020.10.14   22:04:00::0015
20201014::220400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.6dbar, CTD 34.5psu, index 1.34, Packet 45953
20201014::220400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220408_wf.raa
20201014::220417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220418_wf.raa
20201014::220427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220428_wf.raa
20201014::220430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.1dbar, CTD 34.5psu, index 1.34, Packet 46008
20201014::220430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220438_wf.raa
20201014::220447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220448_wf.raa
20201014::220457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220458_wf.raa
20201014::220459: Head 1: Time Synchronization: 2020.10.14   22:05:00::0017
20201014::220459: Head 2: Time Synchronization: 2020.10.14   22:05:00::0017
20201014::220500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 46062
20201014::220500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220508_wf.raa
20201014::220517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220518_wf.raa
20201014::220527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220528_wf.raa
20201014::220530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 46117
20201014::220530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220538_wf.raa
20201014::220547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220548_wf.raa
20201014::220557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220558_wf.raa
20201014::220559: Head 1: Time Synchronization: 2020.10.14   22:06:00::0016
20201014::220600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 46171
20201014::220600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220608_wf.raa
20201014::220617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220618_wf.raa
20201014::220627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220628_wf.raa
20201014::220630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 46226
20201014::220630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220638_wf.raa
20201014::220647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220648_wf.raa
20201014::220657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220658_wf.raa
20201014::220659: Head 1: Time Synchronization: 2020.10.14   22:07:00::0015
20201014::220700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 46280
20201014::220700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220708_wf.raa
20201014::220717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220718_wf.raa
20201014::220727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220728_wf.raa
20201014::220730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 46335
20201014::220730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220738_wf.raa
20201014::220747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220748_wf.raa
20201014::220757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220758_wf.raa
20201014::220800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.1dbar, CTD 34.5psu, index 1.34, Packet 46390
20201014::220800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220808_wf.raa
20201014::220817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220818_wf.raa
20201014::220827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220828_wf.raa
20201014::220830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 46444
20201014::220830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220838_wf.raa
20201014::220847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220848_wf.raa
20201014::220857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220858_wf.raa
20201014::220900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.2dbar, CTD 34.5psu, index 1.34, Packet 46499
20201014::220900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220908_wf.raa
20201014::220917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220918_wf.raa
20201014::220927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220928_wf.raa
20201014::220930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.2dbar, CTD 34.5psu, index 1.34, Packet 46554
20201014::220930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::220937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220938_wf.raa
20201014::220947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220948_wf.raa
20201014::220957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_220958_wf.raa
20201014::220959: Head 1: Time Synchronization: 2020.10.14   22:10:00::0015
20201014::221000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.0dbar, CTD 34.5psu, index 1.34, Packet 46609
20201014::221000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221008_wf.raa
20201014::221017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221018_wf.raa
20201014::221027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221028_wf.raa
20201014::221030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.6dbar, CTD 34.5psu, index 1.34, Packet 46664
20201014::221030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221038_wf.raa
20201014::221047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221048_wf.raa
20201014::221057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221058_wf.raa
20201014::221100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.3dbar, CTD 34.5psu, index 1.34, Packet 46719
20201014::221100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221108_wf.raa
20201014::221117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221118_wf.raa
20201014::221127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221128_wf.raa
20201014::221130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.2dbar, CTD 34.5psu, index 1.34, Packet 46774
20201014::221130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221138_wf.raa
20201014::221147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221148_wf.raa
20201014::221157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221158_wf.raa
20201014::221159: Head 2: Time Synchronization: 2020.10.14   22:12:00::0015
20201014::221200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.6dbar, CTD 34.5psu, index 1.34, Packet 46828
20201014::221200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221208_wf.raa
20201014::221217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221218_wf.raa
20201014::221227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221228_wf.raa
20201014::221230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.0dbar, CTD 34.5psu, index 1.34, Packet 46882
20201014::221230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221238_wf.raa
20201014::221247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221248_wf.raa
20201014::221257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221258_wf.raa
20201014::221259: Head 1: Time Synchronization: 2020.10.14   22:13:00::0015
20201014::221300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1212.8dbar, CTD 34.5psu, index 1.34, Packet 46937
20201014::221300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221308_wf.raa
20201014::221317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221318_wf.raa
20201014::221327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221328_wf.raa
20201014::221330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.4dbar, CTD 34.5psu, index 1.34, Packet 46992
20201014::221330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221338_wf.raa
20201014::221347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221348_wf.raa
20201014::221357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221358_wf.raa
20201014::221359: Head 1: Time Synchronization: 2020.10.14   22:14:00::0014
20201014::221400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.8dbar, CTD 34.5psu, index 1.34, Packet 47046
20201014::221400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221408_wf.raa
20201014::221417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221418_wf.raa
20201014::221427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221428_wf.raa
20201014::221430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.6dbar, CTD 34.5psu, index 1.34, Packet 47101
20201014::221430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221438_wf.raa
20201014::221447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221448_wf.raa
20201014::221457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221458_wf.raa
20201014::221459: Head 1: Time Synchronization: 2020.10.14   22:15:00::0016
20201014::221500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.2dbar, CTD 34.5psu, index 1.34, Packet 47156
20201014::221500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221508_wf.raa
20201014::221517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221518_wf.raa
20201014::221527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221528_wf.raa
20201014::221530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1214.0dbar, CTD 34.5psu, index 1.34, Packet 47211
20201014::221530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221538_wf.raa
20201014::221547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221548_wf.raa
20201014::221557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221558_wf.raa
20201014::221600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1213.6dbar, CTD 34.5psu, index 1.34, Packet 47265
20201014::221600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221608_wf.raa
20201014::221617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221618_wf.raa
20201014::221627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221628_wf.raa
20201014::221630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.6dbar, CTD 34.5psu, index 1.34, Packet 47320
20201014::221630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221638_wf.raa
20201014::221647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221648_wf.raa
20201014::221657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221658_wf.raa
20201014::221700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.8dbar, CTD 34.5psu, index 1.34, Packet 47374
20201014::221700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221708_wf.raa
20201014::221717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221718_wf.raa
20201014::221727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221728_wf.raa
20201014::221730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.5dbar, CTD 34.5psu, index 1.34, Packet 47429
20201014::221730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221738_wf.raa
20201014::221747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221748_wf.raa
20201014::221757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221758_wf.raa
20201014::221800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.4dbar, CTD 34.5psu, index 1.34, Packet 47484
20201014::221800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221808_wf.raa
20201014::221817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221818_wf.raa
20201014::221827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221828_wf.raa
20201014::221830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.3dbar, CTD 34.5psu, index 1.34, Packet 47538
20201014::221830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221838_wf.raa
20201014::221847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221848_wf.raa
20201014::221857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221858_wf.raa
20201014::221859: Head 1: Time Synchronization: 2020.10.14   22:19:00::0014
20201014::221900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.0dbar, CTD 34.5psu, index 1.34, Packet 47593
20201014::221900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221908_wf.raa
20201014::221917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221918_wf.raa
20201014::221927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221928_wf.raa
20201014::221930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.9dbar, CTD 34.5psu, index 1.34, Packet 47648
20201014::221930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::221937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221938_wf.raa
20201014::221947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221948_wf.raa
20201014::221957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_221958_wf.raa
20201014::222000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.3dbar, CTD 34.5psu, index 1.34, Packet 47703
20201014::222000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222008_wf.raa
20201014::222017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222018_wf.raa
20201014::222027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222028_wf.raa
20201014::222030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.9dbar, CTD 34.5psu, index 1.34, Packet 47757
20201014::222030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222038_wf.raa
20201014::222047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222048_wf.raa
20201014::222057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222058_wf.raa
20201014::222059: Head 2: Time Synchronization: 2020.10.14   22:21:00::0014
20201014::222100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 47812
20201014::222100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222108_wf.raa
20201014::222117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222118_wf.raa
20201014::222127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222128_wf.raa
20201014::222130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 47866
20201014::222130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222138_wf.raa
20201014::222147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222148_wf.raa
20201014::222157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222158_wf.raa
20201014::222159: Head 1: Time Synchronization: 2020.10.14   22:22:00::0014
20201014::222200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 47921
20201014::222200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222208_wf.raa
20201014::222217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222218_wf.raa
20201014::222227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222228_wf.raa
20201014::222230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 47976
20201014::222230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222238_wf.raa
20201014::222247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222248_wf.raa
20201014::222257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222258_wf.raa
20201014::222300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 48030
20201014::222300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222308_wf.raa
20201014::222317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222318_wf.raa
20201014::222327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222328_wf.raa
20201014::222330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.4dbar, CTD 34.5psu, index 1.34, Packet 48085
20201014::222330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222338_wf.raa
20201014::222347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222348_wf.raa
20201014::222357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222358_wf.raa
20201014::222400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 48140
20201014::222400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222408_wf.raa
20201014::222417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222418_wf.raa
20201014::222427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222428_wf.raa
20201014::222430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.2dbar, CTD 34.5psu, index 1.34, Packet 48194
20201014::222430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222438_wf.raa
20201014::222447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222448_wf.raa
20201014::222457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222458_wf.raa
20201014::222459: Head 1: Time Synchronization: 2020.10.14   22:25:00::0017
20201014::222500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.1dbar, CTD 34.5psu, index 1.34, Packet 48249
20201014::222500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222508_wf.raa
20201014::222517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222518_wf.raa
20201014::222527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222528_wf.raa
20201014::222530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.5dbar, CTD 34.5psu, index 1.34, Packet 48304
20201014::222530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222538_wf.raa
20201014::222547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222548_wf.raa
20201014::222557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222558_wf.raa
20201014::222600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.6dbar, CTD 34.5psu, index 1.34, Packet 48359
20201014::222600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222608_wf.raa
20201014::222617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222618_wf.raa
20201014::222627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222628_wf.raa
20201014::222630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1236.7dbar, CTD 34.5psu, index 1.34, Packet 48413
20201014::222630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222638_wf.raa
20201014::222647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222648_wf.raa
20201014::222657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222658_wf.raa
20201014::222700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1238.2dbar, CTD 34.5psu, index 1.34, Packet 48469
20201014::222700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222708_wf.raa
20201014::222717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222718_wf.raa
20201014::222727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222728_wf.raa
20201014::222730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.0dbar, CTD 34.5psu, index 1.34, Packet 48523
20201014::222730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222738_wf.raa
20201014::222747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222748_wf.raa
20201014::222757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222758_wf.raa
20201014::222800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1234.7dbar, CTD 34.5psu, index 1.34, Packet 48578
20201014::222800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222808_wf.raa
20201014::222817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222818_wf.raa
20201014::222827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222828_wf.raa
20201014::222830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.7dbar, CTD 34.5psu, index 1.34, Packet 48632
20201014::222830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222838_wf.raa
20201014::222847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222848_wf.raa
20201014::222857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222858_wf.raa
20201014::222859: Head 1: Time Synchronization: 2020.10.14   22:29:00::0014
20201014::222900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.3dbar, CTD 34.5psu, index 1.34, Packet 48687
20201014::222900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222908_wf.raa
20201014::222917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222918_wf.raa
20201014::222927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222928_wf.raa
20201014::222930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.7dbar, CTD 34.5psu, index 1.34, Packet 48742
20201014::222930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::222937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222938_wf.raa
20201014::222947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222948_wf.raa
20201014::222957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_222958_wf.raa
20201014::223000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 48797
20201014::223000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223008_wf.raa
20201014::223017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223018_wf.raa
20201014::223027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223028_wf.raa
20201014::223030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 48852
20201014::223030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223038_wf.raa
20201014::223047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223048_wf.raa
20201014::223057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223058_wf.raa
20201014::223100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 48906
20201014::223100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223108_wf.raa
20201014::223117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223118_wf.raa
20201014::223127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223128_wf.raa
20201014::223130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 48961
20201014::223130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223138_wf.raa
20201014::223147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223148_wf.raa
20201014::223157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223158_wf.raa
20201014::223159: Head 1: Time Synchronization: 2020.10.14   22:32:00::0015
20201014::223200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 49015
20201014::223200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223208_wf.raa
20201014::223217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223218_wf.raa
20201014::223227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223228_wf.raa
20201014::223230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.5dbar, CTD 34.5psu, index 1.34, Packet 49070
20201014::223230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223238_wf.raa
20201014::223247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223248_wf.raa
20201014::223257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223258_wf.raa
20201014::223300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 49125
20201014::223300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223308_wf.raa
20201014::223317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223318_wf.raa
20201014::223327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223328_wf.raa
20201014::223330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.7dbar, CTD 34.5psu, index 1.34, Packet 49179
20201014::223330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223338_wf.raa
20201014::223347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223348_wf.raa
20201014::223357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223358_wf.raa
20201014::223359: Head 1: Time Synchronization: 2020.10.14   22:34:00::0014
20201014::223400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.2dbar, CTD 34.5psu, index 1.34, Packet 49234
20201014::223400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223408_wf.raa
20201014::223417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223418_wf.raa
20201014::223427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223428_wf.raa
20201014::223430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.9dbar, CTD 34.5psu, index 1.34, Packet 49289
20201014::223430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223438_wf.raa
20201014::223447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223448_wf.raa
20201014::223457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223458_wf.raa
20201014::223459: Head 2: Time Synchronization: 2020.10.14   22:35:00::0014
20201014::223459: Head 1: Time Synchronization: 2020.10.14   22:35:00::0014
20201014::223500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.9dbar, CTD 34.5psu, index 1.34, Packet 49343
20201014::223500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223508_wf.raa
20201014::223517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223518_wf.raa
20201014::223527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223528_wf.raa
20201014::223530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.1dbar, CTD 34.5psu, index 1.34, Packet 49398
20201014::223530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223538_wf.raa
20201014::223547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223548_wf.raa
20201014::223557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223558_wf.raa
20201014::223559: Head 1: Time Synchronization: 2020.10.14   22:36:00::0017
20201014::223600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.3dbar, CTD 34.5psu, index 1.34, Packet 49453
20201014::223600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223608_wf.raa
20201014::223617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223618_wf.raa
20201014::223627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223628_wf.raa
20201014::223630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.7dbar, CTD 34.5psu, index 1.34, Packet 49507
20201014::223630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223638_wf.raa
20201014::223647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223648_wf.raa
20201014::223657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223658_wf.raa
20201014::223700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.8dbar, CTD 34.5psu, index 1.34, Packet 49562
20201014::223700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223708_wf.raa
20201014::223717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223718_wf.raa
20201014::223727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223728_wf.raa
20201014::223730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.3dbar, CTD 34.5psu, index 1.34, Packet 49617
20201014::223730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223738_wf.raa
20201014::223747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223748_wf.raa
20201014::223757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223758_wf.raa
20201014::223800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1214.2dbar, CTD 34.5psu, index 1.34, Packet 49672
20201014::223800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223808_wf.raa
20201014::223817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223818_wf.raa
20201014::223827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223828_wf.raa
20201014::223830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.8dbar, CTD 34.5psu, index 1.34, Packet 49726
20201014::223830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223838_wf.raa
20201014::223847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223848_wf.raa
20201014::223857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223858_wf.raa
20201014::223859: Head 1: Time Synchronization: 2020.10.14   22:39:00::0016
20201014::223900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.3dbar, CTD 34.5psu, index 1.34, Packet 49781
20201014::223900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223908_wf.raa
20201014::223917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223918_wf.raa
20201014::223927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223928_wf.raa
20201014::223930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.9dbar, CTD 34.5psu, index 1.34, Packet 49835
20201014::223930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::223937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223938_wf.raa
20201014::223947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223948_wf.raa
20201014::223957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_223958_wf.raa
20201014::224000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.6dbar, CTD 34.5psu, index 1.34, Packet 49889
20201014::224000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224008_wf.raa
20201014::224017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224018_wf.raa
20201014::224027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224028_wf.raa
20201014::224030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1215.2dbar, CTD 34.5psu, index 1.34, Packet 49944
20201014::224030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224038_wf.raa
20201014::224047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224048_wf.raa
20201014::224057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224058_wf.raa
20201014::224059: Head 1: Time Synchronization: 2020.10.14   22:41:00::0015
20201014::224100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.2dbar, CTD 34.5psu, index 1.34, Packet 50000
20201014::224100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224108_wf.raa
20201014::224117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224118_wf.raa
20201014::224127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224128_wf.raa
20201014::224130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.8dbar, CTD 34.5psu, index 1.34, Packet 50054
20201014::224130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224138_wf.raa
20201014::224147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224148_wf.raa
20201014::224157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224158_wf.raa
20201014::224159: Head 1: Time Synchronization: 2020.10.14   22:42:00::0016
20201014::224200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.8dbar, CTD 34.5psu, index 1.34, Packet 50109
20201014::224200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224208_wf.raa
20201014::224217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224218_wf.raa
20201014::224227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224228_wf.raa
20201014::224230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.7dbar, CTD 34.5psu, index 1.34, Packet 50164
20201014::224230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224238_wf.raa
20201014::224247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224248_wf.raa
20201014::224257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224258_wf.raa
20201014::224259: Head 1: Time Synchronization: 2020.10.14   22:43:00::0016
20201014::224300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1223.5dbar, CTD 34.5psu, index 1.34, Packet 50219
20201014::224300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224308_wf.raa
20201014::224317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224318_wf.raa
20201014::224327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224328_wf.raa
20201014::224330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.2dbar, CTD 34.5psu, index 1.34, Packet 50274
20201014::224330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224338_wf.raa
20201014::224347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224348_wf.raa
20201014::224357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224358_wf.raa
20201014::224400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.4dbar, CTD 34.5psu, index 1.34, Packet 50329
20201014::224400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224408_wf.raa
20201014::224417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224418_wf.raa
20201014::224427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224428_wf.raa
20201014::224430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.0dbar, CTD 34.5psu, index 1.34, Packet 50384
20201014::224430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224438_wf.raa
20201014::224447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224448_wf.raa
20201014::224457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224458_wf.raa
20201014::224459: Head 1: Time Synchronization: 2020.10.14   22:45:00::0015
20201014::224500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 50439
20201014::224500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224508_wf.raa
20201014::224517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224518_wf.raa
20201014::224527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224528_wf.raa
20201014::224530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 50493
20201014::224530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224538_wf.raa
20201014::224547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224548_wf.raa
20201014::224557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224558_wf.raa
20201014::224559: Head 1: Time Synchronization: 2020.10.14   22:46:00::0014
20201014::224600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 50548
20201014::224600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224608_wf.raa
20201014::224617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224618_wf.raa
20201014::224627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224628_wf.raa
20201014::224630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 50603
20201014::224630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224638: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224638_wf.raa
20201014::224647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224648_wf.raa
20201014::224657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224658_wf.raa
20201014::224659: Head 1: Time Synchronization: 2020.10.14   22:47:00::0014
20201014::224700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.9dbar, CTD 34.5psu, index 1.34, Packet 50659
20201014::224700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224708_wf.raa
20201014::224717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224718_wf.raa
20201014::224727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224728_wf.raa
20201014::224730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 50713
20201014::224730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224738_wf.raa
20201014::224747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224748_wf.raa
20201014::224757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224758_wf.raa
20201014::224800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 50768
20201014::224800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224808_wf.raa
20201014::224817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224818_wf.raa
20201014::224827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224828_wf.raa
20201014::224830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.4dbar, CTD 34.5psu, index 1.34, Packet 50823
20201014::224830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224838_wf.raa
20201014::224847: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224848_wf.raa
20201014::224857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224858_wf.raa
20201014::224900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1229.7dbar, CTD 34.5psu, index 1.34, Packet 50878
20201014::224900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224908_wf.raa
20201014::224917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224918_wf.raa
20201014::224927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224928_wf.raa
20201014::224930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1231.4dbar, CTD 34.5psu, index 1.34, Packet 50933
20201014::224930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::224937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224938_wf.raa
20201014::224947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224948_wf.raa
20201014::224957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_224958_wf.raa
20201014::224959: Head 2: Time Synchronization: 2020.10.14   22:50:00::0013
20201014::224959: Head 1: Time Synchronization: 2020.10.14   22:50:00::0013
20201014::225000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.2dbar, CTD 34.5psu, index 1.34, Packet 50987
20201014::225000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225008_wf.raa
20201014::225017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225018_wf.raa
20201014::225027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225028_wf.raa
20201014::225030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.2dbar, CTD 34.5psu, index 1.34, Packet 51042
20201014::225030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225038_wf.raa
20201014::225047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225048_wf.raa
20201014::225057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225058_wf.raa
20201014::225100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1237.3dbar, CTD 34.5psu, index 1.34, Packet 51097
20201014::225100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225108_wf.raa
20201014::225117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225118_wf.raa
20201014::225127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225128_wf.raa
20201014::225130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1235.7dbar, CTD 34.5psu, index 1.34, Packet 51152
20201014::225130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225138_wf.raa
20201014::225147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225148_wf.raa
20201014::225157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225158_wf.raa
20201014::225200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1233.9dbar, CTD 34.5psu, index 1.34, Packet 51206
20201014::225200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225208_wf.raa
20201014::225217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225218_wf.raa
20201014::225227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225228_wf.raa
20201014::225230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1232.1dbar, CTD 34.5psu, index 1.34, Packet 51261
20201014::225230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225238_wf.raa
20201014::225247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225248_wf.raa
20201014::225257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225258_wf.raa
20201014::225300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1230.1dbar, CTD 34.5psu, index 1.34, Packet 51315
20201014::225300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225308_wf.raa
20201014::225317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225318_wf.raa
20201014::225327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225328_wf.raa
20201014::225330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.7dbar, CTD 34.5psu, index 1.34, Packet 51369
20201014::225330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225338_wf.raa
20201014::225347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225348_wf.raa
20201014::225357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225358_wf.raa
20201014::225359: Head 1: Time Synchronization: 2020.10.14   22:54:00::0015
20201014::225400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 51424
20201014::225400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225408_wf.raa
20201014::225417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225418_wf.raa
20201014::225427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225428_wf.raa
20201014::225430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 51479
20201014::225430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225438_wf.raa
20201014::225447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225448_wf.raa
20201014::225457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225458_wf.raa
20201014::225459: Head 1: Time Synchronization: 2020.10.14   22:55:00::0016
20201014::225500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 51533
20201014::225500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225508_wf.raa
20201014::225517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225518_wf.raa
20201014::225527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225528_wf.raa
20201014::225530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 51588
20201014::225530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225537: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225538_wf.raa
20201014::225547: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225548_wf.raa
20201014::225557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225558_wf.raa
20201014::225559: Head 1: Time Synchronization: 2020.10.14   22:56:00::0014
20201014::225600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 51642
20201014::225600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225607: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225608_wf.raa
20201014::225617: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225618_wf.raa
20201014::225627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225628_wf.raa
20201014::225630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 51697
20201014::225630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225637: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225638_wf.raa
20201014::225647: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225648_wf.raa
20201014::225657: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225658_wf.raa
20201014::225700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 51751
20201014::225700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225707: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225708_wf.raa
20201014::225717: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225718_wf.raa
20201014::225727: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225728_wf.raa
20201014::225730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.3dbar, CTD 34.5psu, index 1.34, Packet 51806
20201014::225730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225737: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225738_wf.raa
20201014::225747: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225748_wf.raa
20201014::225757: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225758_wf.raa
20201014::225800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.8dbar, CTD 34.5psu, index 1.34, Packet 51861
20201014::225800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225808_wf.raa
20201014::225817: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225818_wf.raa
20201014::225827: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225828_wf.raa
20201014::225830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.5dbar, CTD 34.5psu, index 1.34, Packet 51916
20201014::225830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225837: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225838_wf.raa
20201014::225852: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225848_wf.raa
20201014::225857: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225858_wf.raa
20201014::225859: Head 1: Time Synchronization: 2020.10.14   22:59:00::0014
20201014::225900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.2dbar, CTD 34.5psu, index 1.34, Packet 51970
20201014::225900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225907: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225908_wf.raa
20201014::225917: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225918_wf.raa
20201014::225927: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225928_wf.raa
20201014::225930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.8dbar, CTD 34.5psu, index 1.34, Packet 52024
20201014::225930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::225937: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225938_wf.raa
20201014::225947: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225948_wf.raa
20201014::225957: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_225958_wf.raa
20201014::230000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1221.3dbar, CTD 34.5psu, index 1.34, Packet 52079
20201014::230000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230007: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230008_wf.raa
20201014::230017: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230018_wf.raa
20201014::230027: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230028_wf.raa
20201014::230030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1219.2dbar, CTD 34.5psu, index 1.34, Packet 52133
20201014::230030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230037: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230038_wf.raa
20201014::230047: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230048_wf.raa
20201014::230057: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230058_wf.raa
20201014::230100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230100: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.1dbar, CTD 34.5psu, index 1.34, Packet 52188
20201014::230100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230107: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230108_wf.raa
20201014::230117: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230118_wf.raa
20201014::230127: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230128_wf.raa
20201014::230130: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.4dbar, CTD 34.5psu, index 1.34, Packet 52242
20201014::230130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230137: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230138_wf.raa
20201014::230147: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230148_wf.raa
20201014::230157: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230158_wf.raa
20201014::230200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230200: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1216.9dbar, CTD 34.5psu, index 1.34, Packet 52297
20201014::230200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230207: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230208_wf.raa
20201014::230217: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230218_wf.raa
20201014::230227: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230228_wf.raa
20201014::230230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230230: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.3dbar, CTD 34.5psu, index 1.34, Packet 52352
20201014::230230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230237: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230238_wf.raa
20201014::230247: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230248_wf.raa
20201014::230257: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230258_wf.raa
20201014::230300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230300: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.0dbar, CTD 34.5psu, index 1.34, Packet 52406
20201014::230300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230307: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230308_wf.raa
20201014::230317: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230318_wf.raa
20201014::230327: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230328_wf.raa
20201014::230330: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.4dbar, CTD 34.5psu, index 1.34, Packet 52461
20201014::230330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230337: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230338_wf.raa
20201014::230347: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230348_wf.raa
20201014::230357: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230358_wf.raa
20201014::230400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230400: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.2dbar, CTD 34.5psu, index 1.34, Packet 52516
20201014::230400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230407: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230408_wf.raa
20201014::230417: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230418_wf.raa
20201014::230427: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230428_wf.raa
20201014::230430: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1217.5dbar, CTD 34.5psu, index 1.34, Packet 52570
20201014::230430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230437: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230438_wf.raa
20201014::230447: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230448_wf.raa
20201014::230457: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230458_wf.raa
20201014::230459: Head 1: Time Synchronization: 2020.10.14   23:05:00::0015
20201014::230500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230500: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1218.5dbar, CTD 34.5psu, index 1.34, Packet 52625
20201014::230500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230507: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230508_wf.raa
20201014::230517: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230518_wf.raa
20201014::230527: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230528_wf.raa
20201014::230530: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1220.1dbar, CTD 34.5psu, index 1.34, Packet 52679
20201014::230530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230538: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230538_wf.raa
20201014::230548: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230548_wf.raa
20201014::230557: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230558_wf.raa
20201014::230600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230600: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1222.4dbar, CTD 34.5psu, index 1.34, Packet 52734
20201014::230600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230616: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230608_wf.raa
20201014::230620: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230618_wf.raa
20201014::230627: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230628_wf.raa
20201014::230630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230630: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.1dbar, CTD 34.5psu, index 1.34, Packet 52788
20201014::230631: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 22.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230643: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230638_wf.raa
20201014::230648: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230648_wf.raa
20201014::230659: Head 1: Time Synchronization: 2020.10.14   23:07:00::0017
20201014::230700: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1224.9dbar, CTD 34.5psu, index 1.34, Packet 52841
20201014::230700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230700: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230658_wf.raa
20201014::230714: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230708_wf.raa
20201014::230719: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230718_wf.raa
20201014::230728: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230728_wf.raa
20201014::230730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230730: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1226.3dbar, CTD 34.5psu, index 1.34, Packet 52896
20201014::230730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 15.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 27.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230738: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230738_wf.raa
20201014::230748: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230748_wf.raa
20201014::230758: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230758_wf.raa
20201014::230759: Head 1: Time Synchronization: 2020.10.14   23:08:00::0019
20201014::230800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230800: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.2dbar, CTD 34.5psu, index 1.34, Packet 52950
20201014::230800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230807: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230808_wf.raa
20201014::230818: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230818_wf.raa
20201014::230828: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230828_wf.raa
20201014::230830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230830: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.7dbar, CTD 34.5psu, index 1.34, Packet 53004
20201014::230830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 13.5Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230838: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230838_wf.raa
20201014::230848: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230848_wf.raa
20201014::230858: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230858_wf.raa
20201014::230859: Head 1: Time Synchronization: 2020.10.14   23:09:00::0019
20201014::230900: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.8dbar, CTD 34.5psu, index 1.34, Packet 53059
20201014::230900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230909: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230908_wf.raa
20201014::230918: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230918_wf.raa
20201014::230928: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230928_wf.raa
20201014::230930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230930: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.0dbar, CTD 34.5psu, index 1.34, Packet 53113
20201014::230930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 23.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::230938: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230938_wf.raa
20201014::230948: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230948_wf.raa
20201014::230959: Head 1: Time Synchronization: 2020.10.14   23:10:00::0020
20201014::230959: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_230959_wf.raa
20201014::231000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::231000: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.3dbar, CTD 34.5psu, index 1.34, Packet 53168
20201014::231000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::231009: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_231009_wf.raa
20201014::231019: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_231019_wf.raa
20201014::231029: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_231029_wf.raa
20201014::231030: System  Initialized, Gain 8, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1228.1dbar, CTD 34.5psu, index 1.34, Packet 53222
20201014::231030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 14.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 3, laser state 1
20201014::231030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 21.5Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 3, laser state 1
20201014::231038: GUI: Archiving data to file --> C:\Data\20201014d2\20201014_231039_wf.raa
20201014::231048: GUI: Live mode ON.
20201014::231048: GUI: Requesing STOP operation, Head 2
20201014::231048: GUI: Requesing STOP operation, Head 1
20201014::231048: Head 2: Received request: STOP
20201014::231048: Head 1: Received request: STOP
20201014::231049: Head 2: Stopping Scan Operation
20201014::231049: Head 1: Stopping Scan Operation
20201014::231051: Head 2: ProcessingMgr stopped all worker threads.
20201014::231051: Head 1: ProcessingMgr stopped all worker threads.
20201014::231051: Head 2:       Stop finished, may now recover.
20201014::231051: Head 1:       Stop finished, may now recover.
20201014::231053: Head 1: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::231053: Head 1: Eye Safe Optical Filter check Passed
20201014::231054: Head 2: Eye Safe Optical Filter State there 5, not there 25, transition 1
20201014::231055: Head 2: Eye Safe Optical Filter check Passed
20201014::231100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 21.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231100: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1227.6dbar, CTD 34.5psu, index 1.34, Packet 53276
20201014::231100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 22.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 20.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231130: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.1C, CTD 1225.7dbar, CTD 34.5psu, index 1.34, Packet 53330
20201014::231130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231200: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1215.5dbar, CTD 34.5psu, index 1.34, Packet 53385
20201014::231200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231230: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.2C, CTD 1201.4dbar, CTD 34.5psu, index 1.34, Packet 53438
20201014::231230: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231300: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1186.0dbar, CTD 34.5psu, index 1.34, Packet 53492
20201014::231300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 21.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231330: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.3C, CTD 1171.2dbar, CTD 34.5psu, index 1.34, Packet 53545
20201014::231330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 19.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231400: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1154.1dbar, CTD 34.5psu, index 1.34, Packet 53599
20201014::231400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231430: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1137.6dbar, CTD 34.5psu, index 1.34, Packet 53652
20201014::231430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231500: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.4C, CTD 1120.3dbar, CTD 34.5psu, index 1.34, Packet 53706
20201014::231500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231530: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1103.6dbar, CTD 34.5psu, index 1.34, Packet 53759
20201014::231530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231600: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.5C, CTD 1087.1dbar, CTD 34.5psu, index 1.34, Packet 53815
20201014::231600: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231630: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1070.4dbar, CTD 34.5psu, index 1.34, Packet 53869
20201014::231630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 20.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231700: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.6C, CTD 1054.8dbar, CTD 34.5psu, index 1.34, Packet 53923
20201014::231700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231730: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.7C, CTD 1039.4dbar, CTD 34.5psu, index 1.34, Packet 53976
20201014::231730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231800: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1023.9dbar, CTD 34.5psu, index 1.34, Packet 54030
20201014::231800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231830: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 1008.1dbar, CTD 34.5psu, index 1.34, Packet 54083
20201014::231830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231900: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 991.3dbar, CTD 34.5psu, index 1.34, Packet 54137
20201014::231900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::231930: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 975.3dbar, CTD 34.5psu, index 1.34, Packet 54190
20201014::231930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232000: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232000: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.8C, CTD 958.8dbar, CTD 34.5psu, index 1.34, Packet 54244
20201014::232000: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232030: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.9C, CTD 942.5dbar, CTD 34.4psu, index 1.34, Packet 54297
20201014::232030: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232030: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232100: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 3.9C, CTD 926.0dbar, CTD 34.4psu, index 1.34, Packet 54350
20201014::232100: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232100: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232130: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232130: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.0C, CTD 910.1dbar, CTD 34.4psu, index 1.34, Packet 54404
20201014::232130: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232200: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232200: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.1C, CTD 894.6dbar, CTD 34.4psu, index 1.34, Packet 54457
20201014::232200: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232230: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232231: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 878.8dbar, CTD 34.4psu, index 1.34, Packet 54511
20201014::232231: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232300: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.2C, CTD 863.1dbar, CTD 34.4psu, index 1.34, Packet 54562
20201014::232300: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232300: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232330: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 847.2dbar, CTD 34.4psu, index 1.34, Packet 54615
20201014::232330: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 19.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232330: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232400: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 831.4dbar, CTD 34.4psu, index 1.34, Packet 54669
20201014::232400: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 18.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232400: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232430: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.3C, CTD 815.6dbar, CTD 34.4psu, index 1.34, Packet 54722
20201014::232430: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232430: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232500: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232500: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 799.4dbar, CTD 34.4psu, index 1.34, Packet 54776
20201014::232500: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232530: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 783.6dbar, CTD 34.4psu, index 1.34, Packet 54828
20201014::232530: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232530: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232600: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232600: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.4C, CTD 767.2dbar, CTD 34.4psu, index 1.34, Packet 54882
20201014::232601: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232630: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232630: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.5C, CTD 751.2dbar, CTD 34.4psu, index 1.34, Packet 54934
20201014::232630: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232700: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232700: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 734.9dbar, CTD 34.4psu, index 1.34, Packet 54987
20201014::232700: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232730: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232730: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.6C, CTD 718.7dbar, CTD 34.4psu, index 1.34, Packet 55040
20201014::232730: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232800: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232800: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.7C, CTD 702.3dbar, CTD 34.4psu, index 1.34, Packet 55094
20201014::232800: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232822: Head 2: Comm CTD Error, disconnecting
20201014::232822: Head 1: Comm CTD Error, disconnecting
20201014::232823: Head 2: Warning, CTD not recieved within 2 minutes.
20201014::232823: Head 1: Warning, CTD not recieved within 2 minutes.
20201014::232823: Head 2: Restarting CTD Ethernet connection ...
20201014::232823: Head 1: Restarting CTD Ethernet connection ...
20201014::232830: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232830: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 692.4dbar, CTD 34.4psu, index 1.34, Packet 55148
20201014::232830: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232900: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232900: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 692.4dbar, CTD 34.4psu, index 1.34, Packet 55202
20201014::232900: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232930: Head #2, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 25%, OPB 9C, Laser 17.0C, Dig 32.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232930: System  Initialized, Gain 1, Elec PB 16.1C, Elec PB 26.4%, Elec PB 5V 5.0V, Elec PB 3V 3.4V, CTD 4.8C, CTD 692.4dbar, CTD 34.4psu, index 1.34, Packet 55256
20201014::232930: Head #1, Init state OK, comm ctrl 1, comm data 1, Scan rate 0.0Hz, OCB Init 1, OCB 17C, OCB 26%, OPB 10C, Laser 18.0C, Dig 26.0C, Scan Az fault 0, gain 0, laser state 0
20201014::232947: GUI: OnBnClickedOk
20201014::232947: GUI: Exiting the WiSSL GUI..
20201014::232947: GUI: Writing configuration data to file --> C:\3D\CFG\WiSSL_Gui.cfg
20201014::232947: GUI: Wrote configuration data.
