Power Can Connector
J1 MINK10/L
	Connector Name
	Bulkhead Type
	Vendor
	Function(s)
	Bulkhead Thread
	Spotface Diameter

	J1
	MINK10/L
	Seaconn
	GigE & AC Power In
	¾-20
	1.22’’

	J2
	MINK16
	Seaconn
	Camera 24V Pwr, Gige, Cam trigger in
	¾-20
	1.22’’

	J3
	MINK16
	Seaconn
	Camera 24V Pwr, Gige, Cam Trigger out
	¾-20
	1.22’’

	J4
	MINK16
	Seacon
	Spare, 24V Pwr, GigE
	¾-20
	1.22’’

	J5
	MINK16
	Seacon
	Spare, 24V Pwr, GigE
	¾-20
	1.22’’

	J6
	MHDG16
	Impulse
	Reson 7125, 24V Pwr, Gige, 1PPS, Sonar Trigger
	9/16-18

	1.1’’

	J7
	MCBH3F
	Subconn
	RS232 Serial configured as 1PPS
	7/16-20

	1.0’’

	J8
	MHDL16BCR
	Impulse
	LIDAR 48V pwr, 1PPS, 10/100BT
	7/8-20
	1.35’’

	J9
	BH5F
	Subconn
	Strobe Power & Trigger
	7/16-20

	1.0’’
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