Baud rate 9600bps, 8 data bits, one stop bit, no parity. Each data frame contains eight bytes..

Control command format:
	Bytes Number
	1
	2
	3
	4
	5
	6
	7
	8

	
	Frame head
	Reserved bytes
	Channel
	Command
	checksum

	Reading status
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	00
	0xAB

0xAC

0xAD

0xAE

0xAF

0xB0
0xB1

0xB2

	Relay open
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	01
	0xAD

0xAE

0xAF

0xB0
0xB1

0xB2

0xB3

0xB4

	Relay close
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	02
	0xAE

0xAF

0xB0

0xB1
0xB2

0xB3

0xB4
0xB5

	Relay toggle
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	03
	0xAF

0xB0

0xB1

0xB2
0xB3

0xB4

0xB5

0xB6

	Relay momentary
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	04
	0xB0

0xB1

0xB2

0xB3
0xB4

0xB5

0xB6

0xB7

	Relay

 Interlock
	0x5556
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4

0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	05
	0xB1
0xB2
0xB3
0xB4
0xB5

0xB6

0xB7

0xB8


5 Control commands：

1. Reading status（reading the satus of the relay (on/off)）

Channel 1 ：55 56 00 00 00 01 00 AC
Channel 2 ：55 56 00 00 00 02 00 AD
Channel 3 ：55 56 00 00 00 03 00 AE
Channel 4 ：55 56 00 00 00 04 00 AF

Channel 5 ：55 56 00 00 00 05 00 B0
Channel 6 ：55 56 00 00 00 06 00 B1
Channel 7 ：55 56 00 00 00 07 00 B2
Channel 8 ：55 56 00 00 00 08 00 B3

2. Relay open (issue this command ，Relay open , COM connect to NO ）
Channel 1 ：55 56 00 00 00 01 01 AD
Channel 2 ：55 56 00 00 00 02 01 AE
Channel 3 ：55 56 00 00 00 03 01 AF
Channel 4 ：55 56 00 00 00 04 01 B0
Channel 5 ：55 56 00 00 00 05 01 B1
Channel 6 ：55 56 00 00 00 06 01 B2
Channel 7 ：55 56 00 00 00 07 01 B3
Channel 8 ：55 56 00 00 00 08 01 B4

3. Relay close (issue this command ，Relay close , COM disconnect NO , and COM connect to NC ）
Channel 1 ：55 56 00 00 00 01 02 AE
Channel 2 ：55 56 00 00 00 02 02 AF
Channel 3 ：55 56 00 00 00 03 02 B0
Channel 4 ：55 56 00 00 00 04 02 B1
Channel 5 ：55 56 00 00 00 05 02 B2
Channel 6 ：55 56 00 00 00 06 02 B3
Channel 7 ：55 56 00 00 00 07 02 B4
Channel 8 ：55 56 00 00 00 08 02 B5

4. Relay toggle（Relay status reversal，if COM connect to NO，this commands will Disconnect COM to NO and Reverse COM connect to NC，and vice versa）
Channel 1 ：55 56 00 00 00 01 03 AF
Channel 2 ：55 56 00 00 00 02 03 B0
Channel 3 ：55 56 00 00 00 03 03 B1
Channel 4 ：55 56 00 00 00 04 03 B2
Channel 5 ：55 56 00 00 00 05 03 B3
Channel 6 ：55 56 00 00 00 06 03 B4
Channel 7 ：55 56 00 00 00 07 03 B5
Channel 8 ：55 56 00 00 00 08 03 B6

5. Relay momentary（Relay COM connect to NO，disconnect after 200MS ）
Channel 1 ：55 56 00 00 00 01 04 B0
Channel 2 ：55 56 00 00 00 02 04 B1
Channel 3 ：55 56 00 00 00 03 04 B2
Channel 4 ：55 56 00 00 00 04 04 B3
Channel 5 ：55 56 00 00 00 05 04 B4
Channel 6 ：55 56 00 00 00 06 04 B5
Channel 7 ：55 56 00 00 00 07 04 B6
Channel 8 ：55 56 00 00 00 08 04 B7

6. Relay Interlock
Channel 1 ：55 56 00 00 00 01 05 B1
Channel 2 ：55 56 00 00 00 02 05 B2
Channel 3 ：55 56 00 00 00 03 05 B3
Channel 4 ：55 56 00 00 00 04 05 B4
Channel 5 ：55 56 00 00 00 05 05 B5
Channel 6 ：55 56 00 00 00 06 05 B6
Channel 7 ：55 56 00 00 00 07 05 B7
Channel 8 ：55 56 00 00 00 08 05 B8

Once issue a command, will have a return fame , 7th byte of return fame mean the satus of realy .
Return command format:
	Bytes Number
	1
	2
	3
	4
	5
	6
	7
	8

	
	Frame head
	Reserved bytes
	Channel
	Command
	checksum

	Return relay open 
	0x333C
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4
0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	01
	0x71

0x72

0x73

0x74
0x75
0x76
0x77
0x78

	Return relay close
	0x333C
	0x000000
	0x01 Channel 1

0x02 Channel 2

0x03 Channel 3

0x04 Channel 4
0x05 Channel 5
0x06 Channel 6
0x07 Channel 7
0x08 Channel 8
	02
	0x72

0x73

0x74

0x75
0x76
0x77
0x78
0x79


2 return command 
1、Return relay open（return this command，mean COM connect to NO ）
Channel 1 ：33 3C 00 00 00 01 01 71

Channel 2 ：33 3C 00 00 00 02 01 72

Channel 3 ：33 3C 00 00 00 03 01 73

Channel 4 ：33 3C 00 00 00 04 01 74
Channel 5 ：33 3C 00 00 00 05 01 75

Channel 6 ：33 3C 00 00 00 06 01 76

Channel 7 ：33 3C 00 00 00 07 01 77

Channel 8 ：33 3C 00 00 00 08 01 78

2、Return relay close（return this command，mean COM disconnect NO , and COM connect to NC ）
Channel 1 ：33 3C 00 00 00 01 02 72

Channel 2 ：33 3C 00 00 00 02 02 73

Channel 3 ：33 3C 00 00 00 03 02 74

Channel 4 ：33 3C 00 00 00 04 02 75

Channel 5 ：33 3C 00 00 00 05 02 76

Channel 6 ：33 3C 00 00 00 06 02 77

Channel 7 ：33 3C 00 00 00 07 02 78

Channel 8 ：33 3C 00 00 00 08 02 79

