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LIDAR:
· 50 degrees each
· 94 degrees total on 10.5” baseline located at bottom of LIDAR mount frame.

Reson:
· Receiver array:  120 degrees on 20” baseline at transducer face

Kearfott:
· Each beam 30 degress on 2.5” baseline
· Each beam it oriented 30 degrees from vertical, centered on a 5.75” baseline
· Net Port-Starboard beam width = 90 degrees on 8” baseline at base of instrument (approx.)

Cameras:
· Relatively Narrow

