	Button control
	

	t app button: shutter/power/wifi -P = Press, R = Release PR = Press and Release (click)
	Example: t app button shutter PR

	Time between actions
	

	sleep: time in seconds
	Example: sleep 6

	Camera Modes
	

	t app appmode: video/photo/photo_burst (Burst) /photo_pes (Timelapse) /settings
	Example: t app appmode photo_burst

	Custom text on LCD
	

	t app fp_show 4
sleep 2
t app fp_string 'custom text here'
t app fp_show 4 will show a blank screen before the text
	Example: t app fp_show 4
sleep 2
t app fp_string 'i will kill you'

	LEDs Settings
	

	t app led_count: 4/2/0
	Example: t app led_count 0

	LED control
	

	t app led: red_front/red_top_bottom/red_back/ {on/off}
	Example: t app led red_front on

	Video Format
	

	t app video_format: ntsc/pal
	Example: t app video_format pal

	One Button Mode
	

	t app obm: on/off
	Example: t app obm on

	White Balance
	

	t app white_balance: auto/3000/5500/6500/camraw
	Example: t app white_balance 3000

	Loop
	

	d:\autoexec.ash
REBOOT yes
	Example:
sleep 1 
t app appmode photo 
sleep 120 
t app button shutter PR 
d:\autoexec.ash 
REBOOT yes

	Protune
	

	t app protune: on/off
	Example: t app protune on

	Lock exposure
	

	t app protune: on/off
	Example: t app protune on

	Video Loop
	

	t ia2 -exp lock: 1=on 0=off
	Example: t ia2 -exp lock 1

	Video+Photo
	

	t app video_photo: off/5/10/30/60
	Example: t app video_photo 5

	Spot Meter
	

	t app spot_meter: on/off
	Example: t app spot_meter on

	Mirror Flip
	

	t app flip_mirror: enable=1/disable=0
	Example: t app flip_mirror 1

	Delete a directory (such as DCIM) (works with all cameras!)
	

	deletedir: SD card port d:\ + DCIM folder
	Example: deletedir d:\DCIM

	Timelapse Settings
	

	t app pes_settings: 0.5/1/2/5/10/20/60
	Example: t app pes_settings 5

	Burst Settings
	

	t app burst_settings: 3-1/5-1/10-1/10-2/30-1/30-2/30-3
	Example: t app burst_settings 30-2

	Continuous Photo Settings
	

	t app sps_settings: single=1/3/5/10
	Example: t app sps_settings 10

	Photo Resoultion
	

	t app photo_size: 12W/7M/7W/5M
	Example: t app photo_size 7W

	Rotation /basic/
	

	t app test vin_rotate: 0/90/180/270
	Example: t app test vin_rotate 90

	Rotation /advanced/
	

	t app test rec_fmt_rotate: Normal=0x01/Flip&Horizontal=0x02/
Rotate180=0x03/Flip&Vertical=0x04/Transpose=0x05/
Rotate90=0x06/Transverse=0x07/Rotate270=0x08
	Example: t app test rec_fmt_rotate 0x04

	Key
	

	t app key: up/up_rel/down/down_rel/left/left_rel/right/right_rel/zoomin/zoomin_rel/
zoomout/zoomout_rel/set/focus/focus_rel/shutter/shutter_rel/record/
mode/menu/power/del/format/copydir/switchosd
	Example: t app key zoomin

	Default mode
	

	t app default_mode: last/video/photo/photo_burst(Burst)/photo_pes (Timelapse)
	Example: t app default_mode photo

	Auto-power off
	

	t app shutdown_mode: manual/60/120/300
	Example: t app shutdown_mode 120

	HERO3Plus Black Power 0ff
	

	poweroff yes reboot yes
	Example: poweroff yes reboot yes

	HERO3Plus Black Boss Boot
	

	t app test boss_boot: enable=1/disable=0
	Example: t app test boss_boot 1

	HERO3Plus Black SB sensor
	

	t app sensor_sb: enable/disable
	Example: t app sensor_sb enable

	HERO3Plus Black Photo Resolution
	

	t app photo_size: 12W/10W/7M/7W/5M
	Example: t app photo_size 10W

	HERO3Plus Black LCD Images
	

	t app test fp_display: splash_screen.bmp/video.bmp/photo.bmp/one_button.bmp/
blank.bmp/background.bmp
	Example: t app test fp_display video.bmp

	HERO3Plus Black Rotation
	

	t app test vin_rotate: 0/90/180/270/flip_h/flip_v
	Example: t app test vin_rotate 270

	HERO3Plus Black HDMI Settings (PES)
	

	t app hdmi_set_pes: none/10%/20%/30%
	Example: t app hdmi_set_pes 10%

	HERO3Plus Black HDMI Settings (PIV)
	

	t app hdmi_set_pib: 0mA/0.6mA/1.2mA/1.8mA
	Example: t app hdmi_set_piv 1.3mA

	HERO3Plus button status
v2.0
	

	t app btn_status: enable(1) / disable(0)
	Example: t app btn_status 1

	HERO3Plus 3D Smarty Master
v2.0
	

	t app master_set_for_smarty: start(1) / stop(0)
	Example: t app master_set_for_smarty 1

	HERO3Plus 3D Smarty Slave
v2.0
	

	t app slave_set_for_smarty: start(1) / stop(0)
	Example: t app slave_set_for_smarty 1

	HERO3Plus Heart beat for 3D
v2.0
	

	t app heart_beat_3d: on(1) / off(0)
	Example: t app heart_beat_3d 1

	HERO3Plus 3D Video Start/Stop recording (?)
v2.0
	

	t app test bacpac3d I2C SY: START_RECORD / STOP_RECORD
	Example: t app test bacpac3d I2C SY START RECORD

	HERO3Plus WB Gain Set
	

	t ia2 -awb: [set][][][]
	Example: t ia2 -awb [788][][][]

	HERO3Plus ISO Still Set
	

	t ia2 -ae still_iso: [iso]
	Example: t ia2 -ae still_iso 1200

	HERO3Plus Shutter Still Set
	

	t ia2 -ae still_shutter: [shutter]
	Example: t ia2 -ae still_shutter 126

	HERO3Plus ISO Still Set
	

	t ia2 -ae still_iris: [iris]
	Example: t ia2 -ae still_iris 45

	The commands tagged with v2.0 ONLY work with GoPro HERO3 Plus Black cameras with the firmware 2.0 of 6 March 2014
t app, t ia2, deletedir work for all gopro models, t cal works only for hero3 black/plus black/plus silver
	

	Video/Photo Digital Filters
For HERO3 Black / HERO3+ Black / HERO3+ Silver
	

	t cal -de: 1/2/3/4/5/6/7/8/9/10

· 1: Art effect
· 2: Sepia Effect
· 3: Negative Effect
· 4: Black White Effect
· 5: Vivid Effect
· 6: 70s Film Effect
· 7: Punk Effect
· 8: Popart Effect
· 9: Wedding Effect
· 10:Pinhole Effect
	Example: t cal -de 4
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