## Control Center Serial

#### Batch Instruction Commands

Notes on Batch Instructions:

- Unless specified otherwise, all arguments to a batch instruction are "1" to enable/request the specified parameter, or "0" to disable/not request the specified parameter.
- Name of root element can be either aardvark or adapter.

General Commands

- configure
- sleep

I2C Commands

- i2c_bitrate
- i2c_write
- i2c_read
- i2c_free_bus

SPI Commands

- spi_config
- spi_bitrate
- spi_write
- spi_read

GPIO Commands

- gpio_config
- gpio_get
- gpio_set