Budget for fabrication of 4000m rated housing for SeeStar camera:


[image: ]
Approximate dimensions and specs:
Outside diameter: 5.5”
Inside diameter: 5”.
Length (including encaps): 17”
Flat port (BK7 or sapphire), 4” diameter
Lens: 16mm Sony e-mount.
Cost of components:

	
	Material cost (USD)
	Vendor
	Machine shop time (hours)

	Titanium endcap
	191
	titanium industries
	20

	Titanium tube
	1825
	titanium industries
	20

	Titanium port ring
	191
	titanium industries
	15

	Flat port
	727.5
	EP Oceanographic
	NA

	Aluminum chassis
	50
	McMaster
	8

	Vent plug
	200
	Prevco
	NA

	Fasteners
	50
	McMaster, United Ti
	NA

	Misc. hardware
	100
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	NA

	total
	3154.50
	 
	67
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