O-rings for SeeStar deep. Created 8/19/15 by Francois
[bookmark: _GoBack]All o-rings should be EPDM or buna-N, 70 durometer and should be very sparingly lubricated with o-ring grease
Camera housing:
1 endcap o-ring: 2-039
1 port o-ring: 2-023
2 connector o-rings: 2-014
Battery housing:
2 endcap o-rings: 2-147
1 connector o-rings: 2-014
Light housing
1 or two endcap or rings: 2-147
1 port o-ring: 2-033
1 connector o-ring: 2-014

o-ring list for SeeStar 1 (PVC housings):
Camera housing:
2 endcap o-rings: 2-151
2 connector o-rings: 2-014
Battery housing:
2 endcap o-rings: 2-151
1 connector o-ring: 2-014
Light housing:
2 endcap o-rings: 2-151
1 connector o-ring: 2-014
