1.Run DirectUSB_Setup_a2s_20090710.exe file.
2.After installation,copy the board.ini file to the installation directory.
3.Run the DirectUSB software.
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4. There are three red Circle marks in above picture, set parameters according to these.

5. Press the Snap key of DV, then connect the usb cable with it(it means power on the dv).
6. Press “connect” button to check whether the usb connection is ok or no. If it is not ok, then

Do step 5 again.

7. Press “choose” button to select the firmware file(dv600d_USB_txd_PAR_PAR1207071X.elf). 

8. Press “Download” button to download.

9. The download ok message will appear in above window after finish the download, it will be about 20 Sec.

