Plankton imager design requiremenst

1. white light source (FR- color images)
2. Resolution of camera should be such that we achieve X pixels for each 0.5 cm object (at what distance?)
This seems like a design requirement. What are the objects to be imaged and how much resolution do you need to study them? Do you need to count the legs, identify species of ?? and at what distance, i.e. across what field of view.
3. Flat port. Not sure why this is a functional requirement. Sounds possible given 50 degree field of view. This should really be driven by 8, 10 and 17.
