SCPI Function Requirements
1. System must be able to distinguish a target of TBD cm (0.5-1)
2. System shall take color images therefore white light source
3. System shall have a programmable sample rate
4. System shall be triggerable externally
5. System shall be rated for 500m depth
6. System shall be self-contained- onboard power and storage
7. System shall have a cabled option for using remote power and data comms
8. System shall have a field of view of 1 m x 1.5 m – 50 deg
9. Depth of field
10. Resolution of camera should be such that we achieve X pixels for each 0.5 cm object
11. Have computer to control camera
12. Shall be able to acquire X images per mission
13. Synchronize time with external source at the start of mission
14. Shall be battery operated
15. Flat port
16. Size, weight < 2 kg
17. 

