MBARI’S MINI ROV CONTROL/WORK VAN SPECIFICATIONS
[bookmark: _GoBack]
Single trip 20’ ISO container
Insulate interior with R13 insulation and install ¾” plywood liner on walls and ceiling
Retain double doors
Install water tight personnel door (located on side of van)
Install Roxtec regular cable gland
Install recess for 2t AC unit and “Mains” power connection (1 x 230 3 phase @ 20A) and (1 x 230/220 1 phase @ 60A)
Install (inside) 100A service breaker panel for the 230/220 1 phase main supply
Paint exterior with industry standard marine epoxy paint

