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Notes

In attendance: Alana Sherman, Jose Rosal, Paul McGill, Ed Mellinger, Andy Hamilton, Dale Graves, Ken Smith, Brett Hobson, Charlie Paull, Doug Au


Vehicle to have LED lights - similar in lumens to current phantom.

Ground faulting OTS - agency safety rated for topside (tether).

Shanna Rae - 6kW, 110V, single phase available.

Overvoltage protection for Vicors needed

Tether: 14AWGx4 SouthBay specificed 8A max - under what conditions? 
	Heating on the drum - water cooled?

Possible power solutions:	
	Running Vicor modules in series (at input) and parallel the outputs.
	Shunt regulation	


Question about multiple busses for the thruster 48Vdc. 2 Horz + 1 Vert per bus
	Combining busses in the event of a Vicor failure?
	Utilize shutdown feature of Vicor modules to maximize bus efficiency?

Excess tether only 10% longer. Why? No consensus.

Ed - noted to specify DC voltage for new tether.


