File Name:  10020690rA
QTY: 5-10
Turn Time: 5-10 Days 
Layers: 2
Layer Orientation:
1.	10020690RA_SSTOP
2.	10020690RA_SMTOP
3.	10020690RA_CUTOP
4.	10020690RA_CUBOT
5.	10020690RA_SMBOT

Thickness:  0.062 "" FR4 
Dimensions: 2.165" X 1.831”
Plating: SMOBC 
Cu Weight: 
1.	Signal: 2oz
Trace width/space: 0.007”/0.007”
Smallest hole size: 0.010" 
Sides to solder mask: Both Sides (GREEN)
Sides to silk screen:  Top Side only (WHITE)
