Maximum Voltage 425 VDC

Maximum voltage drop over cable 125 VDC
Max current 12 A

Min 2 power conductors

Small gauge wire for frame ground/continuity circuit

Working load min 1500 lbs

4 single mode fibers

Weight in water min -10 lbs/1000ft

Length 1700 m + 5% -0%

Operation depth 1500 m 

Terminated into oil-filled j-box (currently oil Shell Tellus 15, we are open to changing oil type)

