I2MAP Camera Upgrades and supplies

1. Re-spin PCB to separate camera and recorder power (lower heat load for long download times).
2. Route over-temp flag to digital input!
3. Change port pin mapping.
4. Add voltage and current sensing.
5. Waterproof and spare test cable. MINL.
6. Upgrade connector that was wrong bulkhead configuration.
7. [bookmark: _GoBack]Remote power and coms test cable (replacement for AUV connection).
