For CAN-1 Operation:
CCA cable must connect from BPU-4000 to CNA-1 (mostly for power but it is rumored the Ethernet cable with POE can be used also), then a Ethernet cable connects from CNA-1 to BPU-4000. A USB mouse connects from the CNA-1. To change IP Address you must log on and as I found out the hard way please use Chrome, IE just does not work. Then log on to the browser enter the IP address of the CNA-1 and you can change the address of the BPU or mouse. There are a few other items I still need to investigate, but here is some information:

User and Password for CAN-1
User: admin
Password: password
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