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[bookmark: _GoBack]The modified camera port and modified titanium ring were assembled for pressure testing. A LVTD was placed inside the assembly. The purpose of the LVDT is to measure the displacement of the glass port during pressure testing. The range of the LVDT is -0.100” to +0.100”.  The LVDT was calibrated today in the cold room at 4oC.  0V output is -0.100” and 10V output is +0.100”.
An 8-pin, right angle, bulkhead connector is used to connect the LVDT. The pin out is as follows:
· Pin 1, black, Primary coil 1
· Pin 2, white, primary coil 2
· Pin 3, red, secondary coil 1
· Pin 4, green, secondary coil 2
The output of the signal conditioner is a 0 to 10VDC. (1/1000” = 0.05VDC) 

