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Communications
Verify Ethernet comms to Matchport
Verify both serial outputs of Matchport
Verify serial debug port


Power
Verify 24V Vicor
Verify 12V Vicor
Turn on Vicors
Read back Vicor states
Measure DC output of each
Turn on each Node
Read back Node states
Turn on fans
Read back fan states

** attach a load to each node output and check volt/curr calibration **


ADCs
Read back Node 1 volt/curr
Read back Node 2 volt/curr
Read back the 4 Vicor temperature sensors
Read back 24V volt/curr
Measure DC output
Read back 3.3V volt/curr
Measure DC output
Read back ambient temp/hum


Ground Fault Circuit
Verify correct voltage levels
Read back gf_curr measurement (ADC)
Verify H2O sensors

[bookmark: _GoBack]
