[bookmark: _GoBack]xinit - chip 2 pin 07 [addr:71]
init_pin - c:2 p:07 setting dir OUTPUT
init_pin - c:2 p:07 setting act ACTIVE_LOW
init_pin - c:2 p:07 setting val HIGH
xinit - chip 2 pin 06 [addr:70]
init_pin - c:2 p:06 setting dir OUTPUT
init_pin - c:2 p:06 setting act ACTIVE_LOW
init_pin - c:2 p:06 setting val HIGH
xinit - chip 2 pin 09 [addr:73]
init_pin - c:2 p:09 setting dir OUTPUT
init_pin - c:2 p:09 setting act ACTIVE_LOW
init_pin - c:2 p:09 setting val HIGH
xinit - chip 2 pin 08 [addr:72]
init_pin - c:2 p:08 setting dir OUTPUT
init_pin - c:2 p:08 setting act ACTIVE_LOW
init_pin - c:2 p:08 setting val HIGH
xinit - chip 2 pin 11 [addr:75]
init_pin - c:2 p:11 setting dir OUTPUT
init_pin - c:2 p:11 setting act ACTIVE_LOW
init_pin - c:2 p:11 setting val HIGH
xinit - chip 2 pin 10 [addr:74]
init_pin - c:2 p:10 setting dir OUTPUT
init_pin - c:2 p:10 setting act ACTIVE_LOW
init_pin - c:2 p:10 setting val HIGH
xinit - chip 2 pin 13 [addr:77]
init_pin - c:2 p:13 setting dir OUTPUT
init_pin - c:2 p:13 setting act ACTIVE_LOW
init_pin - c:2 p:13 setting val HIGH
xinit - chip 2 pin 12 [addr:76]
init_pin - c:2 p:12 setting dir OUTPUT
init_pin - c:2 p:12 setting act ACTIVE_LOW
init_pin - c:2 p:12 setting val HIGH
xinit - chip 1 pin 14 [addr:46]
init_pin - c:1 p:14 setting dir OUTPUT
init_pin - c:1 p:14 setting act ACTIVE_LOW
init_pin - c:1 p:14 setting val HIGH
xinit - chip 1 pin 15 [addr:47]
init_pin - c:1 p:15 setting dir OUTPUT
init_pin - c:1 p:15 setting act ACTIVE_LOW
init_pin - c:1 p:15 setting val HIGH
xinit - chip 2 pin 22 [addr:86]
*** NODE_1_STATE ***
init_pin - c:2 p:22 setting dir INPUT
init_pin - c:2 p:22 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:2 p:22 not setting val
*** NODE_2_OFF ***
xinit - chip 1 pin 12 [addr:44]
init_pin - c:1 p:12 setting dir OUTPUT
init_pin - c:1 p:12 setting act ACTIVE_LOW
init_pin - c:1 p:12 setting val HIGH
*** NODE_2_ON***
xinit - chip 1 pin 13 [addr:45]
init_pin - c:1 p:13 setting dir OUTPUT
init_pin - c:1 p:13 setting act ACTIVE_LOW
init_pin - c:1 p:13 setting val HIGH
***NODE_2_STATE***
xinit - chip 2 pin 23 [addr:87]
init_pin - c:2 p:23 setting dir INPUT
init_pin - c:2 p:23 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:2 p:23 not setting val
***NODE_3_OFF***
xinit - chip 1 pin 03 [addr:35]
init_pin - c:1 p:03 setting dir OUTPUT
gpio_set_dir: could not open dir path [/sys/class/gpio/gpio35/direction]
init_pin - c:1 p:03 setting act ACTIVE_HIGH <- Should be ACTIVE_LOW
gpio_set_act: could not open act path [/sys/class/gpio/gpio35/active_low]
init_pin - c:1 p:03 setting val LOW <- Should be HIGH
gpio_get_dir: error reading GPIO dir [/sys/class/gpio/gpio35/direction]
gpio_set_val: GPIO is not an output [/sys/class/gpio/gpio35]
***NODE_3_ON***
xinit - chip 1 pin 02 [addr:34]
init_pin - c:1 p:02 setting dir OUTPUT
init_pin - c:1 p:02 setting act ACTIVE_HIGH  <- Should be ACTIVE_LOW
init_pin - c:1 p:02 setting val LOW  <- Should be HIGH
***NODE_3_STATE***
xinit - chip 2 pin 24 [addr:88]
init_pin - c:2 p:24 setting dir INPUT
init_pin - c:2 p:24 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:2 p:24 not setting val
***NODE_4_OFF***
xinit - chip 1 pin 07 [addr:39]
init_pin - c:1 p:07 setting dir OUTPUT
init_pin - c:1 p:07 setting act ACTIVE_HIGH   <- Should be ACTIVE_LOW
init_pin - c:1 p:07 setting val LOW   <- Should be HIGH

***NODE_4_ON***
xinit - chip 1 pin 06 [addr:38]
init_pin - c:1 p:06 setting dir OUTPUT
init_pin - c:1 p:06 setting act ACTIVE_HIGH <- Should be ACTIVE_LOW
init_pin - c:1 p:06 setting val LOW  <- Should be HIGH
***NODE_4_STATE***
xinit - chip 2 pin 25 [addr:89]
init_pin - c:2 p:25 setting dir INPUT
init_pin - c:2 p:25 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:2 p:25 not setting val
***48V_RET_GF***
xinit - chip 1 pin 04 [addr:36]
init_pin - c:1 p:04 setting dir OUTPUT
init_pin - c:1 p:04 setting act ACTIVE_HIGH
init_pin - c:1 p:04 setting val LOW
***48V_GF***
xinit - chip 1 pin 00 [addr:32]
init_pin - c:1 p:00 setting dir OUTPUT
init_pin - c:1 p:00 setting act ACTIVE_HIGH
init_pin - c:1 p:00 setting val LOW
***TEST_RET_GF***
xinit - chip 1 pin 01 [addr:33]
init_pin - c:1 p:01 setting dir OUTPUT
init_pin - c:1 p:01 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:1 p:01 setting val LOW
***SPARE***
xinit - chip 1 pin 28 [addr:60]
init_pin - c:1 p:28 setting dir OUTPUT
init_pin - c:1 p:28 setting act ACTIVE_LOW
init_pin - c:1 p:28 setting val LOW
***TEST_GF***
xinit - chip 1 pin 29 [addr:61]
init_pin - c:1 p:29 setting dir OUTPUT
init_pin - c:1 p:29 setting act ACTIVE_LOW  <- Should be ACTIVE_HIGH
init_pin - c:1 p:29 setting val LOW
***H2O_ALARM***
xinit - chip 1 pin 05 [addr:37]
init_pin - c:1 p:05 setting dir INPUT
init_pin - c:1 p:05 setting act ACTIVE_LOW   <- Should be ACTIVE_HIGH
init_pin - c:1 p:05 not setting val
***ENVR_ALARM***
xinit - chip 1 pin 31 [addr:63]
init_pin - c:1 p:31 setting dir INPUT
init_pin - c:1 p:31 setting act ACTIVE_LOW
init_pin - c:1 p:31 not setting val
***EEPROM_WP***
xinit - chip 1 pin 30 [addr:62]
init_pin - c:1 p:30 setting dir OUTPUT
init_pin - c:1 p:30 setting act ACTIVE_HIGH   <- Should be ACTIVE_LOW
init_pin - c:1 p:30 setting val LOW <- Should be HIGH
