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Network Ports
· 5 auto-sensing UTP ports
Forwarding Mode
· Store-and-forward
· 128 KB on-chip packet buffering
Performance
· Bandwidth: 10 Gbps (non-blocking)
· Forwarding rate: 
- 10 Mbps port: 14,800 packets/sec 
- 100 Mbps port: 148,000 packets/sec 
- 1000 Mbps port: 1,480,000 packets/sec
· Latency (using 1500-byte packets): 
- 10 Mbps: 30μs (max) 
- 100 Mbps: 6μs (max) 
- 1000 Mbps: 4μs (max)
· MAC address database: 4,000
· Mean time between failures (MTBF): 
>1 million hours (~114 years)
Status LEDs
· System power
· Link, speed, and activity indicators per port built into each RJ-45 port
AC Power
· Power adapter: 12W, 12V DC, 1A
· Maximum power consumption: 3.5W
Physical Specifications
· Dimensions (w x d x h): 94 x 104 x 28 mm (3.7 x 4.1 x 1.1 in)
· Weight: 0.30 kg (0.66 lb)
Environmental Specifications
· Operating temperature: 0º to 50º C (32º to 122º F)
· Operating humidity: 10% to 90% non-condensing
· Storage temperature: -20º to 70° C (-4º to 158º F)
· Storage humidity: 10% to 95% relative humidity
p>Standards Compliance
· IEEE 802.3i 10BASE-T Ethernet
· IEEE 802.3u 100BASE-TX Fast Ethernet
· IEEE 802.3ab 1000BASE-T Gigabit Ethernet
· Honors IEEE 802.1p and DSCP priority tags
· Jumbo frame: up to 9,720 bytes
Safety Agency Approvals
· C-Tick, CE Mark
Electromagnetic Compliance
· FCC Class B, VCCI Class B
System Requirements
· Windows®, Linux®, Mac OS®
· 10 Mbps: UTP Cat 3 (or better)
· 100 Mbps: UTP Cat 5 (or better)
· 1000 Mbps: UTP Cat 5e (or better)
· Network card for each PC or server
Warranty
· Switch: NETGEAR Lifetime Warranty††
· Power adapter: NETGEAR 2-year warranty
ProSupport Service Packs Available
OnCall 24x7, Category 1
· PMB0331-100 (US)
· PMB0331 (non-US)
XPressHW, Category 1
· PRR0331
Package Contents
· ProSafe 5-port or 8-port Gigabit Desktop Switch 10/100/1000 Mbps (GS105v3 or GS108v3)
· Wall-mount kit
· AC adapter
· Installation guide
· Warranty/support information card
NETGEAR Related Products
· Gigabit Ethernet PCI Adapter (GA311)
· Gigabit Ethernet PC Card (GA511)
· ProSafe® 16-port Gigabit Desktop Switch (GS116)
Ordering Information
· North America: GS105NA
· Europe - General: GS105GE
· UK: GS105UK
· Asia: GS105AU
· Japan: GS105A-300JPS

