	PST-INV2424
	Function: DC/AC Inverter with 24VAC output

	Country of Origin
	USA, NAFTA qualified

	Output power
	40VA continuous (40 Watts) (24VAC 1.6Amps nominal)
50VA for 1 minute at 50% duty factor( 1 minute above 40VAC, one minute below 40VA

	Output Current
	1.6 Amps continuous, 2 amps peak

	Input voltage
	DC 22VDC to 29VDC start-up, 
20VDC to 30VDC operating.

	Output voltage
	AC 24VAC

	Output voltage regulation
	± 10%

	Output wave form
	Pure sine wave

	Output frequency
	60Hz ± 1% (50Hz available, ask)

	Standby current
	0.2A, 200 mA typical

	Efficiency
	90% max.

	Operating Temperature
	-10°C to +45°C

	Cooling
	Convection cooling, no fan

	Protections
	Output short 
Polarity reverse
Under voltage input

	Under voltage protection
	Unit will shut itself down when the input voltage is less than 20VDC ±5%. It will restart when the voltage is above 22VDC

	DC Input
	Screw terminals

	AC output
	Screw Terminals

	Isolation
	DC input is galvanically isolated from the AC output, greater than 100V hipot

	Dimensions
	132 X 75 X 38 mm , 5.2 x 3 x 1.5 inches

	Weight
	277 gms., 10oz, 0.6 lbs

	Drawing
	Drawing and Mounting dimensions click here

	More options
	Please ask if you need different input voltages, output voltage, output power, surge protection, connectorization, or form factor.
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