Possible test plan for determining the source of the MVC rebooting issue. 

[bookmark: _GoBack]I propose we turn on one chamber at a time in an effort to isolate the source of the problem. It may take less time if we begin by having all of the instruments powered up on the chamber under observation (problem may occur quicker). Once the problem arises, re-initialize the chamber with one less Sensor Node. If the problem is narrowed down to a particular Sensor Node, then we can begin turning off the actual instruments on the Sensor Node one at a time. 

One question is how long do we wait before determining that the rebooting problem will not happen? We have seen instances of it happening within 5 days or up to 3 weeks. 

I propose the following order. Begin with chamber #1, everything on. If the problem does not surface, move onto chamber #2.

Chamber 1 (Camera, no thruster)
All Sensor Nodes and Instruments on
	Turn off Sensor Node SN# 9
	Turn off Sensor Node SN# 8
	Turn off Sensor Node SN# 7
	Turn off Sensor Node SN# 6

Chamber 2 (No camera, thruster)
	All Sensor Nodes and Instruments on
	Turn off Sensor Node SN# 11
	Turn off Sensor Node SN# 18
	Turn off Sensor Node SN# 17
	Turn off Sensor Node SN# 16














	GN SN#/Port
	SN SN#
	Port
	Instrument
	Instr Manuf
	Model #
	Serial #
	SSDS ID#
	Sensor Unit

	#1 / 1
	6
	1
	pH Probe
	SeaBird
	SBE18S
	181067
	1813
	2

	#1 / 1
	6
	2
	pH Probe
	SeaBird
	SBE18S
	181069
	1812
	2

	#1 / 1
	6
	3
	CTD-O2
	SeaBird
	SBE52-43
	624878-0047
	1642
	2

	#1 / 1
	6
	4
	Pump
	Seabird
	SBE5T
	057936
	1850
	2

	#1 / 2
	7
	1
	pH Probe
	SeaBird
	SBE18S
	181066
	1818
	1

	#1 / 2
	7
	2
	pH Probe
	SeaBird
	SBE18S
	181065
	1817
	1

	#1 / 2
	7
	3
	CTD-O2
	SeaBird
	SBE52-43
	5248473-0044
	1733
	1

	#1 / 2
	7
	4
	Pump
	SeaBird
	SBE5T
	054258
	1837
	1

	#1 / 3
	8
	1
	PAR Sensor
	Satlantic
	 
	401
	1824
	 

	#1 / 3
	8
	2
	PAR Sensor
	Satlantic
	 
	400
	1851
	 

	#1 / 3
	8
	3
	[open]
	 
	 
	 
	 
	 

	#1 / 3
	8
	4
	[open]
	 
	 
	 
	 
	 

	#1 / 4
	9
	1
	Valve Box
	MBARI
	N/A
	1
	1846
	 

	#1 / 4
	9
	2
	Motor
	 
	 
	 
	 
	 

	#1 / 4
	9
	3
	Flowmeter
	Omega
	FMG-554
	 
	 
	 

	#1 / 4
	9
	4
	Motor
	 
	 
	 
	 
	 



	#2 / 1
	16
	1
	pH Probe
	SeaBird
	SBE18S
	180943
	1848
	3

	#2 / 1
	16
	2
	pH Probe
	SeaBird
	SBE18S
	181070
	1833
	3

	#2 / 1
	16
	3
	CTD-O2
	SeaBird
	SBE52-43
	5248473-0046
	1752
	3

	#2 / 1
	16
	4
	Pump
	Seabird
	SBE5T
	054310
	1836
	3

	#2 / 2
	17
	1
	[open]
	 
	 
	 
	 
	 

	#2 / 2
	17
	2
	[open]
	 
	 
	 
	 
	 

	#2 / 2
	17
	3
	[open]
	 
	 
	 
	 
	 

	#2 / 2
	17
	4
	[open]
	 
	 
	 
	 
	 

	#2 / 3
	18
	1
	PAR Sensor
	Satlantic
	 
	402
	1820
	 

	#2 / 3
	18
	2
	[open]
	 
	 
	 
	 
	 

	#2 / 3
	18
	3
	[open]
	 
	 
	 
	 
	 

	#2 / 3
	18
	4
	[open]
	 
	 
	 
	 
	 

	#2 / 4
	11
	1
	Valve Box
	MBARI
	N/A
	3
	1847
	 

	#2 / 4
	11
	2
	Motor
	 
	 
	 
	 
	 

	#2 / 4
	11
	3
	Flowmeter
	Omega
	FMG-554
	2
	 
	 

	#2 / 4
	11
	4
	Motor
	 
	 
	 
	 
	 




