FOCE Load Switcher

Functionality:
Individual instrument load switching
	Upto 30V available to each instrument
	Upto 2A available to each instrument
Individual instrument voltage and current monitoring
Undervoltage protection / Overcurrent protection [circuit breaker]

Additional Features:
Direct interface to new ground faulting board
Simplifies power distribution within FOCE
Individual addressable boards in stack (up to xx boards)
Low power consumption
	Latching relays used
Circuit breaker at input allows for rapid power removal
Common bus allows for future board development on same stack
Simple SPI interface to main CPU

Replaces:
RTD Relay Control Boards (x2)
FOCE Distribution Boards (x4)
Power Distribution Cables (x4)

Notes:
Different sized connectors for each input voltage
Digital Potentiometer to set current/voltage levels

