FOCE Chassis Ground Fault Detector Board 

Ground Fault Detectors:
High Voltage Ground Fault Circuits x4 (50V to 400V)
Low-Medium Ground Fault Circutis x12 (0 to 50V)
Need to determine min/max (acceptable?) seawater currents.
Have one test channel (an isolated voltage source?)

Use an SPI based ADC (14+ bit) (PIC only has 10 bits)
	Bidirectional currents possible (offset or pos/neg)
	ADS8341 has differential inputs
Do I need to read channel voltages?
	I can ask Power Board or Load Switcher board instead.


