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[CTD pumping diagnostic - checking CTD status]

& et rom
Target Waypoint

[ L
e e

L [

O —
\Unspecficd [~ operation Type
VirtualRelayCell Commurication Chamnel =] yioad rie

[write Console seript [<]

|
|
[ —
|

(2049

e
N | - |
N | - |
N | - |
[

2t (deg) Lon (deg) I
81730 12181836
oo ooooo
81770 -121.81926

s1e11 -121.62005

s1849 -121.82090

s1882 2182172

vv v

e Ve e

ln

~ TimeStamp Comma...| Combined Acks | Created By

04/27/2015 1

Command Reason

Command

04/27/2015 10:21 powering up GPCTD+DO to debug pum...  Set Parameters: Payload 2 Power=1 on vehicl..  Acked
0 telem06 reportRate=2m System Info Field Event Created

04/27/2015 10:17 “telem0s.updateReportRate(2) Write Console Seript Acked ox.
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