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	[bookmark: _GoBack]SV2 Wave Glider Pre-Launch Checklist

	Date: 
	Glider Name: 

	Operator: 
	Payload:

	Ship/Op Area: 
	Project: 

	Communication

	Item/Procedure
	Readings
	Specifications
	Initials

	Xbee Connection
	
	Coms Established
	

	WGMS Updating
	
	Coms Established
	

	Configuration 

	Print xbee commands 
	
	<CR>,26,27,97 (attach to this doc)
	

	RDF Frequency
	Top:
Bottom:
	
	

	Tracker name/#
	
	
	

	Float name
	
	
	

	Glider name
	
	
	

	Drybox name
	
	
	

	Vehicle Status

	Battery Wh
	
	>  550 Watt-hours
	

	Solar Power Indicators:
	Panel 1
	Panel 2
	
	

	
	
	
	> 1000 mW
	

	Environmental:
	Pressure
	Temp
	> 135 kpa, < 35 C
<50%
< 105 kpa, < 35 C 
> 135 kpa, < 35 C (Plastic PL ~100 kpa)          
<  50%                                  
> 135 kpa, < 35 C
<  50%
	

	C&C Drybox (Float)
	
	
	
	

	C&C humidity
	
	
	

	Rudder Module (Sub)
	
	
	
	

	Payload 1
	
	
	
	

	Payload humidity
	
	
	

	Payload 2
	
	
	
	

	Payload humidity
	
	
	

	Mechanical Checks

	Float
	
	
	

	Wet-mates connected/lubed
	
	
	

	Connector covers secure
	
	30 in/lbs
	

	Drybox secure
	
	30 in/lbs
	

	Turtledeck secure
	
	30 in/lbs
	

	Contact info secure
	
	
	

	Remove RDF magnet
	
	Top & Bottom RDF
	

	Orange flag attached to mast
	
	
	

	Glider
	
	
	

	Line Terminator secure  
	
	Rubber mallet treatment
	

	Umbilical visual inspection  
	
	Free of voids/defects
	

	Roll pin inserted
	
	
	

	Vehicle Functionality – WGMS

	Tracker report rate/reporting
	Time
	Yes/No
	
	

	
	
	
	
	

	Light on/off
	
	
	

	IPIB sensors powered on
	
	Check all IPIB sensors; Current Draw ~350mA
	

	Rudder moves 360
	
	
	

	Rudder center
	
	
	

	Rudder left
	
	
	

	Rudder right
	
	
	

	Fixed heading test (spin)
	
	Heading used
	

	Vehicle Functionality – WGMS Cont.

	Item/Procedure
	Readings
	Specifications
	Initials

	Waypoint course test (spin)
	
	Waypoint number used
	

	Op area defined
	
	full vehicle
	

	Photo document 
	
	Turtledeck, umbilical, rudder, spring bar, wing spring hardware, etc.
	

	Event definitions 
	
	Compare against standard list
	

	Set default comms
	
	Change to iridium or alt-iridium
	

	Check alarms
	
	
	

	Payload Checks

	Sensor
	Power On/Off
	Current Time
	Last Packet

	AIS
	
	
	

	Weather Station
	
	
	

	Water Speed
	
	
	

	C3 
	
	
	

	Camera
	
	
	

	Wave Sensor
	
	
	

	CTD
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	
	
	
	

	
	
	
	

	
	
	
	

	
	
	
	

	Comments

	

	

	

	

	

	

	

	

	

	

	



Technician Signature:							
Note:  Once vehicle is launched the following tasks must be completed
1. Clear alarms
2. Vehicle on mission
3. Create LAUNCHED comment into Hyperion (WGMS). 
4. Upload photos to box.com with album name: YYYY-MM-DD VehicleName
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