The Benthic Rover is deployed in 870 meters of water near Smooth Ridge (19.8 nm from Moss Landing). Users would like to have the ability to query the Rover for basic health and status information. In the event that an anomaly was reported, the team might be able to deal with the issue sooner than the scheduled bi-annual cruise would allow. The Wave Glider SV3 “Tiny” will be used to communicate acoustically with the Rover with a human in the loop managing specific commands to the Rover. 

Dates:
Tentatively June 25-July 10

Location and Waypoints:
1.) L&R 3nm from MBARI
2.) [bookmark: _GoBack]36.711367,-122.186817 (N 36 42.682, W 122 11.209) 


Configuration:
Configured with skeg mounted Benthos Low  Frequency (LF) modem and 3G modem for user interaction. Tests will be performed using the Iridium link as well since this deployment is a test for the “real thing” at Station M. 

Mission:
Transit direct from L&R, to waypoint and loiter in place in 100 m circle. 
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