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ELECTRICAL CONTACT SIZES
	CONTACT AWG
	DIAMETER (INCHES)
	AMPACITY (AMPS)

	#28 AWG
	0.015
	0.5

	#22 AWG
	0.031
	2.5

	#20 AWG
	0.040
	4

	#16 AWG
	0.062
	13

	#14 AWG
	0.093
	16

	#10 AWG
	0.125
	23

	#8 AWG
	0.156
	50

	#6 AWG
	0.218
	65

	#4 AWG
	0.255
	90

	#1/0 AWG
	0.355
	200


NOTES:
The ampacity is computed at temperature range of +30°F +68°F.
Above 70°F the ampacity drops.
Pins and sockets are brass alloy. Pins are gold plated per MIL-G-45204.
Most contacts conform to MIL-C-24217.

