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1. System components:
a. Laser and laser controller housing:
i. Physical dimensions: O.D. =  8.38”, length = 29.38”
ii. In water weight: 24.9 lbs
iii. In air weight: 84.3 lbs
iv. Electrical Interfaces:
1. Power: 110 VAC, <2A (Needs to be confirmed) (Version 4 would need 6A circuit)
2. Communications: Ethernet (GigE not required)
3. Analog Inputs: 0-5V, 2 Channels, temp and humidity from camera housing
b. Camera Housing:
i. Physical dimensions: : O.D. = 5.875, length = 13.56”
ii. In water weight: 15.5 lbs
iii. In air weight: 22.3 lbs
iv. Electrical Interfaces:
1. Power: 24V, <1A
2. Communications : serial, RS232
3. Video: 3G-SDI, 1080 60p
4. Analog output: 2 channels, 0-5V (temp/humidity)
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